{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Home","Price list","Discount groups","Order","Offer","Terms and Conditions","Claims Handling Rules","Manual"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":63,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Home","index":0,"n_rows":8,"n_cols":4,"rows_kept":8,"cut":false,"hidden":false,"merged":[[3,1,3,6],[5,1,5,2]]}
[]
[]
[]
[null,"Price list NOARK Electric Europe s.r.o."]
[]
[null,"Ukraine"]
[]
[null,"Valid from ",null,"2020-09-14"]

{"sheet":"Price list","index":1,"n_rows":5527,"n_cols":14,"rows_kept":5527,"cut":false,"hidden":false,"merged":[]}
[]
["Price list NOARK Electric Europe s.r.o.",null,null,"Valid from:",{"$f":"Valid","v":"2020-09-14"}]
["Ukraine"]
["Article No.","Type","Description","Discount group","Gross price (EUR)","Discount","Price with discount (EUR)","Product EAN code","Basic package (pc)","EAN/GTIN code of basic package","Carton package (pc)","EAN/GTIN code of carton package","Customs tariff","Unit Weight (kg)"]
[]
["Miniature Circuit  Breakers Ex9BH, 10 kA"]
[100270,"Ex9BH 1P B1 ","Miniature Circuit  Breaker 10 kA, characteristic B, 1 A, 1-pole","NAA",7.08,{"$f":"NAA","v":0},{"$f":"E7*(1-F7)","v":7.08},8592765002716,12,18592765002713,144,28592765002710,"8536201090",0.12]
[100271,"Ex9BH 1P B2 ","Miniature Circuit  Breaker 10 kA, characteristic B, 2 A, 1-pole","NAA",7.08,0,7.08,8592765002723,12,18592765002720,144,28592765002727,"8536201090",0.12]
[100272,"Ex9BH 1P B3 ","Miniature Circuit  Breaker 10 kA, characteristic B, 3 A, 1-pole","NAA",7.08,0,7.08,8592765002730,12,18592765002737,144,28592765002734,"8536201090",0.12]
[100273,"Ex9BH 1P B4 ","Miniature Circuit  Breaker 10 kA, characteristic B, 4 A, 1-pole","NAA",7.08,0,7.08,8592765002747,12,18592765002744,144,28592765002741,"8536201090",0.12]
[100274,"Ex9BH 1P B6 ","Miniature Circuit  Breaker 10 kA, characteristic B, 6 A, 1-pole","NAA",6.86,0,6.86,8592765002754,12,18592765002751,144,28592765002758,"8536201090",0.12]
[100275,"Ex9BH 1P B8 ","Miniature Circuit  Breaker 10 kA, characteristic B, 8 A, 1-pole","NAA",6.86,0,6.86,8592765002761,12,18592765002768,144,28592765002765,"8536201090",0.12]
[100276,"Ex9BH 1P B10 ","Miniature Circuit  Breaker 10 kA, characteristic B, 10 A, 1-pole","NAA",4.84,0,4.84,8592765002778,12,18592765002775,144,28592765002772,"8536201090",0.12]
[100277,"Ex9BH 1P B13 ","Miniature Circuit  Breaker 10 kA, characteristic B, 13 A, 1-pole","NAA",4.84,0,4.84,8592765002785,12,18592765002782,144,28592765002789,"8536201090",0.12]
[100278,"Ex9BH 1P B16 ","Miniature Circuit  Breaker 10 kA, characteristic B, 16 A, 1-pole","NAA",4.84,0,4.84,8592765002792,12,18592765002799,144,28592765002796,"8536201090",0.12]
[100279,"Ex9BH 1P B20 ","Miniature Circuit  Breaker 10 kA, characteristic B, 20 A, 1-pole","NAA",4.84,0,4.84,8592765002808,12,18592765002805,144,28592765002802,"8536201090",0.12]
[100280,"Ex9BH 1P B25 ","Miniature Circuit  Breaker 10 kA, characteristic B, 25 A, 1-pole","NAA",4.84,0,4.84,8592765002815,12,18592765002812,144,28592765002819,"8536201090",0.12]
[100281,"Ex9BH 1P B32 ","Miniature Circuit  Breaker 10 kA, characteristic B, 32 A, 1-pole","NAA",7.64,0,7.64,8592765002822,12,18592765002829,144,28592765002826,"8536201090",0.12]
[100282,"Ex9BH 1P B40 ","Miniature Circuit  Breaker 10 kA, characteristic B, 40 A, 1-pole","NAA",7.64,0,7.64,8592765002839,12,18592765002836,144,28592765002833,"8536201090",0.12]
[100283,"Ex9BH 1P B50 ","Miniature Circuit  Breaker 10 kA, characteristic B, 50 A, 1-pole","NAA",17.52,0,17.52,8592765002846,12,18592765002843,144,28592765002840,"8536201090",0.12]
[100284,"Ex9BH 1P B63 ","Miniature Circuit  Breaker 10 kA, characteristic B, 63 A, 1-pole","NAA",19.350000000000001,0,19.350000000000001,8592765002853,12,18592765002850,144,28592765002857,"8536201090",0.12]
[100285,"Ex9BH 1PN B1 ","Miniature Circuit  Breaker 10 kA, characteristic B, 1 A, 1+Npole","NAA",11.64,0,11.64,8592765002860,6,18592765002867,72,28592765002864,"8536201090",0.24]
[100286,"Ex9BH 1PN B2 ","Miniature Circuit  Breaker 10 kA, characteristic B, 2 A, 1+Npole","NAA",11.64,0,11.64,8592765002877,6,18592765002874,72,28592765002871,"8536201090",0.24]
[100287,"Ex9BH 1PN B3 ","Miniature Circuit  Breaker 10 kA, characteristic B, 3 A, 1+Npole","NAA",11.64,0,11.64,8592765002884,6,18592765002881,72,28592765002888,"8536201090",0.24]
[100288,"Ex9BH 1PN B4 ","Miniature Circuit  Breaker 10 kA, characteristic B, 4 A, 1+Npole","NAA",11.64,0,11.64,8592765002891,6,18592765002898,72,28592765002895,"8536201090",0.24]
[100289,"Ex9BH 1PN B6 ","Miniature Circuit  Breaker 10 kA, characteristic B, 6 A, 1+Npole","NAA",11.64,0,11.64,8592765002907,6,18592765002904,72,28592765002901,"8536201090",0.24]
[100290,"Ex9BH 1PN B8 ","Miniature Circuit  Breaker 10 kA, characteristic B, 8 A, 1+Npole","NAA",11.64,0,11.64,8592765002914,6,18592765002911,72,28592765002918,"8536201090",0.24]
[100291,"Ex9BH 1PN B10 ","Miniature Circuit  Breaker 10 kA, characteristic B, 10 A, 1+Npole","NAA",11.19,0,11.19,8592765002921,6,18592765002928,72,28592765002925,"8536201090",0.24]
[100292,"Ex9BH 1PN B13 ","Miniature Circuit  Breaker 10 kA, characteristic B, 13 A, 1+Npole","NAA",11.19,0,11.19,8592765002938,6,18592765002935,72,28592765002932,"8536201090",0.24]
[100293,"Ex9BH 1PN B16 ","Miniature Circuit  Breaker 10 kA, characteristic B, 16 A, 1+Npole","NAA",11.19,0,11.19,8592765002945,6,18592765002942,72,28592765002949,"8536201090",0.24]
[100294,"Ex9BH 1PN B20 ","Miniature Circuit  Breaker 10 kA, characteristic B, 20 A, 1+Npole","NAA",11.19,0,11.19,8592765002952,6,18592765002959,72,28592765002956,"8536201090",0.24]
[100295,"Ex9BH 1PN B25 ","Miniature Circuit  Breaker 10 kA, characteristic B, 25 A, 1+Npole","NAA",11.19,0,11.19,8592765002969,6,18592765002966,72,28592765002963,"8536201090",0.24]
[100296,"Ex9BH 1PN B32 ","Miniature Circuit  Breaker 10 kA, characteristic B, 32 A, 1+Npole","NAA",13.59,0,13.59,8592765002976,6,18592765002973,72,28592765002970,"8536201090",0.24]
[100297,"Ex9BH 1PN B40 ","Miniature Circuit  Breaker 10 kA, characteristic B, 40 A, 1+Npole","NAA",13.59,0,13.59,8592765002983,6,18592765002980,72,28592765002987,"8536201090",0.24]
[100298,"Ex9BH 1PN B50 ","Miniature Circuit  Breaker 10 kA, characteristic B, 50 A, 1+Npole","NAA",44.41,0,44.41,8592765002990,6,18592765002997,72,28592765002994,"8536201090",0.24]
[100299,"Ex9BH 1PN B63 ","Miniature Circuit  Breaker 10 kA, characteristic B, 63 A, 1+Npole","NAA",44.41,0,44.41,8592765003003,6,18592765003000,72,28592765003007,"8536201090",0.24]
[100300,"Ex9BH 2P B1 ","Miniature Circuit  Breaker 10 kA, characteristic B, 1 A, 2-pole","NAA",16.329999999999998,0,16.329999999999998,8592765003010,6,18592765003017,72,28592765003014,"8536201090",0.24]
[100301,"Ex9BH 2P B2 ","Miniature Circuit  Breaker 10 kA, characteristic B, 2 A, 2-pole","NAA",16.329999999999998,0,16.329999999999998,8592765003027,6,18592765003024,72,28592765003021,"8536201090",0.24]
[100302,"Ex9BH 2P B3 ","Miniature Circuit  Breaker 10 kA, characteristic B, 3 A, 2-pole","NAA",16.329999999999998,0,16.329999999999998,8592765003034,6,18592765003031,72,28592765003038,"8536201090",0.24]
[100303,"Ex9BH 2P B4 ","Miniature Circuit  Breaker 10 kA, characteristic B, 4 A, 2-pole","NAA",16.329999999999998,0,16.329999999999998,8592765003041,6,18592765003048,72,28592765003045,"8536201090",0.24]
[100304,"Ex9BH 2P B6 ","Miniature Circuit  Breaker 10 kA, characteristic B, 6 A, 2-pole","NAA",16.329999999999998,0,16.329999999999998,8592765003058,6,18592765003055,72,28592765003052,"8536201090",0.24]
[100305,"Ex9BH 2P B8 ","Miniature Circuit  Breaker 10 kA, characteristic B, 8 A, 2-pole","NAA",16.329999999999998,0,16.329999999999998,8592765003065,6,18592765003062,72,28592765003069,"8536201090",0.24]
[100306,"Ex9BH 2P B10 ","Miniature Circuit  Breaker 10 kA, characteristic B, 10 A, 2-pole","NAA",15.14,0,15.14,8592765003072,6,18592765003079,72,28592765003076,"8536201090",0.24]
[100307,"Ex9BH 2P B13 ","Miniature Circuit  Breaker 10 kA, characteristic B, 13 A, 2-pole","NAA",15.14,0,15.14,8592765003089,6,18592765003086,72,28592765003083,"8536201090",0.24]
[100308,"Ex9BH 2P B16 ","Miniature Circuit  Breaker 10 kA, characteristic B, 16 A, 2-pole","NAA",15.14,0,15.14,8592765003096,6,18592765003093,72,28592765003090,"8536201090",0.24]
[100309,"Ex9BH 2P B20 ","Miniature Circuit  Breaker 10 kA, characteristic B, 20 A, 2-pole","NAA",15.14,0,15.14,8592765003102,6,18592765003109,72,28592765003106,"8536201090",0.24]
[100310,"Ex9BH 2P B25 ","Miniature Circuit  Breaker 10 kA, characteristic B, 25 A, 2-pole","NAA",15.14,0,15.14,8592765003119,6,18592765003116,72,28592765003113,"8536201090",0.24]
[100311,"Ex9BH 2P B32 ","Miniature Circuit  Breaker 10 kA, characteristic B, 32 A, 2-pole","NAA",19.79,0,19.79,8592765003126,6,18592765003123,72,28592765003120,"8536201090",0.24]
[100312,"Ex9BH 2P B40 ","Miniature Circuit  Breaker 10 kA, characteristic B, 40 A, 2-pole","NAA",19.79,0,19.79,8592765003133,6,18592765003130,72,28592765003137,"8536201090",0.24]
[100313,"Ex9BH 2P B50 ","Miniature Circuit  Breaker 10 kA, characteristic B, 50 A, 2-pole","NAA",36.880000000000003,0,36.880000000000003,8592765003140,6,18592765003147,72,28592765003144,"8536201090",0.24]
[100314,"Ex9BH 2P B63 ","Miniature Circuit  Breaker 10 kA, characteristic B, 63 A, 2-pole","NAA",38.08,0,38.08,8592765003157,6,18592765003154,72,28592765003151,"8536201090",0.24]
[100315,"Ex9BH 3P B1 ","Miniature Circuit  Breaker 10 kA, characteristic B, 1 A, 3-pole","NAA",22.29,0,22.29,8592765003164,4,18592765003161,48,28592765003168,"8536201090",0.36]
[100316,"Ex9BH 3P B2 ","Miniature Circuit  Breaker 10 kA, characteristic B, 2 A, 3-pole","NAA",22.29,0,22.29,8592765003171,4,18592765003178,48,28592765003175,"8536201090",0.36]
[100317,"Ex9BH 3P B3 ","Miniature Circuit  Breaker 10 kA, characteristic B, 3 A, 3-pole","NAA",22.29,0,22.29,8592765003188,4,18592765003185,48,28592765003182,"8536201090",0.36]
[100318,"Ex9BH 3P B4 ","Miniature Circuit  Breaker 10 kA, characteristic B, 4 A, 3-pole","NAA",22.29,0,22.29,8592765003195,4,18592765003192,48,28592765003199,"8536201090",0.36]
[100319,"Ex9BH 3P B6 ","Miniature Circuit  Breaker 10 kA, characteristic B, 6 A, 3-pole","NAA",22.29,0,22.29,8592765003201,4,18592765003208,48,28592765003205,"8536201090",0.36]
[100320,"Ex9BH 3P B8 ","Miniature Circuit  Breaker 10 kA, characteristic B, 8 A, 3-pole","NAA",22.29,0,22.29,8592765003218,4,18592765003215,48,28592765003212,"8536201090",0.36]
[100321,"Ex9BH 3P B10 ","Miniature Circuit  Breaker 10 kA, characteristic B, 10 A, 3-pole","NAA",16.89,0,16.89,8592765003225,4,18592765003222,48,28592765003229,"8536201090",0.36]
[100322,"Ex9BH 3P B13 ","Miniature Circuit  Breaker 10 kA, characteristic B, 13 A, 3-pole","NAA",16.89,0,16.89,8592765003232,4,18592765003239,48,28592765003236,"8536201090",0.36]
[100323,"Ex9BH 3P B16 ","Miniature Circuit  Breaker 10 kA, characteristic B, 16 A, 3-pole","NAA",16.89,0,16.89,8592765003249,4,18592765003246,48,28592765003243,"8536201090",0.36]
[100324,"Ex9BH 3P B20 ","Miniature Circuit  Breaker 10 kA, characteristic B, 20 A, 3-pole","NAA",16.89,0,16.89,8592765003256,4,18592765003253,48,28592765003250,"8536201090",0.36]
[100325,"Ex9BH 3P B25 ","Miniature Circuit  Breaker 10 kA, characteristic B, 25 A, 3-pole","NAA",16.89,0,16.89,8592765003263,4,18592765003260,48,28592765003267,"8536201090",0.36]
[100326,"Ex9BH 3P B32 ","Miniature Circuit  Breaker 10 kA, characteristic B, 32 A, 3-pole","NAA",24.39,0,24.39,8592765003270,4,18592765003277,48,28592765003274,"8536201090",0.36]
[100327,"Ex9BH 3P B40 ","Miniature Circuit  Breaker 10 kA, characteristic B, 40 A, 3-pole","NAA",24.39,0,24.39,8592765003287,4,18592765003284,48,28592765003281,"8536201090",0.36]
[100328,"Ex9BH 3P B50 ","Miniature Circuit  Breaker 10 kA, characteristic B, 50 A, 3-pole","NAA",42.21,0,42.21,8592765003294,4,18592765003291,48,28592765003298,"8536201090",0.36]
[100329,"Ex9BH 3P B63 ","Miniature Circuit  Breaker 10 kA, characteristic B, 63 A, 3-pole","NAA",46.41,0,46.41,8592765003300,4,18592765003307,48,28592765003304,"8536201090",0.36]
[100330,"Ex9BH 3PN B1 ","Miniature Circuit  Breaker 10 kA, characteristic B, 1 A, 3+Npole","NAA",36.83,0,36.83,8592765003317,3,18592765003314,36,28592765003311,"8536201090",0.48]
[100331,"Ex9BH 3PN B2 ","Miniature Circuit  Breaker 10 kA, characteristic B, 2 A, 3+Npole","NAA",36.83,0,36.83,8592765003324,3,18592765003321,36,28592765003328,"8536201090",0.48]
[100332,"Ex9BH 3PN B3 ","Miniature Circuit  Breaker 10 kA, characteristic B, 3 A, 3+Npole","NAA",36.83,0,36.83,8592765003331,3,18592765003338,36,28592765003335,"8536201090",0.48]
[100333,"Ex9BH 3PN B4 ","Miniature Circuit  Breaker 10 kA, characteristic B, 4 A, 3+Npole","NAA",36.83,0,36.83,8592765003348,3,18592765003345,36,28592765003342,"8536201090",0.48]
[100334,"Ex9BH 3PN B6 ","Miniature Circuit  Breaker 10 kA, characteristic B, 6 A, 3+Npole","NAA",36.83,{"$f":"NAA","v":0},{"$f":"E71*(1-F71)","v":36.83},8592765003355,3,18592765003352,36,28592765003359,"8536201090",0.48]
[100335,"Ex9BH 3PN B8 ","Miniature Circuit  Breaker 10 kA, characteristic B, 8 A, 3+Npole","NAA",36.83,0,36.83,8592765003362,3,18592765003369,36,28592765003366,"8536201090",0.48]
[100336,"Ex9BH 3PN B10 ","Miniature Circuit  Breaker 10 kA, characteristic B, 10 A, 3+Npole","NAA",25.99,0,25.99,8592765003379,3,18592765003376,36,28592765003373,"8536201090",0.48]
[100337,"Ex9BH 3PN B13 ","Miniature Circuit  Breaker 10 kA, characteristic B, 13 A, 3+Npole","NAA",25.99,0,25.99,8592765003386,3,18592765003383,36,28592765003380,"8536201090",0.48]
[100338,"Ex9BH 3PN B16 ","Miniature Circuit  Breaker 10 kA, characteristic B, 16 A, 3+Npole","NAA",25.99,0,25.99,8592765003393,3,18592765003390,36,28592765003397,"8536201090",0.48]
[100339,"Ex9BH 3PN B20 ","Miniature Circuit  Breaker 10 kA, characteristic B, 20 A, 3+Npole","NAA",25.99,0,25.99,8592765003409,3,18592765003406,36,28592765003403,"8536201090",0.48]
[100340,"Ex9BH 3PN B25 ","Miniature Circuit  Breaker 10 kA, characteristic B, 25 A, 3+Npole","NAA",25.99,0,25.99,8592765003416,3,18592765003413,36,28592765003410,"8536201090",0.48]
[100341,"Ex9BH 3PN B32 ","Miniature Circuit  Breaker 10 kA, characteristic B, 32 A, 3+Npole","NAA",35.76,0,35.76,8592765003423,3,18592765003420,36,28592765003427,"8536201090",0.48]
[100342,"Ex9BH 3PN B40 ","Miniature Circuit  Breaker 10 kA, characteristic B, 40 A, 3+Npole","NAA",35.76,0,35.76,8592765003430,3,18592765003437,36,28592765003434,"8536201090",0.48]
[100343,"Ex9BH 3PN B50 ","Miniature Circuit  Breaker 10 kA, characteristic B, 50 A, 3+Npole","NAA",63.28,0,63.28,8592765003447,3,18592765003444,36,28592765003441,"8536201090",0.48]
[100344,"Ex9BH 3PN B63 ","Miniature Circuit  Breaker 10 kA, characteristic B, 63 A, 3+Npole","NAA",63.28,0,63.28,8592765003454,3,18592765003451,36,28592765003458,"8536201090",0.48]
[100345,"Ex9BH 4P B1 ","Miniature Circuit  Breaker 10 kA, characteristic B, 1 A, 4-pole","NAA",42.78,0,42.78,8592765003461,3,18592765003468,36,28592765003465,"8536201090",0.48]
[100346,"Ex9BH 4P B2 ","Miniature Circuit  Breaker 10 kA, characteristic B, 2 A, 4-pole","NAA",42.78,0,42.78,8592765003478,3,18592765003475,36,28592765003472,"8536201090",0.48]
[100347,"Ex9BH 4P B3 ","Miniature Circuit  Breaker 10 kA, characteristic B, 3 A, 4-pole","NAA",42.78,0,42.78,8592765003485,3,18592765003482,36,28592765003489,"8536201090",0.48]
[100348,"Ex9BH 4P B4 ","Miniature Circuit  Breaker 10 kA, characteristic B, 4 A, 4-pole","NAA",42.78,0,42.78,8592765003492,3,18592765003499,36,28592765003496,"8536201090",0.48]
[100349,"Ex9BH 4P B6 ","Miniature Circuit  Breaker 10 kA, characteristic B, 6 A, 4-pole","NAA",42.78,0,42.78,8592765003508,3,18592765003505,36,28592765003502,"8536201090",0.48]
[100350,"Ex9BH 4P B8 ","Miniature Circuit  Breaker 10 kA, characteristic B, 8 A, 4-pole","NAA",42.78,0,42.78,8592765003515,3,18592765003512,36,28592765003519,"8536201090",0.48]
[100351,"Ex9BH 4P B10 ","Miniature Circuit  Breaker 10 kA, characteristic B, 10 A, 4-pole","NAA",29.95,0,29.95,8592765003522,3,18592765003529,36,28592765003526,"8536201090",0.48]
[100352,"Ex9BH 4P B13 ","Miniature Circuit  Breaker 10 kA, characteristic B, 13 A, 4-pole","NAA",29.95,0,29.95,8592765003539,3,18592765003536,36,28592765003533,"8536201090",0.48]
[100353,"Ex9BH 4P B16 ","Miniature Circuit  Breaker 10 kA, characteristic B, 16 A, 4-pole","NAA",29.95,0,29.95,8592765003546,3,18592765003543,36,28592765003540,"8536201090",0.48]
[100354,"Ex9BH 4P B20 ","Miniature Circuit  Breaker 10 kA, characteristic B, 20 A, 4-pole","NAA",29.95,0,29.95,8592765003553,3,18592765003550,36,28592765003557,"8536201090",0.48]
[100355,"Ex9BH 4P B25 ","Miniature Circuit  Breaker 10 kA, characteristic B, 25 A, 4-pole","NAA",29.95,0,29.95,8592765003560,3,18592765003567,36,28592765003564,"8536201090",0.48]
[100356,"Ex9BH 4P B32 ","Miniature Circuit  Breaker 10 kA, characteristic B, 32 A, 4-pole","NAA",41.29,0,41.29,8592765003577,3,18592765003574,36,28592765003571,"8536201090",0.48]
[100357,"Ex9BH 4P B40 ","Miniature Circuit  Breaker 10 kA, characteristic B, 40 A, 4-pole","NAA",41.29,0,41.29,8592765003584,3,18592765003581,36,28592765003588,"8536201090",0.48]
[100358,"Ex9BH 4P B50 ","Miniature Circuit  Breaker 10 kA, characteristic B, 50 A, 4-pole","NAA",74.2,0,74.2,8592765003591,3,18592765003598,36,28592765003595,"8536201090",0.48]
[100359,"Ex9BH 4P B63 ","Miniature Circuit  Breaker 10 kA, characteristic B, 63 A, 4-pole","NAA",74.2,0,74.2,8592765003607,3,18592765003604,36,28592765003601,"8536201090",0.48]
[100360,"Ex9BH 1P C1 ","Miniature Circuit  Breaker 10 kA, characteristic C, 1 A, 1-pole","NAA",7.08,0,7.08,8592765003614,12,18592765003611,144,28592765003618,"8536201090",0.12]
[100361,"Ex9BH 1P C2 ","Miniature Circuit  Breaker 10 kA, characteristic C, 2 A, 1-pole","NAA",7.08,0,7.08,8592765003621,12,18592765003628,144,28592765003625,"8536201090",0.12]
[100362,"Ex9BH 1P C3 ","Miniature Circuit  Breaker 10 kA, characteristic C, 3 A, 1-pole","NAA",7.08,0,7.08,8592765003638,12,18592765003635,144,28592765003632,"8536201090",0.12]
[100363,"Ex9BH 1P C4 ","Miniature Circuit  Breaker 10 kA, characteristic C, 4 A, 1-pole","NAA",7.08,0,7.08,8592765003645,12,18592765003642,144,28592765003649,"8536201090",0.12]
[100364,"Ex9BH 1P C6 ","Miniature Circuit  Breaker 10 kA, characteristic C, 6 A, 1-pole","NAA",6.86,0,6.86,8592765003652,12,18592765003659,144,28592765003656,"8536201090",0.12]
[100365,"Ex9BH 1P C8 ","Miniature Circuit  Breaker 10 kA, characteristic C, 8 A, 1-pole","NAA",6.86,0,6.86,8592765003669,12,18592765003666,144,28592765003663,"8536201090",0.12]
[100366,"Ex9BH 1P C10 ","Miniature Circuit  Breaker 10 kA, characteristic C, 10 A, 1-pole","NAA",4.84,0,4.84,8592765003676,12,18592765003673,144,28592765003670,"8536201090",0.12]
[100367,"Ex9BH 1P C13 ","Miniature Circuit  Breaker 10 kA, characteristic C, 13 A, 1-pole","NAA",4.84,0,4.84,8592765003683,12,18592765003680,144,28592765003687,"8536201090",0.12]
[100368,"Ex9BH 1P C16 ","Miniature Circuit  Breaker 10 kA, characteristic C, 16 A, 1-pole","NAA",4.84,0,4.84,8592765003690,12,18592765003697,144,28592765003694,"8536201090",0.12]
[100369,"Ex9BH 1P C20 ","Miniature Circuit  Breaker 10 kA, characteristic C, 20 A, 1-pole","NAA",4.84,0,4.84,8592765003706,12,18592765003703,144,28592765003700,"8536201090",0.12]
[100370,"Ex9BH 1P C25 ","Miniature Circuit  Breaker 10 kA, characteristic C, 25 A, 1-pole","NAA",4.84,0,4.84,8592765003713,12,18592765003710,144,28592765003717,"8536201090",0.12]
[100371,"Ex9BH 1P C32 ","Miniature Circuit  Breaker 10 kA, characteristic C, 32 A, 1-pole","NAA",7.64,0,7.64,8592765003720,12,18592765003727,144,28592765003724,"8536201090",0.12]
[100372,"Ex9BH 1P C40 ","Miniature Circuit  Breaker 10 kA, characteristic C, 40 A, 1-pole","NAA",7.64,0,7.64,8592765003737,12,18592765003734,144,28592765003731,"8536201090",0.12]
[100373,"Ex9BH 1P C50 ","Miniature Circuit  Breaker 10 kA, characteristic C, 50 A, 1-pole","NAA",16.71,0,16.71,8592765003744,12,18592765003741,144,28592765003748,"8536201090",0.12]
[100374,"Ex9BH 1P C63 ","Miniature Circuit  Breaker 10 kA, characteristic C, 63 A, 1-pole","NAA",19.350000000000001,0,19.350000000000001,8592765003751,12,18592765003758,144,28592765003755,"8536201090",0.12]
[100375,"Ex9BH 1PN C1 ","Miniature Circuit  Breaker 10 kA, characteristic C, 1 A, 1+Npole","NAA",11.02,0,11.02,8592765003768,6,18592765003765,72,28592765003762,"8536201090",0.24]
[100376,"Ex9BH 1PN C2 ","Miniature Circuit  Breaker 10 kA, characteristic C, 2 A, 1+Npole","NAA",11.02,0,11.02,8592765003775,6,18592765003772,72,28592765003779,"8536201090",0.24]
[100377,"Ex9BH 1PN C3 ","Miniature Circuit  Breaker 10 kA, characteristic C, 3 A, 1+Npole","NAA",11.02,0,11.02,8592765003782,6,18592765003789,72,28592765003786,"8536201090",0.24]
[100378,"Ex9BH 1PN C4 ","Miniature Circuit  Breaker 10 kA, characteristic C, 4 A, 1+Npole","NAA",11.02,0,11.02,8592765003799,6,18592765003796,72,28592765003793,"8536201090",0.24]
[100379,"Ex9BH 1PN C6 ","Miniature Circuit  Breaker 10 kA, characteristic C, 6 A, 1+Npole","NAA",11.02,0,11.02,8592765003805,6,18592765003802,72,28592765003809,"8536201090",0.24]
[100380,"Ex9BH 1PN C8 ","Miniature Circuit  Breaker 10 kA, characteristic C, 8 A, 1+Npole","NAA",11.02,0,11.02,8592765003812,6,18592765003819,72,28592765003816,"8536201090",0.24]
[100381,"Ex9BH 1PN C10 ","Miniature Circuit  Breaker 10 kA, characteristic C, 10 A, 1+Npole","NAA",8.14,0,8.14,8592765003829,6,18592765003826,72,28592765003823,"8536201090",0.24]
[100382,"Ex9BH 1PN C13 ","Miniature Circuit  Breaker 10 kA, characteristic C, 13 A, 1+Npole","NAA",8.14,0,8.14,8592765003836,6,18592765003833,72,28592765003830,"8536201090",0.24]
[100383,"Ex9BH 1PN C16 ","Miniature Circuit  Breaker 10 kA, characteristic C, 16 A, 1+Npole","NAA",8.14,0,8.14,8592765003843,6,18592765003840,72,28592765003847,"8536201090",0.24]
[100384,"Ex9BH 1PN C20 ","Miniature Circuit  Breaker 10 kA, characteristic C, 20 A, 1+Npole","NAA",8.14,0,8.14,8592765003850,6,18592765003857,72,28592765003854,"8536201090",0.24]
[100385,"Ex9BH 1PN C25 ","Miniature Circuit  Breaker 10 kA, characteristic C, 25 A, 1+Npole","NAA",8.14,0,8.14,8592765003867,6,18592765003864,72,28592765003861,"8536201090",0.24]
[100386,"Ex9BH 1PN C32 ","Miniature Circuit  Breaker 10 kA, characteristic C, 32 A, 1+Npole","NAA",13.29,0,13.29,8592765003874,6,18592765003871,72,28592765003878,"8536201090",0.24]
[100387,"Ex9BH 1PN C40 ","Miniature Circuit  Breaker 10 kA, characteristic C, 40 A, 1+Npole","NAA",13.29,0,13.29,8592765003881,6,18592765003888,72,28592765003885,"8536201090",0.24]
[100388,"Ex9BH 1PN C50 ","Miniature Circuit  Breaker 10 kA, characteristic C, 50 A, 1+Npole","NAA",39.69,0,39.69,8592765003898,6,18592765003895,72,28592765003892,"8536201090",0.24]
[100389,"Ex9BH 1PN C63 ","Miniature Circuit  Breaker 10 kA, characteristic C, 63 A, 1+Npole","NAA",39.69,0,39.69,8592765003904,6,18592765003901,72,28592765003908,"8536201090",0.24]
[100390,"Ex9BH 2P C1 ","Miniature Circuit  Breaker 10 kA, characteristic C, 1 A, 2-pole","NAA",16.399999999999999,0,16.399999999999999,8592765003911,6,18592765003918,72,28592765003915,"8536201090",0.24]
[100391,"Ex9BH 2P C2 ","Miniature Circuit  Breaker 10 kA, characteristic C, 2 A, 2-pole","NAA",16.399999999999999,0,16.399999999999999,8592765003928,6,18592765003925,72,28592765003922,"8536201090",0.24]
[100392,"Ex9BH 2P C3 ","Miniature Circuit  Breaker 10 kA, characteristic C, 3 A, 2-pole","NAA",16.399999999999999,0,16.399999999999999,8592765003935,6,18592765003932,72,28592765003939,"8536201090",0.24]
[100393,"Ex9BH 2P C4 ","Miniature Circuit  Breaker 10 kA, characteristic C, 4 A, 2-pole","NAA",16.399999999999999,0,16.399999999999999,8592765003942,6,18592765003949,72,28592765003946,"8536201090",0.24]
[100394,"Ex9BH 2P C6 ","Miniature Circuit  Breaker 10 kA, characteristic C, 6 A, 2-pole","NAA",16.399999999999999,0,16.399999999999999,8592765003959,6,18592765003956,72,28592765003953,"8536201090",0.24]
[100395,"Ex9BH 2P C8 ","Miniature Circuit  Breaker 10 kA, characteristic C, 8 A, 2-pole","NAA",16.399999999999999,0,16.399999999999999,8592765003966,6,18592765003963,72,28592765003960,"8536201090",0.24]
[100396,"Ex9BH 2P C10 ","Miniature Circuit  Breaker 10 kA, characteristic C, 10 A, 2-pole","NAA",11.42,0,11.42,8592765003973,6,18592765003970,72,28592765003977,"8536201090",0.24]
[100397,"Ex9BH 2P C13 ","Miniature Circuit  Breaker 10 kA, characteristic C, 13 A, 2-pole","NAA",11.42,0,11.42,8592765003980,6,18592765003987,72,28592765003984,"8536201090",0.24]
[100398,"Ex9BH 2P C16 ","Miniature Circuit  Breaker 10 kA, characteristic C, 16 A, 2-pole","NAA",11.42,{"$f":"NAA","v":0},{"$f":"E135*(1-F135)","v":11.42},8592765003997,6,18592765003994,72,28592765003991,"8536201090",0.24]
[100399,"Ex9BH 2P C20 ","Miniature Circuit  Breaker 10 kA, characteristic C, 20 A, 2-pole","NAA",11.42,0,11.42,8592765004000,6,18592765004007,72,28592765004004,"8536201090",0.24]
[100400,"Ex9BH 2P C25 ","Miniature Circuit  Breaker 10 kA, characteristic C, 25 A, 2-pole","NAA",11.42,0,11.42,8592765004017,6,18592765004014,72,28592765004011,"8536201090",0.24]
[100401,"Ex9BH 2P C32 ","Miniature Circuit  Breaker 10 kA, characteristic C, 32 A, 2-pole","NAA",18.36,0,18.36,8592765004024,6,18592765004021,72,28592765004028,"8536201090",0.24]
[100402,"Ex9BH 2P C40 ","Miniature Circuit  Breaker 10 kA, characteristic C, 40 A, 2-pole","NAA",18.36,0,18.36,8592765004031,6,18592765004038,72,28592765004035,"8536201090",0.24]
[100403,"Ex9BH 2P C50 ","Miniature Circuit  Breaker 10 kA, characteristic C, 50 A, 2-pole","NAA",49.6,0,49.6,8592765004048,6,18592765004045,72,28592765004042,"8536201090",0.24]
[100404,"Ex9BH 2P C63 ","Miniature Circuit  Breaker 10 kA, characteristic C, 63 A, 2-pole","NAA",49.6,0,49.6,8592765004055,6,18592765004052,72,28592765004059,"8536201090",0.24]
[100405,"Ex9BH 3P C1 ","Miniature Circuit  Breaker 10 kA, characteristic C, 1 A, 3-pole","NAA",22.29,0,22.29,8592765004062,4,18592765004069,48,28592765004066,"8536201090",0.36]
[100406,"Ex9BH 3P C2 ","Miniature Circuit  Breaker 10 kA, characteristic C, 2 A, 3-pole","NAA",22.29,0,22.29,8592765004079,4,18592765004076,48,28592765004073,"8536201090",0.36]
[100407,"Ex9BH 3P C3 ","Miniature Circuit  Breaker 10 kA, characteristic C, 3 A, 3-pole","NAA",22.29,0,22.29,8592765004086,4,18592765004083,48,28592765004080,"8536201090",0.36]
[100408,"Ex9BH 3P C4 ","Miniature Circuit  Breaker 10 kA, characteristic C, 4 A, 3-pole","NAA",22.29,0,22.29,8592765004093,4,18592765004090,48,28592765004097,"8536201090",0.36]
[100409,"Ex9BH 3P C6 ","Miniature Circuit  Breaker 10 kA, characteristic C, 6 A, 3-pole","NAA",22.29,0,22.29,8592765004109,4,18592765004106,48,28592765004103,"8536201090",0.36]
[100410,"Ex9BH 3P C8 ","Miniature Circuit  Breaker 10 kA, characteristic C, 8 A, 3-pole","NAA",22.29,0,22.29,8592765004116,4,18592765004113,48,28592765004110,"8536201090",0.36]
[100411,"Ex9BH 3P C10 ","Miniature Circuit  Breaker 10 kA, characteristic C, 10 A, 3-pole","NAA",16.89,0,16.89,8592765004123,4,18592765004120,48,28592765004127,"8536201090",0.36]
[100412,"Ex9BH 3P C13 ","Miniature Circuit  Breaker 10 kA, characteristic C, 13 A, 3-pole","NAA",16.89,0,16.89,8592765004130,4,18592765004137,48,28592765004134,"8536201090",0.36]
[100413,"Ex9BH 3P C16 ","Miniature Circuit  Breaker 10 kA, characteristic C, 16 A, 3-pole","NAA",16.89,0,16.89,8592765004147,4,18592765004144,48,28592765004141,"8536201090",0.36]
[100414,"Ex9BH 3P C20 ","Miniature Circuit  Breaker 10 kA, characteristic C, 20 A, 3-pole","NAA",16.89,0,16.89,8592765004154,4,18592765004151,48,28592765004158,"8536201090",0.36]
[100415,"Ex9BH 3P C25 ","Miniature Circuit  Breaker 10 kA, characteristic C, 25 A, 3-pole","NAA",16.89,0,16.89,8592765004161,4,18592765004168,48,28592765004165,"8536201090",0.36]
[100416,"Ex9BH 3P C32 ","Miniature Circuit  Breaker 10 kA, characteristic C, 32 A, 3-pole","NAA",24.39,0,24.39,8592765004178,4,18592765004175,48,28592765004172,"8536201090",0.36]
[100417,"Ex9BH 3P C40 ","Miniature Circuit  Breaker 10 kA, characteristic C, 40 A, 3-pole","NAA",24.39,0,24.39,8592765004185,4,18592765004182,48,28592765004189,"8536201090",0.36]
[100418,"Ex9BH 3P C50 ","Miniature Circuit  Breaker 10 kA, characteristic C, 50 A, 3-pole","NAA",46.84,0,46.84,8592765004192,4,18592765004199,48,28592765004196,"8536201090",0.36]
[100419,"Ex9BH 3P C63 ","Miniature Circuit  Breaker 10 kA, characteristic C, 63 A, 3-pole","NAA",51.39,0,51.39,8592765004208,4,18592765004205,48,28592765004202,"8536201090",0.36]
[100420,"Ex9BH 3PN C1 ","Miniature Circuit  Breaker 10 kA, characteristic C, 1 A, 3+Npole","NAA",36.08,0,36.08,8592765004215,3,18592765004212,36,28592765004219,"8536201090",0.48]
[100421,"Ex9BH 3PN C2 ","Miniature Circuit  Breaker 10 kA, characteristic C, 2 A, 3+Npole","NAA",36.08,0,36.08,8592765004222,3,18592765004229,36,28592765004226,"8536201090",0.48]
[100422,"Ex9BH 3PN C3 ","Miniature Circuit  Breaker 10 kA, characteristic C, 3 A, 3+Npole","NAA",36.08,0,36.08,8592765004239,3,18592765004236,36,28592765004233,"8536201090",0.48]
[100423,"Ex9BH 3PN C4 ","Miniature Circuit  Breaker 10 kA, characteristic C, 4 A, 3+Npole","NAA",36.08,0,36.08,8592765004246,3,18592765004243,36,28592765004240,"8536201090",0.48]
[100424,"Ex9BH 3PN C6 ","Miniature Circuit  Breaker 10 kA, characteristic C, 6 A, 3+Npole","NAA",36.08,0,36.08,8592765004253,3,18592765004250,36,28592765004257,"8536201090",0.48]
[100425,"Ex9BH 3PN C8 ","Miniature Circuit  Breaker 10 kA, characteristic C, 8 A, 3+Npole","NAA",36.08,0,36.08,8592765004260,3,18592765004267,36,28592765004264,"8536201090",0.48]
[100426,"Ex9BH 3PN C10 ","Miniature Circuit  Breaker 10 kA, characteristic C, 10 A, 3+Npole","NAA",24.29,0,24.29,8592765004277,3,18592765004274,36,28592765004271,"8536201090",0.48]
[100427,"Ex9BH 3PN C13 ","Miniature Circuit  Breaker 10 kA, characteristic C, 13 A, 3+Npole","NAA",24.29,0,24.29,8592765004284,3,18592765004281,36,28592765004288,"8536201090",0.48]
[100428,"Ex9BH 3PN C16 ","Miniature Circuit  Breaker 10 kA, characteristic C, 16 A, 3+Npole","NAA",24.29,0,24.29,8592765004291,3,18592765004298,36,28592765004295,"8536201090",0.48]
[100429,"Ex9BH 3PN C20 ","Miniature Circuit  Breaker 10 kA, characteristic C, 20 A, 3+Npole","NAA",24.29,0,24.29,8592765004307,3,18592765004304,36,28592765004301,"8536201090",0.48]
[100430,"Ex9BH 3PN C25 ","Miniature Circuit  Breaker 10 kA, characteristic C, 25 A, 3+Npole","NAA",24.29,0,24.29,8592765004314,3,18592765004311,36,28592765004318,"8536201090",0.48]
[100431,"Ex9BH 3PN C32 ","Miniature Circuit  Breaker 10 kA, characteristic C, 32 A, 3+Npole","NAA",33.69,0,33.69,8592765004321,3,18592765004328,36,28592765004325,"8536201090",0.48]
[100432,"Ex9BH 3PN C40 ","Miniature Circuit  Breaker 10 kA, characteristic C, 40 A, 3+Npole","NAA",33.69,0,33.69,8592765004338,3,18592765004335,36,28592765004332,"8536201090",0.48]
[100433,"Ex9BH 3PN C50 ","Miniature Circuit  Breaker 10 kA, characteristic C, 50 A, 3+Npole","NAA",65.77,0,65.77,8592765004345,3,18592765004342,36,28592765004349,"8536201090",0.48]
[100434,"Ex9BH 3PN C63 ","Miniature Circuit  Breaker 10 kA, characteristic C, 63 A, 3+Npole","NAA",65.77,0,65.77,8592765004352,3,18592765004359,36,28592765004356,"8536201090",0.48]
[100435,"Ex9BH 4P C1 ","Miniature Circuit  Breaker 10 kA, characteristic C, 1 A, 4-pole","NAA",41.41,0,41.41,8592765004369,3,18592765004366,36,28592765004363,"8536201090",0.48]
[100436,"Ex9BH 4P C2 ","Miniature Circuit  Breaker 10 kA, characteristic C, 2 A, 4-pole","NAA",41.41,0,41.41,8592765004376,3,18592765004373,36,28592765004370,"8536201090",0.48]
[100437,"Ex9BH 4P C3 ","Miniature Circuit  Breaker 10 kA, characteristic C, 3 A, 4-pole","NAA",41.41,0,41.41,8592765004383,3,18592765004380,36,28592765004387,"8536201090",0.48]
[100438,"Ex9BH 4P C4 ","Miniature Circuit  Breaker 10 kA, characteristic C, 4 A, 4-pole","NAA",41.41,0,41.41,8592765004390,3,18592765004397,36,28592765004394,"8536201090",0.48]
[100439,"Ex9BH 4P C6 ","Miniature Circuit  Breaker 10 kA, characteristic C, 6 A, 4-pole","NAA",41.41,0,41.41,8592765004406,3,18592765004403,36,28592765004400,"8536201090",0.48]
[100440,"Ex9BH 4P C8 ","Miniature Circuit  Breaker 10 kA, characteristic C, 8 A, 4-pole","NAA",41.41,0,41.41,8592765004413,3,18592765004410,36,28592765004417,"8536201090",0.48]
[100441,"Ex9BH 4P C10 ","Miniature Circuit  Breaker 10 kA, characteristic C, 10 A, 4-pole","NAA",27.99,0,27.99,8592765004420,3,18592765004427,36,28592765004424,"8536201090",0.48]
[100442,"Ex9BH 4P C13 ","Miniature Circuit  Breaker 10 kA, characteristic C, 13 A, 4-pole","NAA",27.99,0,27.99,8592765004437,3,18592765004434,36,28592765004431,"8536201090",0.48]
[100443,"Ex9BH 4P C16 ","Miniature Circuit  Breaker 10 kA, characteristic C, 16 A, 4-pole","NAA",27.99,0,27.99,8592765004444,3,18592765004441,36,28592765004448,"8536201090",0.48]
[100444,"Ex9BH 4P C20 ","Miniature Circuit  Breaker 10 kA, characteristic C, 20 A, 4-pole","NAA",27.99,0,27.99,8592765004451,3,18592765004458,36,28592765004455,"8536201090",0.48]
[100445,"Ex9BH 4P C25 ","Miniature Circuit  Breaker 10 kA, characteristic C, 25 A, 4-pole","NAA",27.99,0,27.99,8592765004468,3,18592765004465,36,28592765004462,"8536201090",0.48]
[100446,"Ex9BH 4P C32 ","Miniature Circuit  Breaker 10 kA, characteristic C, 32 A, 4-pole","NAA",39.229999999999997,0,39.229999999999997,8592765004475,3,18592765004472,36,28592765004479,"8536201090",0.48]
[100447,"Ex9BH 4P C40 ","Miniature Circuit  Breaker 10 kA, characteristic C, 40 A, 4-pole","NAA",39.229999999999997,0,39.229999999999997,8592765004482,3,18592765004489,36,28592765004486,"8536201090",0.48]
[100448,"Ex9BH 4P C50 ","Miniature Circuit  Breaker 10 kA, characteristic C, 50 A, 4-pole","NAA",75.37,0,75.37,8592765004499,3,18592765004496,36,28592765004493,"8536201090",0.48]
[100449,"Ex9BH 4P C63 ","Miniature Circuit  Breaker 10 kA, characteristic C, 63 A, 4-pole","NAA",75.37,0,75.37,8592765004505,3,18592765004502,36,28592765004509,"8536201090",0.48]
[100450,"Ex9BH 1P D1 ","Miniature Circuit  Breaker 10 kA, characteristic D, 1 A, 1-pole","NAA",9.91,0,9.91,8592765004512,12,18592765004519,144,28592765004516,"8536201090",0.12]
[100451,"Ex9BH 1P D2 ","Miniature Circuit  Breaker 10 kA, characteristic D, 2 A, 1-pole","NAA",9.91,0,9.91,8592765004529,12,18592765004526,144,28592765004523,"8536201090",0.12]
[100452,"Ex9BH 1P D3 ","Miniature Circuit  Breaker 10 kA, characteristic D, 3 A, 1-pole","NAA",9.91,0,9.91,8592765004536,12,18592765004533,144,28592765004530,"8536201090",0.12]
[100453,"Ex9BH 1P D4 ","Miniature Circuit  Breaker 10 kA, characteristic D, 4 A, 1-pole","NAA",9.91,0,9.91,8592765004543,12,18592765004540,144,28592765004547,"8536201090",0.12]
[100454,"Ex9BH 1P D6 ","Miniature Circuit  Breaker 10 kA, characteristic D, 6 A, 1-pole","NAA",9.91,0,9.91,8592765004550,12,18592765004557,144,28592765004554,"8536201090",0.12]
[100455,"Ex9BH 1P D8 ","Miniature Circuit  Breaker 10 kA, characteristic D, 8 A, 1-pole","NAA",9.91,0,9.91,8592765004567,12,18592765004564,144,28592765004561,"8536201090",0.12]
[100456,"Ex9BH 1P D10 ","Miniature Circuit  Breaker 10 kA, characteristic D, 10 A, 1-pole","NAA",9.18,0,9.18,8592765004574,12,18592765004571,144,28592765004578,"8536201090",0.12]
[100457,"Ex9BH 1P D13 ","Miniature Circuit  Breaker 10 kA, characteristic D, 13 A, 1-pole","NAA",9.18,0,9.18,8592765004581,12,18592765004588,144,28592765004585,"8536201090",0.12]
[100458,"Ex9BH 1P D16 ","Miniature Circuit  Breaker 10 kA, characteristic D, 16 A, 1-pole","NAA",9.18,0,9.18,8592765004598,12,18592765004595,144,28592765004592,"8536201090",0.12]
[100459,"Ex9BH 1P D20 ","Miniature Circuit  Breaker 10 kA, characteristic D, 20 A, 1-pole","NAA",9.18,0,9.18,8592765004604,12,18592765004601,144,28592765004608,"8536201090",0.12]
[100460,"Ex9BH 1P D25 ","Miniature Circuit  Breaker 10 kA, characteristic D, 25 A, 1-pole","NAA",9.18,0,9.18,8592765004611,12,18592765004618,144,28592765004615,"8536201090",0.12]
[100461,"Ex9BH 1P D32 ","Miniature Circuit  Breaker 10 kA, characteristic D, 32 A, 1-pole","NAA",9.18,0,9.18,8592765004628,12,18592765004625,144,28592765004622,"8536201090",0.12]
[100462,"Ex9BH 1P D40 ","Miniature Circuit  Breaker 10 kA, characteristic D, 40 A, 1-pole","NAA",11.49,{"$f":"NAA","v":0},{"$f":"E199*(1-F199)","v":11.49},8592765004635,12,18592765004632,144,28592765004639,"8536201090",0.12]
[100463,"Ex9BH 1P D50 ","Miniature Circuit  Breaker 10 kA, characteristic D, 50 A, 1-pole","NAA",32.520000000000003,0,32.520000000000003,8592765004642,12,18592765004649,144,28592765004646,"8536201090",0.12]
[100464,"Ex9BH 1P D63 ","Miniature Circuit  Breaker 10 kA, characteristic D, 63 A, 1-pole","NAA",32.520000000000003,0,32.520000000000003,8592765004659,12,18592765004656,144,28592765004653,"8536201090",0.12]
[100465,"Ex9BH 1PN D1 ","Miniature Circuit  Breaker 10 kA, characteristic D, 1 A, 1+Npole","NAA",16.75,0,16.75,8592765004666,6,18592765004663,72,28592765004660,"8536201090",0.24]
[100466,"Ex9BH 1PN D2 ","Miniature Circuit  Breaker 10 kA, characteristic D, 2 A, 1+Npole","NAA",16.75,0,16.75,8592765004673,6,18592765004670,72,28592765004677,"8536201090",0.24]
[100467,"Ex9BH 1PN D3 ","Miniature Circuit  Breaker 10 kA, characteristic D, 3 A, 1+Npole","NAA",16.75,0,16.75,8592765004680,6,18592765004687,72,28592765004684,"8536201090",0.24]
[100468,"Ex9BH 1PN D4 ","Miniature Circuit  Breaker 10 kA, characteristic D, 4 A, 1+Npole","NAA",16.75,0,16.75,8592765004697,6,18592765004694,72,28592765004691,"8536201090",0.24]
[100469,"Ex9BH 1PN D6 ","Miniature Circuit  Breaker 10 kA, characteristic D, 6 A, 1+Npole","NAA",16.75,0,16.75,8592765004703,6,18592765004700,72,28592765004707,"8536201090",0.24]
[100470,"Ex9BH 1PN D8 ","Miniature Circuit  Breaker 10 kA, characteristic D, 8 A, 1+Npole","NAA",16.75,0,16.75,8592765004710,6,18592765004717,72,28592765004714,"8536201090",0.24]
[100471,"Ex9BH 1PN D10 ","Miniature Circuit  Breaker 10 kA, characteristic D, 10 A, 1+Npole","NAA",15.7,0,15.7,8592765004727,6,18592765004724,72,28592765004721,"8536201090",0.24]
[100472,"Ex9BH 1PN D13 ","Miniature Circuit  Breaker 10 kA, characteristic D, 13 A, 1+Npole","NAA",15.7,0,15.7,8592765004734,6,18592765004731,72,28592765004738,"8536201090",0.24]
[100473,"Ex9BH 1PN D16 ","Miniature Circuit  Breaker 10 kA, characteristic D, 16 A, 1+Npole","NAA",15.7,0,15.7,8592765004741,6,18592765004748,72,28592765004745,"8536201090",0.24]
[100474,"Ex9BH 1PN D20 ","Miniature Circuit  Breaker 10 kA, characteristic D, 20 A, 1+Npole","NAA",15.7,0,15.7,8592765004758,6,18592765004755,72,28592765004752,"8536201090",0.24]
[100475,"Ex9BH 1PN D25 ","Miniature Circuit  Breaker 10 kA, characteristic D, 25 A, 1+Npole","NAA",15.7,0,15.7,8592765004765,6,18592765004762,72,28592765004769,"8536201090",0.24]
[100476,"Ex9BH 1PN D32 ","Miniature Circuit  Breaker 10 kA, characteristic D, 32 A, 1+Npole","NAA",19.45,0,19.45,8592765004772,6,18592765004779,72,28592765004776,"8536201090",0.24]
[100477,"Ex9BH 1PN D40 ","Miniature Circuit  Breaker 10 kA, characteristic D, 40 A, 1+Npole","NAA",19.45,0,19.45,8592765004789,6,18592765004786,72,28592765004783,"8536201090",0.24]
[100478,"Ex9BH 1PN D50 ","Miniature Circuit  Breaker 10 kA, characteristic D, 50 A, 1+Npole","NAA",53.86,0,53.86,8592765004796,6,18592765004793,72,28592765004790,"8536201090",0.24]
[100479,"Ex9BH 1PN D63 ","Miniature Circuit  Breaker 10 kA, characteristic D, 63 A, 1+Npole","NAA",53.86,0,53.86,8592765004802,6,18592765004809,72,28592765004806,"8536201090",0.24]
[100480,"Ex9BH 2P D1 ","Miniature Circuit  Breaker 10 kA, characteristic D, 1 A, 2-pole","NAA",19.52,0,19.52,8592765004819,6,18592765004816,72,28592765004813,"8536201090",0.24]
[100481,"Ex9BH 2P D2 ","Miniature Circuit  Breaker 10 kA, characteristic D, 2 A, 2-pole","NAA",19.52,0,19.52,8592765004826,6,18592765004823,72,28592765004820,"8536201090",0.24]
[100482,"Ex9BH 2P D3 ","Miniature Circuit  Breaker 10 kA, characteristic D, 3 A, 2-pole","NAA",19.52,0,19.52,8592765004833,6,18592765004830,72,28592765004837,"8536201090",0.24]
[100483,"Ex9BH 2P D4 ","Miniature Circuit  Breaker 10 kA, characteristic D, 4 A, 2-pole","NAA",19.52,0,19.52,8592765004840,6,18592765004847,72,28592765004844,"8536201090",0.24]
[100484,"Ex9BH 2P D6 ","Miniature Circuit  Breaker 10 kA, characteristic D, 6 A, 2-pole","NAA",19.52,0,19.52,8592765004857,6,18592765004854,72,28592765004851,"8536201090",0.24]
[100485,"Ex9BH 2P D8 ","Miniature Circuit  Breaker 10 kA, characteristic D, 8 A, 2-pole","NAA",19.52,0,19.52,8592765004864,6,18592765004861,72,28592765004868,"8536201090",0.24]
[100486,"Ex9BH 2P D10 ","Miniature Circuit  Breaker 10 kA, characteristic D, 10 A, 2-pole","NAA",19.16,0,19.16,8592765004871,6,18592765004878,72,28592765004875,"8536201090",0.24]
[100487,"Ex9BH 2P D13 ","Miniature Circuit  Breaker 10 kA, characteristic D, 13 A, 2-pole","NAA",19.16,0,19.16,8592765004888,6,18592765004885,72,28592765004882,"8536201090",0.24]
[100488,"Ex9BH 2P D16 ","Miniature Circuit  Breaker 10 kA, characteristic D, 16 A, 2-pole","NAA",19.16,0,19.16,8592765004895,6,18592765004892,72,28592765004899,"8536201090",0.24]
[100489,"Ex9BH 2P D20 ","Miniature Circuit  Breaker 10 kA, characteristic D, 20 A, 2-pole","NAA",19.16,0,19.16,8592765004901,6,18592765004908,72,28592765004905,"8536201090",0.24]
[100490,"Ex9BH 2P D25 ","Miniature Circuit  Breaker 10 kA, characteristic D, 25 A, 2-pole","NAA",19.16,0,19.16,8592765004918,6,18592765004915,72,28592765004912,"8536201090",0.24]
[100491,"Ex9BH 2P D32 ","Miniature Circuit  Breaker 10 kA, characteristic D, 32 A, 2-pole","NAA",25.15,0,25.15,8592765004925,6,18592765004922,72,28592765004929,"8536201090",0.24]
[100492,"Ex9BH 2P D40 ","Miniature Circuit  Breaker 10 kA, characteristic D, 40 A, 2-pole","NAA",25.15,0,25.15,8592765004932,6,18592765004939,72,28592765004936,"8536201090",0.24]
[100493,"Ex9BH 2P D50 ","Miniature Circuit  Breaker 10 kA, characteristic D, 50 A, 2-pole","NAA",71.260000000000005,0,71.260000000000005,8592765004949,6,18592765004946,72,28592765004943,"8536201090",0.24]
[100494,"Ex9BH 2P D63 ","Miniature Circuit  Breaker 10 kA, characteristic D, 63 A, 2-pole","NAA",71.260000000000005,0,71.260000000000005,8592765004956,6,18592765004953,72,28592765004950,"8536201090",0.24]
[100495,"Ex9BH 3P D1 ","Miniature Circuit  Breaker 10 kA, characteristic D, 1 A, 3-pole","NAA",34.14,0,34.14,8592765004963,4,18592765004960,48,28592765004967,"8536201090",0.36]
[100496,"Ex9BH 3P D2 ","Miniature Circuit  Breaker 10 kA, characteristic D, 2 A, 3-pole","NAA",34.14,0,34.14,8592765004970,4,18592765004977,48,28592765004974,"8536201090",0.36]
[100497,"Ex9BH 3P D3 ","Miniature Circuit  Breaker 10 kA, characteristic D, 3 A, 3-pole","NAA",34.14,0,34.14,8592765004987,4,18592765004984,48,28592765004981,"8536201090",0.36]
[100498,"Ex9BH 3P D4 ","Miniature Circuit  Breaker 10 kA, characteristic D, 4 A, 3-pole","NAA",34.14,0,34.14,8592765004994,4,18592765004991,48,28592765004998,"8536201090",0.36]
[100499,"Ex9BH 3P D6 ","Miniature Circuit  Breaker 10 kA, characteristic D, 6 A, 3-pole","NAA",34.14,0,34.14,8592765005007,4,18592765005004,48,28592765005001,"8536201090",0.36]
[100500,"Ex9BH 3P D8 ","Miniature Circuit  Breaker 10 kA, characteristic D, 8 A, 3-pole","NAA",34.14,0,34.14,8592765005014,4,18592765005011,48,28592765005018,"8536201090",0.36]
[100501,"Ex9BH 3P D10 ","Miniature Circuit  Breaker 10 kA, characteristic D, 10 A, 3-pole","NAA",29.67,0,29.67,8592765005021,4,18592765005028,48,28592765005025,"8536201090",0.36]
[100502,"Ex9BH 3P D13 ","Miniature Circuit  Breaker 10 kA, characteristic D, 13 A, 3-pole","NAA",29.67,0,29.67,8592765005038,4,18592765005035,48,28592765005032,"8536201090",0.36]
[100503,"Ex9BH 3P D16 ","Miniature Circuit  Breaker 10 kA, characteristic D, 16 A, 3-pole","NAA",29.67,0,29.67,8592765005045,4,18592765005042,48,28592765005049,"8536201090",0.36]
[100504,"Ex9BH 3P D20 ","Miniature Circuit  Breaker 10 kA, characteristic D, 20 A, 3-pole","NAA",29.67,0,29.67,8592765005052,4,18592765005059,48,28592765005056,"8536201090",0.36]
[100505,"Ex9BH 3P D25 ","Miniature Circuit  Breaker 10 kA, characteristic D, 25 A, 3-pole","NAA",29.67,0,29.67,8592765005069,4,18592765005066,48,28592765005063,"8536201090",0.36]
[100506,"Ex9BH 3P D32 ","Miniature Circuit  Breaker 10 kA, characteristic D, 32 A, 3-pole","NAA",30.48,0,30.48,8592765005076,4,18592765005073,48,28592765005070,"8536201090",0.36]
[100507,"Ex9BH 3P D40 ","Miniature Circuit  Breaker 10 kA, characteristic D, 40 A, 3-pole","NAA",40.18,0,40.18,8592765005083,4,18592765005080,48,28592765005087,"8536201090",0.36]
[100508,"Ex9BH 3P D50 ","Miniature Circuit  Breaker 10 kA, characteristic D, 50 A, 3-pole","NAA",111.53,0,111.53,8592765005090,4,18592765005097,48,28592765005094,"8536201090",0.36]
[100509,"Ex9BH 3P D63 ","Miniature Circuit  Breaker 10 kA, characteristic D, 63 A, 3-pole","NAA",111.53,0,111.53,8592765005106,4,18592765005103,48,28592765005100,"8536201090",0.36]
[100510,"Ex9BH 3PN D1 ","Miniature Circuit  Breaker 10 kA, characteristic D, 1 A, 3+Npole","NAA",46.51,0,46.51,8592765005113,3,18592765005110,36,28592765005117,"8536201090",0.48]
[100511,"Ex9BH 3PN D2 ","Miniature Circuit  Breaker 10 kA, characteristic D, 2 A, 3+Npole","NAA",46.51,0,46.51,8592765005120,3,18592765005127,36,28592765005124,"8536201090",0.48]
[100512,"Ex9BH 3PN D3 ","Miniature Circuit  Breaker 10 kA, characteristic D, 3 A, 3+Npole","NAA",46.51,0,46.51,8592765005137,3,18592765005134,36,28592765005131,"8536201090",0.48]
[100513,"Ex9BH 3PN D4 ","Miniature Circuit  Breaker 10 kA, characteristic D, 4 A, 3+Npole","NAA",46.51,0,46.51,8592765005144,3,18592765005141,36,28592765005148,"8536201090",0.48]
[100514,"Ex9BH 3PN D6 ","Miniature Circuit  Breaker 10 kA, characteristic D, 6 A, 3+Npole","NAA",46.51,0,46.51,8592765005151,3,18592765005158,36,28592765005155,"8536201090",0.48]
[100515,"Ex9BH 3PN D8 ","Miniature Circuit  Breaker 10 kA, characteristic D, 8 A, 3+Npole","NAA",46.51,0,46.51,8592765005168,3,18592765005165,36,28592765005162,"8536201090",0.48]
[100516,"Ex9BH 3PN D10 ","Miniature Circuit  Breaker 10 kA, characteristic D, 10 A, 3+Npole","NAA",42.39,0,42.39,8592765005175,3,18592765005172,36,28592765005179,"8536201090",0.48]
[100517,"Ex9BH 3PN D13 ","Miniature Circuit  Breaker 10 kA, characteristic D, 13 A, 3+Npole","NAA",42.39,0,42.39,8592765005182,3,18592765005189,36,28592765005186,"8536201090",0.48]
[100518,"Ex9BH 3PN D16 ","Miniature Circuit  Breaker 10 kA, characteristic D, 16 A, 3+Npole","NAA",42.39,0,42.39,8592765005199,3,18592765005196,36,28592765005193,"8536201090",0.48]
[100519,"Ex9BH 3PN D20 ","Miniature Circuit  Breaker 10 kA, characteristic D, 20 A, 3+Npole","NAA",42.39,0,42.39,8592765005205,3,18592765005202,36,28592765005209,"8536201090",0.48]
[100520,"Ex9BH 3PN D25 ","Miniature Circuit  Breaker 10 kA, characteristic D, 25 A, 3+Npole","NAA",42.39,0,42.39,8592765005212,3,18592765005219,36,28592765005216,"8536201090",0.48]
[100521,"Ex9BH 3PN D32 ","Miniature Circuit  Breaker 10 kA, characteristic D, 32 A, 3+Npole","NAA",56.72,0,56.72,8592765005229,3,18592765005226,36,28592765005223,"8536201090",0.48]
[100522,"Ex9BH 3PN D40 ","Miniature Circuit  Breaker 10 kA, characteristic D, 40 A, 3+Npole","NAA",56.72,0,56.72,8592765005236,3,18592765005233,36,28592765005230,"8536201090",0.48]
[100523,"Ex9BH 3PN D50 ","Miniature Circuit  Breaker 10 kA, characteristic D, 50 A, 3+Npole","NAA",159.26,0,159.26,8592765005243,3,18592765005240,36,28592765005247,"8536201090",0.48]
[100524,"Ex9BH 3PN D63 ","Miniature Circuit  Breaker 10 kA, characteristic D, 63 A, 3+Npole","NAA",159.26,0,159.26,8592765005250,3,18592765005257,36,28592765005254,"8536201090",0.48]
[100525,"Ex9BH 4P D1 ","Miniature Circuit  Breaker 10 kA, characteristic D, 1 A, 4-pole","NAA",53.21,0,53.21,8592765005267,3,18592765005264,36,28592765005261,"8536201090",0.48]
[100526,"Ex9BH 4P D2 ","Miniature Circuit  Breaker 10 kA, characteristic D, 2 A, 4-pole","NAA",53.21,{"$f":"NAA","v":0},{"$f":"E263*(1-F263)","v":53.21},8592765005274,3,18592765005271,36,28592765005278,"8536201090",0.48]
[100527,"Ex9BH 4P D3 ","Miniature Circuit  Breaker 10 kA, characteristic D, 3 A, 4-pole","NAA",53.21,0,53.21,8592765005281,3,18592765005288,36,28592765005285,"8536201090",0.48]
[100528,"Ex9BH 4P D4 ","Miniature Circuit  Breaker 10 kA, characteristic D, 4 A, 4-pole","NAA",53.21,0,53.21,8592765005298,3,18592765005295,36,28592765005292,"8536201090",0.48]
[100529,"Ex9BH 4P D6 ","Miniature Circuit  Breaker 10 kA, characteristic D, 6 A, 4-pole","NAA",53.21,0,53.21,8592765005304,3,18592765005301,36,28592765005308,"8536201090",0.48]
[100530,"Ex9BH 4P D8 ","Miniature Circuit  Breaker 10 kA, characteristic D, 8 A, 4-pole","NAA",53.21,0,53.21,8592765005311,3,18592765005318,36,28592765005315,"8536201090",0.48]
[100531,"Ex9BH 4P D10 ","Miniature Circuit  Breaker 10 kA, characteristic D, 10 A, 4-pole","NAA",48.98,0,48.98,8592765005328,3,18592765005325,36,28592765005322,"8536201090",0.48]
[100532,"Ex9BH 4P D13 ","Miniature Circuit  Breaker 10 kA, characteristic D, 13 A, 4-pole","NAA",48.98,0,48.98,8592765005335,3,18592765005332,36,28592765005339,"8536201090",0.48]
[100533,"Ex9BH 4P D16 ","Miniature Circuit  Breaker 10 kA, characteristic D, 16 A, 4-pole","NAA",48.98,0,48.98,8592765005342,3,18592765005349,36,28592765005346,"8536201090",0.48]
[100534,"Ex9BH 4P D20 ","Miniature Circuit  Breaker 10 kA, characteristic D, 20 A, 4-pole","NAA",48.98,0,48.98,8592765005359,3,18592765005356,36,28592765005353,"8536201090",0.48]
[100535,"Ex9BH 4P D25 ","Miniature Circuit  Breaker 10 kA, characteristic D, 25 A, 4-pole","NAA",48.98,0,48.98,8592765005366,3,18592765005363,36,28592765005360,"8536201090",0.48]
[100536,"Ex9BH 4P D32 ","Miniature Circuit  Breaker 10 kA, characteristic D, 32 A, 4-pole","NAA",65.41,0,65.41,8592765005373,3,18592765005370,36,28592765005377,"8536201090",0.48]
[100537,"Ex9BH 4P D40 ","Miniature Circuit  Breaker 10 kA, characteristic D, 40 A, 4-pole","NAA",65.41,0,65.41,8592765005380,3,18592765005387,36,28592765005384,"8536201090",0.48]
[100538,"Ex9BH 4P D50 ","Miniature Circuit  Breaker 10 kA, characteristic D, 50 A, 4-pole","NAA",183.87,0,183.87,8592765005397,3,18592765005394,36,28592765005391,"8536201090",0.48]
[100539,"Ex9BH 4P D63 ","Miniature Circuit  Breaker 10 kA, characteristic D, 63 A, 4-pole","NAA",183.87,0,183.87,8592765005403,3,18592765005400,36,28592765005407,"8536201090",0.48]
[]
["Miniature Circuit  Breakers Ex9BN, 6 kA"]
[100000,"Ex9BN 1P B1 ","Miniature Circuit  Breaker 6 kA, characteristic B, 1 A, 1-pole","NAB",4.32,{"$f":"NAB","v":0},{"$f":"E279*(1-F279)","v":4.32},8592765000019,12,18592765000016,144,28592765000013,"8536201090",0.12]
[100001,"Ex9BN 1P B2 ","Miniature Circuit  Breaker 6 kA, characteristic B, 2 A, 1-pole","NAB",4.32,0,4.32,8592765000026,12,18592765000023,144,28592765000020,"8536201090",0.12]
[100002,"Ex9BN 1P B3 ","Miniature Circuit  Breaker 6 kA, characteristic B, 3 A, 1-pole","NAB",4.32,0,4.32,8592765000033,12,18592765000030,144,28592765000037,"8536201090",0.12]
[100003,"Ex9BN 1P B4 ","Miniature Circuit  Breaker 6 kA, characteristic B, 4 A, 1-pole","NAB",4.32,0,4.32,8592765000040,12,18592765000047,144,28592765000044,"8536201090",0.12]
[100004,"Ex9BN 1P B6 ","Miniature Circuit  Breaker 6 kA, characteristic B, 6 A, 1-pole","NAB",4.13,0,4.13,8592765000057,12,18592765000054,144,28592765000051,"8536201090",0.12]
[100005,"Ex9BN 1P B8 ","Miniature Circuit  Breaker 6 kA, characteristic B, 8 A, 1-pole","NAB",4.13,0,4.13,8592765000064,12,18592765000061,144,28592765000068,"8536201090",0.12]
[100006,"Ex9BN 1P B10 ","Miniature Circuit  Breaker 6 kA, characteristic B, 10 A, 1-pole","NAB",3.65,0,3.65,8592765000071,12,18592765000078,144,28592765000075,"8536201090",0.12]
[100007,"Ex9BN 1P B13 ","Miniature Circuit  Breaker 6 kA, characteristic B, 13 A, 1-pole","NAB",3.65,0,3.65,8592765000088,12,18592765000085,144,28592765000082,"8536201090",0.12]
[100008,"Ex9BN 1P B16 ","Miniature Circuit  Breaker 6 kA, characteristic B, 16 A, 1-pole","NAB",3.65,0,3.65,8592765000095,12,18592765000092,144,28592765000099,"8536201090",0.12]
[100009,"Ex9BN 1P B20 ","Miniature Circuit  Breaker 6 kA, characteristic B, 20 A, 1-pole","NAB",3.65,0,3.65,8592765000101,12,18592765000108,144,28592765000105,"8536201090",0.12]
[100010,"Ex9BN 1P B25 ","Miniature Circuit  Breaker 6 kA, characteristic B, 25 A, 1-pole","NAB",3.65,0,3.65,8592765000118,12,18592765000115,144,28592765000112,"8536201090",0.12]
[100011,"Ex9BN 1P B32 ","Miniature Circuit  Breaker 6 kA, characteristic B, 32 A, 1-pole","NAB",4.6100000000000003,0,4.6100000000000003,8592765000125,12,18592765000122,144,28592765000129,"8536201090",0.12]
[100012,"Ex9BN 1P B40 ","Miniature Circuit  Breaker 6 kA, characteristic B, 40 A, 1-pole","NAB",4.6100000000000003,0,4.6100000000000003,8592765000132,12,18592765000139,144,28592765000136,"8536201090",0.12]
[100013,"Ex9BN 1P B50 ","Miniature Circuit  Breaker 6 kA, characteristic B, 50 A, 1-pole","NAB",8.09,0,8.09,8592765000149,12,18592765000146,144,28592765000143,"8536201090",0.12]
[100014,"Ex9BN 1P B63 ","Miniature Circuit  Breaker 6 kA, characteristic B, 63 A, 1-pole","NAB",8.09,0,8.09,8592765000156,12,18592765000153,144,28592765000150,"8536201090",0.12]
[100015,"Ex9BN 1PN B1 ","Miniature Circuit  Breaker 6 kA, characteristic B, 1 A, 1+Npole","NAB",7.71,0,7.71,8592765000163,6,18592765000160,72,28592765000167,"8536201090",0.24]
[100016,"Ex9BN 1PN B2 ","Miniature Circuit  Breaker 6 kA, characteristic B, 2 A, 1+Npole","NAB",7.71,0,7.71,8592765000170,6,18592765000177,72,28592765000174,"8536201090",0.24]
[100017,"Ex9BN 1PN B3 ","Miniature Circuit  Breaker 6 kA, characteristic B, 3 A, 1+Npole","NAB",7.71,0,7.71,8592765000187,6,18592765000184,72,28592765000181,"8536201090",0.24]
[100018,"Ex9BN 1PN B4 ","Miniature Circuit  Breaker 6 kA, characteristic B, 4 A, 1+Npole","NAB",7.71,0,7.71,8592765000194,6,18592765000191,72,28592765000198,"8536201090",0.24]
[100019,"Ex9BN 1PN B6 ","Miniature Circuit  Breaker 6 kA, characteristic B, 6 A, 1+Npole","NAB",7.71,0,7.71,8592765000200,6,18592765000207,72,28592765000204,"8536201090",0.24]
[100020,"Ex9BN 1PN B8 ","Miniature Circuit  Breaker 6 kA, characteristic B, 8 A, 1+Npole","NAB",7.71,0,7.71,8592765000217,6,18592765000214,72,28592765000211,"8536201090",0.24]
[100021,"Ex9BN 1PN B10 ","Miniature Circuit  Breaker 6 kA, characteristic B, 10 A, 1+Npole","NAB",8.56,0,8.56,8592765000224,6,18592765000221,72,28592765000228,"8536201090",0.24]
[100022,"Ex9BN 1PN B13 ","Miniature Circuit  Breaker 6 kA, characteristic B, 13 A, 1+Npole","NAB",8.56,0,8.56,8592765000231,6,18592765000238,72,28592765000235,"8536201090",0.24]
[100023,"Ex9BN 1PN B16 ","Miniature Circuit  Breaker 6 kA, characteristic B, 16 A, 1+Npole","NAB",8.56,0,8.56,8592765000248,6,18592765000245,72,28592765000242,"8536201090",0.24]
[100024,"Ex9BN 1PN B20 ","Miniature Circuit  Breaker 6 kA, characteristic B, 20 A, 1+Npole","NAB",8.56,0,8.56,8592765000255,6,18592765000252,72,28592765000259,"8536201090",0.24]
[100025,"Ex9BN 1PN B25 ","Miniature Circuit  Breaker 6 kA, characteristic B, 25 A, 1+Npole","NAB",8.56,0,8.56,8592765000262,6,18592765000269,72,28592765000266,"8536201090",0.24]
[100026,"Ex9BN 1PN B32 ","Miniature Circuit  Breaker 6 kA, characteristic B, 32 A, 1+Npole","NAB",8.8699999999999992,0,8.8699999999999992,8592765000279,6,18592765000276,72,28592765000273,"8536201090",0.24]
[100027,"Ex9BN 1PN B40 ","Miniature Circuit  Breaker 6 kA, characteristic B, 40 A, 1+Npole","NAB",8.8699999999999992,0,8.8699999999999992,8592765000286,6,18592765000283,72,28592765000280,"8536201090",0.24]
[100028,"Ex9BN 1PN B50 ","Miniature Circuit  Breaker 6 kA, characteristic B, 50 A, 1+Npole","NAB",15.52,0,15.52,8592765000293,6,18592765000290,72,28592765000297,"8536201090",0.24]
[100029,"Ex9BN 1PN B63 ","Miniature Circuit  Breaker 6 kA, characteristic B, 63 A, 1+Npole","NAB",15.52,0,15.52,8592765000309,6,18592765000306,72,28592765000303,"8536201090",0.24]
[100030,"Ex9BN 2P B1 ","Miniature Circuit  Breaker 6 kA, characteristic B, 1 A, 2-pole","NAB",9.0500000000000007,0,9.0500000000000007,8592765000316,6,18592765000313,72,28592765000310,"8536201090",0.24]
[100031,"Ex9BN 2P B2 ","Miniature Circuit  Breaker 6 kA, characteristic B, 2 A, 2-pole","NAB",9.0500000000000007,0,9.0500000000000007,8592765000323,6,18592765000320,72,28592765000327,"8536201090",0.24]
[100032,"Ex9BN 2P B3 ","Miniature Circuit  Breaker 6 kA, characteristic B, 3 A, 2-pole","NAB",9.0500000000000007,0,9.0500000000000007,8592765000330,6,18592765000337,72,28592765000334,"8536201090",0.24]
[100033,"Ex9BN 2P B4 ","Miniature Circuit  Breaker 6 kA, characteristic B, 4 A, 2-pole","NAB",9.0500000000000007,0,9.0500000000000007,8592765000347,6,18592765000344,72,28592765000341,"8536201090",0.24]
[100034,"Ex9BN 2P B6 ","Miniature Circuit  Breaker 6 kA, characteristic B, 6 A, 2-pole","NAB",9.0500000000000007,0,9.0500000000000007,8592765000354,6,18592765000351,72,28592765000358,"8536201090",0.24]
[100035,"Ex9BN 2P B8 ","Miniature Circuit  Breaker 6 kA, characteristic B, 8 A, 2-pole","NAB",9.0500000000000007,0,9.0500000000000007,8592765000361,6,18592765000368,72,28592765000365,"8536201090",0.24]
[100036,"Ex9BN 2P B10 ","Miniature Circuit  Breaker 6 kA, characteristic B, 10 A, 2-pole","NAB",10.1,0,10.1,8592765000378,6,18592765000375,72,28592765000372,"8536201090",0.24]
[100037,"Ex9BN 2P B13 ","Miniature Circuit  Breaker 6 kA, characteristic B, 13 A, 2-pole","NAB",10.1,0,10.1,8592765000385,6,18592765000382,72,28592765000389,"8536201090",0.24]
[100038,"Ex9BN 2P B16 ","Miniature Circuit  Breaker 6 kA, characteristic B, 16 A, 2-pole","NAB",10.1,0,10.1,8592765000392,6,18592765000399,72,28592765000396,"8536201090",0.24]
[100039,"Ex9BN 2P B20 ","Miniature Circuit  Breaker 6 kA, characteristic B, 20 A, 2-pole","NAB",10.1,0,10.1,8592765000408,6,18592765000405,72,28592765000402,"8536201090",0.24]
[100040,"Ex9BN 2P B25 ","Miniature Circuit  Breaker 6 kA, characteristic B, 25 A, 2-pole","NAB",10.1,0,10.1,8592765000415,6,18592765000412,72,28592765000419,"8536201090",0.24]
[100041,"Ex9BN 2P B32 ","Miniature Circuit  Breaker 6 kA, characteristic B, 32 A, 2-pole","NAB",10.41,0,10.41,8592765000422,6,18592765000429,72,28592765000426,"8536201090",0.24]
[100042,"Ex9BN 2P B40 ","Miniature Circuit  Breaker 6 kA, characteristic B, 40 A, 2-pole","NAB",10.41,0,10.41,8592765000439,6,18592765000436,72,28592765000433,"8536201090",0.24]
[100043,"Ex9BN 2P B50 ","Miniature Circuit  Breaker 6 kA, characteristic B, 50 A, 2-pole","NAB",18.22,0,18.22,8592765000446,6,18592765000443,72,28592765000440,"8536201090",0.24]
[100044,"Ex9BN 2P B63 ","Miniature Circuit  Breaker 6 kA, characteristic B, 63 A, 2-pole","NAB",18.22,0,18.22,8592765000453,6,18592765000450,72,28592765000457,"8536201090",0.24]
[100045,"Ex9BN 3P B1 ","Miniature Circuit  Breaker 6 kA, characteristic B, 1 A, 3-pole","NAB",13.68,0,13.68,8592765000460,4,18592765000467,48,28592765000464,"8536201090",0.36]
[100046,"Ex9BN 3P B2 ","Miniature Circuit  Breaker 6 kA, characteristic B, 2 A, 3-pole","NAB",13.68,0,13.68,8592765000477,4,18592765000474,48,28592765000471,"8536201090",0.36]
[100047,"Ex9BN 3P B3 ","Miniature Circuit  Breaker 6 kA, characteristic B, 3 A, 3-pole","NAB",13.68,0,13.68,8592765000484,4,18592765000481,48,28592765000488,"8536201090",0.36]
[100048,"Ex9BN 3P B4 ","Miniature Circuit  Breaker 6 kA, characteristic B, 4 A, 3-pole","NAB",13.68,0,13.68,8592765000491,4,18592765000498,48,28592765000495,"8536201090",0.36]
[100049,"Ex9BN 3P B6 ","Miniature Circuit  Breaker 6 kA, characteristic B, 6 A, 3-pole","NAB",13.68,0,13.68,8592765000507,4,18592765000504,48,28592765000501,"8536201090",0.36]
[100050,"Ex9BN 3P B8 ","Miniature Circuit  Breaker 6 kA, characteristic B, 8 A, 3-pole","NAB",13.68,0,13.68,8592765000514,4,18592765000511,48,28592765000518,"8536201090",0.36]
[100051,"Ex9BN 3P B10 ","Miniature Circuit  Breaker 6 kA, characteristic B, 10 A, 3-pole","NAB",12.15,0,12.15,8592765000521,4,18592765000528,48,28592765000525,"8536201090",0.36]
[100052,"Ex9BN 3P B13 ","Miniature Circuit  Breaker 6 kA, characteristic B, 13 A, 3-pole","NAB",12.15,0,12.15,8592765000538,4,18592765000535,48,28592765000532,"8536201090",0.36]
[100053,"Ex9BN 3P B16 ","Miniature Circuit  Breaker 6 kA, characteristic B, 16 A, 3-pole","NAB",12.15,0,12.15,8592765000545,4,18592765000542,48,28592765000549,"8536201090",0.36]
[100054,"Ex9BN 3P B20 ","Miniature Circuit  Breaker 6 kA, characteristic B, 20 A, 3-pole","NAB",12.15,0,12.15,8592765000552,4,18592765000559,48,28592765000556,"8536201090",0.36]
[100055,"Ex9BN 3P B25 ","Miniature Circuit  Breaker 6 kA, characteristic B, 25 A, 3-pole","NAB",12.15,0,12.15,8592765000569,4,18592765000566,48,28592765000563,"8536201090",0.36]
[100056,"Ex9BN 3P B32 ","Miniature Circuit  Breaker 6 kA, characteristic B, 32 A, 3-pole","NAB",13.68,0,13.68,8592765000576,4,18592765000573,48,28592765000570,"8536201090",0.36]
[100057,"Ex9BN 3P B40 ","Miniature Circuit  Breaker 6 kA, characteristic B, 40 A, 3-pole","NAB",13.68,0,13.68,8592765000583,4,18592765000580,48,28592765000587,"8536201090",0.36]
[100058,"Ex9BN 3P B50 ","Miniature Circuit  Breaker 6 kA, characteristic B, 50 A, 3-pole","NAB",22.59,0,22.59,8592765000590,4,18592765000597,48,28592765000594,"8536201090",0.36]
[100059,"Ex9BN 3P B63 ","Miniature Circuit  Breaker 6 kA, characteristic B, 63 A, 3-pole","NAB",22.59,0,22.59,8592765000606,4,18592765000603,48,28592765000600,"8536201090",0.36]
[100060,"Ex9BN 3PN B1 ","Miniature Circuit  Breaker 6 kA, characteristic B, 1 A, 3+Npole","NAB",25.26,0,25.26,8592765000613,3,18592765000610,36,28592765000617,"8536201090",0.48]
[100061,"Ex9BN 3PN B2 ","Miniature Circuit  Breaker 6 kA, characteristic B, 2 A, 3+Npole","NAB",25.26,0,25.26,8592765000620,3,18592765000627,36,28592765000624,"8536201090",0.48]
[100062,"Ex9BN 3PN B3 ","Miniature Circuit  Breaker 6 kA, characteristic B, 3 A, 3+Npole","NAB",25.26,0,25.26,8592765000637,3,18592765000634,36,28592765000631,"8536201090",0.48]
[100063,"Ex9BN 3PN B4 ","Miniature Circuit  Breaker 6 kA, characteristic B, 4 A, 3+Npole","NAB",25.26,0,25.26,8592765000644,3,18592765000641,36,28592765000648,"8536201090",0.48]
[100064,"Ex9BN 3PN B6 ","Miniature Circuit  Breaker 6 kA, characteristic B, 6 A, 3+Npole","NAB",25.26,0,{"$f":"E343*(1-F343)","v":25.26},8592765000651,3,18592765000658,36,28592765000655,"8536201090",0.48]
[100065,"Ex9BN 3PN B8 ","Miniature Circuit  Breaker 6 kA, characteristic B, 8 A, 3+Npole","NAB",25.26,0,25.26,8592765000668,3,18592765000665,36,28592765000662,"8536201090",0.48]
[100066,"Ex9BN 3PN B10 ","Miniature Circuit  Breaker 6 kA, characteristic B, 10 A, 3+Npole","NAB",22.48,0,22.48,8592765000675,3,18592765000672,36,28592765000679,"8536201090",0.48]
[100067,"Ex9BN 3PN B13 ","Miniature Circuit  Breaker 6 kA, characteristic B, 13 A, 3+Npole","NAB",22.48,0,22.48,8592765000682,3,18592765000689,36,28592765000686,"8536201090",0.48]
[100068,"Ex9BN 3PN B16 ","Miniature Circuit  Breaker 6 kA, characteristic B, 16 A, 3+Npole","NAB",22.48,0,22.48,8592765000699,3,18592765000696,36,28592765000693,"8536201090",0.48]
[100069,"Ex9BN 3PN B20 ","Miniature Circuit  Breaker 6 kA, characteristic B, 20 A, 3+Npole","NAB",22.48,0,22.48,8592765000705,3,18592765000702,36,28592765000709,"8536201090",0.48]
[100070,"Ex9BN 3PN B25 ","Miniature Circuit  Breaker 6 kA, characteristic B, 25 A, 3+Npole","NAB",22.48,0,22.48,8592765000712,3,18592765000719,36,28592765000716,"8536201090",0.48]
[100071,"Ex9BN 3PN B32 ","Miniature Circuit  Breaker 6 kA, characteristic B, 32 A, 3+Npole","NAB",33.06,0,33.06,8592765000729,3,18592765000726,36,28592765000723,"8536201090",0.48]
[100072,"Ex9BN 3PN B40 ","Miniature Circuit  Breaker 6 kA, characteristic B, 40 A, 3+Npole","NAB",33.06,0,33.06,8592765000736,3,18592765000733,36,28592765000730,"8536201090",0.48]
[100073,"Ex9BN 3PN B50 ","Miniature Circuit  Breaker 6 kA, characteristic B, 50 A, 3+Npole","NAB",43.93,0,43.93,8592765000743,3,18592765000740,36,28592765000747,"8536201090",0.48]
[100074,"Ex9BN 3PN B63 ","Miniature Circuit  Breaker 6 kA, characteristic B, 63 A, 3+Npole","NAB",43.93,0,43.93,8592765000750,3,18592765000757,36,28592765000754,"8536201090",0.48]
[100075,"Ex9BN 4P B1 ","Miniature Circuit  Breaker 6 kA, characteristic B, 1 A, 4-pole","NAB",29.02,0,29.02,8592765000767,3,18592765000764,36,28592765000761,"8536201090",0.48]
[100076,"Ex9BN 4P B2 ","Miniature Circuit  Breaker 6 kA, characteristic B, 2 A, 4-pole","NAB",29.02,0,29.02,8592765000774,3,18592765000771,36,28592765000778,"8536201090",0.48]
[100077,"Ex9BN 4P B3 ","Miniature Circuit  Breaker 6 kA, characteristic B, 3 A, 4-pole","NAB",29.02,0,29.02,8592765000781,3,18592765000788,36,28592765000785,"8536201090",0.48]
[100078,"Ex9BN 4P B4 ","Miniature Circuit  Breaker 6 kA, characteristic B, 4 A, 4-pole","NAB",29.02,0,29.02,8592765000798,3,18592765000795,36,28592765000792,"8536201090",0.48]
[100079,"Ex9BN 4P B6 ","Miniature Circuit  Breaker 6 kA, characteristic B, 6 A, 4-pole","NAB",29.02,0,29.02,8592765000804,3,18592765000801,36,28592765000808,"8536201090",0.48]
[100080,"Ex9BN 4P B8 ","Miniature Circuit  Breaker 6 kA, characteristic B, 8 A, 4-pole","NAB",29.02,0,29.02,8592765000811,3,18592765000818,36,28592765000815,"8536201090",0.48]
[100081,"Ex9BN 4P B10 ","Miniature Circuit  Breaker 6 kA, characteristic B, 10 A, 4-pole","NAB",25.86,0,25.86,8592765000828,3,18592765000825,36,28592765000822,"8536201090",0.48]
[100082,"Ex9BN 4P B13 ","Miniature Circuit  Breaker 6 kA, characteristic B, 13 A, 4-pole","NAB",25.86,0,25.86,8592765000835,3,18592765000832,36,28592765000839,"8536201090",0.48]
[100083,"Ex9BN 4P B16 ","Miniature Circuit  Breaker 6 kA, characteristic B, 16 A, 4-pole","NAB",25.86,0,25.86,8592765000842,3,18592765000849,36,28592765000846,"8536201090",0.48]
[100084,"Ex9BN 4P B20 ","Miniature Circuit  Breaker 6 kA, characteristic B, 20 A, 4-pole","NAB",25.86,0,25.86,8592765000859,3,18592765000856,36,28592765000853,"8536201090",0.48]
[100085,"Ex9BN 4P B25 ","Miniature Circuit  Breaker 6 kA, characteristic B, 25 A, 4-pole","NAB",25.86,0,25.86,8592765000866,3,18592765000863,36,28592765000860,"8536201090",0.48]
[100086,"Ex9BN 4P B32 ","Miniature Circuit  Breaker 6 kA, characteristic B, 32 A, 4-pole","NAB",38.04,0,38.04,8592765000873,3,18592765000870,36,28592765000877,"8536201090",0.48]
[100087,"Ex9BN 4P B40 ","Miniature Circuit  Breaker 6 kA, characteristic B, 40 A, 4-pole","NAB",38.04,0,38.04,8592765000880,3,18592765000887,36,28592765000884,"8536201090",0.48]
[100088,"Ex9BN 4P B50 ","Miniature Circuit  Breaker 6 kA, characteristic B, 50 A, 4-pole","NAB",50.52,0,50.52,8592765000897,3,18592765000894,36,28592765000891,"8536201090",0.48]
[100089,"Ex9BN 4P B63 ","Miniature Circuit  Breaker 6 kA, characteristic B, 63 A, 4-pole","NAB",50.52,0,50.52,8592765000903,3,18592765000900,36,28592765000907,"8536201090",0.48]
[100090,"Ex9BN 1P C1 ","Miniature Circuit  Breaker 6 kA, characteristic C, 1 A, 1-pole","NAB",4.2699999999999996,0,4.2699999999999996,8592765000910,12,18592765000917,144,28592765000914,"8536201090",0.12]
[100091,"Ex9BN 1P C2 ","Miniature Circuit  Breaker 6 kA, characteristic C, 2 A, 1-pole","NAB",4.2699999999999996,0,4.2699999999999996,8592765000927,12,18592765000924,144,28592765000921,"8536201090",0.12]
[100092,"Ex9BN 1P C3 ","Miniature Circuit  Breaker 6 kA, characteristic C, 3 A, 1-pole","NAB",4.2699999999999996,{"$f":"NAB","v":0},4.2699999999999996,8592765000934,12,18592765000931,144,28592765000938,"8536201090",0.12]
[100093,"Ex9BN 1P C4 ","Miniature Circuit  Breaker 6 kA, characteristic C, 4 A, 1-pole","NAB",4.2699999999999996,0,4.2699999999999996,8592765000941,12,18592765000948,144,28592765000945,"8536201090",0.12]
[100094,"Ex9BN 1P C6 ","Miniature Circuit  Breaker 6 kA, characteristic C, 6 A, 1-pole","NAB",4.09,0,4.09,8592765000958,12,18592765000955,144,28592765000952,"8536201090",0.12]
[100095,"Ex9BN 1P C8 ","Miniature Circuit  Breaker 6 kA, characteristic C, 8 A, 1-pole","NAB",4.09,0,4.09,8592765000965,12,18592765000962,144,28592765000969,"8536201090",0.12]
[100096,"Ex9BN 1P C10 ","Miniature Circuit  Breaker 6 kA, characteristic C, 10 A, 1-pole","NAB",3.62,0,3.62,8592765000972,12,18592765000979,144,28592765000976,"8536201090",0.12]
[100097,"Ex9BN 1P C13 ","Miniature Circuit  Breaker 6 kA, characteristic C, 13 A, 1-pole","NAB",3.62,0,3.62,8592765000989,12,18592765000986,144,28592765000983,"8536201090",0.12]
[100098,"Ex9BN 1P C16 ","Miniature Circuit  Breaker 6 kA, characteristic C, 16 A, 1-pole","NAB",3.62,0,3.62,8592765000996,12,18592765000993,144,28592765000990,"8536201090",0.12]
[100099,"Ex9BN 1P C20 ","Miniature Circuit  Breaker 6 kA, characteristic C, 20 A, 1-pole","NAB",3.62,0,3.62,8592765001009,12,18592765001006,144,28592765001003,"8536201090",0.12]
[100100,"Ex9BN 1P C25 ","Miniature Circuit  Breaker 6 kA, characteristic C, 25 A, 1-pole","NAB",3.62,0,3.62,8592765001016,12,18592765001013,144,28592765001010,"8536201090",0.12]
[100101,"Ex9BN 1P C32 ","Miniature Circuit  Breaker 6 kA, characteristic C, 32 A, 1-pole","NAB",4.6100000000000003,0,4.6100000000000003,8592765001023,12,18592765001020,144,28592765001027,"8536201090",0.12]
[100102,"Ex9BN 1P C40 ","Miniature Circuit  Breaker 6 kA, characteristic C, 40 A, 1-pole","NAB",4.6100000000000003,0,4.6100000000000003,8592765001030,12,18592765001037,144,28592765001034,"8536201090",0.12]
[100103,"Ex9BN 1P C50 ","Miniature Circuit  Breaker 6 kA, characteristic C, 50 A, 1-pole","NAB",8.09,0,8.09,8592765001047,12,18592765001044,144,28592765001041,"8536201090",0.12]
[100104,"Ex9BN 1P C63 ","Miniature Circuit  Breaker 6 kA, characteristic C, 63 A, 1-pole","NAB",8.09,0,8.09,8592765001054,12,18592765001051,144,28592765001058,"8536201090",0.12]
[100105,"Ex9BN 1PN C1 ","Miniature Circuit  Breaker 6 kA, characteristic C, 1 A, 1+Npole","NAB",8.82,0,8.82,8592765001061,6,18592765001068,72,28592765001065,"8536201090",0.24]
[100106,"Ex9BN 1PN C2 ","Miniature Circuit  Breaker 6 kA, characteristic C, 2 A, 1+Npole","NAB",8.82,0,8.82,8592765001078,6,18592765001075,72,28592765001072,"8536201090",0.24]
[100107,"Ex9BN 1PN C3 ","Miniature Circuit  Breaker 6 kA, characteristic C, 3 A, 1+Npole","NAB",8.82,0,8.82,8592765001085,6,18592765001082,72,28592765001089,"8536201090",0.24]
[100108,"Ex9BN 1PN C4 ","Miniature Circuit  Breaker 6 kA, characteristic C, 4 A, 1+Npole","NAB",8.82,0,8.82,8592765001092,6,18592765001099,72,28592765001096,"8536201090",0.24]
[100109,"Ex9BN 1PN C6 ","Miniature Circuit  Breaker 6 kA, characteristic C, 6 A, 1+Npole","NAB",8.82,0,8.82,8592765001108,6,18592765001105,72,28592765001102,"8536201090",0.24]
[100110,"Ex9BN 1PN C8 ","Miniature Circuit  Breaker 6 kA, characteristic C, 8 A, 1+Npole","NAB",8.82,0,8.82,8592765001115,6,18592765001112,72,28592765001119,"8536201090",0.24]
[100111,"Ex9BN 1PN C10 ","Miniature Circuit  Breaker 6 kA, characteristic C, 10 A, 1+Npole","NAB",7.82,0,7.82,8592765001122,6,18592765001129,72,28592765001126,"8536201090",0.24]
[100112,"Ex9BN 1PN C13 ","Miniature Circuit  Breaker 6 kA, characteristic C, 13 A, 1+Npole","NAB",7.82,0,7.82,8592765001139,6,18592765001136,72,28592765001133,"8536201090",0.24]
[100113,"Ex9BN 1PN C16 ","Miniature Circuit  Breaker 6 kA, characteristic C, 16 A, 1+Npole","NAB",7.82,0,7.82,8592765001146,6,18592765001143,72,28592765001140,"8536201090",0.24]
[100114,"Ex9BN 1PN C20 ","Miniature Circuit  Breaker 6 kA, characteristic C, 20 A, 1+Npole","NAB",7.82,0,7.82,8592765001153,6,18592765001150,72,28592765001157,"8536201090",0.24]
[100115,"Ex9BN 1PN C25 ","Miniature Circuit  Breaker 6 kA, characteristic C, 25 A, 1+Npole","NAB",7.82,0,7.82,8592765001160,6,18592765001167,72,28592765001164,"8536201090",0.24]
[100116,"Ex9BN 1PN C32 ","Miniature Circuit  Breaker 6 kA, characteristic C, 32 A, 1+Npole","NAB",9.94,0,9.94,8592765001177,6,18592765001174,72,28592765001171,"8536201090",0.24]
[100117,"Ex9BN 1PN C40 ","Miniature Circuit  Breaker 6 kA, characteristic C, 40 A, 1+Npole","NAB",9.94,0,9.94,8592765001184,6,18592765001181,72,28592765001188,"8536201090",0.24]
[100118,"Ex9BN 1PN C50 ","Miniature Circuit  Breaker 6 kA, characteristic C, 50 A, 1+Npole","NAB",17.440000000000001,0,17.440000000000001,8592765001191,6,18592765001198,72,28592765001195,"8536201090",0.24]
[100119,"Ex9BN 1PN C63 ","Miniature Circuit  Breaker 6 kA, characteristic C, 63 A, 1+Npole","NAB",17.440000000000001,0,17.440000000000001,8592765001207,6,18592765001204,72,28592765001201,"8536201090",0.24]
[100120,"Ex9BN 2P C1 ","Miniature Circuit  Breaker 6 kA, characteristic C, 1 A, 2-pole","NAB",10.48,0,10.48,8592765001214,6,18592765001211,72,28592765001218,"8536201090",0.24]
[100121,"Ex9BN 2P C2 ","Miniature Circuit  Breaker 6 kA, characteristic C, 2 A, 2-pole","NAB",10.48,0,10.48,8592765001221,6,18592765001228,72,28592765001225,"8536201090",0.24]
[100122,"Ex9BN 2P C3 ","Miniature Circuit  Breaker 6 kA, characteristic C, 3 A, 2-pole","NAB",10.48,0,10.48,8592765001238,6,18592765001235,72,28592765001232,"8536201090",0.24]
[100123,"Ex9BN 2P C4 ","Miniature Circuit  Breaker 6 kA, characteristic C, 4 A, 2-pole","NAB",10.48,0,10.48,8592765001245,6,18592765001242,72,28592765001249,"8536201090",0.24]
[100124,"Ex9BN 2P C6 ","Miniature Circuit  Breaker 6 kA, characteristic C, 6 A, 2-pole","NAB",10.48,0,10.48,8592765001252,6,18592765001259,72,28592765001256,"8536201090",0.24]
[100125,"Ex9BN 2P C8 ","Miniature Circuit  Breaker 6 kA, characteristic C, 8 A, 2-pole","NAB",10.48,0,10.48,8592765001269,6,18592765001266,72,28592765001263,"8536201090",0.24]
[100126,"Ex9BN 2P C10 ","Miniature Circuit  Breaker 6 kA, characteristic C, 10 A, 2-pole","NAB",8.92,0,8.92,8592765001276,6,18592765001273,72,28592765001270,"8536201090",0.24]
[100127,"Ex9BN 2P C13 ","Miniature Circuit  Breaker 6 kA, characteristic C, 13 A, 2-pole","NAB",8.92,0,8.92,8592765001283,6,18592765001280,72,28592765001287,"8536201090",0.24]
[100128,"Ex9BN 2P C16 ","Miniature Circuit  Breaker 6 kA, characteristic C, 16 A, 2-pole","NAB",8.92,0,{"$f":"E407*(1-F407)","v":8.92},8592765001290,6,18592765001297,72,28592765001294,"8536201090",0.24]
[100129,"Ex9BN 2P C20 ","Miniature Circuit  Breaker 6 kA, characteristic C, 20 A, 2-pole","NAB",8.92,0,8.92,8592765001306,6,18592765001303,72,28592765001300,"8536201090",0.24]
[100130,"Ex9BN 2P C25 ","Miniature Circuit  Breaker 6 kA, characteristic C, 25 A, 2-pole","NAB",8.92,0,8.92,8592765001313,6,18592765001310,72,28592765001317,"8536201090",0.24]
[100131,"Ex9BN 2P C32 ","Miniature Circuit  Breaker 6 kA, characteristic C, 32 A, 2-pole","NAB",11.89,0,11.89,8592765001320,6,18592765001327,72,28592765001324,"8536201090",0.24]
[100132,"Ex9BN 2P C40 ","Miniature Circuit  Breaker 6 kA, characteristic C, 40 A, 2-pole","NAB",11.89,0,11.89,8592765001337,6,18592765001334,72,28592765001331,"8536201090",0.24]
[100133,"Ex9BN 2P C50 ","Miniature Circuit  Breaker 6 kA, characteristic C, 50 A, 2-pole","NAB",22.08,0,22.08,8592765001344,6,18592765001341,72,28592765001348,"8536201090",0.24]
[100134,"Ex9BN 2P C63 ","Miniature Circuit  Breaker 6 kA, characteristic C, 63 A, 2-pole","NAB",22.08,0,22.08,8592765001351,6,18592765001358,72,28592765001355,"8536201090",0.24]
[100135,"Ex9BN 3P C1 ","Miniature Circuit  Breaker 6 kA, characteristic C, 1 A, 3-pole","NAB",13.68,0,13.68,8592765001368,4,18592765001365,48,28592765001362,"8536201090",0.36]
[100136,"Ex9BN 3P C2 ","Miniature Circuit  Breaker 6 kA, characteristic C, 2 A, 3-pole","NAB",13.68,0,13.68,8592765001375,4,18592765001372,48,28592765001379,"8536201090",0.36]
[100137,"Ex9BN 3P C3 ","Miniature Circuit  Breaker 6 kA, characteristic C, 3 A, 3-pole","NAB",13.68,0,13.68,8592765001382,4,18592765001389,48,28592765001386,"8536201090",0.36]
[100138,"Ex9BN 3P C4 ","Miniature Circuit  Breaker 6 kA, characteristic C, 4 A, 3-pole","NAB",13.68,0,13.68,8592765001399,4,18592765001396,48,28592765001393,"8536201090",0.36]
[100139,"Ex9BN 3P C6 ","Miniature Circuit  Breaker 6 kA, characteristic C, 6 A, 3-pole","NAB",13.68,0,13.68,8592765001405,4,18592765001402,48,28592765001409,"8536201090",0.36]
[100140,"Ex9BN 3P C8 ","Miniature Circuit  Breaker 6 kA, characteristic C, 8 A, 3-pole","NAB",13.68,0,13.68,8592765001412,4,18592765001419,48,28592765001416,"8536201090",0.36]
[100141,"Ex9BN 3P C10 ","Miniature Circuit  Breaker 6 kA, characteristic C, 10 A, 3-pole","NAB",12.15,0,12.15,8592765001429,4,18592765001426,48,28592765001423,"8536201090",0.36]
[100142,"Ex9BN 3P C13 ","Miniature Circuit  Breaker 6 kA, characteristic C, 13 A, 3-pole","NAB",12.15,0,12.15,8592765001436,4,18592765001433,48,28592765001430,"8536201090",0.36]
[100143,"Ex9BN 3P C16 ","Miniature Circuit  Breaker 6 kA, characteristic C, 16 A, 3-pole","NAB",12.15,0,12.15,8592765001443,4,18592765001440,48,28592765001447,"8536201090",0.36]
[100144,"Ex9BN 3P C20 ","Miniature Circuit  Breaker 6 kA, characteristic C, 20 A, 3-pole","NAB",12.15,0,12.15,8592765001450,4,18592765001457,48,28592765001454,"8536201090",0.36]
[100145,"Ex9BN 3P C25 ","Miniature Circuit  Breaker 6 kA, characteristic C, 25 A, 3-pole","NAB",12.15,0,12.15,8592765001467,4,18592765001464,48,28592765001461,"8536201090",0.36]
[100146,"Ex9BN 3P C32 ","Miniature Circuit  Breaker 6 kA, characteristic C, 32 A, 3-pole","NAB",13.68,0,13.68,8592765001474,4,18592765001471,48,28592765001478,"8536201090",0.36]
[100147,"Ex9BN 3P C40 ","Miniature Circuit  Breaker 6 kA, characteristic C, 40 A, 3-pole","NAB",13.68,0,13.68,8592765001481,4,18592765001488,48,28592765001485,"8536201090",0.36]
[100148,"Ex9BN 3P C50 ","Miniature Circuit  Breaker 6 kA, characteristic C, 50 A, 3-pole","NAB",22.59,0,22.59,8592765001498,4,18592765001495,48,28592765001492,"8536201090",0.36]
[100149,"Ex9BN 3P C63 ","Miniature Circuit  Breaker 6 kA, characteristic C, 63 A, 3-pole","NAB",22.59,0,22.59,8592765001504,4,18592765001501,48,28592765001508,"8536201090",0.36]
[100150,"Ex9BN 3PN C1 ","Miniature Circuit  Breaker 6 kA, characteristic C, 1 A, 3+Npole","NAB",25.19,0,25.19,8592765001511,3,18592765001518,36,28592765001515,"8536201090",0.48]
[100151,"Ex9BN 3PN C2 ","Miniature Circuit  Breaker 6 kA, characteristic C, 2 A, 3+Npole","NAB",25.19,0,25.19,8592765001528,3,18592765001525,36,28592765001522,"8536201090",0.48]
[100152,"Ex9BN 3PN C3 ","Miniature Circuit  Breaker 6 kA, characteristic C, 3 A, 3+Npole","NAB",25.19,0,25.19,8592765001535,3,18592765001532,36,28592765001539,"8536201090",0.48]
[100153,"Ex9BN 3PN C4 ","Miniature Circuit  Breaker 6 kA, characteristic C, 4 A, 3+Npole","NAB",25.19,0,25.19,8592765001542,3,18592765001549,36,28592765001546,"8536201090",0.48]
[100154,"Ex9BN 3PN C6 ","Miniature Circuit  Breaker 6 kA, characteristic C, 6 A, 3+Npole","NAB",25.19,0,25.19,8592765001559,3,18592765001556,36,28592765001553,"8536201090",0.48]
[100155,"Ex9BN 3PN C8 ","Miniature Circuit  Breaker 6 kA, characteristic C, 8 A, 3+Npole","NAB",25.19,0,25.19,8592765001566,3,18592765001563,36,28592765001560,"8536201090",0.48]
[100156,"Ex9BN 3PN C10 ","Miniature Circuit  Breaker 6 kA, characteristic C, 10 A, 3+Npole","NAB",22.27,{"$f":"NAB","v":0},22.27,8592765001573,3,18592765001570,36,28592765001577,"8536201090",0.48]
[100157,"Ex9BN 3PN C13 ","Miniature Circuit  Breaker 6 kA, characteristic C, 13 A, 3+Npole","NAB",22.27,0,22.27,8592765001580,3,18592765001587,36,28592765001584,"8536201090",0.48]
[100158,"Ex9BN 3PN C16 ","Miniature Circuit  Breaker 6 kA, characteristic C, 16 A, 3+Npole","NAB",22.27,0,22.27,8592765001597,3,18592765001594,36,28592765001591,"8536201090",0.48]
[100159,"Ex9BN 3PN C20 ","Miniature Circuit  Breaker 6 kA, characteristic C, 20 A, 3+Npole","NAB",22.27,0,22.27,8592765001603,3,18592765001600,36,28592765001607,"8536201090",0.48]
[100160,"Ex9BN 3PN C25 ","Miniature Circuit  Breaker 6 kA, characteristic C, 25 A, 3+Npole","NAB",22.27,0,22.27,8592765001610,3,18592765001617,36,28592765001614,"8536201090",0.48]
[100161,"Ex9BN 3PN C32 ","Miniature Circuit  Breaker 6 kA, characteristic C, 32 A, 3+Npole","NAB",25.24,0,25.24,8592765001627,3,18592765001624,36,28592765001621,"8536201090",0.48]
[100162,"Ex9BN 3PN C40 ","Miniature Circuit  Breaker 6 kA, characteristic C, 40 A, 3+Npole","NAB",25.24,0,25.24,8592765001634,3,18592765001631,36,28592765001638,"8536201090",0.48]
[100163,"Ex9BN 3PN C50 ","Miniature Circuit  Breaker 6 kA, characteristic C, 50 A, 3+Npole","NAB",44.18,0,44.18,8592765001641,3,18592765001648,36,28592765001645,"8536201090",0.48]
[100164,"Ex9BN 3PN C63 ","Miniature Circuit  Breaker 6 kA, characteristic C, 63 A, 3+Npole","NAB",44.18,0,44.18,8592765001658,3,18592765001655,36,28592765001652,"8536201090",0.48]
[100165,"Ex9BN 4P C1 ","Miniature Circuit  Breaker 6 kA, characteristic C, 1 A, 4-pole","NAB",28.97,0,28.97,8592765001665,3,18592765001662,36,28592765001669,"8536201090",0.48]
[100166,"Ex9BN 4P C2 ","Miniature Circuit  Breaker 6 kA, characteristic C, 2 A, 4-pole","NAB",28.97,0,28.97,8592765001672,3,18592765001679,36,28592765001676,"8536201090",0.48]
[100167,"Ex9BN 4P C3 ","Miniature Circuit  Breaker 6 kA, characteristic C, 3 A, 4-pole","NAB",28.97,0,28.97,8592765001689,3,18592765001686,36,28592765001683,"8536201090",0.48]
[100168,"Ex9BN 4P C4 ","Miniature Circuit  Breaker 6 kA, characteristic C, 4 A, 4-pole","NAB",28.97,0,28.97,8592765001696,3,18592765001693,36,28592765001690,"8536201090",0.48]
[100169,"Ex9BN 4P C6 ","Miniature Circuit  Breaker 6 kA, characteristic C, 6 A, 4-pole","NAB",28.97,0,28.97,8592765001702,3,18592765001709,36,28592765001706,"8536201090",0.48]
[100170,"Ex9BN 4P C8 ","Miniature Circuit  Breaker 6 kA, characteristic C, 8 A, 4-pole","NAB",28.97,0,28.97,8592765001719,3,18592765001716,36,28592765001713,"8536201090",0.48]
[100171,"Ex9BN 4P C10 ","Miniature Circuit  Breaker 6 kA, characteristic C, 10 A, 4-pole","NAB",25.72,0,25.72,8592765001726,3,18592765001723,36,28592765001720,"8536201090",0.48]
[100172,"Ex9BN 4P C13 ","Miniature Circuit  Breaker 6 kA, characteristic C, 13 A, 4-pole","NAB",25.72,0,25.72,8592765001733,3,18592765001730,36,28592765001737,"8536201090",0.48]
[100173,"Ex9BN 4P C16 ","Miniature Circuit  Breaker 6 kA, characteristic C, 16 A, 4-pole","NAB",25.72,0,25.72,8592765001740,3,18592765001747,36,28592765001744,"8536201090",0.48]
[100174,"Ex9BN 4P C20 ","Miniature Circuit  Breaker 6 kA, characteristic C, 20 A, 4-pole","NAB",25.72,0,25.72,8592765001757,3,18592765001754,36,28592765001751,"8536201090",0.48]
[100175,"Ex9BN 4P C25 ","Miniature Circuit  Breaker 6 kA, characteristic C, 25 A, 4-pole","NAB",25.72,0,25.72,8592765001764,3,18592765001761,36,28592765001768,"8536201090",0.48]
[100176,"Ex9BN 4P C32 ","Miniature Circuit  Breaker 6 kA, characteristic C, 32 A, 4-pole","NAB",29.11,0,29.11,8592765001771,3,18592765001778,36,28592765001775,"8536201090",0.48]
[100177,"Ex9BN 4P C40 ","Miniature Circuit  Breaker 6 kA, characteristic C, 40 A, 4-pole","NAB",29.11,0,29.11,8592765001788,3,18592765001785,36,28592765001782,"8536201090",0.48]
[100178,"Ex9BN 4P C50 ","Miniature Circuit  Breaker 6 kA, characteristic C, 50 A, 4-pole","NAB",51.79,0,51.79,8592765001795,3,18592765001792,36,28592765001799,"8536201090",0.48]
[100179,"Ex9BN 4P C63 ","Miniature Circuit  Breaker 6 kA, characteristic C, 63 A, 4-pole","NAB",51.79,0,51.79,8592765001801,3,18592765001808,36,28592765001805,"8536201090",0.48]
[100180,"Ex9BN 1P D1 ","Miniature Circuit  Breaker 6 kA, characteristic D, 1 A, 1-pole","NAB",6.33,0,6.33,8592765001818,12,18592765001815,144,28592765001812,"8536201090",0.12]
[100181,"Ex9BN 1P D2 ","Miniature Circuit  Breaker 6 kA, characteristic D, 2 A, 1-pole","NAB",6.33,0,6.33,8592765001825,12,18592765001822,144,28592765001829,"8536201090",0.12]
[100182,"Ex9BN 1P D3 ","Miniature Circuit  Breaker 6 kA, characteristic D, 3 A, 1-pole","NAB",6.33,0,6.33,8592765001832,12,18592765001839,144,28592765001836,"8536201090",0.12]
[100183,"Ex9BN 1P D4 ","Miniature Circuit  Breaker 6 kA, characteristic D, 4 A, 1-pole","NAB",6.33,0,6.33,8592765001849,12,18592765001846,144,28592765001843,"8536201090",0.12]
[100184,"Ex9BN 1P D6 ","Miniature Circuit  Breaker 6 kA, characteristic D, 6 A, 1-pole","NAB",6.21,0,6.21,8592765001856,12,18592765001853,144,28592765001850,"8536201090",0.12]
[100185,"Ex9BN 1P D8 ","Miniature Circuit  Breaker 6 kA, characteristic D, 8 A, 1-pole","NAB",6.21,0,6.21,8592765001863,12,18592765001860,144,28592765001867,"8536201090",0.12]
[100186,"Ex9BN 1P D10 ","Miniature Circuit  Breaker 6 kA, characteristic D, 10 A, 1-pole","NAB",5.22,0,5.22,8592765001870,12,18592765001877,144,28592765001874,"8536201090",0.12]
[100187,"Ex9BN 1P D13 ","Miniature Circuit  Breaker 6 kA, characteristic D, 13 A, 1-pole","NAB",5.22,0,5.22,8592765001887,12,18592765001884,144,28592765001881,"8536201090",0.12]
[100188,"Ex9BN 1P D16 ","Miniature Circuit  Breaker 6 kA, characteristic D, 16 A, 1-pole","NAB",5.22,0,5.22,8592765001894,12,18592765001891,144,28592765001898,"8536201090",0.12]
[100189,"Ex9BN 1P D20 ","Miniature Circuit  Breaker 6 kA, characteristic D, 20 A, 1-pole","NAB",5.22,0,5.22,8592765001900,12,18592765001907,144,28592765001904,"8536201090",0.12]
[100190,"Ex9BN 1P D25 ","Miniature Circuit  Breaker 6 kA, characteristic D, 25 A, 1-pole","NAB",5.22,0,5.22,8592765001917,12,18592765001914,144,28592765001911,"8536201090",0.12]
[100191,"Ex9BN 1P D32 ","Miniature Circuit  Breaker 6 kA, characteristic D, 32 A, 1-pole","NAB",7.21,0,7.21,8592765001924,12,18592765001921,144,28592765001928,"8536201090",0.12]
[100192,"Ex9BN 1P D40 ","Miniature Circuit  Breaker 6 kA, characteristic D, 40 A, 1-pole","NAB",7.21,0,{"$f":"E471*(1-F471)","v":7.21},8592765001931,12,18592765001938,144,28592765001935,"8536201090",0.12]
[100193,"Ex9BN 1P D50 ","Miniature Circuit  Breaker 6 kA, characteristic D, 50 A, 1-pole","NAB",18.690000000000001,0,18.690000000000001,8592765001948,12,18592765001945,144,28592765001942,"8536201090",0.12]
[100194,"Ex9BN 1P D63 ","Miniature Circuit  Breaker 6 kA, characteristic D, 63 A, 1-pole","NAB",18.690000000000001,0,18.690000000000001,8592765001955,12,18592765001952,144,28592765001959,"8536201090",0.12]
[100195,"Ex9BN 1PN D1 ","Miniature Circuit  Breaker 6 kA, characteristic D, 1 A, 1+Npole","NAB",11.36,0,11.36,8592765001962,6,18592765001969,72,28592765001966,"8536201090",0.24]
[100196,"Ex9BN 1PN D2 ","Miniature Circuit  Breaker 6 kA, characteristic D, 2 A, 1+Npole","NAB",11.36,0,11.36,8592765001979,6,18592765001976,72,28592765001973,"8536201090",0.24]
[100197,"Ex9BN 1PN D3 ","Miniature Circuit  Breaker 6 kA, characteristic D, 3 A, 1+Npole","NAB",11.36,0,11.36,8592765001986,6,18592765001983,72,28592765001980,"8536201090",0.24]
[100198,"Ex9BN 1PN D4 ","Miniature Circuit  Breaker 6 kA, characteristic D, 4 A, 1+Npole","NAB",11.36,0,11.36,8592765001993,6,18592765001990,72,28592765001997,"8536201090",0.24]
[100199,"Ex9BN 1PN D6 ","Miniature Circuit  Breaker 6 kA, characteristic D, 6 A, 1+Npole","NAB",11.36,0,11.36,8592765002006,6,18592765002003,72,28592765002000,"8536201090",0.24]
[100200,"Ex9BN 1PN D8 ","Miniature Circuit  Breaker 6 kA, characteristic D, 8 A, 1+Npole","NAB",11.36,0,11.36,8592765002013,6,18592765002010,72,28592765002017,"8536201090",0.24]
[100201,"Ex9BN 1PN D10 ","Miniature Circuit  Breaker 6 kA, characteristic D, 10 A, 1+Npole","NAB",11,0,11,8592765002020,6,18592765002027,72,28592765002024,"8536201090",0.24]
[100202,"Ex9BN 1PN D13 ","Miniature Circuit  Breaker 6 kA, characteristic D, 13 A, 1+Npole","NAB",11,0,11,8592765002037,6,18592765002034,72,28592765002031,"8536201090",0.24]
[100203,"Ex9BN 1PN D16 ","Miniature Circuit  Breaker 6 kA, characteristic D, 16 A, 1+Npole","NAB",11,0,11,8592765002044,6,18592765002041,72,28592765002048,"8536201090",0.24]
[100204,"Ex9BN 1PN D20 ","Miniature Circuit  Breaker 6 kA, characteristic D, 20 A, 1+Npole","NAB",11,0,11,8592765002051,6,18592765002058,72,28592765002055,"8536201090",0.24]
[100205,"Ex9BN 1PN D25 ","Miniature Circuit  Breaker 6 kA, characteristic D, 25 A, 1+Npole","NAB",11,0,11,8592765002068,6,18592765002065,72,28592765002062,"8536201090",0.24]
[100206,"Ex9BN 1PN D32 ","Miniature Circuit  Breaker 6 kA, characteristic D, 32 A, 1+Npole","NAB",13.6,0,13.6,8592765002075,6,18592765002072,72,28592765002079,"8536201090",0.24]
[100207,"Ex9BN 1PN D40 ","Miniature Circuit  Breaker 6 kA, characteristic D, 40 A, 1+Npole","NAB",13.6,0,13.6,8592765002082,6,18592765002089,72,28592765002086,"8536201090",0.24]
[100208,"Ex9BN 1PN D50 ","Miniature Circuit  Breaker 6 kA, characteristic D, 50 A, 1+Npole","NAB",30.45,0,30.45,8592765002099,6,18592765002096,72,28592765002093,"8536201090",0.24]
[100209,"Ex9BN 1PN D63 ","Miniature Circuit  Breaker 6 kA, characteristic D, 63 A, 1+Npole","NAB",30.45,0,30.45,8592765002105,6,18592765002102,72,28592765002109,"8536201090",0.24]
[100210,"Ex9BN 2P D1 ","Miniature Circuit  Breaker 6 kA, characteristic D, 1 A, 2-pole","NAB",13.35,0,13.35,8592765002112,6,18592765002119,72,28592765002116,"8536201090",0.24]
[100211,"Ex9BN 2P D2 ","Miniature Circuit  Breaker 6 kA, characteristic D, 2 A, 2-pole","NAB",13.35,0,13.35,8592765002129,6,18592765002126,72,28592765002123,"8536201090",0.24]
[100212,"Ex9BN 2P D3 ","Miniature Circuit  Breaker 6 kA, characteristic D, 3 A, 2-pole","NAB",13.35,0,13.35,8592765002136,6,18592765002133,72,28592765002130,"8536201090",0.24]
[100213,"Ex9BN 2P D4 ","Miniature Circuit  Breaker 6 kA, characteristic D, 4 A, 2-pole","NAB",13.35,0,13.35,8592765002143,6,18592765002140,72,28592765002147,"8536201090",0.24]
[100214,"Ex9BN 2P D6 ","Miniature Circuit  Breaker 6 kA, characteristic D, 6 A, 2-pole","NAB",13.35,0,13.35,8592765002150,6,18592765002157,72,28592765002154,"8536201090",0.24]
[100215,"Ex9BN 2P D8 ","Miniature Circuit  Breaker 6 kA, characteristic D, 8 A, 2-pole","NAB",13.35,0,13.35,8592765002167,6,18592765002164,72,28592765002161,"8536201090",0.24]
[100216,"Ex9BN 2P D10 ","Miniature Circuit  Breaker 6 kA, characteristic D, 10 A, 2-pole","NAB",12.97,0,12.97,8592765002174,6,18592765002171,72,28592765002178,"8536201090",0.24]
[100217,"Ex9BN 2P D13 ","Miniature Circuit  Breaker 6 kA, characteristic D, 13 A, 2-pole","NAB",12.97,0,12.97,8592765002181,6,18592765002188,72,28592765002185,"8536201090",0.24]
[100218,"Ex9BN 2P D16 ","Miniature Circuit  Breaker 6 kA, characteristic D, 16 A, 2-pole","NAB",12.97,0,12.97,8592765002198,6,18592765002195,72,28592765002192,"8536201090",0.24]
[100219,"Ex9BN 2P D20 ","Miniature Circuit  Breaker 6 kA, characteristic D, 20 A, 2-pole","NAB",12.97,0,12.97,8592765002204,6,18592765002201,72,28592765002208,"8536201090",0.24]
[100220,"Ex9BN 2P D25 ","Miniature Circuit  Breaker 6 kA, characteristic D, 25 A, 2-pole","NAB",12.97,{"$f":"NAB","v":0},12.97,8592765002211,6,18592765002218,72,28592765002215,"8536201090",0.24]
[100221,"Ex9BN 2P D32 ","Miniature Circuit  Breaker 6 kA, characteristic D, 32 A, 2-pole","NAB",15.94,0,15.94,8592765002228,6,18592765002225,72,28592765002222,"8536201090",0.24]
[100222,"Ex9BN 2P D40 ","Miniature Circuit  Breaker 6 kA, characteristic D, 40 A, 2-pole","NAB",15.94,0,15.94,8592765002235,6,18592765002232,72,28592765002239,"8536201090",0.24]
[100223,"Ex9BN 2P D50 ","Miniature Circuit  Breaker 6 kA, characteristic D, 50 A, 2-pole","NAB",37.6,0,37.6,8592765002242,6,18592765002249,72,28592765002246,"8536201090",0.24]
[100224,"Ex9BN 2P D63 ","Miniature Circuit  Breaker 6 kA, characteristic D, 63 A, 2-pole","NAB",37.6,0,37.6,8592765002259,6,18592765002256,72,28592765002253,"8536201090",0.24]
[100225,"Ex9BN 3P D1 ","Miniature Circuit  Breaker 6 kA, characteristic D, 1 A, 3-pole","NAB",21.83,{"$f":"NAB","v":0},21.83,8592765002266,4,18592765002263,48,28592765002260,"8536201090",0.36]
[100226,"Ex9BN 3P D2 ","Miniature Circuit  Breaker 6 kA, characteristic D, 2 A, 3-pole","NAB",21.83,0,21.83,8592765002273,4,18592765002270,48,28592765002277,"8536201090",0.36]
[100227,"Ex9BN 3P D3 ","Miniature Circuit  Breaker 6 kA, characteristic D, 3 A, 3-pole","NAB",21.83,0,21.83,8592765002280,4,18592765002287,48,28592765002284,"8536201090",0.36]
[100228,"Ex9BN 3P D4 ","Miniature Circuit  Breaker 6 kA, characteristic D, 4 A, 3-pole","NAB",21.83,0,21.83,8592765002297,4,18592765002294,48,28592765002291,"8536201090",0.36]
[100229,"Ex9BN 3P D6 ","Miniature Circuit  Breaker 6 kA, characteristic D, 6 A, 3-pole","NAB",21.83,0,21.83,8592765002303,4,18592765002300,48,28592765002307,"8536201090",0.36]
[100230,"Ex9BN 3P D8 ","Miniature Circuit  Breaker 6 kA, characteristic D, 8 A, 3-pole","NAB",21.83,0,21.83,8592765002310,4,18592765002317,48,28592765002314,"8536201090",0.36]
[100231,"Ex9BN 3P D10 ","Miniature Circuit  Breaker 6 kA, characteristic D, 10 A, 3-pole","NAB",19.010000000000002,0,19.010000000000002,8592765002327,4,18592765002324,48,28592765002321,"8536201090",0.36]
[100232,"Ex9BN 3P D13 ","Miniature Circuit  Breaker 6 kA, characteristic D, 13 A, 3-pole","NAB",19.010000000000002,0,19.010000000000002,8592765002334,4,18592765002331,48,28592765002338,"8536201090",0.36]
[100233,"Ex9BN 3P D16 ","Miniature Circuit  Breaker 6 kA, characteristic D, 16 A, 3-pole","NAB",19.010000000000002,0,19.010000000000002,8592765002341,4,18592765002348,48,28592765002345,"8536201090",0.36]
[100234,"Ex9BN 3P D20 ","Miniature Circuit  Breaker 6 kA, characteristic D, 20 A, 3-pole","NAB",19.010000000000002,0,19.010000000000002,8592765002358,4,18592765002355,48,28592765002352,"8536201090",0.36]
[100235,"Ex9BN 3P D25 ","Miniature Circuit  Breaker 6 kA, characteristic D, 25 A, 3-pole","NAB",19.010000000000002,0,19.010000000000002,8592765002365,4,18592765002362,48,28592765002369,"8536201090",0.36]
[100236,"Ex9BN 3P D32 ","Miniature Circuit  Breaker 6 kA, characteristic D, 32 A, 3-pole","NAB",25.44,0,25.44,8592765002372,4,18592765002379,48,28592765002376,"8536201090",0.36]
[100237,"Ex9BN 3P D40 ","Miniature Circuit  Breaker 6 kA, characteristic D, 40 A, 3-pole","NAB",25.44,0,25.44,8592765002389,4,18592765002386,48,28592765002383,"8536201090",0.36]
[100238,"Ex9BN 3P D50 ","Miniature Circuit  Breaker 6 kA, characteristic D, 50 A, 3-pole","NAB",31.21,0,31.21,8592765002396,4,18592765002393,48,28592765002390,"8536201090",0.36]
[100239,"Ex9BN 3P D63 ","Miniature Circuit  Breaker 6 kA, characteristic D, 63 A, 3-pole","NAB",31.21,0,31.21,8592765002402,4,18592765002409,48,28592765002406,"8536201090",0.36]
[100240,"Ex9BN 3PN D1 ","Miniature Circuit  Breaker 6 kA, characteristic D, 1 A, 3+Npole","NAB",33.15,0,33.15,8592765002419,3,18592765002416,36,28592765002413,"8536201090",0.48]
[100241,"Ex9BN 3PN D2 ","Miniature Circuit  Breaker 6 kA, characteristic D, 2 A, 3+Npole","NAB",33.15,0,33.15,8592765002426,3,18592765002423,36,28592765002420,"8536201090",0.48]
[100242,"Ex9BN 3PN D3 ","Miniature Circuit  Breaker 6 kA, characteristic D, 3 A, 3+Npole","NAB",33.15,0,33.15,8592765002433,3,18592765002430,36,28592765002437,"8536201090",0.48]
[100243,"Ex9BN 3PN D4 ","Miniature Circuit  Breaker 6 kA, characteristic D, 4 A, 3+Npole","NAB",33.15,0,33.15,8592765002440,3,18592765002447,36,28592765002444,"8536201090",0.48]
[100244,"Ex9BN 3PN D6 ","Miniature Circuit  Breaker 6 kA, characteristic D, 6 A, 3+Npole","NAB",33.15,0,33.15,8592765002457,3,18592765002454,36,28592765002451,"8536201090",0.48]
[100245,"Ex9BN 3PN D8 ","Miniature Circuit  Breaker 6 kA, characteristic D, 8 A, 3+Npole","NAB",33.15,0,33.15,8592765002464,3,18592765002461,36,28592765002468,"8536201090",0.48]
[100246,"Ex9BN 3PN D10 ","Miniature Circuit  Breaker 6 kA, characteristic D, 10 A, 3+Npole","NAB",31.32,0,31.32,8592765002471,3,18592765002478,36,28592765002475,"8536201090",0.48]
[100247,"Ex9BN 3PN D13 ","Miniature Circuit  Breaker 6 kA, characteristic D, 13 A, 3+Npole","NAB",31.32,0,31.32,8592765002488,3,18592765002485,36,28592765002482,"8536201090",0.48]
[100248,"Ex9BN 3PN D16 ","Miniature Circuit  Breaker 6 kA, characteristic D, 16 A, 3+Npole","NAB",31.32,{"$f":"NAB","v":0},31.32,8592765002495,3,18592765002492,36,28592765002499,"8536201090",0.48]
[100249,"Ex9BN 3PN D20 ","Miniature Circuit  Breaker 6 kA, characteristic D, 20 A, 3+Npole","NAB",31.32,0,31.32,8592765002501,3,18592765002508,36,28592765002505,"8536201090",0.48]
[100250,"Ex9BN 3PN D25 ","Miniature Circuit  Breaker 6 kA, characteristic D, 25 A, 3+Npole","NAB",31.32,0,31.32,8592765002518,3,18592765002515,36,28592765002512,"8536201090",0.48]
[100251,"Ex9BN 3PN D32 ","Miniature Circuit  Breaker 6 kA, characteristic D, 32 A, 3+Npole","NAB",40.74,0,40.74,8592765002525,3,18592765002522,36,28592765002529,"8536201090",0.48]
[100252,"Ex9BN 3PN D40 ","Miniature Circuit  Breaker 6 kA, characteristic D, 40 A, 3+Npole","NAB",40.74,0,40.74,8592765002532,3,18592765002539,36,28592765002536,"8536201090",0.48]
[100253,"Ex9BN 3PN D50 ","Miniature Circuit  Breaker 6 kA, characteristic D, 50 A, 3+Npole","NAB",44.36,0,44.36,8592765002549,3,18592765002546,36,28592765002543,"8536201090",0.48]
[100254,"Ex9BN 3PN D63 ","Miniature Circuit  Breaker 6 kA, characteristic D, 63 A, 3+Npole","NAB",44.36,0,44.36,8592765002556,3,18592765002553,36,28592765002550,"8536201090",0.48]
[100255,"Ex9BN 4P D1 ","Miniature Circuit  Breaker 6 kA, characteristic D, 1 A, 4-pole","NAB",38.33,0,38.33,8592765002563,3,18592765002560,36,28592765002567,"8536201090",0.48]
[100256,"Ex9BN 4P D2 ","Miniature Circuit  Breaker 6 kA, characteristic D, 2 A, 4-pole","NAB",38.33,0,{"$f":"E535*(1-F535)","v":38.33},8592765002570,3,18592765002577,36,28592765002574,"8536201090",0.48]
[100257,"Ex9BN 4P D3 ","Miniature Circuit  Breaker 6 kA, characteristic D, 3 A, 4-pole","NAB",38.33,0,38.33,8592765002587,3,18592765002584,36,28592765002581,"8536201090",0.48]
[100258,"Ex9BN 4P D4 ","Miniature Circuit  Breaker 6 kA, characteristic D, 4 A, 4-pole","NAB",38.33,0,38.33,8592765002594,3,18592765002591,36,28592765002598,"8536201090",0.48]
[100259,"Ex9BN 4P D6 ","Miniature Circuit  Breaker 6 kA, characteristic D, 6 A, 4-pole","NAB",38.33,0,38.33,8592765002600,3,18592765002607,36,28592765002604,"8536201090",0.48]
[100260,"Ex9BN 4P D8 ","Miniature Circuit  Breaker 6 kA, characteristic D, 8 A, 4-pole","NAB",38.33,0,38.33,8592765002617,3,18592765002614,36,28592765002611,"8536201090",0.48]
[100261,"Ex9BN 4P D10 ","Miniature Circuit  Breaker 6 kA, characteristic D, 10 A, 4-pole","NAB",36.01,0,36.01,8592765002624,3,18592765002621,36,28592765002628,"8536201090",0.48]
[100262,"Ex9BN 4P D13 ","Miniature Circuit  Breaker 6 kA, characteristic D, 13 A, 4-pole","NAB",36.01,0,36.01,8592765002631,3,18592765002638,36,28592765002635,"8536201090",0.48]
[100263,"Ex9BN 4P D16 ","Miniature Circuit  Breaker 6 kA, characteristic D, 16 A, 4-pole","NAB",36.01,0,36.01,8592765002648,3,18592765002645,36,28592765002642,"8536201090",0.48]
[100264,"Ex9BN 4P D20 ","Miniature Circuit  Breaker 6 kA, characteristic D, 20 A, 4-pole","NAB",36.01,0,36.01,8592765002655,3,18592765002652,36,28592765002659,"8536201090",0.48]
[100265,"Ex9BN 4P D25 ","Miniature Circuit  Breaker 6 kA, characteristic D, 25 A, 4-pole","NAB",36.01,0,36.01,8592765002662,3,18592765002669,36,28592765002666,"8536201090",0.48]
[100266,"Ex9BN 4P D32 ","Miniature Circuit  Breaker 6 kA, characteristic D, 32 A, 4-pole","NAB",46.94,0,46.94,8592765002679,3,18592765002676,36,28592765002673,"8536201090",0.48]
[100267,"Ex9BN 4P D40 ","Miniature Circuit  Breaker 6 kA, characteristic D, 40 A, 4-pole","NAB",46.94,0,46.94,8592765002686,3,18592765002683,36,28592765002680,"8536201090",0.48]
[100268,"Ex9BN 4P D50 ","Miniature Circuit  Breaker 6 kA, characteristic D, 50 A, 4-pole","NAB",49.92,0,49.92,8592765002693,3,18592765002690,36,28592765002697,"8536201090",0.48]
[100269,"Ex9BN 4P D63 ","Miniature Circuit  Breaker 6 kA, characteristic D, 63 A, 4-pole","NAB",49.92,0,49.92,8592765002709,3,18592765002706,36,28592765002703,"8536201090",0.48]
[]
["Miniature Circuit  Breakers Ex9BS, 4,5 kA"]
[102030,"Ex9BS 1P B6 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 6 A, 1-pole","NAK",3.58,{"$f":"NAK","v":0},{"$f":"E551*(1-F551)","v":3.58},8592765020314,12,18592765020311,144,28592765020318,"8536201090",0.12]
[102031,"Ex9BS 1P B8 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 8 A, 1-pole","NAK",3.58,0,3.58,8592765020321,12,18592765020328,144,28592765020325,"8536201090",0.12]
[102032,"Ex9BS 1P B10 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 10 A, 1-pole","NAK",3.18,0,3.18,8592765020338,12,18592765020335,144,28592765020332,"8536201090",0.12]
[102033,"Ex9BS 1P B13 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 13 A, 1-pole","NAK",3.18,0,3.18,8592765020345,12,18592765020342,144,28592765020349,"8536201090",0.12]
[102034,"Ex9BS 1P B16 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 16 A, 1-pole","NAK",3.18,0,3.18,8592765020352,12,18592765020359,144,28592765020356,"8536201090",0.12]
[102035,"Ex9BS 1P B20 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 20 A, 1-pole","NAK",3.18,0,3.18,8592765020369,12,18592765020366,144,28592765020363,"8536201090",0.12]
[102036,"Ex9BS 1P B25 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 25 A, 1-pole","NAK",3.18,0,3.18,8592765020376,12,18592765020373,144,28592765020370,"8536201090",0.12]
[102037,"Ex9BS 1P B32 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 32 A, 1-pole","NAK",4.0599999999999996,0,4.0599999999999996,8592765020383,12,18592765020380,144,28592765020387,"8536201090",0.12]
[102038,"Ex9BS 1P B40 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 40 A, 1-pole","NAK",4.0599999999999996,0,4.0599999999999996,8592765020390,12,18592765020397,144,28592765020394,"8536201090",0.12]
[102039,"Ex9BS 1P B50 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 50 A, 1-pole","NAK",7.11,0,7.11,8592765020406,12,18592765020403,144,28592765020400,"8536201090",0.12]
[102040,"Ex9BS 1P B63 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 63 A, 1-pole","NAK",7.11,0,7.11,8592765020413,12,18592765020410,144,28592765020417,"8536201090",0.12]
[102060,"Ex9BS 2P B6 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 6 A, 2-pole","NAK",7.95,{"$f":"NAK","v":0},7.95,8592765020611,6,18592765020618,72,28592765020615,"8536201090",0.24]
[102061,"Ex9BS 2P B8 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 8 A, 2-pole","NAK",7.95,0,7.95,8592765020628,6,18592765020625,72,28592765020622,"8536201090",0.24]
[102062,"Ex9BS 2P B10 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 10 A, 2-pole","NAK",8.89,0,8.89,8592765020635,6,18592765020632,72,28592765020639,"8536201090",0.24]
[102063,"Ex9BS 2P B13 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 13 A, 2-pole","NAK",8.89,0,8.89,8592765020642,6,18592765020649,72,28592765020646,"8536201090",0.24]
[102064,"Ex9BS 2P B16 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 16 A, 2-pole","NAK",8.89,0,8.89,8592765020659,6,18592765020656,72,28592765020653,"8536201090",0.24]
[102065,"Ex9BS 2P B20 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 20 A, 2-pole","NAK",8.89,0,8.89,8592765020666,6,18592765020663,72,28592765020660,"8536201090",0.24]
[102066,"Ex9BS 2P B25 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 25 A, 2-pole","NAK",8.89,0,8.89,8592765020673,6,18592765020670,72,28592765020677,"8536201090",0.24]
[102067,"Ex9BS 2P B32 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 32 A, 2-pole","NAK",9.18,0,9.18,8592765020680,6,18592765020687,72,28592765020684,"8536201090",0.24]
[102068,"Ex9BS 2P B40 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 40 A, 2-pole","NAK",9.18,0,9.18,8592765020697,6,18592765020694,72,28592765020691,"8536201090",0.24]
[102069,"Ex9BS 2P B50 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 50 A, 2-pole","NAK",16.05,0,16.05,8592765020703,6,18592765020700,72,28592765020707,"8536201090",0.24]
[102070,"Ex9BS 2P B63 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 63 A, 2-pole","NAK",16.05,0,16.05,8592765020710,6,18592765020717,72,28592765020714,"8536201090",0.24]
[102075,"Ex9BS 3P B6 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 6 A, 3-pole","NAK",12.02,0,12.02,8592765020765,4,18592765020762,48,28592765020769,"8536201090",0.36]
[102076,"Ex9BS 3P B8 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 8 A, 3-pole","NAK",12.02,0,12.02,8592765020772,4,18592765020779,48,28592765020776,"8536201090",0.36]
[102077,"Ex9BS 3P B10 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 10 A, 3-pole","NAK",10.69,0,10.69,8592765020789,4,18592765020786,48,28592765020783,"8536201090",0.36]
[102078,"Ex9BS 3P B13 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 13 A, 3-pole","NAK",10.69,0,10.69,8592765020796,4,18592765020793,48,28592765020790,"8536201090",0.36]
[102079,"Ex9BS 3P B16 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 16 A, 3-pole","NAK",10.69,0,10.69,8592765020802,4,18592765020809,48,28592765020806,"8536201090",0.36]
[102080,"Ex9BS 3P B20 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 20 A, 3-pole","NAK",10.69,0,10.69,8592765020819,4,18592765020816,48,28592765020813,"8536201090",0.36]
[102081,"Ex9BS 3P B25 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 25 A, 3-pole","NAK",10.69,0,10.69,8592765020826,4,18592765020823,48,28592765020820,"8536201090",0.36]
[102082,"Ex9BS 3P B32 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 32 A, 3-pole","NAK",12.02,0,12.02,8592765020833,4,18592765020830,48,28592765020837,"8536201090",0.36]
[102083,"Ex9BS 3P B40 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 40 A, 3-pole","NAK",12.02,0,12.02,8592765020840,4,18592765020847,48,28592765020844,"8536201090",0.36]
[102084,"Ex9BS 3P B50 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 50 A, 3-pole","NAK",19.88,0,19.88,8592765020857,4,18592765020854,48,28592765020851,"8536201090",0.36]
[102085,"Ex9BS 3P B63 ","Miniature Circuit  Breaker 4,5 kA, characteristic B, 63 A, 3-pole","NAK",19.88,0,19.88,8592765020864,4,18592765020861,48,28592765020868,"8536201090",0.36]
[102120,"Ex9BS 1P C6 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 6 A, 1-pole","NAK",3.58,{"$f":"NAK","v":0},3.58,8592765021212,12,18592765021219,144,28592765021216,"8536201090",0.12]
[102121,"Ex9BS 1P C8 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 8 A, 1-pole","NAK",3.58,0,3.58,8592765021229,12,18592765021226,144,28592765021223,"8536201090",0.12]
[102122,"Ex9BS 1P C10 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 10 A, 1-pole","NAK",3.18,0,3.18,8592765021236,12,18592765021233,144,28592765021230,"8536201090",0.12]
[102123,"Ex9BS 1P C13 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 13 A, 1-pole","NAK",3.18,0,3.18,8592765021243,12,18592765021240,144,28592765021247,"8536201090",0.12]
[102124,"Ex9BS 1P C16 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 16 A, 1-pole","NAK",3.18,0,3.18,8592765021250,12,18592765021257,144,28592765021254,"8536201090",0.12]
[102125,"Ex9BS 1P C20 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 20 A, 1-pole","NAK",3.18,0,3.18,8592765021267,12,18592765021264,144,28592765021261,"8536201090",0.12]
[102126,"Ex9BS 1P C25 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 25 A, 1-pole","NAK",3.18,0,3.18,8592765021274,12,18592765021271,144,28592765021278,"8536201090",0.12]
[102127,"Ex9BS 1P C32 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 32 A, 1-pole","NAK",4.0599999999999996,0,4.0599999999999996,8592765021281,12,18592765021288,144,28592765021285,"8536201090",0.12]
[102128,"Ex9BS 1P C40 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 40 A, 1-pole","NAK",4.0599999999999996,0,4.0599999999999996,8592765021298,12,18592765021295,144,28592765021292,"8536201090",0.12]
[102129,"Ex9BS 1P C50 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 50 A, 1-pole","NAK",7.11,0,7.11,8592765021304,12,18592765021301,144,28592765021308,"8536201090",0.12]
[102130,"Ex9BS 1P C63 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 63 A, 1-pole","NAK",7.11,0,7.11,8592765021311,12,18592765021318,144,28592765021315,"8536201090",0.12]
[102150,"Ex9BS 2P C6 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 6 A, 2-pole","NAK",9.24,{"$f":"NAK","v":0},9.24,8592765021519,6,18592765021516,72,28592765021513,"8536201090",0.24]
[102151,"Ex9BS 2P C8 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 8 A, 2-pole","NAK",9.24,0,9.24,8592765021526,6,18592765021523,72,28592765021520,"8536201090",0.24]
[102152,"Ex9BS 2P C10 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 10 A, 2-pole","NAK",7.85,0,7.85,8592765021533,6,18592765021530,72,28592765021537,"8536201090",0.24]
[102153,"Ex9BS 2P C13 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 13 A, 2-pole","NAK",7.85,0,7.85,8592765021540,6,18592765021547,72,28592765021544,"8536201090",0.24]
[102154,"Ex9BS 2P C16 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 16 A, 2-pole","NAK",7.85,0,7.85,8592765021557,6,18592765021554,72,28592765021551,"8536201090",0.24]
[102155,"Ex9BS 2P C20 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 20 A, 2-pole","NAK",7.85,{"$f":"NAK","v":0},7.85,8592765021564,6,18592765021561,72,28592765021568,"8536201090",0.24]
[102156,"Ex9BS 2P C25 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 25 A, 2-pole","NAK",7.85,0,7.85,8592765021571,6,18592765021578,72,28592765021575,"8536201090",0.24]
[102157,"Ex9BS 2P C32 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 32 A, 2-pole","NAK",10.46,0,10.46,8592765021588,6,18592765021585,72,28592765021582,"8536201090",0.24]
[102158,"Ex9BS 2P C40 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 40 A, 2-pole","NAK",10.46,0,10.46,8592765021595,6,18592765021592,72,28592765021599,"8536201090",0.24]
[102159,"Ex9BS 2P C50 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 50 A, 2-pole","NAK",19.45,0,19.45,8592765021601,6,18592765021608,72,28592765021605,"8536201090",0.24]
[102160,"Ex9BS 2P C63 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 63 A, 2-pole","NAK",19.45,0,19.45,8592765021618,6,18592765021615,72,28592765021612,"8536201090",0.24]
[102165,"Ex9BS 3P C6 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 6 A, 3-pole","NAK",12.02,{"$f":"NAK","v":0},12.02,8592765021663,4,18592765021660,48,28592765021667,"8536201090",0.36]
[102166,"Ex9BS 3P C8 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 8 A, 3-pole","NAK",12.02,0,12.02,8592765021670,4,18592765021677,48,28592765021674,"8536201090",0.36]
[102167,"Ex9BS 3P C10 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 10 A, 3-pole","NAK",10.69,0,10.69,8592765021687,4,18592765021684,48,28592765021681,"8536201090",0.36]
[102168,"Ex9BS 3P C13 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 13 A, 3-pole","NAK",10.69,0,10.69,8592765021694,4,18592765021691,48,28592765021698,"8536201090",0.36]
[102169,"Ex9BS 3P C16 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 16 A, 3-pole","NAK",10.69,0,10.69,8592765021700,4,18592765021707,48,28592765021704,"8536201090",0.36]
[102170,"Ex9BS 3P C20 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 20 A, 3-pole","NAK",10.69,0,10.69,8592765021717,4,18592765021714,48,28592765021711,"8536201090",0.36]
[102171,"Ex9BS 3P C25 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 25 A, 3-pole","NAK",10.69,0,10.69,8592765021724,4,18592765021721,48,28592765021728,"8536201090",0.36]
[102172,"Ex9BS 3P C32 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 32 A, 3-pole","NAK",12.02,0,12.02,8592765021731,4,18592765021738,48,28592765021735,"8536201090",0.36]
[102173,"Ex9BS 3P C40 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 40 A, 3-pole","NAK",12.02,0,12.02,8592765021748,4,18592765021745,48,28592765021742,"8536201090",0.36]
[102174,"Ex9BS 3P C50 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 50 A, 3-pole","NAK",19.88,0,19.88,8592765021755,4,18592765021752,48,28592765021759,"8536201090",0.36]
[102175,"Ex9BS 3P C63 ","Miniature Circuit  Breaker 4,5 kA, characteristic C, 63 A, 3-pole","NAK",19.88,0,19.88,8592765021762,4,18592765021769,48,28592765021766,"8536201090",0.36]
[]
["Slim MCB Ex9B40J, 6 kA"]
[110719,"Ex9B40J 1P B1","Slim MCB 13,5 mm, 6 kA, characteristic B, 1 A, 1-pole","NAAB",4.1900000000000004,{"$f":"_xlfn.SINGLE(NAAB)","v":0},{"$f":"E619*(1-F619)","v":4.1900000000000004},8592765107190,16,18592765107197,192,28592765107194,8536201090,8.5999999999999993E-2]
[110720,"Ex9B40J 1P B2","Slim MCB 13,5 mm, 6 kA, characteristic B, 2 A, 1-pole","NAAB",4.1900000000000004,0,{"$f":"E620*(1-F620)","v":4.1900000000000004},8592765107206,16,18592765107203,192,28592765107200,8536201090,8.6999999999999994E-2]
[110721,"Ex9B40J 1P B3","Slim MCB 13,5 mm, 6 kA, characteristic B, 3 A, 1-pole","NAAB",4.1900000000000004,0,4.1900000000000004,8592765107213,16,18592765107210,192,28592765107217,8536201090,8.6999999999999994E-2]
[110722,"Ex9B40J 1P B4","Slim MCB 13,5 mm, 6 kA, characteristic B, 4 A, 1-pole","NAAB",4.1900000000000004,0,4.1900000000000004,8592765107220,16,18592765107227,192,28592765107224,8536201090,8.5999999999999993E-2]
[110723,"Ex9B40J 1P B6","Slim MCB 13,5 mm, 6 kA, characteristic B, 6 A, 1-pole","NAAB",4.01,0,4.01,8592765107237,16,18592765107234,192,28592765107231,8536201090,8.6999999999999994E-2]
[110724,"Ex9B40J 1P B10","Slim MCB 13,5 mm, 6 kA, characteristic B, 10 A, 1-pole","NAAB",3.54,0,3.54,8592765107244,16,18592765107241,192,28592765107248,8536201090,8.5000000000000006E-2]
[110725,"Ex9B40J 1P B16","Slim MCB 13,5 mm, 6 kA, characteristic B, 16 A, 1-pole","NAAB",3.54,0,3.54,8592765107251,16,18592765107258,192,28592765107255,8536201090,8.4000000000000005E-2]
[110726,"Ex9B40J 1P B20","Slim MCB 13,5 mm, 6 kA, characteristic B, 20 A, 1-pole","NAAB",3.54,0,3.54,8592765107268,16,18592765107265,192,28592765107262,8536201090,8.5999999999999993E-2]
[110727,"Ex9B40J 1P B25","Slim MCB 13,5 mm, 6 kA, characteristic B, 25 A, 1-pole","NAAB",3.54,0,3.54,8592765107275,16,18592765107272,192,28592765107279,8536201090,8.5999999999999993E-2]
[110728,"Ex9B40J 1P B32","Slim MCB 13,5 mm, 6 kA, characteristic B, 32 A, 1-pole","NAAB",4.47,0,4.47,8592765107282,16,18592765107289,192,28592765107286,8536201090,8.5999999999999993E-2]
[110729,"Ex9B40J 1P B40","Slim MCB 13,5 mm, 6 kA, characteristic B, 40 A, 1-pole","NAAB",4.47,0,4.47,8592765107299,16,18592765107296,192,28592765107293,8536201090,8.6999999999999994E-2]
[110730,"Ex9B40J 2P B1","Slim MCB 27 mm, 6 kA, characteristic B, 1 A, 2-pole","NAAB",8.7799999999999994,0,8.7799999999999994,8592765107305,8,18592765107302,96,28592765107309,8536201090,0.17299999999999999]
[110731,"Ex9B40J 2P B2","Slim MCB 27 mm, 6 kA, characteristic B, 2 A, 2-pole","NAAB",8.7799999999999994,0,8.7799999999999994,8592765107312,8,18592765107319,96,28592765107316,8536201090,0.17499999999999999]
[110732,"Ex9B40J 2P B3","Slim MCB 27 mm, 6 kA, characteristic B, 3 A, 2-pole","NAAB",8.7799999999999994,0,8.7799999999999994,8592765107329,8,18592765107326,96,28592765107323,8536201090,0.17499999999999999]
[110733,"Ex9B40J 2P B4","Slim MCB 27 mm, 6 kA, characteristic B, 4 A, 2-pole","NAAB",8.7799999999999994,0,8.7799999999999994,8592765107336,8,18592765107333,96,28592765107330,8536201090,0.17299999999999999]
[110734,"Ex9B40J 2P B6","Slim MCB 27 mm, 6 kA, characteristic B, 6 A, 2-pole","NAAB",8.7799999999999994,0,8.7799999999999994,8592765107343,8,18592765107340,96,28592765107347,8536201090,0.17499999999999999]
[110735,"Ex9B40J 2P B10","Slim MCB 27 mm, 6 kA, characteristic B, 10 A, 2-pole","NAAB",9.8000000000000007,0,9.8000000000000007,8592765107350,8,18592765107357,96,28592765107354,8536201090,0.17100000000000001]
[110736,"Ex9B40J 2P B16","Slim MCB 27 mm, 6 kA, characteristic B, 16 A, 2-pole","NAAB",9.8000000000000007,0,9.8000000000000007,8592765107367,8,18592765107364,96,28592765107361,8536201090,0.16900000000000001]
[110737,"Ex9B40J 2P B20","Slim MCB 27 mm, 6 kA, characteristic B, 20 A, 2-pole","NAAB",9.8000000000000007,0,9.8000000000000007,8592765107374,8,18592765107371,96,28592765107378,8536201090,0.17299999999999999]
[110738,"Ex9B40J 2P B25","Slim MCB 27 mm, 6 kA, characteristic B, 25 A, 2-pole","NAAB",9.8000000000000007,0,9.8000000000000007,8592765107381,8,18592765107388,96,28592765107385,8536201090,0.17299999999999999]
[110739,"Ex9B40J 2P B32","Slim MCB 27 mm, 6 kA, characteristic B, 32 A, 2-pole","NAAB",10.1,0,10.1,8592765107398,8,18592765107395,96,28592765107392,8536201090,0.17299999999999999]
[110740,"Ex9B40J 2P B40","Slim MCB 27 mm, 6 kA, characteristic B, 40 A, 2-pole","NAAB",10.1,0,10.1,8592765107404,8,18592765107401,96,28592765107408,8536201090,0.17499999999999999]
[110741,"Ex9B40J 3P B1","Slim MCB 40,5 mm, 6 kA, characteristic B, 1 A, 3-pole","NAAB",13.27,0,13.27,8592765107411,5,18592765107418,60,28592765107415,8536201090,0.25800000000000001]
[110742,"Ex9B40J 3P B2","Slim MCB 40,5 mm, 6 kA, characteristic B, 2 A, 3-pole","NAAB",13.27,0,13.27,8592765107428,5,18592765107425,60,28592765107422,8536201090,0.26100000000000001]
[110743,"Ex9B40J 3P B3","Slim MCB 40,5 mm, 6 kA, characteristic B, 3 A, 3-pole","NAAB",13.27,0,13.27,8592765107435,5,18592765107432,60,28592765107439,8536201090,0.26100000000000001]
[110744,"Ex9B40J 3P B4","Slim MCB 40,5 mm, 6 kA, characteristic B, 4 A, 3-pole","NAAB",13.27,0,13.27,8592765107442,5,18592765107449,60,28592765107446,8536201090,0.25800000000000001]
[110745,"Ex9B40J 3P B6","Slim MCB 40,5 mm, 6 kA, characteristic B, 6 A, 3-pole","NAAB",13.27,0,13.27,8592765107459,5,18592765107456,60,28592765107453,8536201090,0.26100000000000001]
[110746,"Ex9B40J 3P B10","Slim MCB 40,5 mm, 6 kA, characteristic B, 10 A, 3-pole","NAAB",11.79,0,11.79,8592765107466,5,18592765107463,60,28592765107460,8536201090,0.255]
[110747,"Ex9B40J 3P B16","Slim MCB 40,5 mm, 6 kA, characteristic B, 16 A, 3-pole","NAAB",11.79,0,11.79,8592765107473,5,18592765107470,60,28592765107477,8536201090,0.252]
[110748,"Ex9B40J 3P B20","Slim MCB 40,5 mm, 6 kA, characteristic B, 20 A, 3-pole","NAAB",11.79,0,11.79,8592765107480,5,18592765107487,60,28592765107484,8536201090,0.25800000000000001]
[110749,"Ex9B40J 3P B25","Slim MCB 40,5 mm, 6 kA, characteristic B, 25 A, 3-pole","NAAB",11.79,0,11.79,8592765107497,5,18592765107494,60,28592765107491,8536201090,0.25800000000000001]
[110750,"Ex9B40J 3P B32","Slim MCB 40,5 mm, 6 kA, characteristic B, 32 A, 3-pole","NAAB",13.27,0,13.27,8592765107503,5,18592765107500,60,28592765107507,8536201090,0.25800000000000001]
[110751,"Ex9B40J 3P B40","Slim MCB 40,5 mm, 6 kA, characteristic B, 40 A, 3-pole","NAAB",13.27,0,13.27,8592765107510,5,18592765107517,60,28592765107514,8536201090,0.26100000000000001]
[110752,"Ex9B40J 4P B1","Slim MCB 54 mm, 6 kA, characteristic B, 1 A, 4-pole","NAAB",28.15,0,28.15,8592765107527,4,18592765107524,48,28592765107521,8536201090,0.34399999999999997]
[110753,"Ex9B40J 4P B2","Slim MCB 54 mm, 6 kA, characteristic B, 2 A, 4-pole","NAAB",28.15,0,28.15,8592765107534,4,18592765107531,48,28592765107538,8536201090,0.34799999999999998]
[110754,"Ex9B40J 4P B3","Slim MCB 54 mm, 6 kA, characteristic B, 3 A, 4-pole","NAAB",28.15,0,28.15,8592765107541,4,18592765107548,48,28592765107545,8536201090,0.34799999999999998]
[110755,"Ex9B40J 4P B4","Slim MCB 54 mm, 6 kA, characteristic B, 4 A, 4-pole","NAAB",28.15,0,28.15,8592765107558,4,18592765107555,48,28592765107552,8536201090,0.34399999999999997]
[110756,"Ex9B40J 4P B6","Slim MCB 54 mm, 6 kA, characteristic B, 6 A, 4-pole","NAAB",28.15,0,28.15,8592765107565,4,18592765107562,48,28592765107569,8536201090,0.34799999999999998]
[110757,"Ex9B40J 4P B10","Slim MCB 54 mm, 6 kA, characteristic B, 10 A, 4-pole","NAAB",25.08,0,25.08,8592765107572,4,18592765107579,48,28592765107576,8536201090,0.34]
[110758,"Ex9B40J 4P B16","Slim MCB 54 mm, 6 kA, characteristic B, 16 A, 4-pole","NAAB",25.08,0,25.08,8592765107589,4,18592765107586,48,28592765107583,8536201090,0.33600000000000002]
[110759,"Ex9B40J 4P B20","Slim MCB 54 mm, 6 kA, characteristic B, 20 A, 4-pole","NAAB",25.08,0,25.08,8592765107596,4,18592765107593,48,28592765107590,8536201090,0.34399999999999997]
[110760,"Ex9B40J 4P B25","Slim MCB 54 mm, 6 kA, characteristic B, 25 A, 4-pole","NAAB",25.08,0,25.08,8592765107602,4,18592765107609,48,28592765107606,8536201090,0.34399999999999997]
[110761,"Ex9B40J 4P B32","Slim MCB 54 mm, 6 kA, characteristic B, 32 A, 4-pole","NAAB",36.9,0,36.9,8592765107619,4,18592765107616,48,28592765107613,8536201090,0.34399999999999997]
[110762,"Ex9B40J 4P B40","Slim MCB 54 mm, 6 kA, characteristic B, 40 A, 4-pole","NAAB",36.9,0,36.9,8592765107626,4,18592765107623,48,28592765107620,8536201090,0.34799999999999998]
[110763,"Ex9B40J 1P C1","Slim MCB 13,5 mm, 6 kA, characteristic C, 1 A, 1-pole","NAAB",4.1399999999999997,0,4.1399999999999997,8592765107633,16,18592765107630,192,28592765107637,8536201090,8.5999999999999993E-2]
[110764,"Ex9B40J 1P C2","Slim MCB 13,5 mm, 6 kA, characteristic C, 2 A, 1-pole","NAAB",4.1399999999999997,0,4.1399999999999997,8592765107640,16,18592765107647,192,28592765107644,8536201090,8.6999999999999994E-2]
[110765,"Ex9B40J 1P C3","Slim MCB 13,5 mm, 6 kA, characteristic C, 3 A, 1-pole","NAAB",4.1399999999999997,0,4.1399999999999997,8592765107657,16,18592765107654,192,28592765107651,8536201090,8.6999999999999994E-2]
[110766,"Ex9B40J 1P C4","Slim MCB 13,5 mm, 6 kA, characteristic C, 4 A, 1-pole","NAAB",4.1399999999999997,0,4.1399999999999997,8592765107664,16,18592765107661,192,28592765107668,8536201090,8.5999999999999993E-2]
[110767,"Ex9B40J 1P C6","Slim MCB 13,5 mm, 6 kA, characteristic C, 6 A, 1-pole","NAAB",3.97,0,3.97,8592765107671,16,18592765107678,192,28592765107675,8536201090,8.6999999999999994E-2]
[110768,"Ex9B40J 1P C10","Slim MCB 13,5 mm, 6 kA, characteristic C, 10 A, 1-pole","NAAB",3.51,0,3.51,8592765107688,16,18592765107685,192,28592765107682,8536201090,8.5000000000000006E-2]
[110769,"Ex9B40J 1P C16","Slim MCB 13,5 mm, 6 kA, characteristic C, 16 A, 1-pole","NAAB",3.51,0,3.51,8592765107695,16,18592765107692,192,28592765107699,8536201090,8.4000000000000005E-2]
[110770,"Ex9B40J 1P C20","Slim MCB 13,5 mm, 6 kA, characteristic C, 20 A, 1-pole","NAAB",3.51,0,3.51,8592765107701,16,18592765107708,192,28592765107705,8536201090,8.5999999999999993E-2]
[110771,"Ex9B40J 1P C25","Slim MCB 13,5 mm, 6 kA, characteristic C, 25 A, 1-pole","NAAB",3.51,0,3.51,8592765107718,16,18592765107715,192,28592765107712,8536201090,8.5999999999999993E-2]
[110772,"Ex9B40J 1P C32","Slim MCB 13,5 mm, 6 kA, characteristic C, 32 A, 1-pole","NAAB",4.47,0,4.47,8592765107725,16,18592765107722,192,28592765107729,8536201090,8.5999999999999993E-2]
[110773,"Ex9B40J 1P C40","Slim MCB 13,5 mm, 6 kA, characteristic C, 40 A, 1-pole","NAAB",4.47,0,4.47,8592765107732,16,18592765107739,192,28592765107736,8536201090,8.6999999999999994E-2]
[110774,"Ex9B40J 2P C1","Slim MCB 27 mm, 6 kA, characteristic C, 1 A, 2-pole","NAAB",10.17,0,10.17,8592765107749,8,18592765107746,96,28592765107743,8536201090,0.17299999999999999]
[110775,"Ex9B40J 2P C2","Slim MCB 27 mm, 6 kA, characteristic C, 2 A, 2-pole","NAAB",10.17,0,10.17,8592765107756,8,18592765107753,96,28592765107750,8536201090,0.17499999999999999]
[110776,"Ex9B40J 2P C3","Slim MCB 27 mm, 6 kA, characteristic C, 3 A, 2-pole","NAAB",10.17,0,10.17,8592765107763,8,18592765107760,96,28592765107767,8536201090,0.17499999999999999]
[110777,"Ex9B40J 2P C4","Slim MCB 27 mm, 6 kA, characteristic C, 4 A, 2-pole","NAAB",10.17,0,10.17,8592765107770,8,18592765107777,96,28592765107774,8536201090,0.17299999999999999]
[110778,"Ex9B40J 2P C6","Slim MCB 27 mm, 6 kA, characteristic C, 6 A, 2-pole","NAAB",10.17,0,10.17,8592765107787,8,18592765107784,96,28592765107781,8536201090,0.17499999999999999]
[110779,"Ex9B40J 2P C10","Slim MCB 27 mm, 6 kA, characteristic C, 10 A, 2-pole","NAAB",8.65,0,8.65,8592765107794,8,18592765107791,96,28592765107798,8536201090,0.17100000000000001]
[110780,"Ex9B40J 2P C16","Slim MCB 27 mm, 6 kA, characteristic C, 16 A, 2-pole","NAAB",8.65,0,8.65,8592765107800,8,18592765107807,96,28592765107804,8536201090,0.16900000000000001]
[110781,"Ex9B40J 2P C20","Slim MCB 27 mm, 6 kA, characteristic C, 20 A, 2-pole","NAAB",8.65,0,8.65,8592765107817,8,18592765107814,96,28592765107811,8536201090,0.17299999999999999]
[110782,"Ex9B40J 2P C25","Slim MCB 27 mm, 6 kA, characteristic C, 25 A, 2-pole","NAAB",8.65,0,8.65,8592765107824,8,18592765107821,96,28592765107828,8536201090,0.17299999999999999]
[110783,"Ex9B40J 2P C32","Slim MCB 27 mm, 6 kA, characteristic C, 32 A, 2-pole","NAAB",11.53,{"$f":"_xlfn.SINGLE(NAAB)","v":0},11.53,8592765107831,8,18592765107838,96,28592765107835,8536201090,0.17299999999999999]
[110784,"Ex9B40J 2P C40","Slim MCB 27 mm, 6 kA, characteristic C, 40 A, 2-pole","NAAB",11.53,0,{"$f":"E684*(1-F684)","v":11.53},8592765107848,8,18592765107845,96,28592765107842,8536201090,0.17499999999999999]
[110785,"Ex9B40J 3P C1","Slim MCB 40,5 mm, 6 kA, characteristic C, 1 A, 3-pole","NAAB",13.27,0,13.27,8592765107855,5,18592765107852,60,28592765107859,8536201090,0.25800000000000001]
[110786,"Ex9B40J 3P C2","Slim MCB 40,5 mm, 6 kA, characteristic C, 2 A, 3-pole","NAAB",13.27,0,13.27,8592765107862,5,18592765107869,60,28592765107866,8536201090,0.26100000000000001]
[110787,"Ex9B40J 3P C3","Slim MCB 40,5 mm, 6 kA, characteristic C, 3 A, 3-pole","NAAB",13.27,0,13.27,8592765107879,5,18592765107876,60,28592765107873,8536201090,0.26100000000000001]
[110788,"Ex9B40J 3P C4","Slim MCB 40,5 mm, 6 kA, characteristic C, 4 A, 3-pole","NAAB",13.27,0,13.27,8592765107886,5,18592765107883,60,28592765107880,8536201090,0.25800000000000001]
[110789,"Ex9B40J 3P C6","Slim MCB 40,5 mm, 6 kA, characteristic C, 6 A, 3-pole","NAAB",13.27,0,13.27,8592765107893,5,18592765107890,60,28592765107897,8536201090,0.26100000000000001]
[110790,"Ex9B40J 3P C10","Slim MCB 40,5 mm, 6 kA, characteristic C, 10 A, 3-pole","NAAB",11.79,0,11.79,8592765107909,5,18592765107906,60,28592765107903,8536201090,0.255]
[110791,"Ex9B40J 3P C16","Slim MCB 40,5 mm, 6 kA, characteristic C, 16 A, 3-pole","NAAB",11.79,0,11.79,8592765107916,5,18592765107913,60,28592765107910,8536201090,0.252]
[110792,"Ex9B40J 3P C20","Slim MCB 40,5 mm, 6 kA, characteristic C, 20 A, 3-pole","NAAB",11.79,0,11.79,8592765107923,5,18592765107920,60,28592765107927,8536201090,0.25800000000000001]
[110793,"Ex9B40J 3P C25","Slim MCB 40,5 mm, 6 kA, characteristic C, 25 A, 3-pole","NAAB",11.79,0,11.79,8592765107930,5,18592765107937,60,28592765107934,8536201090,0.25800000000000001]
[110794,"Ex9B40J 3P C32","Slim MCB 40,5 mm, 6 kA, characteristic C, 32 A, 3-pole","NAAB",13.27,0,13.27,8592765107947,5,18592765107944,60,28592765107941,8536201090,0.25800000000000001]
[110795,"Ex9B40J 3P C40","Slim MCB 40,5 mm, 6 kA, characteristic C, 40 A, 3-pole","NAAB",13.27,0,13.27,8592765107954,5,18592765107951,60,28592765107958,8536201090,0.26100000000000001]
[110796,"Ex9B40J 4P C1","Slim MCB 54 mm, 6 kA, characteristic C, 1 A, 4-pole","NAAB",28.1,0,28.1,8592765107961,4,18592765107968,48,28592765107965,8536201090,0.34399999999999997]
[110797,"Ex9B40J 4P C2","Slim MCB 54 mm, 6 kA, characteristic C, 2 A, 4-pole","NAAB",28.1,0,28.1,8592765107978,4,18592765107975,48,28592765107972,8536201090,0.34799999999999998]
[110798,"Ex9B40J 4P C3","Slim MCB 54 mm, 6 kA, characteristic C, 3 A, 4-pole","NAAB",28.1,0,28.1,8592765107985,4,18592765107982,48,28592765107989,8536201090,0.34799999999999998]
[110799,"Ex9B40J 4P C4","Slim MCB 54 mm, 6 kA, characteristic C, 4 A, 4-pole","NAAB",28.1,0,28.1,8592765107992,4,18592765107999,48,28592765107996,8536201090,0.34399999999999997]
[110800,"Ex9B40J 4P C6","Slim MCB 54 mm, 6 kA, characteristic C, 6 A, 4-pole","NAAB",28.1,0,28.1,8592765108005,4,18592765108002,48,28592765108009,8536201090,0.34799999999999998]
[110801,"Ex9B40J 4P C10","Slim MCB 54 mm, 6 kA, characteristic C, 10 A, 4-pole","NAAB",24.95,0,24.95,8592765108012,4,18592765108019,48,28592765108016,8536201090,0.34]
[110802,"Ex9B40J 4P C16","Slim MCB 54 mm, 6 kA, characteristic C, 16 A, 4-pole","NAAB",24.95,0,24.95,8592765108029,4,18592765108026,48,28592765108023,8536201090,0.33600000000000002]
[110803,"Ex9B40J 4P C20","Slim MCB 54 mm, 6 kA, characteristic C, 20 A, 4-pole","NAAB",24.95,0,24.95,8592765108036,4,18592765108033,48,28592765108030,8536201090,0.34399999999999997]
[110804,"Ex9B40J 4P C25","Slim MCB 54 mm, 6 kA, characteristic C, 25 A, 4-pole","NAAB",24.95,0,24.95,8592765108043,4,18592765108040,48,28592765108047,8536201090,0.34399999999999997]
[110805,"Ex9B40J 4P C32","Slim MCB 54 mm, 6 kA, characteristic C, 32 A, 4-pole","NAAB",28.24,0,28.24,8592765108050,4,18592765108057,48,28592765108054,8536201090,0.34399999999999997]
[110806,"Ex9B40J 4P C40","Slim MCB 54 mm, 6 kA, characteristic C, 40 A, 4-pole","NAAB",28.24,0,28.24,8592765108067,4,18592765108064,48,28592765108061,8536201090,0.34799999999999998]
[]
["Miniature Circuit  Breakers Ex9PN-N, 6 kA"]
[101600,"Ex9PN-N 1PN B1","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 1 A, 1+Npole","NAI",11.06,{"$f":"NAI","v":0},{"$f":"E709*(1-F709)","v":11.06},8592765016010,12,18592765016017,144,28592765016014,"8536201090",0.12]
[101601,"Ex9PN-N 1PN B2 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 2 A, 1+Npole","NAI",10.87,0,10.87,8592765016027,12,18592765016024,144,28592765016021,"8536201090",0.12]
[101602,"Ex9PN-N 1PN B3 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 3 A, 1+Npole","NAI",10.14,0,10.14,8592765016034,12,18592765016031,144,28592765016038,"8536201090",0.12]
[101603,"Ex9PN-N 1PN B4 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 4 A, 1+Npole","NAI",10.01,0,10.01,8592765016041,12,18592765016048,144,28592765016045,"8536201090",0.12]
[101604,"Ex9PN-N 1PN B6 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 6 A, 1+Npole","NAI",9.98,0,9.98,8592765016058,12,18592765016055,144,28592765016052,"8536201090",0.12]
[101605,"Ex9PN-N 1PN B10 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 10 A, 1+Npole","NAI",9.8699999999999992,0,9.8699999999999992,8592765016065,12,18592765016062,144,28592765016069,"8536201090",0.12]
[102354,"Ex9PN-N 1PN B13 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 13 A, 1+Npole","NAI",9.99,0,9.99,8592765023551,12,18592765023558,144,28592765023555,"8536201090",0.12]
[101606,"Ex9PN-N 1PN B16 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 16 A, 1+Npole","NAI",9.4499999999999993,0,9.4499999999999993,8592765016072,12,18592765016079,144,28592765016076,"8536201090",0.12]
[101607,"Ex9PN-N 1PN B20 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 20 A, 1+Npole","NAI",10.06,0,10.06,8592765016089,12,18592765016086,144,28592765016083,"8536201090",0.12]
[101608,"Ex9PN-N 1PN B25 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 25 A, 1+Npole","NAI",10.4,0,10.4,8592765016096,12,18592765016093,144,28592765016090,"8536201090",0.12]
[101609,"Ex9PN-N 1PN B32 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 32 A, 1+Npole","NAI",11.11,0,11.11,8592765016102,12,18592765016109,144,28592765016106,"8536201090",0.12]
[101610,"Ex9PN-N 1PN B40 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic B, 40 A, 1+Npole","NAI",11.53,0,11.53,8592765016119,12,18592765016116,144,28592765016113,"8536201090",0.12]
[101611,"Ex9PN-N 1PN C1","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 1 A, 1+Npole","NAI",12.65,0,12.65,8592765016126,12,18592765016123,144,28592765016120,"8536201090",0.12]
[101612,"Ex9PN-N 1PN C2 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 2 A, 1+Npole","NAI",11.53,0,11.53,8592765016133,12,18592765016130,144,28592765016137,"8536201090",0.12]
[101613,"Ex9PN-N 1PN C3 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 3 A, 1+Npole","NAI",11.38,0,11.38,8592765016140,12,18592765016147,144,28592765016144,"8536201090",0.12]
[101614,"Ex9PN-N 1PN C4 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 4 A, 1+Npole","NAI",11.11,0,11.11,8592765016157,12,18592765016154,144,28592765016151,"8536201090",0.12]
[101615,"Ex9PN-N 1PN C6 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 6 A, 1+Npole","NAI",10.65,0,10.65,8592765016164,12,18592765016161,144,28592765016168,"8536201090",0.12]
[101616,"Ex9PN-N 1PN C10 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 10 A, 1+Npole","NAI",10.31,0,10.31,8592765016171,12,18592765016178,144,28592765016175,"8536201090",0.12]
[102355,"Ex9PN-N 1PN C13 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 13 A, 1+Npole","NAI",10.75,0,10.75,8592765023568,12,18592765023565,144,28592765023562,"8536201090",0.12]
[101617,"Ex9PN-N 1PN C16 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 16 A, 1+Npole","NAI",10.17,0,10.17,8592765016188,12,18592765016185,144,28592765016182,"8536201090",0.12]
[101618,"Ex9PN-N 1PN C20 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 20 A, 1+Npole","NAI",10.75,0,10.75,8592765016195,12,18592765016192,144,28592765016199,"8536201090",0.12]
[101619,"Ex9PN-N 1PN C25 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 25 A, 1+Npole","NAI",11.19,0,11.19,8592765016201,12,18592765016208,144,28592765016205,"8536201090",0.12]
[101620,"Ex9PN-N 1PN C32 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 32 A, 1+Npole","NAI",11.92,0,11.92,8592765016218,12,18592765016215,144,28592765016212,"8536201090",0.12]
[101621,"Ex9PN-N 1PN C40 ","Miniature Circuit  Breaker, width 1 module, 6 kA, characteristic C, 40 A, 1+Npole","NAI",13.18,0,13.18,8592765016225,12,18592765016222,144,28592765016229,"8536201090",0.12]
[]
["Miniature Circuit  Breakers Ex9B125, up to 100 A"]
[102684,"Ex9B125 1P B16A ","Miniature Circuit  Breaker 25 kA, characteristic B, 16 A, 1-pole","NAW",28.97,{"$f":"NAW","v":0},{"$f":"E735*(1-F735)","v":28.97},8592765026859,12,18592765026856,null,18592765026856,"8536201090",0.2]
[102685,"Ex9B125 1P B20A ","Miniature Circuit  Breaker 25 kA, characteristic B, 20 A, 1-pole","NAW",28.97,{"$f":"NAW","v":0},{"$f":"E736*(1-F736)","v":28.97},8592765026866,12,18592765026863,null,18592765026863,"8536201090",0.2]
[102686,"Ex9B125 1P B25A","Miniature Circuit  Breaker 25 kA, characteristic B, 25 A, 1-pole","NAW",29.79,0,29.79,8592765026873,12,18592765026870,null,18592765026870,"8536201090",0.2]
[102687,"Ex9B125 1P B32A","Miniature Circuit  Breaker 25 kA, characteristic B, 32 A, 1-pole","NAW",29.79,0,29.79,8592765026880,12,18592765026887,null,18592765026887,"8536201090",0.2]
[102688,"Ex9B125 1P B40A","Miniature Circuit  Breaker 25 kA, characteristic B, 40 A, 1-pole","NAW",36.409999999999997,0,36.409999999999997,8592765026897,12,18592765026894,null,18592765026894,"8536201090",0.2]
[102689,"Ex9B125 1P B50A","Miniature Circuit  Breaker 25 kA, characteristic B, 50 A, 1-pole","NAW",51.11,0,51.11,8592765026903,12,18592765026900,null,18592765026900,"8536201090",0.2]
[102690,"Ex9B125 1P B63A","Miniature Circuit  Breaker 25 kA, characteristic B, 63 A, 1-pole","NAW",55.51,0,55.51,8592765026910,12,18592765026917,null,18592765026917,"8536201090",0.2]
[102691,"Ex9B125 1P B80A","Miniature Circuit  Breaker 20 kA, characteristic B, 80 A, 1-pole","NAW",56.03,0,56.03,8592765026927,12,18592765026924,null,18592765026924,"8536209090",0.2]
[102692,"Ex9B125 1P B100A","Miniature Circuit  Breaker 20 kA, characteristic B, 100 A, 1-pole","NAW",57.91,0,57.91,8592765026934,12,18592765026931,null,18592765026931,"8536209090",0.2]
[102714,"Ex9B125 1PN B16A","Miniature Circuit  Breaker 25 kA, characteristic B, 16 A, 1+Npole","NAW",64.790000000000006,0,64.790000000000006,8592765027153,6,18592765027150,null,18592765027150,"8536201090",0.4]
[102715,"Ex9B125 1PN B20A","Miniature Circuit  Breaker 25 kA, characteristic B, 20 A, 1+Npole","NAW",68.09,0,68.09,8592765027160,6,18592765027167,null,18592765027167,"8536201090",0.4]
[102716,"Ex9B125 1PN B25A","Miniature Circuit  Breaker 25 kA, characteristic B, 25 A, 1+Npole","NAW",69.97,0,69.97,8592765027177,6,18592765027174,null,18592765027174,"8536201090",0.4]
[102717,"Ex9B125 1PN B32A","Miniature Circuit  Breaker 25 kA, characteristic B, 32 A, 1+Npole","NAW",69.97,0,69.97,8592765027184,6,18592765027181,null,18592765027181,"8536201090",0.4]
[102718,"Ex9B125 1PN B40A","Miniature Circuit  Breaker 25 kA, characteristic B, 40 A, 1+Npole","NAW",82.39,0,82.39,8592765027191,6,18592765027198,null,18592765027198,"8536201090",0.4]
[102719,"Ex9B125 1PN B50A","Miniature Circuit  Breaker 25 kA, characteristic B, 50 A, 1+Npole","NAW",91.23,0,91.23,8592765027207,6,18592765027204,null,18592765027204,"8536201090",0.4]
[102720,"Ex9B125 1PN B63A","Miniature Circuit  Breaker 25 kA, characteristic B, 63 A, 1+Npole","NAW",96.6,0,96.6,8592765027214,6,18592765027211,null,18592765027211,"8536201090",0.4]
[102721,"Ex9B125 1PN B80A","Miniature Circuit  Breaker 20 kA, characteristic B, 80 A, 1+Npole","NAW",96.58,0,96.58,8592765027221,6,18592765027228,null,18592765027228,"8536201090",0.4]
[102722,"Ex9B125 1PN B100A","Miniature Circuit  Breaker 20 kA, characteristic B, 100 A, 1+Npole","NAW",101.95,0,101.95,8592765027238,6,18592765027235,null,18592765027235,"8536201090",0.4]
[102744,"Ex9B125 2P B16A","Miniature Circuit  Breaker 25 kA, characteristic B, 16 A, 2-pole","NAW",64.790000000000006,0,64.790000000000006,8592765027450,6,18592765027457,null,18592765027457,"8536201090",0.4]
[102745,"Ex9B125 2P B20A","Miniature Circuit  Breaker 25 kA, characteristic B, 20 A, 2-pole","NAW",68.09,0,68.09,8592765027467,6,18592765027464,null,18592765027464,"8536201090",0.4]
[102746,"Ex9B125 2P B25A","Miniature Circuit  Breaker 25 kA, characteristic B, 25 A, 2-pole","NAW",69.97,0,69.97,8592765027474,6,18592765027471,null,18592765027471,"8536201090",0.4]
[102747,"Ex9B125 2P B32A","Miniature Circuit  Breaker 25 kA, characteristic B, 32 A, 2-pole","NAW",69.97,0,69.97,8592765027481,6,18592765027488,null,18592765027488,"8536201090",0.4]
[102748,"Ex9B125 2P B40A","Miniature Circuit  Breaker 25 kA, characteristic B, 40 A, 2-pole","NAW",82.39,0,82.39,8592765027498,6,18592765027495,null,18592765027495,"8536201090",0.4]
[102749,"Ex9B125 2P B50A","Miniature Circuit  Breaker 25 kA, characteristic B, 50 A, 2-pole","NAW",91.23,0,91.23,8592765027504,6,18592765027501,null,18592765027501,"8536201090",0.4]
[102750,"Ex9B125 2P B63A","Miniature Circuit  Breaker 25 kA, characteristic B, 63 A, 2-pole","NAW",96.6,0,96.6,8592765027511,6,18592765027518,null,18592765027518,"8536201090",0.4]
[102751,"Ex9B125 2P B80A","Miniature Circuit  Breaker 20 kA, characteristic B, 80 A, 2-pole","NAW",96.58,0,96.58,8592765027528,6,18592765027525,null,18592765027525,"8536201090",0.4]
[102752,"Ex9B125 2P B100A","Miniature Circuit  Breaker 20 kA, characteristic B, 100 A, 2-pole","NAW",101.95,0,101.95,8592765027535,6,18592765027532,null,18592765027532,"8536201090",0.4]
[102774,"Ex9B125 3P B16A","Miniature Circuit  Breaker 25 kA, characteristic B, 16 A, 3-pole","NAW",99.25,0,99.25,8592765027757,4,18592765027754,null,18592765027754,"8536201090",0.6]
[102775,"Ex9B125 3P B20A","Miniature Circuit  Breaker 25 kA, characteristic B, 20 A, 3-pole","NAW",104.27,0,104.27,8592765027764,4,18592765027761,null,18592765027761,"8536201090",0.6]
[102776,"Ex9B125 3P B25A","Miniature Circuit  Breaker 25 kA, characteristic B, 25 A, 3-pole","NAW",107.2,0,107.2,8592765027771,4,18592765027778,null,18592765027778,"8536201090",0.6]
[102777,"Ex9B125 3P B32A","Miniature Circuit  Breaker 25 kA, characteristic B, 32 A, 3-pole","NAW",107.2,0,107.2,8592765027788,4,18592765027785,null,18592765027785,"8536201090",0.6]
[102778,"Ex9B125 3P B40A","Miniature Circuit  Breaker 25 kA, characteristic B, 40 A, 3-pole","NAW",108.58,0,108.58,8592765027795,4,18592765027792,null,18592765027792,"8536201090",0.6]
[102779,"Ex9B125 3P B50A","Miniature Circuit  Breaker 25 kA, characteristic B, 50 A, 3-pole","NAW",128.75,0,128.75,8592765027801,4,18592765027808,null,18592765027808,"8536201090",0.6]
[102780,"Ex9B125 3P B63A","Miniature Circuit  Breaker 25 kA, characteristic B, 63 A, 3-pole","NAW",126.98,0,126.98,8592765027818,4,18592765027815,null,18592765027815,"8536201090",0.6]
[102781,"Ex9B125 3P B80A","Miniature Circuit  Breaker 20 kA, characteristic B, 80 A, 3-pole","NAW",134.19,0,134.19,8592765027825,4,18592765027822,null,18592765027822,"8536209090",0.6]
[102782,"Ex9B125 3P B100A","Miniature Circuit  Breaker 20 kA, characteristic B, 100 A, 3-pole","NAW",135.04,0,135.04,8592765027832,4,18592765027839,null,18592765027839,"8536209090",0.6]
[102804,"Ex9B125 3PN B16A","Miniature Circuit  Breaker 25 kA, characteristic B, 16 A, 3+Npole","NAW",142.77000000000001,0,142.77000000000001,8592765028051,3,18592765028058,null,18592765028058,"8536201090",0.8]
[102805,"Ex9B125 3PN B20A","Miniature Circuit  Breaker 25 kA, characteristic B, 20 A, 3+Npole","NAW",149.91,0,149.91,8592765028068,3,18592765028065,null,18592765028065,"8536201090",0.8]
[102806,"Ex9B125 3PN B25A","Miniature Circuit  Breaker 25 kA, characteristic B, 25 A, 3+Npole","NAW",154.21,0,154.21,8592765028075,3,18592765028072,null,18592765028072,"8536201090",0.8]
[102807,"Ex9B125 3PN B32A","Miniature Circuit  Breaker 25 kA, characteristic B, 32 A, 3+Npole","NAW",164.84,0,164.84,8592765028082,3,18592765028089,null,18592765028089,"8536201090",0.8]
[102808,"Ex9B125 3PN B40A","Miniature Circuit  Breaker 25 kA, characteristic B, 40 A, 3+Npole","NAW",156.16999999999999,0,156.16999999999999,8592765028099,3,18592765028096,null,18592765028096,"8536201090",0.8]
[102809,"Ex9B125 3PN B50A","Miniature Circuit  Breaker 25 kA, characteristic B, 50 A, 3+Npole","NAW",184.41,0,184.41,8592765028105,3,18592765028102,null,18592765028102,"8536201090",0.8]
[102810,"Ex9B125 3PN B63A","Miniature Circuit  Breaker 25 kA, characteristic B, 63 A, 3+Npole","NAW",193.66,0,193.66,8592765028112,3,18592765028119,null,18592765028119,"8536201090",0.8]
[102811,"Ex9B125 3PN B80A","Miniature Circuit  Breaker 20 kA, characteristic B, 80 A, 3+Npole","NAW",193.57,0,193.57,8592765028129,3,18592765028126,null,18592765028126,"8536209090",0.8]
[102812,"Ex9B125 3PN B100A","Miniature Circuit  Breaker 20 kA, characteristic B, 100 A, 3+Npole","NAW",192.79,0,192.79,8592765028136,3,18592765028133,null,18592765028133,"8536209090",0.8]
[102834,"Ex9B125 4P B16A","Miniature Circuit  Breaker 25 kA, characteristic B, 16 A, 4-pole","NAW",135.12,0,135.12,8592765028358,3,18592765028355,null,18592765028355,"8536201090",0.8]
[102835,"Ex9B125 4P B20A","Miniature Circuit  Breaker 25 kA, characteristic B, 20 A, 4-pole","NAW",141.85,0,141.85,8592765028365,3,18592765028362,null,18592765028362,"8536201090",0.8]
[102836,"Ex9B125 4P B25A","Miniature Circuit  Breaker 25 kA, characteristic B, 25 A, 4-pole","NAW",145.94,0,145.94,8592765028372,3,18592765028379,null,18592765028379,"8536201090",0.8]
[102837,"Ex9B125 4P B32A","Miniature Circuit  Breaker 25 kA, characteristic B, 32 A, 4-pole","NAW",154.54,0,154.54,8592765028389,3,18592765028386,null,18592765028386,"8536201090",0.8]
[102838,"Ex9B125 4P B40A","Miniature Circuit  Breaker 25 kA, characteristic B, 40 A, 4-pole","NAW",178.37,0,178.37,8592765028396,3,18592765028393,null,18592765028393,"8536201090",0.8]
[102839,"Ex9B125 4P B50A","Miniature Circuit  Breaker 25 kA, characteristic B, 50 A, 4-pole","NAW",191.36,0,191.36,8592765028402,3,18592765028409,null,18592765028409,"8536201090",0.8]
[102840,"Ex9B125 4P B63A","Miniature Circuit  Breaker 25 kA, characteristic B, 63 A, 4-pole","NAW",198.5,0,198.5,8592765028419,3,18592765028416,null,18592765028416,"8536201090",0.8]
[102841,"Ex9B125 4P B80A","Miniature Circuit  Breaker 20 kA, characteristic B, 80 A, 4-pole","NAW",205.67,0,205.67,8592765028426,3,18592765028423,null,18592765028423,"8536201090",0.8]
[102842,"Ex9B125 4P B100A","Miniature Circuit  Breaker 20 kA, characteristic B, 100 A, 4-pole","NAW",212.84,0,212.84,8592765028433,3,18592765028430,null,18592765028430,"8536201090",0.8]
[102694,"Ex9B125 1P C16A","Miniature Circuit  Breaker 25 kA, characteristic C, 16 A, 1-pole","NAW",28.97,0,28.97,8592765026958,12,18592765026955,null,18592765026955,"8536201090",0.2]
[102695,"Ex9B125 1P C20A","Miniature Circuit  Breaker 25 kA, characteristic C, 20 A, 1-pole","NAW",28.97,0,28.97,8592765026965,12,18592765026962,null,18592765026962,"8536201090",0.2]
[102696,"Ex9B125 1P C25A","Miniature Circuit  Breaker 25 kA, characteristic C, 25 A, 1-pole","NAW",29.79,0,29.79,8592765026972,12,18592765026979,null,18592765026979,"8536201090",0.2]
[102697,"Ex9B125 1P C32A","Miniature Circuit  Breaker 25 kA, characteristic C, 32 A, 1-pole","NAW",29.79,0,29.79,8592765026989,12,18592765026986,null,18592765026986,"8536201090",0.2]
[102698,"Ex9B125 1P C40A","Miniature Circuit  Breaker 25 kA, characteristic C, 40 A, 1-pole","NAW",36.409999999999997,{"$f":"NAW","v":0},36.409999999999997,8592765026996,12,18592765026993,null,18592765026993,"8536201090",0.2]
[102699,"Ex9B125 1P C50A","Miniature Circuit  Breaker 25 kA, characteristic C, 50 A, 1-pole","NAW",51.11,0,{"$f":"E794*(1-F794)","v":51.11},8592765027009,12,18592765027006,null,18592765027006,"8536201090",0.2]
[102700,"Ex9B125 1P C63A","Miniature Circuit  Breaker 25 kA, characteristic C, 63 A, 1-pole","NAW",46.29,0,46.29,8592765027016,12,18592765027013,null,18592765027013,"8536201090",0.2]
[102701,"Ex9B125 1P C80A","Miniature Circuit  Breaker 20 kA, characteristic C, 80 A, 1-pole","NAW",46.57,0,46.57,8592765027023,12,18592765027020,null,18592765027020,"8536209090",0.2]
[102702,"Ex9B125 1P C100A","Miniature Circuit  Breaker 20 kA, characteristic C, 100 A, 1-pole","NAW",49.22,0,49.22,8592765027030,12,18592765027037,null,18592765027037,"8536209090",0.2]
[102724,"Ex9B125 1PN C16A","Miniature Circuit  Breaker 25 kA, characteristic C, 16 A, 1+Npole","NAW",64.790000000000006,0,64.790000000000006,8592765027252,6,18592765027259,null,18592765027259,"8536201090",0.4]
[102725,"Ex9B125 1PN C20A","Miniature Circuit  Breaker 25 kA, characteristic C, 20 A, 1+Npole","NAW",68.09,0,68.09,8592765027269,6,18592765027266,null,18592765027266,"8536201090",0.4]
[102726,"Ex9B125 1PN C25A","Miniature Circuit  Breaker 25 kA, characteristic C, 25 A, 1+Npole","NAW",69.97,0,69.97,8592765027276,6,18592765027273,null,18592765027273,"8536201090",0.4]
[102727,"Ex9B125 1PN C32A","Miniature Circuit  Breaker 25 kA, characteristic C, 32 A, 1+Npole","NAW",69.97,0,69.97,8592765027283,6,18592765027280,null,18592765027280,"8536201090",0.4]
[102728,"Ex9B125 1PN C40A","Miniature Circuit  Breaker 25 kA, characteristic C, 40 A, 1+Npole","NAW",85.61,0,85.61,8592765027290,6,18592765027297,null,18592765027297,"8536201090",0.4]
[102729,"Ex9B125 1PN C50A","Miniature Circuit  Breaker 25 kA, characteristic C, 50 A, 1+Npole","NAW",91.23,0,91.23,8592765027306,6,18592765027303,null,18592765027303,"8536201090",0.4]
[102730,"Ex9B125 1PN C63A","Miniature Circuit  Breaker 25 kA, characteristic C, 63 A, 1+Npole","NAW",94.84,0,94.84,8592765027313,6,18592765027310,null,18592765027310,"8536201090",0.4]
[102731,"Ex9B125 1PN C80A","Miniature Circuit  Breaker 20 kA, characteristic C, 80 A, 1+Npole","NAW",96.39,0,96.39,8592765027320,6,18592765027327,null,18592765027327,"8536201090",0.4]
[102732,"Ex9B125 1PN C100A","Miniature Circuit  Breaker 20 kA, characteristic C, 100 A, 1+Npole","NAW",107.2,0,107.2,8592765027337,6,18592765027334,null,18592765027334,"8536201090",0.4]
[102754,"Ex9B125 2P C16A","Miniature Circuit  Breaker 25 kA, characteristic C, 16 A, 2-pole","NAW",64.790000000000006,0,64.790000000000006,8592765027559,6,18592765027556,null,18592765027556,"8536201090",0.4]
[102755,"Ex9B125 2P C20A","Miniature Circuit  Breaker 25 kA, characteristic C, 20 A, 2-pole","NAW",68.09,0,68.09,8592765027566,6,18592765027563,null,18592765027563,"8536201090",0.4]
[102756,"Ex9B125 2P C25A","Miniature Circuit  Breaker 25 kA, characteristic C, 25 A, 2-pole","NAW",69.97,0,69.97,8592765027573,6,18592765027570,null,18592765027570,"8536201090",0.4]
[102757,"Ex9B125 2P C32A","Miniature Circuit  Breaker 25 kA, characteristic C, 32 A, 2-pole","NAW",69.97,0,69.97,8592765027580,6,18592765027587,null,18592765027587,"8536201090",0.4]
[102758,"Ex9B125 2P C40A","Miniature Circuit  Breaker 25 kA, characteristic C, 40 A, 2-pole","NAW",85.61,0,85.61,8592765027597,6,18592765027594,null,18592765027594,"8536201090",0.4]
[102759,"Ex9B125 2P C50A","Miniature Circuit  Breaker 25 kA, characteristic C, 50 A, 2-pole","NAW",91.23,0,91.23,8592765027603,6,18592765027600,null,18592765027600,"8536201090",0.4]
[102760,"Ex9B125 2P C63A","Miniature Circuit  Breaker 25 kA, characteristic C, 63 A, 2-pole","NAW",94.84,0,94.84,8592765027610,6,18592765027617,null,18592765027617,"8536201090",0.4]
[102761,"Ex9B125 2P C80A","Miniature Circuit  Breaker 20 kA, characteristic C, 80 A, 2-pole","NAW",96.39,0,96.39,8592765027627,6,18592765027624,null,18592765027624,"8536209090",0.4]
[102762,"Ex9B125 2P C100A","Miniature Circuit  Breaker 20 kA, characteristic C, 100 A, 2-pole","NAW",107.2,0,107.2,8592765027634,6,18592765027631,null,18592765027631,"8536209090",0.4]
[102784,"Ex9B125 3P C16A","Miniature Circuit  Breaker 25 kA, characteristic C, 16 A, 3-pole","NAW",99.25,0,99.25,8592765027856,4,18592765027853,null,18592765027853,"8536201090",0.6]
[102785,"Ex9B125 3P C20A","Miniature Circuit  Breaker 25 kA, characteristic C, 20 A, 3-pole","NAW",104.27,0,104.27,8592765027863,4,18592765027860,null,18592765027860,"8536201090",0.6]
[102786,"Ex9B125 3P C25A","Miniature Circuit  Breaker 25 kA, characteristic C, 25 A, 3-pole","NAW",107.2,0,107.2,8592765027870,4,18592765027877,null,18592765027877,"8536201090",0.6]
[102787,"Ex9B125 3P C32A","Miniature Circuit  Breaker 25 kA, characteristic C, 32 A, 3-pole","NAW",107.2,0,107.2,8592765027887,4,18592765027884,null,18592765027884,"8536201090",0.6]
[102788,"Ex9B125 3P C40A","Miniature Circuit  Breaker 25 kA, characteristic C, 40 A, 3-pole","NAW",108.58,0,108.58,8592765027894,4,18592765027891,null,18592765027891,"8536201090",0.6]
[102789,"Ex9B125 3P C50A","Miniature Circuit  Breaker 25 kA, characteristic C, 50 A, 3-pole","NAW",116.31,0,116.31,8592765027900,4,18592765027907,null,18592765027907,"8536201090",0.6]
[102790,"Ex9B125 3P C63A","Miniature Circuit  Breaker 25 kA, characteristic C, 63 A, 3-pole","NAW",116.97,0,116.97,8592765027917,4,18592765027914,null,18592765027914,"8536201090",0.6]
[102791,"Ex9B125 3P C80A","Miniature Circuit  Breaker 20 kA, characteristic C, 80 A, 3-pole","NAW",120.36,0,120.36,8592765027924,4,18592765027921,null,18592765027921,"8536209090",0.6]
[102792,"Ex9B125 3P C100A","Miniature Circuit  Breaker 20 kA, characteristic C, 100 A, 3-pole","NAW",127.31,0,127.31,8592765027931,4,18592765027938,null,18592765027938,"8536209090",0.6]
[102814,"Ex9B125 3PN C16A","Miniature Circuit  Breaker 25 kA, characteristic C, 16 A, 3+Npole","NAW",198.52,0,198.52,8592765028150,3,18592765028157,null,18592765028157,"8536201090",0.8]
[102815,"Ex9B125 3PN C20A","Miniature Circuit  Breaker 25 kA, characteristic C, 20 A, 3+Npole","NAW",198.52,0,198.52,8592765028167,3,18592765028164,null,18592765028164,"8536201090",0.8]
[102816,"Ex9B125 3PN C25A","Miniature Circuit  Breaker 25 kA, characteristic C, 25 A, 3+Npole","NAW",198.52,0,198.52,8592765028174,3,18592765028171,null,18592765028171,"8536201090",0.8]
[102817,"Ex9B125 3PN C32A","Miniature Circuit  Breaker 25 kA, characteristic C, 32 A, 3+Npole","NAW",198.52,0,198.52,8592765028181,3,18592765028188,null,18592765028188,"8536201090",0.8]
[102818,"Ex9B125 3PN C40A","Miniature Circuit  Breaker 25 kA, characteristic C, 40 A, 3+Npole","NAW",198.52,0,198.52,8592765028198,3,18592765028195,null,18592765028195,"8536201090",0.8]
[102819,"Ex9B125 3PN C50A","Miniature Circuit  Breaker 25 kA, characteristic C, 50 A, 3+Npole","NAW",198.52,0,198.52,8592765028204,3,18592765028201,null,18592765028201,"8536201090",0.8]
[102820,"Ex9B125 3PN C63A","Miniature Circuit  Breaker 25 kA, characteristic C, 63 A, 3+Npole","NAW",166.05,0,166.05,8592765028211,3,18592765028218,null,18592765028218,"8536201090",0.8]
[102821,"Ex9B125 3PN C80A","Miniature Circuit  Breaker 20 kA, characteristic C, 80 A, 3+Npole","NAW",166.05,0,166.05,8592765028228,3,18592765028225,null,18592765028225,"8536209090",0.8]
[102822,"Ex9B125 3PN C100A","Miniature Circuit  Breaker 20 kA, characteristic C, 100 A, 3+Npole","NAW",177.51,0,177.51,8592765028235,3,18592765028232,null,18592765028232,"8536209090",0.8]
[102844,"Ex9B125 4P C16A","Miniature Circuit  Breaker 25 kA, characteristic C, 16 A, 4-pole","NAW",135.12,0,135.12,8592765028457,3,18592765028454,null,18592765028454,"8536201090",0.8]
[102845,"Ex9B125 4P C20A","Miniature Circuit  Breaker 25 kA, characteristic C, 20 A, 4-pole","NAW",141.85,0,141.85,8592765028464,3,18592765028461,null,18592765028461,"8536201090",0.8]
[102846,"Ex9B125 4P C25A","Miniature Circuit  Breaker 25 kA, characteristic C, 25 A, 4-pole","NAW",145.94,0,145.94,8592765028471,3,18592765028478,null,18592765028478,"8536201090",0.8]
[102847,"Ex9B125 4P C32A","Miniature Circuit  Breaker 25 kA, characteristic C, 32 A, 4-pole","NAW",154.54,0,154.54,8592765028488,3,18592765028485,null,18592765028485,"8536201090",0.8]
[102848,"Ex9B125 4P C40A","Miniature Circuit  Breaker 25 kA, characteristic C, 40 A, 4-pole","NAW",178.37,0,178.37,8592765028495,3,18592765028492,null,18592765028492,"8536201090",0.8]
[102849,"Ex9B125 4P C50A","Miniature Circuit  Breaker 25 kA, characteristic C, 50 A, 4-pole","NAW",191.36,0,191.36,8592765028501,3,18592765028508,null,18592765028508,"8536201090",0.8]
[102850,"Ex9B125 4P C63A","Miniature Circuit  Breaker 25 kA, characteristic C, 63 A, 4-pole","NAW",198.5,0,198.5,8592765028518,3,18592765028515,null,18592765028515,"8536201090",0.8]
[102851,"Ex9B125 4P C80A","Miniature Circuit  Breaker 20 kA, characteristic C, 80 A, 4-pole","NAW",205.67,0,205.67,8592765028525,3,18592765028522,null,18592765028522,"8536209090",0.8]
[102852,"Ex9B125 4P C100A","Miniature Circuit  Breaker 20 kA, characteristic C, 100 A, 4-pole","NAW",212.84,0,212.84,8592765028532,3,18592765028539,null,18592765028539,"8536209090",0.8]
[102704,"Ex9B125 1P D16A","Miniature Circuit  Breaker 25 kA, characteristic D, 16 A, 1-pole","NAW",32.619999999999997,0,32.619999999999997,8592765027054,12,18592765027051,null,18592765027051,"8536201090",0.2]
[102705,"Ex9B125 1P D20A","Miniature Circuit  Breaker 25 kA, characteristic D, 20 A, 1-pole","NAW",34.270000000000003,0,34.270000000000003,8592765027061,12,18592765027068,null,18592765027068,"8536201090",0.2]
[102706,"Ex9B125 1P D25A","Miniature Circuit  Breaker 25 kA, characteristic D, 25 A, 1-pole","NAW",35.200000000000003,0,35.200000000000003,8592765027078,12,18592765027075,null,18592765027075,"8536201090",0.2]
[102707,"Ex9B125 1P D32A","Miniature Circuit  Breaker 25 kA, characteristic D, 32 A, 1-pole","NAW",35.200000000000003,0,35.200000000000003,8592765027085,12,18592765027082,null,18592765027082,"8536201090",0.2]
[102708,"Ex9B125 1P D40A","Miniature Circuit  Breaker 25 kA, characteristic D, 40 A, 1-pole","NAW",42.98,0,42.98,8592765027092,12,18592765027099,null,18592765027099,"8536201090",0.2]
[102709,"Ex9B125 1P D50A","Miniature Circuit  Breaker 25 kA, characteristic D, 50 A, 1-pole","NAW",60.44,0,60.44,8592765027108,12,18592765027105,null,18592765027105,"8536201090",0.2]
[102710,"Ex9B125 1P D63A","Miniature Circuit  Breaker 25 kA, characteristic D, 63 A, 1-pole","NAW",53.75,0,53.75,8592765027115,12,18592765027112,null,18592765027112,"8536201090",0.2]
[102711,"Ex9B125 1P D80A","Miniature Circuit  Breaker 20 kA, characteristic D, 80 A, 1-pole","NAW",53.61,{"$f":"NAW","v":0},53.61,8592765027122,12,18592765027129,null,18592765027129,"8536209090",0.2]
[102712,"Ex9B125 1P D100A","Miniature Circuit  Breaker 20 kA, characteristic D, 100 A, 1-pole","NAW",55.49,0,55.49,8592765027139,12,18592765027136,null,18592765027136,"8536201090",0.2]
[102734,"Ex9B125 1PN D16A","Miniature Circuit  Breaker 25 kA, characteristic D, 16 A, 1+Npole","NAW",76.650000000000006,0,{"$f":"E852*(1-F852)","v":76.650000000000006},8592765027351,6,18592765027358,null,18592765027358,"8536201090",0.4]
[102735,"Ex9B125 1PN D20A","Miniature Circuit  Breaker 25 kA, characteristic D, 20 A, 1+Npole","NAW",80.5,0,80.5,8592765027368,6,18592765027365,null,18592765027365,"8536201090",0.4]
[102736,"Ex9B125 1PN D25A","Miniature Circuit  Breaker 25 kA, characteristic D, 25 A, 1+Npole","NAW",82.79,0,82.79,8592765027375,6,18592765027372,null,18592765027372,"8536201090",0.4]
[102737,"Ex9B125 1PN D32A","Miniature Circuit  Breaker 25 kA, characteristic D, 32 A, 1+Npole","NAW",82.79,0,82.79,8592765027382,6,18592765027389,null,18592765027389,"8536201090",0.4]
[102738,"Ex9B125 1PN D40A","Miniature Circuit  Breaker 25 kA, characteristic D, 40 A, 1+Npole","NAW",85.07,0,85.07,8592765027399,6,18592765027396,null,18592765027396,"8536201090",0.4]
[102739,"Ex9B125 1PN D50A","Miniature Circuit  Breaker 25 kA, characteristic D, 50 A, 1+Npole","NAW",107.86,0,107.86,8592765027405,6,18592765027402,null,18592765027402,"8536201090",0.4]
[102740,"Ex9B125 1PN D63A","Miniature Circuit  Breaker 25 kA, characteristic D, 63 A, 1+Npole","NAW",107.2,0,107.2,8592765027412,6,18592765027419,null,18592765027419,"8536201090",0.4]
[102741,"Ex9B125 1PN D80A","Miniature Circuit  Breaker 20 kA, characteristic D, 80 A, 1+Npole","NAW",107.2,0,107.2,8592765027429,6,18592765027426,null,18592765027426,"8536201090",0.4]
[102742,"Ex9B125 1PN D100A","Miniature Circuit  Breaker 20 kA, characteristic D, 100 A, 1+Npole","NAW",110.63,0,110.63,8592765027436,6,18592765027433,null,18592765027433,"8536201090",0.4]
[102764,"Ex9B125 2P D16A","Miniature Circuit  Breaker 25 kA, characteristic D, 16 A, 2-pole","NAW",76.650000000000006,0,76.650000000000006,8592765027658,6,18592765027655,null,18592765027655,"8536201090",0.4]
[102765,"Ex9B125 2P D20A","Miniature Circuit  Breaker 25 kA, characteristic D, 20 A, 2-pole","NAW",80.5,0,80.5,8592765027665,6,18592765027662,null,18592765027662,"8536201090",0.4]
[102766,"Ex9B125 2P D25A","Miniature Circuit  Breaker 25 kA, characteristic D, 25 A, 2-pole","NAW",82.79,0,82.79,8592765027672,6,18592765027679,null,18592765027679,"8536201090",0.4]
[102767,"Ex9B125 2P D32A","Miniature Circuit  Breaker 25 kA, characteristic D, 32 A, 2-pole","NAW",82.79,0,82.79,8592765027689,6,18592765027686,null,18592765027686,"8536201090",0.4]
[102768,"Ex9B125 2P D40A","Miniature Circuit  Breaker 25 kA, characteristic D, 40 A, 2-pole","NAW",85.07,0,85.07,8592765027696,6,18592765027693,null,18592765027693,"8536201090",0.4]
[102769,"Ex9B125 2P D50A","Miniature Circuit  Breaker 25 kA, characteristic D, 50 A, 2-pole","NAW",107.86,0,107.86,8592765027702,6,18592765027709,null,18592765027709,"8536201090",0.4]
[102770,"Ex9B125 2P D63A","Miniature Circuit  Breaker 25 kA, characteristic D, 63 A, 2-pole","NAW",107.2,0,107.2,8592765027719,6,18592765027716,null,18592765027716,"8536201090",0.4]
[102771,"Ex9B125 2P D80A","Miniature Circuit  Breaker 20 kA, characteristic D, 80 A, 2-pole","NAW",107.2,0,107.2,8592765027726,6,18592765027723,null,18592765027723,"8536201090",0.4]
[102772,"Ex9B125 2P D100A","Miniature Circuit  Breaker 20 kA, characteristic D, 100 A, 2-pole","NAW",110.63,0,110.63,8592765027733,6,18592765027730,null,18592765027730,"8536201090",0.4]
[102794,"Ex9B125 3P D16A","Miniature Circuit  Breaker 25 kA, characteristic D, 16 A, 3-pole","NAW",117.39,0,117.39,8592765027955,4,18592765027952,null,18592765027952,"8536201090",0.6]
[102795,"Ex9B125 3P D20A","Miniature Circuit  Breaker 25 kA, characteristic D, 20 A, 3-pole","NAW",123.28,0,123.28,8592765027962,4,18592765027969,null,18592765027969,"8536201090",0.6]
[102796,"Ex9B125 3P D25A","Miniature Circuit  Breaker 25 kA, characteristic D, 25 A, 3-pole","NAW",126.75,0,126.75,8592765027979,4,18592765027976,null,18592765027976,"8536201090",0.6]
[102797,"Ex9B125 3P D32A","Miniature Circuit  Breaker 25 kA, characteristic D, 32 A, 3-pole","NAW",126.75,0,126.75,8592765027986,4,18592765027983,null,18592765027983,"8536201090",0.6]
[102798,"Ex9B125 3P D40A","Miniature Circuit  Breaker 25 kA, characteristic D, 40 A, 3-pole","NAW",128.33000000000001,0,128.33000000000001,8592765027993,4,18592765027990,null,18592765027990,"8536201090",0.6]
[102799,"Ex9B125 3P D50A","Miniature Circuit  Breaker 25 kA, characteristic D, 50 A, 3-pole","NAW",142.86000000000001,0,142.86000000000001,8592765028006,4,18592765028003,null,18592765028003,"8536201090",0.6]
[102800,"Ex9B125 3P D63A","Miniature Circuit  Breaker 25 kA, characteristic D, 63 A, 3-pole","NAW",135.04,0,135.04,8592765028013,4,18592765028010,null,18592765028010,"8536201090",0.6]
[102801,"Ex9B125 3P D80A","Miniature Circuit  Breaker 20 kA, characteristic D, 80 A, 3-pole","NAW",135.04,0,135.04,8592765028020,4,18592765028027,null,18592765028027,"8536209090",0.6]
[102802,"Ex9B125 3P D100A","Miniature Circuit  Breaker 20 kA, characteristic D, 100 A, 3-pole","NAW",141.99,0,141.99,8592765028037,4,18592765028034,null,18592765028034,"8536209090",0.6]
[102824,"Ex9B125 3PN D16A","Miniature Circuit  Breaker 25 kA, characteristic D, 16 A, 3+Npole","NAW",153.9,0,153.9,8592765028259,3,18592765028256,null,18592765028256,"8536201090",0.8]
[102825,"Ex9B125 3PN D20A","Miniature Circuit  Breaker 25 kA, characteristic D, 20 A, 3+Npole","NAW",153.9,0,153.9,8592765028266,3,18592765028263,null,18592765028263,"8536201090",0.8]
[102826,"Ex9B125 3PN D25A","Miniature Circuit  Breaker 25 kA, characteristic D, 25 A, 3+Npole","NAW",153.9,0,153.9,8592765028273,3,18592765028270,null,18592765028270,"8536201090",0.8]
[102827,"Ex9B125 3PN D32A","Miniature Circuit  Breaker 25 kA, characteristic D, 32 A, 3+Npole","NAW",153.9,0,153.9,8592765028280,3,18592765028287,null,18592765028287,"8536201090",0.8]
[102828,"Ex9B125 3PN D40A","Miniature Circuit  Breaker 25 kA, characteristic D, 40 A, 3+Npole","NAW",164.11,0,164.11,8592765028297,3,18592765028294,null,18592765028294,"8536201090",0.8]
[102829,"Ex9B125 3PN D50A","Miniature Circuit  Breaker 25 kA, characteristic D, 50 A, 3+Npole","NAW",166.63,0,166.63,8592765028303,3,18592765028300,null,18592765028300,"8536201090",0.8]
[102830,"Ex9B125 3PN D63A","Miniature Circuit  Breaker 25 kA, characteristic D, 63 A, 3+Npole","NAW",158.53,0,158.53,8592765028310,3,18592765028317,null,18592765028317,"8536201090",0.8]
[102831,"Ex9B125 3PN D80A","Miniature Circuit  Breaker 20 kA, characteristic D, 80 A, 3+Npole","NAW",158.53,0,158.53,8592765028327,3,18592765028324,null,18592765028324,"8536201090",0.8]
[102832,"Ex9B125 3PN D100A","Miniature Circuit  Breaker 20 kA, characteristic D, 100 A, 3+Npole","NAW",166.42,0,166.42,8592765028334,3,18592765028331,null,18592765028331,"8536201090",0.8]
[102854,"Ex9B125 4P D16A","Miniature Circuit  Breaker 25 kA, characteristic D, 16 A, 4-pole","NAW",159.72,0,159.72,8592765028556,3,18592765028553,null,18592765028553,"8536201090",0.8]
[102855,"Ex9B125 4P D20A","Miniature Circuit  Breaker 25 kA, characteristic D, 20 A, 4-pole","NAW",167.78,0,167.78,8592765028563,3,18592765028560,null,18592765028560,"8536201090",0.8]
[102856,"Ex9B125 4P D25A","Miniature Circuit  Breaker 25 kA, characteristic D, 25 A, 4-pole","NAW",172.57,0,172.57,8592765028570,3,18592765028577,null,18592765028577,"8536201090",0.8]
[102857,"Ex9B125 4P D32A","Miniature Circuit  Breaker 25 kA, characteristic D, 32 A, 4-pole","NAW",182.68,0,182.68,8592765028587,3,18592765028584,null,18592765028584,"8536201090",0.8]
[102858,"Ex9B125 4P D40A","Miniature Circuit  Breaker 25 kA, characteristic D, 40 A, 4-pole","NAW",210.91,0,210.91,8592765028594,3,18592765028591,null,18592765028591,"8536201090",0.8]
[102859,"Ex9B125 4P D50A","Miniature Circuit  Breaker 25 kA, characteristic D, 50 A, 4-pole","NAW",226.27,0,226.27,8592765028600,3,18592765028607,null,18592765028607,"8536201090",0.8]
[102860,"Ex9B125 4P D63A","Miniature Circuit  Breaker 25 kA, characteristic D, 63 A, 4-pole","NAW",234.71,0,234.71,8592765028617,3,18592765028614,null,18592765028614,"8536201090",0.8]
[102861,"Ex9B125 4P D80A","Miniature Circuit  Breaker 20 kA, characteristic D, 80 A, 4-pole","NAW",243.19,0,243.19,8592765028624,3,18592765028621,null,18592765028621,"8536209090",0.8]
[102862,"Ex9B125 4P D100A","Miniature Circuit  Breaker 20 kA, characteristic D, 100 A, 4-pole","NAW",251.62,0,251.62,8592765028631,3,18592765028638,null,18592765028638,"8536201090",0.8]
[]
["DC Miniature Circuit Breakers Ex9BP-JX, 10 kA, 250 V DC per pole, General Purpose, polarized"]
[110067,"Ex9BP-JX(+) 1P C1","DC Miniature Circuit Breaker 10 kA, characteristic C, 1 A, 250 V DC, 1-pole","NAV",14.75,{"$f":"NAV","v":0},{"$f":"E899*(1-F899)","v":14.75},8592765100672,12,18592765100679,144,28592765100676,"8536201090",0.12]
[110068,"Ex9BP-JX(+) 1P C2","DC Miniature Circuit Breaker 10 kA, characteristic C, 3 A, 250 V DC, 1-pole","NAV",14.75,{"$f":"NAV","v":0},{"$f":"E900*(1-F900)","v":14.75},8592765100689,12,18592765100686,144,28592765100683,"8536201090",0.12]
[110069,"Ex9BP-JX(+) 1P C3","DC Miniature Circuit Breaker 10 kA, characteristic C, 3 A, 250 V DC, 1-pole","NAV",14.75,0,14.75,8592765100696,12,18592765100693,144,28592765100690,"8536201090",0.12]
[110070,"Ex9BP-JX(+) 1P C4","DC Miniature Circuit Breaker 10 kA, characteristic C, 4 A, 250 V DC, 1-pole","NAV",14.75,0,14.75,8592765100702,12,18592765100709,144,28592765100706,"8536201090",0.12]
[110071,"Ex9BP-JX(+) 1P C6","DC Miniature Circuit Breaker 10 kA, characteristic C, 6 A, 250 V DC, 1-pole","NAV",9.17,0,9.17,8592765100719,12,18592765100716,144,28592765100713,"8536201090",0.12]
[110072,"Ex9BP-JX(+) 1P C10","DC Miniature Circuit Breaker 10 kA, characteristic C, 10 A, 250 V DC, 1-pole","NAV",9.17,0,9.17,8592765100726,12,18592765100723,144,28592765100720,"8536201090",0.12]
[110073,"Ex9BP-JX(+) 1P C16","DC Miniature Circuit Breaker 10 kA, characteristic C, 16 A, 250 V DC, 1-pole","NAV",9.23,0,9.23,8592765100733,12,18592765100730,144,28592765100737,"8536201090",0.12]
[110074,"Ex9BP-JX(+) 1P C20","DC Miniature Circuit Breaker 10 kA, characteristic C, 20 A, 250 V DC, 1-pole","NAV",9.23,0,9.23,8592765100740,12,18592765100747,144,28592765100744,"8536201090",0.12]
[110075,"Ex9BP-JX(+) 1P C25","DC Miniature Circuit Breaker 10 kA, characteristic C, 25 A, 250 V DC, 1-pole","NAV",9.23,0,9.23,8592765100757,12,18592765100754,144,28592765100751,"8536201090",0.12]
[110076,"Ex9BP-JX(+) 1P C32","DC Miniature Circuit Breaker 10 kA, characteristic C, 32 A, 250 V DC, 1-pole","NAV",9.23,0,9.23,8592765100764,12,18592765100761,144,28592765100768,"8536201090",0.12]
[110077,"Ex9BP-JX(+) 1P C40","DC Miniature Circuit Breaker 10 kA, characteristic C, 40 A, 250 V DC, 1-pole","NAV",10.93,0,10.93,8592765100771,12,18592765100778,144,28592765100775,"8536201090",0.12]
[110078,"Ex9BP-JX(+) 1P C50","DC Miniature Circuit Breaker 10 kA, characteristic C, 50 A, 250 V DC, 1-pole","NAV",17.43,0,17.43,8592765100788,12,18592765100785,144,28592765100782,"8536201090",0.12]
[110079,"Ex9BP-JX(+) 1P C63","DC Miniature Circuit Breaker 10 kA, characteristic C, 63 A, 250 V DC, 1-pole","NAV",19.82,0,19.82,8592765100795,12,18592765100792,144,28592765100799,"8536201090",0.12]
[110080,"Ex9BP-JX(+) 2P C1","DC Miniature Circuit Breaker 10 kA, characteristic C, 1 A, 500 V DC, 2-pole","NAV",33.68,0,33.68,8592765100801,6,18592765100808,72,28592765100805,"8536201090",0.24]
[110081,"Ex9BP-JX(+) 2P C2","DC Miniature Circuit Breaker 10 kA, characteristic C, 2, A, 500 V DC, 2-pole","NAV",33.68,0,33.68,8592765100818,6,18592765100815,72,28592765100812,"8536201090",0.24]
[110082,"Ex9BP-JX(+) 2P C3","DC Miniature Circuit Breaker 10 kA, characteristic C, 3 A, 500 V DC, 2-pole","NAV",33.68,0,33.68,8592765100825,6,18592765100822,72,28592765100829,"8536201090",0.24]
[110083,"Ex9BP-JX(+) 2P C4","DC Miniature Circuit Breaker 10 kA, characteristic C, 4 A, 500 V DC, 2-pole","NAV",33.68,0,33.68,8592765100832,6,18592765100839,72,28592765100836,"8536201090",0.24]
[110084,"Ex9BP-JX(+) 2P C6","DC Miniature Circuit Breaker 10 kA, characteristic C, 6 A, 500 V DC, 2-pole","NAV",20.350000000000001,0,20.350000000000001,8592765100849,6,18592765100846,72,28592765100843,"8536201090",0.24]
[110085,"Ex9BP-JX(+) 2P C10","DC Miniature Circuit Breaker 10 kA, characteristic C, 10 A, 500 V DC, 2-pole","NAV",20.350000000000001,0,20.350000000000001,8592765100856,6,18592765100853,72,28592765100850,"8536201090",0.24]
[110086,"Ex9BP-JX(+) 2P C16","DC Miniature Circuit Breaker 10 kA, characteristic C, 16 A, 500 V DC, 2-pole","NAV",20.350000000000001,0,20.350000000000001,8592765100863,6,18592765100860,72,28592765100867,"8536201090",0.24]
[110087,"Ex9BP-JX(+) 2P C20","DC Miniature Circuit Breaker 10 kA, characteristic C, 20 A, 500 V DC, 2-pole","NAV",20.350000000000001,0,20.350000000000001,8592765100870,6,18592765100877,72,28592765100874,"8536201090",0.24]
[110088,"Ex9BP-JX(+) 2P C25","DC Miniature Circuit Breaker 10 kA, characteristic C, 25 A, 500 V DC, 2-pole","NAV",20.350000000000001,0,20.350000000000001,8592765100887,6,18592765100884,72,28592765100881,"8536201090",0.24]
[110089,"Ex9BP-JX(+) 2P C32","DC Miniature Circuit Breaker 10 kA, characteristic C, 32 A, 500 V DC, 2-pole","NAV",20.350000000000001,0,20.350000000000001,8592765100894,6,18592765100891,72,28592765100898,"8536201090",0.24]
[110090,"Ex9BP-JX(+) 2P C40","DC Miniature Circuit Breaker 10 kA, characteristic C, 40 A, 500 V DC, 2-pole","NAV",23.56,0,23.56,8592765100900,6,18592765100907,72,28592765100904,"8536201090",0.24]
[110091,"Ex9BP-JX(+) 2P C50","DC Miniature Circuit Breaker 10 kA, characteristic C, 50 A, 500 V DC, 2-pole","NAV",40.97,0,40.97,8592765100917,6,18592765100914,72,28592765100911,"8536201090",0.24]
[110092,"Ex9BP-JX(+) 2P C63","DC Miniature Circuit Breaker 10 kA, characteristic C, 63 A, 500 V DC, 2-pole","NAV",47.35,0,47.35,8592765100924,6,18592765100921,72,28592765100928,"8536201090",0.24]
[110093,"Ex9BP-JX(+) 3P C1","DC Miniature Circuit Breaker 10 kA, characteristic C, 1 A, 750 V DC, 3-pole","NAV",39.619999999999997,0,39.619999999999997,8592765100931,4,18592765100938,48,28592765100935,"8536201090",0.36]
[110094,"Ex9BP-JX(+) 3P C2","DC Miniature Circuit Breaker 10 kA, characteristic C, 3 A, 750 V DC, 3-pole","NAV",39.619999999999997,0,39.619999999999997,8592765100948,4,18592765100945,48,28592765100942,"8536201090",0.36]
[110095,"Ex9BP-JX(+) 3P C3","DC Miniature Circuit Breaker 10 kA, characteristic C, 3 A, 750 V DC, 3-pole","NAV",39.619999999999997,0,39.619999999999997,8592765100955,4,18592765100952,48,28592765100959,"8536201090",0.36]
[110096,"Ex9BP-JX(+) 3P C4","DC Miniature Circuit Breaker 10 kA, characteristic C, 4 A, 750 V DC, 3-pole","NAV",39.619999999999997,0,39.619999999999997,8592765100962,4,18592765100969,48,28592765100966,"8536201090",0.36]
[110097,"Ex9BP-JX(+) 3P C6","DC Miniature Circuit Breaker 10 kA, characteristic C, 6 A, 750 V DC, 3-pole","NAV",34.200000000000003,0,34.200000000000003,8592765100979,4,18592765100976,48,28592765100973,"8536201090",0.36]
[110098,"Ex9BP-JX(+) 3P C10","DC Miniature Circuit Breaker 10 kA, characteristic C, 10 A, 750 V DC, 3-pole","NAV",34.200000000000003,0,34.200000000000003,8592765100986,4,18592765100983,48,28592765100980,"8536201090",0.36]
[110099,"Ex9BP-JX(+) 3P C16","DC Miniature Circuit Breaker 10 kA, characteristic C, 16 A, 750 V DC, 3-pole","NAV",34.200000000000003,0,34.200000000000003,8592765100993,4,18592765100990,48,28592765100997,"8536201090",0.36]
[110100,"Ex9BP-JX(+) 3P C20","DC Miniature Circuit Breaker 10 kA, characteristic C, 20 A, 750 V DC, 3-pole","NAV",34.200000000000003,0,34.200000000000003,8592765101006,4,18592765101003,48,28592765101000,"8536201090",0.36]
[110101,"Ex9BP-JX(+) 3P C25","DC Miniature Circuit Breaker 10 kA, characteristic C, 25 A, 750 V DC, 3-pole","NAV",34.200000000000003,0,34.200000000000003,8592765101013,4,18592765101010,48,28592765101017,"8536201090",0.36]
[110102,"Ex9BP-JX(+) 3P C32","DC Miniature Circuit Breaker 10 kA, characteristic C, 32 A, 750 V DC, 3-pole","NAV",34.200000000000003,0,34.200000000000003,8592765101020,4,18592765101027,48,28592765101024,"8536201090",0.36]
[110103,"Ex9BP-JX(+) 3P C40","DC Miniature Circuit Breaker 10 kA, characteristic C, 40 A, 750 V DC, 3-pole","NAV",39.6,0,39.6,8592765101037,4,18592765101034,48,28592765101031,"8536201090",0.36]
[110104,"Ex9BP-JX(+) 3P C50","DC Miniature Circuit Breaker 10 kA, characteristic C, 50 A, 750 V DC, 3-pole","NAV",48.2,0,48.2,8592765101044,4,18592765101041,48,28592765101048,"8536201090",0.36]
[110105,"Ex9BP-JX(+) 3P C63","DC Miniature Circuit Breaker 10 kA, characteristic C, 63 A, 750 V DC, 3-pole","NAV",55.71,0,55.71,8592765101051,4,18592765101058,48,28592765101055,"8536201090",0.36]
[110106,"Ex9BP-JX(+) 4P C1","DC Miniature Circuit Breaker 10 kA, characteristic C, 1 A, 1000 V DC, 4-pole","NAV",44.02,0,44.02,8592765101068,3,18592765101065,36,28592765101062,"8536201090",0.48]
[110107,"Ex9BP-JX(+) 4P C2","DC Miniature Circuit Breaker 10 kA, characteristic C, 2, A, 1000 V DC, 4-pole","NAV",44.02,0,44.02,8592765101075,3,18592765101072,36,28592765101079,"8536201090",0.48]
[110108,"Ex9BP-JX(+) 4P C3","DC Miniature Circuit Breaker 10 kA, characteristic C, 3 A, 1000 V DC, 4-pole","NAV",44.02,0,44.02,8592765101082,3,18592765101089,36,28592765101086,"8536201090",0.48]
[110109,"Ex9BP-JX(+) 4P C4","DC Miniature Circuit Breaker 10 kA, characteristic C, 4 A, 1000 V DC, 4-pole","NAV",44.02,0,44.02,8592765101099,3,18592765101096,36,28592765101093,"8536201090",0.48]
[110110,"Ex9BP-JX(+) 4P C6","DC Miniature Circuit Breaker 10 kA, characteristic C, 6 A, 1000 V DC, 4-pole","NAV",40,0,40,8592765101105,3,18592765101102,36,28592765101109,"8536201090",0.48]
[110111,"Ex9BP-JX(+) 4P C10","DC Miniature Circuit Breaker 10 kA, characteristic C, 10 A, 1000 V DC, 4-pole","NAV",40,0,40,8592765101112,3,18592765101119,36,28592765101116,"8536201090",0.48]
[110112,"Ex9BP-JX(+) 4P C16","DC Miniature Circuit Breaker 10 kA, characteristic C, 16 A, 1000 V DC, 4-pole","NAV",40,0,40,8592765101129,3,18592765101126,36,28592765101123,"8536201090",0.48]
[110113,"Ex9BP-JX(+) 4P C20","DC Miniature Circuit Breaker 10 kA, characteristic C, 20 A, 1000 V DC, 4-pole","NAV",40,0,40,8592765101136,3,18592765101133,36,28592765101130,"8536201090",0.48]
[110114,"Ex9BP-JX(+) 4P C25","DC Miniature Circuit Breaker 10 kA, characteristic C, 25 A, 1000 V DC, 4-pole","NAV",40,0,40,8592765101143,3,18592765101140,36,28592765101147,"8536201090",0.48]
[110115,"Ex9BP-JX(+) 4P C32","DC Miniature Circuit Breaker 10 kA, characteristic C, 32 A, 1000 V DC, 4-pole","NAV",40,0,40,8592765101150,3,18592765101157,36,28592765101154,"8536201090",0.48]
[110116,"Ex9BP-JX(+) 4P C40","DC Miniature Circuit Breaker 10 kA, characteristic C, 40 A, 1000 V DC, 4-pole","NAV",46.32,0,46.32,8592765101167,3,18592765101164,36,28592765101161,"8536201090",0.48]
[110117,"Ex9BP-JX(+) 4P C50","DC Miniature Circuit Breaker 10 kA, characteristic C, 50 A, 1000 V DC, 4-pole","NAV",53.56,0,53.56,8592765101174,3,18592765101171,36,28592765101178,"8536201090",0.48]
[110118,"Ex9BP-JX(+) 4P C63","DC Miniature Circuit Breaker 10 kA, characteristic C, 63 A, 1000 V DC, 4-pole","NAV",61.9,0,61.9,8592765101181,3,18592765101188,36,28592765101185,"8536201090",0.48]
[110119,"Ex9BP-JX(+) 1P K1","DC Miniature Circuit Breaker 10 kA, characteristic K, 1 A, 250 V DC, 1-pole","NAV",16.39,0,16.39,8592765101198,12,18592765101195,144,28592765101192,"8536201090",0.12]
[110120,"Ex9BP-JX(+) 1P K2","DC Miniature Circuit Breaker 10 kA, characteristic K, 3 A, 250 V DC, 1-pole","NAV",16.39,0,16.39,8592765101204,12,18592765101201,144,28592765101208,"8536201090",0.12]
[110121,"Ex9BP-JX(+) 1P K3","DC Miniature Circuit Breaker 10 kA, characteristic K, 3 A, 250 V DC, 1-pole","NAV",16.39,0,16.39,8592765101211,12,18592765101218,144,28592765101215,"8536201090",0.12]
[110122,"Ex9BP-JX(+) 1P K4","DC Miniature Circuit Breaker 10 kA, characteristic K, 4 A, 250 V DC, 1-pole","NAV",16.39,0,16.39,8592765101228,12,18592765101225,144,28592765101222,"8536201090",0.12]
[110123,"Ex9BP-JX(+) 1P K6","DC Miniature Circuit Breaker 10 kA, characteristic K, 6 A, 250 V DC, 1-pole","NAV",10.19,0,10.19,8592765101235,12,18592765101232,144,28592765101239,"8536201090",0.12]
[110124,"Ex9BP-JX(+) 1P K10","DC Miniature Circuit Breaker 10 kA, characteristic K, 10 A, 250 V DC, 1-pole","NAV",10.19,0,10.19,8592765101242,12,18592765101249,144,28592765101246,"8536201090",0.12]
[110125,"Ex9BP-JX(+) 1P K16","DC Miniature Circuit Breaker 10 kA, characteristic K, 16 A, 250 V DC, 1-pole","NAV",10.26,0,10.26,8592765101259,12,18592765101256,144,28592765101253,"8536201090",0.12]
[110126,"Ex9BP-JX(+) 1P K20","DC Miniature Circuit Breaker 10 kA, characteristic K, 20 A, 250 V DC, 1-pole","NAV",10.26,0,10.26,8592765101266,12,18592765101263,144,28592765101260,"8536201090",0.12]
[110127,"Ex9BP-JX(+) 1P K25","DC Miniature Circuit Breaker 10 kA, characteristic K, 25 A, 250 V DC, 1-pole","NAV",10.26,0,10.26,8592765101273,12,18592765101270,144,28592765101277,"8536201090",0.12]
[110128,"Ex9BP-JX(+) 1P K32","DC Miniature Circuit Breaker 10 kA, characteristic K, 32 A, 250 V DC, 1-pole","NAV",10.26,0,10.26,8592765101280,12,18592765101287,144,28592765101284,"8536201090",0.12]
[110129,"Ex9BP-JX(+) 1P K40","DC Miniature Circuit Breaker 10 kA, characteristic K, 40 A, 250 V DC, 1-pole","NAV",12.14,0,12.14,8592765101297,12,18592765101294,144,28592765101291,"8536201090",0.12]
[110130,"Ex9BP-JX(+) 1P K50","DC Miniature Circuit Breaker 10 kA, characteristic K, 50 A, 250 V DC, 1-pole","NAV",19.37,0,19.37,8592765101303,12,18592765101300,144,28592765101307,"8536201090",0.12]
[110131,"Ex9BP-JX(+) 1P K63","DC Miniature Circuit Breaker 10 kA, characteristic K, 63 A, 250 V DC, 1-pole","NAV",22.02,0,22.02,8592765101310,12,18592765101317,144,28592765101314,"8536201090",0.12]
[110132,"Ex9BP-JX(+) 2P K1","DC Miniature Circuit Breaker 10 kA, characteristic K, 1 A, 500 V DC, 2-pole","NAV",37.42,{"$f":"NAV","v":0},{"$f":"E964*(1-F964)","v":37.42},8592765101327,6,18592765101324,72,28592765101321,"8536201090",0.24]
[110133,"Ex9BP-JX(+) 2P K2","DC Miniature Circuit Breaker 10 kA, characteristic K, 2, A, 500 V DC, 2-pole","NAV",37.42,0,37.42,8592765101334,6,18592765101331,72,28592765101338,"8536201090",0.24]
[110134,"Ex9BP-JX(+) 2P K3","DC Miniature Circuit Breaker 10 kA, characteristic K, 3 A, 500 V DC, 2-pole","NAV",37.42,0,37.42,8592765101341,6,18592765101348,72,28592765101345,"8536201090",0.24]
[110135,"Ex9BP-JX(+) 2P K4","DC Miniature Circuit Breaker 10 kA, characteristic K, 4 A, 500 V DC, 2-pole","NAV",37.42,0,37.42,8592765101358,6,18592765101355,72,28592765101352,"8536201090",0.24]
[110136,"Ex9BP-JX(+) 2P K6","DC Miniature Circuit Breaker 10 kA, characteristic K, 6 A, 500 V DC, 2-pole","NAV",22.61,0,22.61,8592765101365,6,18592765101362,72,28592765101369,"8536201090",0.24]
[110137,"Ex9BP-JX(+) 2P K10","DC Miniature Circuit Breaker 10 kA, characteristic K, 10 A, 500 V DC, 2-pole","NAV",22.61,0,22.61,8592765101372,6,18592765101379,72,28592765101376,"8536201090",0.24]
[110138,"Ex9BP-JX(+) 2P K16","DC Miniature Circuit Breaker 10 kA, characteristic K, 16 A, 500 V DC, 2-pole","NAV",22.61,0,22.61,8592765101389,6,18592765101386,72,28592765101383,"8536201090",0.24]
[110139,"Ex9BP-JX(+) 2P K20","DC Miniature Circuit Breaker 10 kA, characteristic K, 20 A, 500 V DC, 2-pole","NAV",22.61,0,22.61,8592765101396,6,18592765101393,72,28592765101390,"8536201090",0.24]
[110140,"Ex9BP-JX(+) 2P K25","DC Miniature Circuit Breaker 10 kA, characteristic K, 25 A, 500 V DC, 2-pole","NAV",22.61,0,22.61,8592765101402,6,18592765101409,72,28592765101406,"8536201090",0.24]
[110141,"Ex9BP-JX(+) 2P K32","DC Miniature Circuit Breaker 10 kA, characteristic K, 32 A, 500 V DC, 2-pole","NAV",22.61,0,22.61,8592765101419,6,18592765101416,72,28592765101413,"8536201090",0.24]
[110142,"Ex9BP-JX(+) 2P K40","DC Miniature Circuit Breaker 10 kA, characteristic K, 40 A, 500 V DC, 2-pole","NAV",26.18,0,26.18,8592765101426,6,18592765101423,72,28592765101420,"8536201090",0.24]
[110143,"Ex9BP-JX(+) 2P K50","DC Miniature Circuit Breaker 10 kA, characteristic K, 50 A, 500 V DC, 2-pole","NAV",45.52,0,45.52,8592765101433,6,18592765101430,72,28592765101437,"8536201090",0.24]
[110144,"Ex9BP-JX(+) 2P K63","DC Miniature Circuit Breaker 10 kA, characteristic K, 63 A, 500 V DC, 2-pole","NAV",52.61,0,52.61,8592765101440,6,18592765101447,72,28592765101444,"8536201090",0.24]
[110145,"Ex9BP-JX(+) 3P K1","DC Miniature Circuit Breaker 10 kA, characteristic K, 1 A, 750 V DC, 3-pole","NAV",42.33,0,42.33,8592765101457,4,18592765101454,48,28592765101451,"8536201090",0.36]
[110146,"Ex9BP-JX(+) 3P K2","DC Miniature Circuit Breaker 10 kA, characteristic K, 3 A, 750 V DC, 3-pole","NAV",42.33,0,42.33,8592765101464,4,18592765101461,48,28592765101468,"8536201090",0.36]
[110147,"Ex9BP-JX(+) 3P K3","DC Miniature Circuit Breaker 10 kA, characteristic K, 3 A, 750 V DC, 3-pole","NAV",42.33,0,42.33,8592765101471,4,18592765101478,48,28592765101475,"8536201090",0.36]
[110148,"Ex9BP-JX(+) 3P K4","DC Miniature Circuit Breaker 10 kA, characteristic K, 4 A, 750 V DC, 3-pole","NAV",42.33,0,42.33,8592765101488,4,18592765101485,48,28592765101482,"8536201090",0.36]
[110149,"Ex9BP-JX(+) 3P K6","DC Miniature Circuit Breaker 10 kA, characteristic K, 6 A, 750 V DC, 3-pole","NAV",36.54,0,36.54,8592765101495,4,18592765101492,48,28592765101499,"8536201090",0.36]
[110150,"Ex9BP-JX(+) 3P K10","DC Miniature Circuit Breaker 10 kA, characteristic K, 10 A, 750 V DC, 3-pole","NAV",36.54,0,36.54,8592765101501,4,18592765101508,48,28592765101505,"8536201090",0.36]
[110151,"Ex9BP-JX(+) 3P K16","DC Miniature Circuit Breaker 10 kA, characteristic K, 16 A, 750 V DC, 3-pole","NAV",36.54,0,36.54,8592765101518,4,18592765101515,48,28592765101512,"8536201090",0.36]
[110152,"Ex9BP-JX(+) 3P K20","DC Miniature Circuit Breaker 10 kA, characteristic K, 20 A, 750 V DC, 3-pole","NAV",36.54,0,36.54,8592765101525,4,18592765101522,48,28592765101529,"8536201090",0.36]
[110153,"Ex9BP-JX(+) 3P K25","DC Miniature Circuit Breaker 10 kA, characteristic K, 25 A, 750 V DC, 3-pole","NAV",36.54,0,36.54,8592765101532,4,18592765101539,48,28592765101536,"8536201090",0.36]
[110154,"Ex9BP-JX(+) 3P K32","DC Miniature Circuit Breaker 10 kA, characteristic K, 32 A, 750 V DC, 3-pole","NAV",36.54,0,36.54,8592765101549,4,18592765101546,48,28592765101543,"8536201090",0.36]
[110155,"Ex9BP-JX(+) 3P K40","DC Miniature Circuit Breaker 10 kA, characteristic K, 40 A, 750 V DC, 3-pole","NAV",42.31,0,42.31,8592765101556,4,18592765101553,48,28592765101550,"8536201090",0.36]
[110156,"Ex9BP-JX(+) 3P K50","DC Miniature Circuit Breaker 10 kA, characteristic K, 50 A, 750 V DC, 3-pole","NAV",51.5,0,51.5,8592765101563,4,18592765101560,48,28592765101567,"8536201090",0.36]
[110157,"Ex9BP-JX(+) 3P K63","DC Miniature Circuit Breaker 10 kA, characteristic K, 63 A, 750 V DC, 3-pole","NAV",59.52,0,59.52,8592765101570,4,18592765101577,48,28592765101574,"8536201090",0.36]
[110158,"Ex9BP-JX(+) 4P K1","DC Miniature Circuit Breaker 10 kA, characteristic K, 1 A, 1000 V DC, 4-pole","NAV",47.03,0,47.03,8592765101587,3,18592765101584,36,28592765101581,"8536201090",0.48]
[110159,"Ex9BP-JX(+) 4P K2","DC Miniature Circuit Breaker 10 kA, characteristic K, 2, A, 1000 V DC, 4-pole","NAV",47.03,0,47.03,8592765101594,3,18592765101591,36,28592765101598,"8536201090",0.48]
[110160,"Ex9BP-JX(+) 4P K3","DC Miniature Circuit Breaker 10 kA, characteristic K, 3 A, 1000 V DC, 4-pole","NAV",47.03,0,47.03,8592765101600,3,18592765101607,36,28592765101604,"8536201090",0.48]
[110161,"Ex9BP-JX(+) 4P K4","DC Miniature Circuit Breaker 10 kA, characteristic K, 4 A, 1000 V DC, 4-pole","NAV",47.03,0,47.03,8592765101617,3,18592765101614,36,28592765101611,"8536201090",0.48]
[110162,"Ex9BP-JX(+) 4P K6","DC Miniature Circuit Breaker 10 kA, characteristic K, 6 A, 1000 V DC, 4-pole","NAV",42.74,0,42.74,8592765101624,3,18592765101621,36,28592765101628,"8536201090",0.48]
[110163,"Ex9BP-JX(+) 4P K10","DC Miniature Circuit Breaker 10 kA, characteristic K, 10 A, 1000 V DC, 4-pole","NAV",42.74,0,42.74,8592765101631,3,18592765101638,36,28592765101635,"8536201090",0.48]
[110164,"Ex9BP-JX(+) 4P K16","DC Miniature Circuit Breaker 10 kA, characteristic K, 16 A, 1000 V DC, 4-pole","NAV",42.74,0,42.74,8592765101648,3,18592765101645,36,28592765101642,"8536201090",0.48]
[110165,"Ex9BP-JX(+) 4P K20","DC Miniature Circuit Breaker 10 kA, characteristic K, 20 A, 1000 V DC, 4-pole","NAV",42.74,0,42.74,8592765101655,3,18592765101652,36,28592765101659,"8536201090",0.48]
[110166,"Ex9BP-JX(+) 4P K25","DC Miniature Circuit Breaker 10 kA, characteristic K, 25 A, 1000 V DC, 4-pole","NAV",42.74,0,42.74,8592765101662,3,18592765101669,36,28592765101666,"8536201090",0.48]
[110167,"Ex9BP-JX(+) 4P K32","DC Miniature Circuit Breaker 10 kA, characteristic K, 32 A, 1000 V DC, 4-pole","NAV",42.74,0,42.74,8592765101679,3,18592765101676,36,28592765101673,"8536201090",0.48]
[110168,"Ex9BP-JX(+) 4P K40","DC Miniature Circuit Breaker 10 kA, characteristic K, 40 A, 1000 V DC, 4-pole","NAV",49.49,0,49.49,8592765101686,3,18592765101683,36,28592765101680,"8536201090",0.48]
[110169,"Ex9BP-JX(+) 4P K50","DC Miniature Circuit Breaker 10 kA, characteristic K, 50 A, 1000 V DC, 4-pole","NAV",57.22,0,57.22,8592765101693,3,18592765101690,36,28592765101697,"8536201090",0.48]
[110170,"Ex9BP-JX(+) 4P K63","DC Miniature Circuit Breaker 10 kA, characteristic K, 63 A, 1000 V DC, 4-pole","NAV",66.13,0,66.13,8592765101709,3,18592765101706,36,28592765101703,"8536201090",0.48]
[]
["Accessories for Miniature Circuit Breakers Ex9B, Ex9PN and Isolators Ex9BI, Ex9IP"]
[100540,"AX3111","Auxiliary contact, 1 change over","NAA",7.43,{"$f":"NAA","v":0},{"$f":"E1005*(1-F1005)","v":7.43},8592765005410,1,8592765005410,96,28592765005414,"8536508090",0.06]
[100541,"AL3111","Signal contact, 1 change over","NAA",12.49,0,12.49,8592765005427,1,8592765005427,96,28592765005421,"8536508090",0.06]
[100542,"AX3122","Auxiliary contact, 2 change over","NAA",21.22,0,21.22,8592765005434,1,8592765005434,96,28592765005438,"8536508090",0.06]
[100543,"AXL31","Auxiliary + Signal contact, 1 CO + 1 CO","NAA",21.22,0,21.22,8592765005441,1,8592765005441,96,28592765005445,"8536508090",0.06]
[100544,"SHT31 110V-415V AC/110V-130V DC","Shunt trip release, 110-415 V AC, 110-130 V DC","NAA",8.5399999999999991,0,8.5399999999999991,8592765005458,1,8592765005458,96,28592765005452,"8536490099",0.12]
[100545,"SHT31 48V AC/DC","Shunt trip release, 48 V AC, 48 V DC","NAA",22.22,0,22.22,8592765005465,1,8592765005465,96,28592765005469,"8536419089",0.12]
[100546,"SHT31 12-24V AC/DC","Shunt trip release, 12-24 V AC, 12-24 V DC","NAA",22.22,0,22.22,8592765005472,1,8592765005472,96,28592765005476,"8536419089",0.12]
[100547,"SHT3111 110V-415V AC/110V-130V DC","Shunt trip release, 110-415 V AC, 110-130 V DC, 1 change over auxiliary contact","NAA",25.3,0,25.3,8592765005489,1,8592765005489,96,28592765005483,"8536490099",0.12]
[100548,"SHT3111 48V AC/DC","Shunt trip release, 48 V AC, 48 V DC, 1 change over auxiliary contact","NAA",25.3,0,25.3,8592765005496,1,8592765005496,96,28592765005490,"8538909999",0.12]
[100549,"SHT3111 12-24V AC/DC","Shunt trip release, 12-24 V AC, 12-24 V DC, 1 change over auxiliary contact","NAA",25.3,0,25.3,8592765005502,1,8592765005502,96,28592765005506,"8536419089",0.12]
[100550,"UVT31 220-240V AC","Undervoltage release, 220-240 V AC","NAA",34.31,0,34.31,8592765005519,1,8592765005519,96,28592765005513,"8536490099",0.12]
[100552,"UVT3101 220-240V AC","Undervoltage release, 220-240 V AC, 1 NC auxiliary contact","NAA",37.53,0,37.53,8592765005533,1,8592765005533,96,28592765005537,"8536490099",0.12]
[100554,"UVT3110 220-240V AC","Undervoltage release, 220-240 V AC, 1 NO auxiliary contact","NAA",37.53,0,37.53,8592765005557,1,8592765005557,96,28592765005551,"8536490099",0.12]
[100556,"OVT31 280V AC±5%","Overvoltage release, 280 V AC","NAA",38.380000000000003,0,38.380000000000003,8592765005571,1,8592765005571,96,28592765005575,"8536490099",0.12]
[110193,"LK-I","Locking mechanism suitable for devices - Ex9BH, Ex9BN, Ex9BD, Ex9BP, Ex9BL, Ex9BI, Ex9PN, Ex9IP, Ex9I125, Ex9I40, Ex9BT, SHT31, UVT31, OVT31","NAA",3.85,{"$f":"NAA","v":0},{"$f":"E1019*(1-F1019)","v":3.85},8592765101938,16,18592765101935,240,28592765101932,"8538909999",4.0000000000000001E-3]
[]
["Residual Current Circuit Breakers Ex9L-H, 10 kA",null,null,null,null,null,null,"","","","","",null,""]
[108156,"Ex9L-H 2P 16A 10mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=10mA, type  AC","NAC",40.78,{"$f":"NAC","v":0},{"$f":"E1022*(1-F1022)","v":40.78},8592765081568,1,18592765081565,81,28592765081562,"8536201090",0.21]
[108158,"Ex9L-H 2P 16A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=30mA, type  AC","NAC",40.78,{"$f":"NAC","v":0},40.78,8592765081582,1,18592765081589,81,28592765081586,"8536201090",0.216]
[108162,"Ex9L-H 2P 16A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=100mA, type  AC","NAC",61.3,0,61.3,8592765081629,1,18592765081626,81,28592765081623,"8536201090",0.216]
[108166,"Ex9L-H 2P 16A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=300mA, type  AC","NAC",61.3,0,61.3,8592765081667,1,18592765081664,81,28592765081661,"8536201090",0.20899999999999999]
[108170,"Ex9L-H 2P 16A 500mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=500mA, type  AC","NAC",66.55,0,66.55,8592765081704,1,18592765081701,81,28592765081708,"8536201090",0.21]
[108157,"Ex9L-H 2P 25A 10mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=10mA, type  AC","NAC",40.78,0,40.78,8592765081575,1,18592765081572,81,28592765081579,"8536201090",0.21]
[108159,"Ex9L-H 2P 25A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=30mA, type  AC","NAC",40.78,0,40.78,8592765081599,1,18592765081596,81,28592765081593,"8536201090",0.216]
[108163,"Ex9L-H 2P 25A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, type  AC","NAC",65.09,0,65.09,8592765081636,1,18592765081633,81,28592765081630,"8536201090",0.216]
[108167,"Ex9L-H 2P 25A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, type  AC","NAC",65.09,0,65.09,8592765081674,1,18592765081671,81,28592765081678,"8536201090",0.20899999999999999]
[108171,"Ex9L-H 2P 25A 500mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=500mA, type  AC","NAC",70.349999999999994,0,70.349999999999994,8592765081711,1,18592765081718,81,28592765081715,"8536201090",0.21]
[108160,"Ex9L-H 2P 40A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=30mA, type  AC","NAC",56.12,0,56.12,8592765081605,1,18592765081602,81,28592765081609,"8536201090",0.216]
[108164,"Ex9L-H 2P 40A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, type  AC","NAC",70.2,0,70.2,8592765081643,1,18592765081640,81,28592765081647,"8536201090",0.216]
[108168,"Ex9L-H 2P 40A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, type  AC","NAC",70.2,0,70.2,8592765081681,1,18592765081688,81,28592765081685,"8536201090",0.20899999999999999]
[108172,"Ex9L-H 2P 40A 500mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=500mA, type  AC","NAC",75.47,0,75.47,8592765081728,1,18592765081725,81,28592765081722,"8536201090",0.21]
[108161,"Ex9L-H 2P 63A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=30mA, type  AC","NAC",78.78,0,78.78,8592765081612,1,18592765081619,81,28592765081616,"8536201090",0.216]
[108165,"Ex9L-H 2P 63A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, type  AC","NAC",80.47,0,80.47,8592765081650,1,18592765081657,81,28592765081654,"8536201090",0.216]
[108169,"Ex9L-H 2P 63A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, type  AC","NAC",80.47,0,80.47,8592765081698,1,18592765081695,81,28592765081692,"8536201090",0.20899999999999999]
[108173,"Ex9L-H 2P 63A 500mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=500mA, type  AC","NAC",85.73,0,85.73,8592765081735,1,18592765081732,81,28592765081739,"8536201090",0.21]
[108174,"Ex9L-H 4P 16A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=30mA, type  AC","NAC",40.78,0,40.78,8592765081742,1,18592765081749,45,28592765081746,"8536201090",0.35599999999999998]
[108178,"Ex9L-H 4P 16A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=100mA, type  AC","NAC",64.349999999999994,0,64.349999999999994,8592765081780,1,18592765081787,45,28592765081784,"8536201090",0.36699999999999999]
[108182,"Ex9L-H 4P 16A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=300mA, type  AC","NAC",66.42,0,66.42,8592765081827,1,18592765081824,45,28592765081821,"8536201090",0.36699999999999999]
[108186,"Ex9L-H 4P 16A 500mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=500mA, type  AC","NAC",71.680000000000007,0,71.680000000000007,8592765081865,1,18592765081862,45,28592765081869,"8536201090",0.36699999999999999]
[108175,"Ex9L-H 4P 25A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=30mA, type  AC","NAC",44.95,0,44.95,8592765081759,1,18592765081756,45,28592765081753,"8536201090",0.35599999999999998]
[108179,"Ex9L-H 4P 25A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, type  AC","NAC",70.14,0,70.14,8592765081797,1,18592765081794,45,28592765081791,"8536201090",0.36699999999999999]
[108183,"Ex9L-H 4P 25A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, type  AC","NAC",70.14,0,70.14,8592765081834,1,18592765081831,45,28592765081838,"8536201090",0.36699999999999999]
[108187,"Ex9L-H 4P 25A 500mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=500mA, type  AC","NAC",75.400000000000006,0,75.400000000000006,8592765081872,1,18592765081879,45,28592765081876,"8536201090",0.36699999999999999]
[108176,"Ex9L-H 4P 40A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=30mA, type  AC","NAC",61.81,0,61.81,8592765081766,1,18592765081763,45,28592765081760,"8536201090",0.35599999999999998]
[108180,"Ex9L-H 4P 40A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, type  AC","NAC",70.959999999999994,0,70.959999999999994,8592765081803,1,18592765081800,45,28592765081807,"8536201090",0.36699999999999999]
[108184,"Ex9L-H 4P 40A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, type  AC","NAC",70.959999999999994,0,70.959999999999994,8592765081841,1,18592765081848,45,28592765081845,"8536201090",0.36699999999999999]
[108188,"Ex9L-H 4P 40A 500mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=500mA, type  AC","NAC",76.209999999999994,0,76.209999999999994,8592765081889,1,18592765081886,45,28592765081883,"8536201090",0.36699999999999999]
[108177,"Ex9L-H 4P 63A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=30mA, type  AC","NAC",83.12,0,83.12,8592765081773,1,18592765081770,45,28592765081777,"8536201090",0.35599999999999998]
[108181,"Ex9L-H 4P 63A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, type  AC","NAC",83.12,0,83.12,8592765081810,1,18592765081817,45,28592765081814,"8536201090",0.35499999999999998]
[108185,"Ex9L-H 4P 63A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, type  AC","NAC",83.12,0,83.12,8592765081858,1,18592765081855,45,28592765081852,"8536201090",0.35599999999999998]
[108189,"Ex9L-H 4P 63A 500mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=500mA, type  AC","NAC",88.38,0,88.38,8592765081896,1,18592765081893,45,28592765081890,"8536201090",0.36699999999999999]
[108190,"Ex9L-H 2P 16A A 10mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=10mA, type  A","NAC",51.18,0,51.18,8592765081902,1,18592765081909,81,28592765081906,"8536201090",0.21]
[108192,"Ex9L-H 2P 16A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=30mA, type  A","NAC",51.18,0,51.18,8592765081926,1,18592765081923,81,28592765081920,"8536201090",0.216]
[108196,"Ex9L-H 2P 16A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=100mA, type  A","NAC",69.58,0,69.58,8592765081964,1,18592765081961,81,28592765081968,"8536201090",0.216]
[108200,"Ex9L-H 2P 16A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=300mA, type  A","NAC",69.58,0,69.58,8592765082008,1,18592765082005,81,28592765082002,"8536201090",0.216]
[108191,"Ex9L-H 2P 25A A 10mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=10mA, type  A","NAC",51.18,0,51.18,8592765081919,1,18592765081916,81,28592765081913,"8536201090",0.21]
[108193,"Ex9L-H 2P 25A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=30mA, type  A","NAC",51.18,0,51.18,8592765081933,1,18592765081930,81,28592765081937,"8536201090",0.216]
[108197,"Ex9L-H 2P 25A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, type  A","NAC",71.680000000000007,0,71.680000000000007,8592765081971,1,18592765081978,81,28592765081975,"8536201090",0.216]
[108201,"Ex9L-H 2P 25A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, type  A","NAC",71.680000000000007,0,71.680000000000007,8592765082015,1,18592765082012,81,28592765082019,"8536201090",0.216]
[108194,"Ex9L-H 2P 40A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=30mA, type  A","NAC",61.73,0,61.73,8592765081940,1,18592765081947,81,28592765081944,"8536201090",0.216]
[108198,"Ex9L-H 2P 40A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, type  A","NAC",77.260000000000005,0,77.260000000000005,8592765081988,1,18592765081985,81,28592765081982,"8536201090",0.216]
[108202,"Ex9L-H 2P 40A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, type  A","NAC",77.260000000000005,0,77.260000000000005,8592765082022,1,18592765082029,81,28592765082026,"8536201090",0.216]
[108195,"Ex9L-H 2P 63A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=30mA, type  A","NAC",86.71,0,86.71,8592765081957,1,18592765081954,81,28592765081951,"8536201090",0.216]
[108199,"Ex9L-H 2P 63A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, type  A","NAC",88.54,0,88.54,8592765081995,1,18592765081992,81,28592765081999,"8536201090",0.216]
[108203,"Ex9L-H 2P 63A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, type  A","NAC",88.54,0,88.54,8592765082039,1,18592765082036,81,28592765082033,"8536201090",0.216]
[108204,"Ex9L-H 4P 16A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=30mA, type  A","NAC",57.46,0,57.46,8592765082046,1,18592765082043,45,28592765082040,"8536201090",0.38900000000000001]
[108208,"Ex9L-H 4P 16A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=100mA, type  A","NAC",77.19,0,77.19,8592765082084,1,18592765082081,45,28592765082088,"8536201090",0.36699999999999999]
[108212,"Ex9L-H 4P 16A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=300mA, type  A","NAC",77.19,0,77.19,8592765082121,1,18592765082128,45,28592765082125,"8536201090",0.36699999999999999]
[108205,"Ex9L-H 4P 25A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=30mA, type  A","NAC",57.46,0,57.46,8592765082053,1,18592765082050,45,28592765082057,"8536201090",0.38900000000000001]
[108209,"Ex9L-H 4P 25A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, type  A","NAC",77.19,0,77.19,8592765082091,1,18592765082098,45,28592765082095,"8536201090",0.36699999999999999]
[108213,"Ex9L-H 4P 25A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, type  A","NAC",77.19,0,77.19,8592765082138,1,18592765082135,45,28592765082132,"8536201090",0.36699999999999999]
[108206,"Ex9L-H 4P 40A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=30mA, type  A","NAC",71.22,0,71.22,8592765082060,1,18592765082067,45,28592765082064,"8536201090",0.38900000000000001]
[108210,"Ex9L-H 4P 40A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, type  A","NAC",78.05,0,78.05,8592765082107,1,18592765082104,45,28592765082101,"8536201090",0.36699999999999999]
[108214,"Ex9L-H 4P 40A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, type  A","NAC",78.05,0,78.05,8592765082145,1,18592765082142,45,28592765082149,"8536201090",0.36699999999999999]
[108207,"Ex9L-H 4P 63A A 30mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=30mA, type  A","NAC",91.45,0,91.45,8592765082077,1,18592765082074,45,28592765082071,"8536201090",0.378]
[108211,"Ex9L-H 4P 63A A 100mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, type  A","NAC",91.45,0,91.45,8592765082114,1,18592765082111,45,28592765082118,"8536201090",0.36699999999999999]
[108215,"Ex9L-H 4P 63A A 300mA","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, type  A","NAC",91.45,0,91.45,8592765082152,1,18592765082159,45,28592765082156,"8536201090",0.36699999999999999]
[108216,"Ex9L-H 2P 16A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=100mA, type  S+AC","NAC",64.349999999999994,0,64.349999999999994,8592765082169,1,18592765082166,81,28592765082163,"8536201090",0.20300000000000001]
[108220,"Ex9L-H 2P 16A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=300mA, type  S+AC","NAC",64.349999999999994,0,64.349999999999994,8592765082206,1,18592765082203,81,28592765082200,"8536201090",0.20300000000000001]
[108224,"Ex9L-H 2P 16A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=500mA, type  S+AC","NAC",74.41,0,74.41,8592765082244,1,18592765082241,81,28592765082248,"8536201090",0.20300000000000001]
[108217,"Ex9L-H 2P 25A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, type  S+AC","NAC",70.14,0,70.14,8592765082176,1,18592765082173,81,28592765082170,"8536201090",0.20300000000000001]
[108221,"Ex9L-H 2P 25A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, type  S+AC","NAC",70.14,0,{"$f":"E1086*(1-F1086)","v":70.14},8592765082213,1,18592765082210,81,28592765082217,"8536201090",0.20300000000000001]
[108225,"Ex9L-H 2P 25A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=500mA, type  S+AC","NAC",80.209999999999994,{"$f":"NAC","v":0},80.209999999999994,8592765082251,1,18592765082258,81,28592765082255,"8536201090",0.20300000000000001]
[108218,"Ex9L-H 2P 40A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, type  S+AC","NAC",70.959999999999994,0,70.959999999999994,8592765082183,1,18592765082180,81,28592765082187,"8536201090",0.20300000000000001]
[108222,"Ex9L-H 2P 40A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, type  S+AC","NAC",70.959999999999994,0,70.959999999999994,8592765082220,1,18592765082227,81,28592765082224,"8536201090",0.20300000000000001]
[108226,"Ex9L-H 2P 40A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=500mA, type  S+AC","NAC",81.010000000000005,0,81.010000000000005,8592765082268,1,18592765082265,81,28592765082262,"8536201090",0.20300000000000001]
[108219,"Ex9L-H 2P 63A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, type  S+AC","NAC",105.82,0,105.82,8592765082190,1,18592765082197,81,28592765082194,"8536201090",0.20300000000000001]
[108223,"Ex9L-H 2P 63A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, type  S+AC","NAC",105.82,0,105.82,8592765082237,1,18592765082234,81,28592765082231,"8536201090",0.20300000000000001]
[108227,"Ex9L-H 2P 63A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=500mA, type  S+AC","NAC",115.89,0,115.89,8592765082275,1,18592765082272,81,28592765082279,"8536201090",0.20300000000000001]
[108228,"Ex9L-H 4P 16A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=100mA, type  S+AC","NAC",90.85,0,90.85,8592765082282,1,18592765082289,45,28592765082286,"8536201090",0.35599999999999998]
[108232,"Ex9L-H 4P 16A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=300mA, type  S+AC","NAC",90.85,0,90.85,8592765082329,1,18592765082326,45,28592765082323,"8536201090",0.35599999999999998]
[108236,"Ex9L-H 4P 16A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=500mA, type  S+AC","NAC",99.71,0,99.71,8592765082367,1,18592765082364,45,28592765082361,"8536201090",0.35599999999999998]
[108229,"Ex9L-H 4P 25A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, type  S+AC","NAC",90.85,0,90.85,8592765082299,1,18592765082296,45,28592765082293,"8536201090",0.35599999999999998]
[108233,"Ex9L-H 4P 25A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, type  S+AC","NAC",90.85,0,90.85,8592765082336,1,18592765082333,45,28592765082330,"8536201090",0.35599999999999998]
[108237,"Ex9L-H 4P 25A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=500mA, type  S+AC","NAC",99.71,0,99.71,8592765082374,1,18592765082371,45,28592765082378,"8536201090",0.35599999999999998]
[108230,"Ex9L-H 4P 40A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, type  S+AC","NAC",91.71,0,91.71,8592765082305,1,18592765082302,45,28592765082309,"8536201090",0.35599999999999998]
[108234,"Ex9L-H 4P 40A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, type  S+AC","NAC",91.71,0,91.71,8592765082343,1,18592765082340,45,28592765082347,"8536201090",0.35599999999999998]
[108238,"Ex9L-H 4P 40A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=500mA, type  S+AC","NAC",100.57,0,100.57,8592765082381,1,18592765082388,45,28592765082385,"8536201090",0.35599999999999998]
[108231,"Ex9L-H 4P 63A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, type  S+AC","NAC",116.95,0,116.95,8592765082312,1,18592765082319,45,28592765082316,"8536201090",0.35599999999999998]
[108235,"Ex9L-H 4P 63A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, type  S+AC","NAC",116.95,0,116.95,8592765082350,1,18592765082357,45,28592765082354,"8536201090",0.35599999999999998]
[108239,"Ex9L-H 4P 63A 500mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=500mA, type  S+AC","NAC",125.8,0,125.8,8592765082398,1,18592765082395,45,28592765082392,"8536201090",0.35599999999999998]
[108240,"Ex9L-H 2P 16A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=100mA, type  S+A","NAC",64.349999999999994,0,64.349999999999994,8592765082404,1,18592765082401,81,28592765082408,"8536201090",0.20300000000000001]
[108244,"Ex9L-H 2P 16A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=300mA, type  S+A","NAC",64.349999999999994,0,64.349999999999994,8592765082442,1,18592765082449,81,28592765082446,"8536201090",0.20300000000000001]
[108241,"Ex9L-H 2P 25A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, type  S+A","NAC",70.14,0,70.14,8592765082411,1,18592765082418,81,28592765082415,"8536201090",0.20300000000000001]
[108245,"Ex9L-H 2P 25A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, type  S+A","NAC",70.14,0,70.14,8592765082459,1,18592765082456,81,28592765082453,"8536201090",0.20300000000000001]
[108242,"Ex9L-H 2P 40A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, type  S+A","NAC",70.959999999999994,0,70.959999999999994,8592765082428,1,18592765082425,81,28592765082422,"8536201090",0.20300000000000001]
[108246,"Ex9L-H 2P 40A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, type  S+A","NAC",70.959999999999994,0,70.959999999999994,8592765082466,1,18592765082463,81,28592765082460,"8536201090",0.20300000000000001]
[108243,"Ex9L-H 2P 63A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, type  S+A","NAC",116.44,0,116.44,8592765082435,1,18592765082432,81,28592765082439,"8536201090",0.20300000000000001]
[108247,"Ex9L-H 2P 63A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, type  S+A","NAC",116.44,0,116.44,8592765082473,1,18592765082470,81,28592765082477,"8536201090",0.20300000000000001]
[108248,"Ex9L-H 4P 16A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=100mA, type  S+A","NAC",74.849999999999994,0,74.849999999999994,8592765082480,1,18592765082487,45,28592765082484,"8536201090",0.35599999999999998]
[108252,"Ex9L-H 4P 16A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=300mA, type  S+A","NAC",74.849999999999994,0,74.849999999999994,8592765082527,1,18592765082524,45,28592765082521,"8536201090",0.35599999999999998]
[108249,"Ex9L-H 4P 25A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, type  S+A","NAC",80.650000000000006,0,80.650000000000006,8592765082497,1,18592765082494,45,28592765082491,"8536201090",0.35599999999999998]
[108253,"Ex9L-H 4P 25A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, type  S+A","NAC",80.650000000000006,0,80.650000000000006,8592765082534,1,18592765082531,45,28592765082538,"8536201090",0.35599999999999998]
[108250,"Ex9L-H 4P 40A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, type  S+A","NAC",81.45,0,81.45,8592765082503,1,18592765082500,45,28592765082507,"8536201090",0.35599999999999998]
[108254,"Ex9L-H 4P 40A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, type  S+A","NAC",81.45,0,81.45,8592765082541,1,18592765082548,45,28592765082545,"8536201090",0.35599999999999998]
[108251,"Ex9L-H 4P 63A A 100mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, type  S+A","NAC",128.68,0,128.68,8592765082510,1,18592765082517,45,28592765082514,"8536201090",0.35599999999999998]
[108255,"Ex9L-H 4P 63A A 300mA S","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, type  S+A","NAC",128.68,0,128.68,8592765082558,1,18592765082555,45,28592765082552,"8536201090",0.35599999999999998]
[108256,"Ex9L-H 2P 16A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=30mA, type  G+AC","NAC",64.89,0,64.89,8592765082565,1,18592765082562,81,28592765082569,"8536201090",0.20300000000000001]
[108259,"Ex9L-H 2P 16A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=100mA, type  G+AC","NAC",70.14,0,70.14,8592765082596,1,18592765082593,81,28592765082590,"8536201090",0.20300000000000001]
[108264,"Ex9L-H 2P 16A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=300mA, type  G+AC","NAC",73.290000000000006,0,73.290000000000006,8592765082640,1,18592765082647,81,28592765082644,"8536201090",0.20300000000000001]
[108268,"Ex9L-H 2P 16A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=500mA, type  G+AC","NAC",82.68,0,82.68,8592765082688,1,18592765082685,81,28592765082682,"8536201090",0.20300000000000001]
[108257,"Ex9L-H 2P 25A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=30mA, type  G+AC","NAC",64.89,0,64.89,8592765082572,1,18592765082579,81,28592765082576,"8536201090",0.20300000000000001]
[108261,"Ex9L-H 2P 25A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, type  G+AC","NAC",70.14,0,70.14,8592765082619,1,18592765082616,81,28592765082613,"8536201090",0.20300000000000001]
[108265,"Ex9L-H 2P 25A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, type  G+AC","NAC",73.12,0,73.12,8592765082657,1,18592765082654,81,28592765082651,"8536201090",0.20300000000000001]
[108269,"Ex9L-H 2P 25A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=500mA, type  G+AC","NAC",82.49,0,82.49,8592765082695,1,18592765082692,81,28592765082699,"8536201090",0.20300000000000001]
[108258,"Ex9L-H 2P 40A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=30mA, type  G+AC","NAC",65.7,0,65.7,8592765082589,1,18592765082586,81,28592765082583,"8536201090",0.20300000000000001]
[108262,"Ex9L-H 2P 40A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, type  G+AC","NAC",70.959999999999994,0,70.959999999999994,8592765082626,1,18592765082623,81,28592765082620,"8536201090",0.20300000000000001]
[108266,"Ex9L-H 2P 40A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, type  G+AC","NAC",73.930000000000007,0,73.930000000000007,8592765082664,1,18592765082661,81,28592765082668,"8536201090",0.20300000000000001]
[108270,"Ex9L-H 2P 40A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=500mA, type  G+AC","NAC",83.31,0,83.31,8592765082701,1,18592765082708,81,28592765082705,"8536201090",0.20300000000000001]
[108260,"Ex9L-H 2P 63A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=30mA, type  G+AC","NAC",116.44,0,{"$f":"E1134*(1-F1134)","v":116.44},8592765082602,1,18592765082609,81,28592765082606,"8536201090",0.20300000000000001]
[108263,"Ex9L-H 2P 63A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, type  G+AC","NAC",116.44,{"$f":"NAC","v":0},116.44,8592765082633,1,18592765082630,81,28592765082637,"8536201090",0.20300000000000001]
[108267,"Ex9L-H 2P 63A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, type  G+AC","NAC",119.42,0,119.42,8592765082671,1,18592765082678,81,28592765082675,"8536201090",0.20300000000000001]
[108271,"Ex9L-H 2P 63A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=500mA, type  G+AC","NAC",128.79,0,128.79,8592765082718,1,18592765082715,81,28592765082712,"8536201090",0.20300000000000001]
[108272,"Ex9L-H 4P 16A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=30mA, type  G+AC","NAC",70.650000000000006,0,70.650000000000006,8592765082725,1,18592765082722,45,28592765082729,"8536201090",0.35599999999999998]
[108276,"Ex9L-H 4P 16A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=100mA, type  G+AC","NAC",83.27,0,83.27,8592765082763,1,18592765082760,45,28592765082767,"8536201090",0.35599999999999998]
[108280,"Ex9L-H 4P 16A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=300mA, type  G+AC","NAC",83.27,0,83.27,8592765082800,1,18592765082807,45,28592765082804,"8536201090",0.35599999999999998]
[108284,"Ex9L-H 4P 16A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=500mA, type  G+AC","NAC",95.87,0,95.87,8592765082848,1,18592765082845,45,28592765082842,"8536201090",0.35599999999999998]
[108273,"Ex9L-H 4P 25A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=30mA, type  G+AC","NAC",76.44,0,76.44,8592765082732,1,18592765082739,45,28592765082736,"8536201090",0.35599999999999998]
[108277,"Ex9L-H 4P 25A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, type  G+AC","NAC",89.05,0,89.05,8592765082770,1,18592765082777,45,28592765082774,"8536201090",0.35599999999999998]
[108281,"Ex9L-H 4P 25A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, type  G+AC","NAC",89.05,0,89.05,8592765082817,1,18592765082814,45,28592765082811,"8536201090",0.35599999999999998]
[108285,"Ex9L-H 4P 25A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=500mA, type  G+AC","NAC",101.66,0,101.66,8592765082855,1,18592765082852,45,28592765082859,"8536201090",0.35599999999999998]
[108274,"Ex9L-H 4P 40A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=30mA, type  G+AC","NAC",77.25,0,77.25,8592765082749,1,18592765082746,45,28592765082743,"8536201090",0.35599999999999998]
[108278,"Ex9L-H 4P 40A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, type  G+AC","NAC",89.86,0,89.86,8592765082787,1,18592765082784,45,28592765082781,"8536201090",0.35599999999999998]
[108282,"Ex9L-H 4P 40A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, type  G+AC","NAC",89.86,0,89.86,8592765082824,1,18592765082821,45,28592765082828,"8536201090",0.35599999999999998]
[108286,"Ex9L-H 4P 40A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=500mA, type  G+AC","NAC",102.47,0,102.47,8592765082862,1,18592765082869,45,28592765082866,"8536201090",0.35599999999999998]
[108275,"Ex9L-H 4P 63A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=30mA, type  G+AC","NAC",124.48,0,124.48,8592765082756,1,18592765082753,45,28592765082750,"8536201090",0.35599999999999998]
[108279,"Ex9L-H 4P 63A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, type  G+AC","NAC",137.08000000000001,0,137.08000000000001,8592765082794,1,18592765082791,45,28592765082798,"8536201090",0.35599999999999998]
[108283,"Ex9L-H 4P 63A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, type  G+AC","NAC",137.08000000000001,0,137.08000000000001,8592765082831,1,18592765082838,45,28592765082835,"8536201090",0.35599999999999998]
[108287,"Ex9L-H 4P 63A 500mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=500mA, type  G+AC","NAC",149.69999999999999,0,149.69999999999999,8592765082879,1,18592765082876,45,28592765082873,"8536201090",0.35599999999999998]
[108288,"Ex9L-H 2P 16A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=30mA, type  G+A","NAC",66.989999999999995,0,66.989999999999995,8592765082886,1,18592765082883,81,28592765082880,"8536201090",0.20300000000000001]
[108292,"Ex9L-H 2P 16A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=100mA, type  G+A","NAC",72.239999999999995,0,72.239999999999995,8592765082923,1,18592765082920,81,28592765082927,"8536201090",0.20300000000000001]
[108296,"Ex9L-H 2P 16A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=16A, IΔn=300mA, type  G+A","NAC",74.98,0,74.98,8592765082961,1,18592765082968,81,28592765082965,"8536201090",0.20300000000000001]
[108289,"Ex9L-H 2P 25A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=30mA, type  G+A","NAC",66.989999999999995,0,66.989999999999995,8592765082893,1,18592765082890,81,28592765082897,"8536201090",0.20300000000000001]
[108293,"Ex9L-H 2P 25A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, type  G+A","NAC",72.239999999999995,0,72.239999999999995,8592765082930,1,18592765082937,81,28592765082934,"8536201090",0.20300000000000001]
[108297,"Ex9L-H 2P 25A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, type  G+A","NAC",80.77,0,80.77,8592765082978,1,18592765082975,81,28592765082972,"8536201090",0.20300000000000001]
[108290,"Ex9L-H 2P 40A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=30mA, type  G+A","NAC",67.8,0,67.8,8592765082909,1,18592765082906,81,28592765082903,"8536201090",0.20300000000000001]
[108294,"Ex9L-H 2P 40A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, type  G+A","NAC",73.06,0,73.06,8592765082947,1,18592765082944,81,28592765082941,"8536201090",0.20300000000000001]
[108298,"Ex9L-H 2P 40A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, type  G+A","NAC",81.58,0,81.58,8592765082985,1,18592765082982,81,28592765082989,"8536201090",0.20300000000000001]
[108291,"Ex9L-H 2P 63A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=30mA, type  G+A","NAC",124.15,0,124.15,8592765082916,1,18592765082913,81,28592765082910,"8536201090",0.20300000000000001]
[108295,"Ex9L-H 2P 63A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, type  G+A","NAC",124.85,0,124.85,8592765082954,1,18592765082951,81,28592765082958,"8536201090",0.20300000000000001]
[108299,"Ex9L-H 2P 63A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, type  G+A","NAC",128.80000000000001,0,128.80000000000001,8592765082992,1,18592765082999,81,28592765082996,"8536201090",0.20300000000000001]
[108300,"Ex9L-H 4P 16A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=30mA, type  G+A","NAC",87.59,0,87.59,8592765083005,1,18592765083002,45,28592765083009,"8536201090",0.35599999999999998]
[108304,"Ex9L-H 4P 16A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=100mA, type  G+A","NAC",87.59,0,87.59,8592765083043,1,18592765083040,45,28592765083047,"8536201090",0.35599999999999998]
[108308,"Ex9L-H 4P 16A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=16A, IΔn=300mA, type  G+A","NAC",100.21,0,100.21,8592765083081,1,18592765083088,45,28592765083085,"8536201090",0.35599999999999998]
[108301,"Ex9L-H 4P 25A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=30mA, type  G+A","NAC",93.38,0,93.38,8592765083012,1,18592765083019,45,28592765083016,"8536201090",0.35599999999999998]
[108305,"Ex9L-H 4P 25A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, type  G+A","NAC",93.38,0,93.38,8592765083050,1,18592765083057,45,28592765083054,"8536201090",0.35599999999999998]
[108309,"Ex9L-H 4P 25A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, type  G+A","NAC",106,0,106,8592765083098,1,18592765083095,45,28592765083092,"8536201090",0.35599999999999998]
[108302,"Ex9L-H 4P 40A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=30mA, type  G+A","NAC",94.19,0,94.19,8592765083029,1,18592765083026,45,28592765083023,"8536201090",0.35599999999999998]
[108306,"Ex9L-H 4P 40A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, type  G+A","NAC",94.19,0,94.19,8592765083067,1,18592765083064,45,28592765083061,"8536201090",0.35599999999999998]
[108310,"Ex9L-H 4P 40A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, type  G+A","NAC",106.8,0,106.8,8592765083104,1,18592765083101,45,28592765083108,"8536201090",0.35599999999999998]
[108303,"Ex9L-H 4P 63A A 30mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=30mA, type  G+A","NAC",141.41999999999999,0,141.41999999999999,8592765083036,1,18592765083033,45,28592765083030,"8536201090",0.35599999999999998]
[108307,"Ex9L-H 4P 63A A 100mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, type  G+A","NAC",141.41999999999999,0,141.41999999999999,8592765083074,1,18592765083071,45,28592765083078,"8536201090",0.35599999999999998]
[108311,"Ex9L-H 4P 63A A 300mA G","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, type  G+A","NAC",149.69999999999999,0,149.69999999999999,8592765083111,1,18592765083118,45,28592765083115,"8536201090",0.35599999999999998]
[]
["Residual Current Circuit Breakers Ex9L-N, 6 kA"]
[108312,"Ex9L-N 2P 16A 10mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=10mA, type  AC","NAD",28.17,{"$f":"NAD","v":0},{"$f":"E1180*(1-F1180)","v":28.17},8592765083128,1,18592765083125,81,28592765083122,"8536201090",0.21]
[108317,"Ex9L-N 2P 16A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=30mA, type  AC","NAD",28.17,{"$f":"NAD","v":0},28.17,8592765083173,1,18592765083170,81,28592765083177,"8536201090",0.216]
[108321,"Ex9L-N 2P 16A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=100mA, type  AC","NAD",28.17,0,28.17,8592765083210,1,18592765083217,81,28592765083214,"8536201090",0.216]
[108325,"Ex9L-N 2P 16A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=300mA, type  AC","NAD",31.32,0,31.32,8592765083258,1,18592765083255,81,28592765083252,"8536201090",0.20899999999999999]
[108329,"Ex9L-N 2P 16A 500mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=500mA, type  AC","NAD",34.47,0,34.47,8592765083296,1,18592765083293,81,28592765083290,"8536201090",0.21]
[108313,"Ex9L-N 2P 25A 10mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=10mA, type  AC","NAD",29.22,0,29.22,8592765083135,1,18592765083132,81,28592765083139,"8536201090",0.21]
[108314,"Ex9L-N 2P 25A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=30mA, type  AC","NAD",28.17,0,28.17,8592765083142,1,18592765083149,81,28592765083146,"8536201090",0.216]
[108318,"Ex9L-N 2P 25A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=100mA, type  AC","NAD",30.8,0,30.8,8592765083180,1,18592765083187,81,28592765083184,"8536201090",0.216]
[108322,"Ex9L-N 2P 25A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=300mA, type  AC","NAD",30.18,0,30.18,8592765083227,1,18592765083224,81,28592765083221,"8536201090",0.20899999999999999]
[108326,"Ex9L-N 2P 25A 500mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=500mA, type  AC","NAD",32.42,0,32.42,8592765083265,1,18592765083262,81,28592765083269,"8536201090",0.21]
[108315,"Ex9L-N 2P 40A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=30mA, type  AC","NAD",30.18,0,30.18,8592765083159,1,18592765083156,81,28592765083153,"8536201090",0.216]
[108319,"Ex9L-N 2P 40A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=100mA, type  AC","NAD",32.81,0,32.81,8592765083197,1,18592765083194,81,28592765083191,"8536201090",0.216]
[108323,"Ex9L-N 2P 40A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=300mA, type  AC","NAD",30.18,0,30.18,8592765083234,1,18592765083231,81,28592765083238,"8536201090",0.20899999999999999]
[108327,"Ex9L-N 2P 40A 500mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=500mA, type  AC","NAD",32.42,0,32.42,8592765083272,1,18592765083279,81,28592765083276,"8536201090",0.21]
[108316,"Ex9L-N 2P 63A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=30mA, type  AC","NAD",37.119999999999997,0,37.119999999999997,8592765083166,1,18592765083163,81,28592765083160,"8536201090",0.216]
[108320,"Ex9L-N 2P 63A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=100mA, type  AC","NAD",39.75,0,39.75,8592765083203,1,18592765083200,81,28592765083207,"8536201090",0.216]
[108324,"Ex9L-N 2P 63A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=300mA, type  AC","NAD",42.37,0,42.37,8592765083241,1,18592765083248,81,28592765083245,"8536201090",0.20899999999999999]
[108328,"Ex9L-N 2P 63A 500mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=500mA, type  AC","NAD",44.63,0,44.63,8592765083289,1,18592765083286,81,28592765083283,"8536201090",0.21]
[108330,"Ex9L-N 4P 16A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=30mA, type  AC","NAD",34.200000000000003,0,34.200000000000003,8592765083302,1,18592765083309,45,28592765083306,"8536201090",0.35599999999999998]
[108334,"Ex9L-N 4P 16A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=100mA, type  AC","NAD",39.46,0,39.46,8592765083340,1,18592765083347,45,28592765083344,"8536201090",0.36699999999999999]
[108338,"Ex9L-N 4P 16A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=300mA, type  AC","NAD",39.46,0,39.46,8592765083388,1,18592765083385,45,28592765083382,"8536201090",0.36699999999999999]
[108342,"Ex9L-N 4P 16A 500mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=500mA, type  AC","NAD",43.35,0,43.35,8592765083425,1,18592765083422,45,28592765083429,"8536201090",0.36699999999999999]
[108331,"Ex9L-N 4P 25A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=30mA, type  AC","NAD",34.200000000000003,0,34.200000000000003,8592765083319,1,18592765083316,45,28592765083313,"8536201090",0.35599999999999998]
[108335,"Ex9L-N 4P 25A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=100mA, type  AC","NAD",41.56,0,41.56,8592765083357,1,18592765083354,45,28592765083351,"8536201090",0.36699999999999999]
[108339,"Ex9L-N 4P 25A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=300mA, type  AC","NAD",36.299999999999997,0,36.299999999999997,8592765083395,1,18592765083392,45,28592765083399,"8536201090",0.36699999999999999]
[108343,"Ex9L-N 4P 25A 500mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=500mA, type  AC","NAD",45.45,0,45.45,8592765083432,1,18592765083439,45,28592765083436,"8536201090",0.36699999999999999]
[108332,"Ex9L-N 4P 40A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=30mA, type  AC","NAD",36.299999999999997,0,36.299999999999997,8592765083326,1,18592765083323,45,28592765083320,"8536201090",0.35599999999999998]
[108336,"Ex9L-N 4P 40A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=100mA, type  AC","NAD",59.41,0,59.41,8592765083364,1,18592765083361,45,28592765083368,"8536201090",0.36699999999999999]
[108340,"Ex9L-N 4P 40A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=300mA, type  AC","NAD",36.299999999999997,0,36.299999999999997,8592765083401,1,18592765083408,45,28592765083405,"8536201090",0.36699999999999999]
[108344,"Ex9L-N 4P 40A 500mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=500mA, type  AC","NAD",50.71,0,50.71,8592765083449,1,18592765083446,45,28592765083443,"8536201090",0.36699999999999999]
[108333,"Ex9L-N 4P 63A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=30mA, type  AC","NAD",54.16,0,54.16,8592765083333,1,18592765083330,45,28592765083337,"8536201090",0.35599999999999998]
[108337,"Ex9L-N 4P 63A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=100mA, type  AC","NAD",44.71,0,44.71,8592765083371,1,18592765083378,45,28592765083375,"8536201090",0.35499999999999998]
[108341,"Ex9L-N 4P 63A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=300mA, type  AC","NAD",54.16,0,54.16,8592765083418,1,18592765083415,45,28592765083412,"8536201090",0.35599999999999998]
[108345,"Ex9L-N 4P 63A 500mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=500mA, type  AC","NAD",58.06,0,58.06,8592765083456,1,18592765083453,45,28592765083450,"8536201090",0.36699999999999999]
[108346,"Ex9L-N 2P 16A A 10mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=10mA, type  A","NAD",37.950000000000003,0,37.950000000000003,8592765083463,1,18592765083460,81,28592765083467,"8536201090",0.21]
[108348,"Ex9L-N 2P 16A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=30mA, type  A","NAD",37.950000000000003,0,37.950000000000003,8592765083487,1,18592765083484,81,28592765083481,"8536201090",0.216]
[108352,"Ex9L-N 2P 16A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=100mA, type  A","NAD",40.57,0,40.57,8592765083524,1,18592765083521,81,28592765083528,"8536201090",0.216]
[108356,"Ex9L-N 2P 16A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=300mA, type  A","NAD",43.2,0,43.2,8592765083562,1,18592765083569,81,28592765083566,"8536201090",0.216]
[108347,"Ex9L-N 2P 25A A 10mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=10mA, type  A","NAD",39,0,39,8592765083470,1,18592765083477,81,28592765083474,"8536201090",0.21]
[108349,"Ex9L-N 2P 25A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=30mA, type  A","NAD",39.950000000000003,0,39.950000000000003,8592765083494,1,18592765083491,81,28592765083498,"8536201090",0.216]
[108353,"Ex9L-N 2P 25A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=100mA, type  A","NAD",42.58,0,42.58,8592765083531,1,18592765083538,81,28592765083535,"8536201090",0.216]
[108357,"Ex9L-N 2P 25A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=300mA, type  A","NAD",45.21,0,45.21,8592765083579,1,18592765083576,81,28592765083573,"8536201090",0.216]
[108350,"Ex9L-N 2P 40A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=30mA, type  A","NAD",46.9,0,46.9,8592765083500,1,18592765083507,81,28592765083504,"8536201090",0.216]
[108354,"Ex9L-N 2P 40A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=100mA, type  A","NAD",49.52,0,49.52,8592765083548,1,18592765083545,81,28592765083542,"8536201090",0.216]
[108358,"Ex9L-N 2P 40A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=300mA, type  A","NAD",52.15,0,52.15,8592765083586,1,18592765083583,81,28592765083580,"8536201090",0.216]
[108351,"Ex9L-N 2P 63A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=30mA, type  A","NAD",53.96,0,53.96,8592765083517,1,18592765083514,81,28592765083511,"8536201090",0.216]
[108355,"Ex9L-N 2P 63A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=100mA, type  A","NAD",56.59,0,56.59,8592765083555,1,18592765083552,81,28592765083559,"8536201090",0.216]
[108359,"Ex9L-N 2P 63A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=300mA, type  A","NAD",59.21,0,59.21,8592765083593,1,18592765083590,81,28592765083597,"8536201090",0.216]
[108360,"Ex9L-N 4P 16A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=30mA, type  A","NAD",45.91,0,45.91,8592765083609,1,18592765083606,45,28592765083603,"8536201090",0.38900000000000001]
[108364,"Ex9L-N 4P 16A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=100mA, type  A","NAD",51.16,0,51.16,8592765083647,1,18592765083644,45,28592765083641,"8536201090",0.36699999999999999]
[108368,"Ex9L-N 4P 16A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=300mA, type  A","NAD",51.16,0,51.16,8592765083685,1,18592765083682,45,28592765083689,"8536201090",0.36699999999999999]
[108361,"Ex9L-N 4P 25A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=30mA, type  A","NAD",45.91,0,45.91,8592765083616,1,18592765083613,45,28592765083610,"8536201090",0.38900000000000001]
[108365,"Ex9L-N 4P 25A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=100mA, type  A","NAD",53.26,0,53.26,8592765083654,1,18592765083651,45,28592765083658,"8536201090",0.36699999999999999]
[108369,"Ex9L-N 4P 25A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=300mA, type  A","NAD",48.01,0,48.01,8592765083692,1,18592765083699,45,28592765083696,"8536201090",0.36699999999999999]
[108362,"Ex9L-N 4P 40A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=30mA, type  A","NAD",48.01,0,48.01,8592765083623,1,18592765083620,45,28592765083627,"8536201090",0.38900000000000001]
[108366,"Ex9L-N 4P 40A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=100mA, type  A","NAD",71.12,0,71.12,8592765083661,1,18592765083668,45,28592765083665,"8536201090",0.36699999999999999]
[108370,"Ex9L-N 4P 40A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=300mA, type  A","NAD",71.12,0,71.12,8592765083708,1,18592765083705,45,28592765083702,"8536201090",0.36699999999999999]
[108363,"Ex9L-N 4P 63A A 30mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=30mA, type  A","NAD",65.87,0,65.87,8592765083630,1,18592765083637,45,28592765083634,"8536201090",0.378]
[108367,"Ex9L-N 4P 63A A 100mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=100mA, type  A","NAD",75.23,0,75.23,8592765083678,1,18592765083675,45,28592765083672,"8536201090",0.36699999999999999]
[108371,"Ex9L-N 4P 63A A 300mA","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=300mA, type  A","NAD",75.23,0,75.23,8592765083715,1,18592765083712,45,28592765083719,"8536201090",0.36699999999999999]
[108372,"Ex9L-N 2P 16A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=100mA, type  S+AC","NAD",40.57,0,40.57,8592765083722,1,18592765083729,81,28592765083726,"8536201090",0.20300000000000001]
[108376,"Ex9L-N 2P 16A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=300mA, type  S+AC","NAD",43.2,0,43.2,8592765083760,1,18592765083767,81,28592765083764,"8536201090",0.20300000000000001]
[108380,"Ex9L-N 2P 16A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=500mA, type  S+AC","NAD",51.6,0,51.6,8592765083807,1,18592765083804,81,28592765083801,"8536201090",0.20300000000000001]
[108373,"Ex9L-N 2P 25A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=100mA, type  S+AC","NAD",42.58,0,42.58,8592765083739,1,18592765083736,81,28592765083733,"8536201090",0.20300000000000001]
[108377,"Ex9L-N 2P 25A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=300mA, type  S+AC","NAD",45.21,0,{"$f":"E1244*(1-F1244)","v":45.21},8592765083777,1,18592765083774,81,28592765083771,"8536201090",0.20300000000000001]
[108381,"Ex9L-N 2P 25A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=500mA, type  S+AC","NAD",53.61,{"$f":"NAD","v":0},53.61,8592765083814,1,18592765083811,81,28592765083818,"8536201090",0.20300000000000001]
[108374,"Ex9L-N 2P 40A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=100mA, type  S+AC","NAD",49.52,0,49.52,8592765083746,1,18592765083743,81,28592765083740,"8536201090",0.20300000000000001]
[108378,"Ex9L-N 2P 40A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=300mA, type  S+AC","NAD",52.15,0,52.15,8592765083784,1,18592765083781,81,28592765083788,"8536201090",0.20300000000000001]
[108382,"Ex9L-N 2P 40A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=500mA, type  S+AC","NAD",60.56,0,60.56,8592765083821,1,18592765083828,81,28592765083825,"8536201090",0.20300000000000001]
[108375,"Ex9L-N 2P 63A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=100mA, type  S+AC","NAD",56.59,0,56.59,8592765083753,1,18592765083750,81,28592765083757,"8536201090",0.20300000000000001]
[108379,"Ex9L-N 2P 63A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=300mA, type  S+AC","NAD",59.21,0,59.21,8592765083791,1,18592765083798,81,28592765083795,"8536201090",0.20300000000000001]
[108383,"Ex9L-N 2P 63A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=500mA, type  S+AC","NAD",67.62,0,67.62,8592765083838,1,18592765083835,81,28592765083832,"8536201090",0.20300000000000001]
[108384,"Ex9L-N 4P 16A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=100mA, type  S+AC","NAD",53.06,0,53.06,8592765083845,1,18592765083842,45,28592765083849,"8536201090",0.35599999999999998]
[108388,"Ex9L-N 4P 16A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=300mA, type  S+AC","NAD",55.16,0,55.16,8592765083883,1,18592765083880,45,28592765083887,"8536201090",0.35599999999999998]
[108392,"Ex9L-N 4P 16A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=500mA, type  S+AC","NAD",67.77,0,67.77,8592765083920,1,18592765083927,45,28592765083924,"8536201090",0.35599999999999998]
[108385,"Ex9L-N 4P 25A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=100mA, type  S+AC","NAD",55.16,0,55.16,8592765083852,1,18592765083859,45,28592765083856,"8536201090",0.35599999999999998]
[108389,"Ex9L-N 4P 25A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=300mA, type  S+AC","NAD",58.31,0,58.31,8592765083890,1,18592765083897,45,28592765083894,"8536201090",0.35599999999999998]
[108393,"Ex9L-N 4P 25A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=500mA, type  S+AC","NAD",70.930000000000007,0,70.930000000000007,8592765083937,1,18592765083934,45,28592765083931,"8536201090",0.35599999999999998]
[108386,"Ex9L-N 4P 40A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=100mA, type  S+AC","NAD",73.02,0,73.02,8592765083869,1,18592765083866,45,28592765083863,"8536201090",0.35599999999999998]
[108390,"Ex9L-N 4P 40A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=300mA, type  S+AC","NAD",73.02,0,73.02,8592765083906,1,18592765083903,45,28592765083900,"8536201090",0.35599999999999998]
[108394,"Ex9L-N 4P 40A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=500mA, type  S+AC","NAD",85.62,0,85.62,8592765083944,1,18592765083941,45,28592765083948,"8536201090",0.35599999999999998]
[108387,"Ex9L-N 4P 63A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=100mA, type  S+AC","NAD",77.13,0,77.13,8592765083876,1,18592765083873,45,28592765083870,"8536201090",0.35599999999999998]
[108391,"Ex9L-N 4P 63A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=300mA, type  S+AC","NAD",77.13,0,77.13,8592765083913,1,18592765083910,45,28592765083917,"8536201090",0.35599999999999998]
[108395,"Ex9L-N 4P 63A 500mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=500mA, type  S+AC","NAD",89.73,0,89.73,8592765083951,1,18592765083958,45,28592765083955,"8536201090",0.35599999999999998]
[108396,"Ex9L-N 2P 16A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=100mA, type  S+A","NAD",40.57,0,40.57,8592765083968,1,18592765083965,81,28592765083962,"8536201090",0.20300000000000001]
[108400,"Ex9L-N 2P 16A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=300mA, type  S+A","NAD",43.2,0,43.2,8592765084002,1,18592765084009,81,28592765084006,"8536201090",0.20300000000000001]
[108397,"Ex9L-N 2P 25A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=100mA, type  S+A","NAD",42.58,0,42.58,8592765083975,1,18592765083972,81,28592765083979,"8536201090",0.20300000000000001]
[108401,"Ex9L-N 2P 25A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=300mA, type  S+A","NAD",45.21,0,45.21,8592765084019,1,18592765084016,81,28592765084013,"8536201090",0.20300000000000001]
[108398,"Ex9L-N 2P 40A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=100mA, type  S+A","NAD",49.52,0,49.52,8592765083982,1,18592765083989,81,28592765083986,"8536201090",0.20300000000000001]
[108402,"Ex9L-N 2P 40A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=300mA, type  S+A","NAD",52.15,0,52.15,8592765084026,1,18592765084023,81,28592765084020,"8536201090",0.20300000000000001]
[108399,"Ex9L-N 2P 63A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=100mA, type  S+A","NAD",56.59,0,56.59,8592765083999,1,18592765083996,81,28592765083993,"8536201090",0.20300000000000001]
[108403,"Ex9L-N 2P 63A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=300mA, type  S+A","NAD",59.21,0,59.21,8592765084033,1,18592765084030,81,28592765084037,"8536201090",0.20300000000000001]
[108404,"Ex9L-N 4P 16A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=100mA, type  S+A","NAD",57.53,0,57.53,8592765084040,1,18592765084047,45,28592765084044,"8536201090",0.35599999999999998]
[108408,"Ex9L-N 4P 16A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=300mA, type  S+A","NAD",59.63,0,59.63,8592765084088,1,18592765084085,45,28592765084082,"8536201090",0.35599999999999998]
[108405,"Ex9L-N 4P 25A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=100mA, type  S+A","NAD",59.63,0,59.63,8592765084057,1,18592765084054,45,28592765084051,"8536201090",0.35599999999999998]
[108409,"Ex9L-N 4P 25A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=300mA, type  S+A","NAD",62.78,0,62.78,8592765084095,1,18592765084092,45,28592765084099,"8536201090",0.35599999999999998]
[108406,"Ex9L-N 4P 40A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=100mA, type  S+A","NAD",77.48,0,77.48,8592765084064,1,18592765084061,45,28592765084068,"8536201090",0.35599999999999998]
[108410,"Ex9L-N 4P 40A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=300mA, type  S+A","NAD",77.48,0,77.48,8592765084101,1,18592765084108,45,28592765084105,"8536201090",0.35599999999999998]
[108407,"Ex9L-N 4P 63A A 100mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=100mA, type  S+A","NAD",81.59,0,81.59,8592765084071,1,18592765084078,45,28592765084075,"8536201090",0.35599999999999998]
[108411,"Ex9L-N 4P 63A A 300mA S","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=300mA, type  S+A","NAD",81.59,0,81.59,8592765084118,1,18592765084115,45,28592765084112,"8536201090",0.35599999999999998]
[108412,"Ex9L-N 2P 16A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=30mA, type  G+AC","NAD",40.76,0,40.76,8592765084125,1,18592765084122,81,28592765084129,"8536201090",0.20300000000000001]
[108416,"Ex9L-N 2P 16A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=100mA, type  G+AC","NAD",43.12,0,43.12,8592765084163,1,18592765084160,81,28592765084167,"8536201090",0.20300000000000001]
[108420,"Ex9L-N 2P 16A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=300mA, type  G+AC","NAD",45.74,0,45.74,8592765084200,1,18592765084207,81,28592765084204,"8536201090",0.20300000000000001]
[108424,"Ex9L-N 2P 16A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=500mA, type  G+AC","NAD",48.41,0,48.41,8592765084248,1,18592765084245,81,28592765084242,"8536201090",0.20300000000000001]
[108413,"Ex9L-N 2P 25A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=30mA, type  G+AC","NAD",42.77,0,42.77,8592765084132,1,18592765084139,81,28592765084136,"8536201090",0.20300000000000001]
[108417,"Ex9L-N 2P 25A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=100mA, type  G+AC","NAD",45.12,0,45.12,8592765084170,1,18592765084177,81,28592765084174,"8536201090",0.20300000000000001]
[108421,"Ex9L-N 2P 25A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=300mA, type  G+AC","NAD",47.75,0,47.75,8592765084217,1,18592765084214,81,28592765084211,"8536201090",0.20300000000000001]
[108425,"Ex9L-N 2P 25A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=500mA, type  G+AC","NAD",50.42,0,50.42,8592765084255,1,18592765084252,81,28592765084259,"8536201090",0.20300000000000001]
[108414,"Ex9L-N 2P 40A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=30mA, type  G+AC","NAD",49.72,0,49.72,8592765084149,1,18592765084146,81,28592765084143,"8536201090",0.20300000000000001]
[108418,"Ex9L-N 2P 40A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=100mA, type  G+AC","NAD",52.07,0,52.07,8592765084187,1,18592765084184,81,28592765084181,"8536201090",0.20300000000000001]
[108422,"Ex9L-N 2P 40A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=300mA, type  G+AC","NAD",54.69,0,54.69,8592765084224,1,18592765084221,81,28592765084228,"8536201090",0.20300000000000001]
[108426,"Ex9L-N 2P 40A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=500mA, type  G+AC","NAD",57.36,0,57.36,8592765084262,1,18592765084269,81,28592765084266,"8536201090",0.20300000000000001]
[108415,"Ex9L-N 2P 63A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=30mA, type  G+AC","NAD",56.77,0,56.77,8592765084156,1,18592765084153,81,28592765084150,"8536201090",0.20300000000000001]
[108419,"Ex9L-N 2P 63A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=100mA, type  G+AC","NAD",59.13,0,59.13,8592765084194,1,18592765084191,81,28592765084198,"8536201090",0.20300000000000001]
[108423,"Ex9L-N 2P 63A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=300mA, type  G+AC","NAD",61.76,0,61.76,8592765084231,1,18592765084238,81,28592765084235,"8536201090",0.20300000000000001]
[108427,"Ex9L-N 2P 63A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=500mA, type  G+AC","NAD",64.430000000000007,0,64.430000000000007,8592765084279,1,18592765084276,81,28592765084273,"8536201090",0.20300000000000001]
[108428,"Ex9L-N 4P 16A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=30mA, type  G+AC","NAD",52.63,0,52.63,8592765084286,1,18592765084283,45,28592765084280,"8536201090",0.35599999999999998]
[108432,"Ex9L-N 4P 16A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=100mA, type  G+AC","NAD",53.06,0,53.06,8592765084323,1,18592765084320,45,28592765084327,"8536201090",0.35599999999999998]
[108436,"Ex9L-N 4P 16A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=300mA, type  G+AC","NAD",55.16,0,55.16,8592765084361,1,18592765084368,45,28592765084365,"8536201090",0.35599999999999998]
[108440,"Ex9L-N 4P 16A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=500mA, type  G+AC","NAD",67.77,0,67.77,8592765084408,1,18592765084405,45,28592765084402,"8536201090",0.35599999999999998]
[108429,"Ex9L-N 4P 25A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=30mA, type  G+AC","NAD",52.63,0,52.63,8592765084293,1,18592765084290,45,28592765084297,"8536201090",0.35599999999999998]
[108433,"Ex9L-N 4P 25A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=100mA, type  G+AC","NAD",55.16,0,55.16,8592765084330,1,18592765084337,45,28592765084334,"8536201090",0.35599999999999998]
[108437,"Ex9L-N 4P 25A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=300mA, type  G+AC","NAD",58.31,0,58.31,8592765084378,1,18592765084375,45,28592765084372,"8536201090",0.35599999999999998]
[108441,"Ex9L-N 4P 25A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=500mA, type  G+AC","NAD",70.930000000000007,0,70.930000000000007,8592765084415,1,18592765084412,45,28592765084419,"8536201090",0.35599999999999998]
[108430,"Ex9L-N 4P 40A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=30mA, type  G+AC","NAD",70.489999999999995,0,70.489999999999995,8592765084309,1,18592765084306,45,28592765084303,"8536201090",0.35599999999999998]
[108434,"Ex9L-N 4P 40A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=100mA, type  G+AC","NAD",73.02,0,73.02,8592765084347,1,18592765084344,45,28592765084341,"8536201090",0.35599999999999998]
[108438,"Ex9L-N 4P 40A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=300mA, type  G+AC","NAD",73.02,0,73.02,8592765084385,1,18592765084382,45,28592765084389,"8536201090",0.35599999999999998]
[108442,"Ex9L-N 4P 40A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=500mA, type  G+AC","NAD",85.62,0,85.62,8592765084422,1,18592765084429,45,28592765084426,"8536201090",0.35599999999999998]
[108431,"Ex9L-N 4P 63A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=30mA, type  G+AC","NAD",74.599999999999994,0,{"$f":"E1308*(1-F1308)","v":74.599999999999994},8592765084316,1,18592765084313,45,28592765084310,"8536201090",0.35599999999999998]
[108435,"Ex9L-N 4P 63A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=100mA, type  G+AC","NAD",77.13,{"$f":"NAD","v":0},77.13,8592765084354,1,18592765084351,45,28592765084358,"8536201090",0.35599999999999998]
[108439,"Ex9L-N 4P 63A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=300mA, type  G+AC","NAD",77.13,0,77.13,8592765084392,1,18592765084399,45,28592765084396,"8536201090",0.35599999999999998]
[108443,"Ex9L-N 4P 63A 500mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=500mA, type  G+AC","NAD",89.73,0,89.73,8592765084439,1,18592765084436,45,28592765084433,"8536201090",0.35599999999999998]
[108444,"Ex9L-N 2P 16A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=30mA, type  G+A","NAD",42.95,0,42.95,8592765084446,1,18592765084443,81,28592765084440,"8536201090",0.20300000000000001]
[108448,"Ex9L-N 2P 16A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=100mA, type  G+A","NAD",45.31,0,45.31,8592765084484,1,18592765084481,81,28592765084488,"8536201090",0.20300000000000001]
[108452,"Ex9L-N 2P 16A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=16A, IΔn=300mA, type  G+A","NAD",47.94,0,47.94,8592765084521,1,18592765084528,81,28592765084525,"8536201090",0.20300000000000001]
[108445,"Ex9L-N 2P 25A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=30mA, type  G+A","NAD",44.96,0,44.96,8592765084453,1,18592765084450,81,28592765084457,"8536201090",0.20300000000000001]
[108449,"Ex9L-N 2P 25A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=100mA, type  G+A","NAD",47.32,0,47.32,8592765084491,1,18592765084498,81,28592765084495,"8536201090",0.20300000000000001]
[108453,"Ex9L-N 2P 25A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=25A, IΔn=300mA, type  G+A","NAD",49.94,0,49.94,8592765084538,1,18592765084535,81,28592765084532,"8536201090",0.20300000000000001]
[108446,"Ex9L-N 2P 40A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=30mA, type  G+A","NAD",51.91,0,51.91,8592765084460,1,18592765084467,81,28592765084464,"8536201090",0.20300000000000001]
[108450,"Ex9L-N 2P 40A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=100mA, type  G+A","NAD",54.26,0,54.26,8592765084507,1,18592765084504,81,28592765084501,"8536201090",0.20300000000000001]
[108454,"Ex9L-N 2P 40A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=40A, IΔn=300mA, type  G+A","NAD",56.89,0,56.89,8592765084545,1,18592765084542,81,28592765084549,"8536201090",0.20300000000000001]
[108447,"Ex9L-N 2P 63A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=30mA, type  G+A","NAD",58.98,0,58.98,8592765084477,1,18592765084474,81,28592765084471,"8536201090",0.20300000000000001]
[108451,"Ex9L-N 2P 63A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=100mA, type  G+A","NAD",61.33,0,61.33,8592765084514,1,18592765084511,81,28592765084518,"8536201090",0.20300000000000001]
[108455,"Ex9L-N 2P 63A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 2-pole, In=63A, IΔn=300mA, type  G+A","NAD",63.95,0,63.95,8592765084552,1,18592765084559,81,28592765084556,"8536201090",0.20300000000000001]
[108456,"Ex9L-N 4P 16A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=30mA, type  G+A","NAD",56.31,0,56.31,8592765084569,1,18592765084566,45,28592765084563,"8536201090",0.35599999999999998]
[108460,"Ex9L-N 4P 16A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=100mA, type  G+A","NAD",56.73,0,56.73,8592765084606,1,18592765084603,45,28592765084600,"8536201090",0.35599999999999998]
[108464,"Ex9L-N 4P 16A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=16A, IΔn=300mA, type  G+A","NAD",58.83,0,58.83,8592765084644,1,18592765084641,45,28592765084648,"8536201090",0.35599999999999998]
[108457,"Ex9L-N 4P 25A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=30mA, type  G+A","NAD",56.31,0,56.31,8592765084576,1,18592765084573,45,28592765084570,"8536201090",0.35599999999999998]
[108461,"Ex9L-N 4P 25A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=100mA, type  G+A","NAD",58.83,0,58.83,8592765084613,1,18592765084610,45,28592765084617,"8536201090",0.35599999999999998]
[108465,"Ex9L-N 4P 25A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=25A, IΔn=300mA, type  G+A","NAD",61.99,0,61.99,8592765084651,1,18592765084658,45,28592765084655,"8536201090",0.35599999999999998]
[108458,"Ex9L-N 4P 40A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=30mA, type  G+A","NAD",74.17,0,74.17,8592765084583,1,18592765084580,45,28592765084587,"8536201090",0.35599999999999998]
[108462,"Ex9L-N 4P 40A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=100mA, type  G+A","NAD",76.69,0,76.69,8592765084620,1,18592765084627,45,28592765084624,"8536201090",0.35599999999999998]
[108466,"Ex9L-N 4P 40A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=40A, IΔn=300mA, type  G+A","NAD",76.69,0,76.69,8592765084668,1,18592765084665,45,28592765084662,"8536201090",0.35599999999999998]
[108459,"Ex9L-N 4P 63A A 30mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=30mA, type  G+A","NAD",78.28,0,78.28,8592765084590,1,18592765084597,45,28592765084594,"8536201090",0.35599999999999998]
[108463,"Ex9L-N 4P 63A A 100mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=100mA, type  G+A","NAD",80.8,0,80.8,8592765084637,1,18592765084634,45,28592765084631,"8536201090",0.35599999999999998]
[108467,"Ex9L-N 4P 63A A 300mA G","Residual Current Circuit Breaker, Icn=6kA, 4-pole, In=63A, IΔn=300mA, type  G+A","NAD",80.8,0,80.8,8592765084675,1,18592765084672,45,28592765084679,"8536201090",0.35599999999999998]
[]
["Residual Current Circuit Breakers Ex9LB63"]
[110212,"Ex9LB63 1P+N 25A 30mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=25A, IΔn=30mA, type  B","NAC",374.01,{"$f":"NAC","v":0},{"$f":"E1338*(1-F1338)","v":374.01},8592765102126,1,18592765102123,72,28592765102120,"8536201090",0.28000000000000003]
[110213,"Ex9LB63 1P+N 40A 30mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=40A, IΔn=30mA, type  B","NAC",379.94,{"$f":"NAC","v":0},{"$f":"E1339*(1-F1339)","v":379.94},8592765102133,1,18592765102130,72,28592765102137,"8536201090",0.28000000000000003]
[110214,"Ex9LB63 1P+N 63A 30mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=63A, IΔn=30mA, type  B","NAC",385.71,0,385.71,8592765102140,1,18592765102147,72,28592765102144,"8536201090",0.28000000000000003]
[110215,"Ex9LB63 1P+N 25A 100mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=25A, IΔn=100mA, type  B","NAC",391.54,0,391.54,8592765102157,1,18592765102154,72,28592765102151,"8536201090",0.28000000000000003]
[110216,"Ex9LB63 1P+N 40A 100mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=40A, IΔn=100mA, type  B","NAC",397.75,0,397.75,8592765102164,1,18592765102161,72,28592765102168,"8536201090",0.28000000000000003]
[110217,"Ex9LB63 1P+N 63A 100mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=63A, IΔn=100mA, type  B","NAC",403.79,0,403.79,8592765102171,1,18592765102178,72,28592765102175,"8536201090",0.28000000000000003]
[110218,"Ex9LB63 1P+N 25A 300mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=25A, IΔn=300mA, type  B","NAC",385.58,0,385.58,8592765102188,1,18592765102185,72,28592765102182,"8536201090",0.28000000000000003]
[110219,"Ex9LB63 1P+N 40A 300mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=40A, IΔn=300mA, type  B","NAC",391.69,0,391.69,8592765102195,1,18592765102192,72,28592765102199,"8536201090",0.28000000000000003]
[110220,"Ex9LB63 1P+N 63A 300mA","Residual Current Circuit Breaker, Icn=10kA, 1P+N, In=63A, IΔn=300mA, type  B","NAC",397.64,0,397.64,8592765102201,1,18592765102208,72,28592765102205,"8536201090",0.28000000000000003]
[110221,"Ex9LB63 3P+N 25A 30mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=25A, IΔn=30mA, type  B","NAC",485.73,0,485.73,8592765102218,1,18592765102215,45,28592765102212,"8536201090",0.43]
[110222,"Ex9LB63 3P+N 40A 30mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=40A, IΔn=30mA, type  B","NAC",493.43,0,493.43,8592765102225,1,18592765102222,45,28592765102229,"8536201090",0.43]
[110223,"Ex9LB63 3P+N 63A 30mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=63A, IΔn=30mA, type  B","NAC",500.92,0,500.92,8592765102232,1,18592765102239,45,28592765102236,"8536201090",0.43]
[110224,"Ex9LB63 3P+N 25A 100mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=25A, IΔn=100mA, type  B","NAC",508.49,0,508.49,8592765102249,1,18592765102246,45,28592765102243,"8536201090",0.43]
[110225,"Ex9LB63 3P+N 40A 100mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=40A, IΔn=100mA, type  B","NAC",516.55999999999995,0,516.55999999999995,8592765102256,1,18592765102253,45,28592765102250,"8536201090",0.43]
[110226,"Ex9LB63 3P+N 63A 100mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=63A, IΔn=100mA, type  B","NAC",524.4,0,524.4,8592765102263,1,18592765102260,45,28592765102267,"8536201090",0.43]
[110227,"Ex9LB63 3P+N 25A 300mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=25A, IΔn=300mA, type  B","NAC",500.75,0,500.75,8592765102270,1,18592765102277,45,28592765102274,"8536201090",0.43]
[110228,"Ex9LB63 3P+N 40A 300mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=40A, IΔn=300mA, type  B","NAC",508.69,0,508.69,8592765102287,1,18592765102284,45,28592765102281,"8536201090",0.43]
[110229,"Ex9LB63 3P+N 63A 300mA","Residual Current Circuit Breaker, Icn=10kA, 3P+N, In=63A, IΔn=300mA, type  B","NAC",516.41,0,516.41,8592765102294,1,18592765102291,45,28592765102298,"8536201090",0.43]
[]
["Residual Current Circuit Breakers Ex9CL-100, 10 kA"]
[100643,"Ex9CL-H 2P 25A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=30mA, typ AC","NAC",40.78,{"$f":"NAC","v":0},{"$f":"E1358*(1-F1358)","v":40.78},8592765006448,1,8592765006448,81,28592765006442,"8536201090",0.24]
[100644,"Ex9CL-H 2P 25A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, typ AC","NAC",65.09,0,65.09,8592765006455,1,8592765006455,81,28592765006459,"8536201090",0.24]
[100645,"Ex9CL-H 2P 25A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, typ AC","NAC",65.09,0,65.09,8592765006462,1,8592765006462,81,28592765006466,"8536201090",0.24]
[100646,"Ex9CL-H 2P 40A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=30mA, typ AC","NAC",56.12,0,56.12,8592765006479,1,8592765006479,81,28592765006473,"8536201090",0.24]
[100647,"Ex9CL-H 2P 40A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, typ AC","NAC",70.2,0,70.2,8592765006486,1,8592765006486,81,28592765006480,"8536201090",0.24]
[100648,"Ex9CL-H 2P 40A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, typ AC","NAC",70.2,0,70.2,8592765006493,1,8592765006493,81,28592765006497,"8536201090",0.24]
[100649,"Ex9CL-H 2P 63A 30mA  ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=30mA, typ AC","NAC",78.78,0,78.78,8592765006509,1,8592765006509,81,28592765006503,"8536201090",0.24]
[100650,"Ex9CL-H 2P 63A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, typ AC","NAC",80.47,0,80.47,8592765006516,1,8592765006516,81,28592765006510,"8536201090",0.24]
[100651,"Ex9CL-H 2P 63A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, typ AC","NAC",80.47,0,80.47,8592765006523,1,8592765006523,81,28592765006527,"8536201090",0.24]
[100652,"Ex9CL-H 4P 25A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=30mA, typ AC","NAC",44.95,0,44.95,8592765006530,1,8592765006530,45,28592765006534,"8536201090",0.48]
[100653,"Ex9CL-H 4P 25A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, typ AC","NAC",70.14,0,70.14,8592765006547,1,8592765006547,45,28592765006541,"8536201090",0.48]
[100654,"Ex9CL-H 4P 25A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, typ AC","NAC",70.14,0,70.14,8592765006554,1,8592765006554,45,28592765006558,"8536201090",0.48]
[100655,"Ex9CL-H 4P 40A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=30mA, typ AC","NAC",61.81,0,61.81,8592765006561,1,8592765006561,45,28592765006565,"8536201090",0.48]
[100656,"Ex9CL-H 4P 40A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, typ AC","NAC",70.959999999999994,0,70.959999999999994,8592765006578,1,8592765006578,45,28592765006572,"8536201090",0.48]
[100657,"Ex9CL-H 4P 40A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, typ AC","NAC",70.959999999999994,0,70.959999999999994,8592765006585,1,8592765006585,45,28592765006589,"8536201090",0.48]
[100658,"Ex9CL-H 4P 63A 30mA  ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=30mA, typ AC","NAC",83.12,0,83.12,8592765006592,1,8592765006592,45,28592765006596,"8536201090",0.48]
[100659,"Ex9CL-H 4P 63A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, typ AC","NAC",83.12,0,83.12,8592765006608,1,8592765006608,45,28592765006602,"8536201090",0.48]
[100660,"Ex9CL-H 4P 63A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, typ AC","NAC",83.12,0,83.12,8592765006615,1,8592765006615,45,28592765006619,"8536201090",0.48]
[100661,"Ex9CL-H 2P 25A A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=30mA, typ A","NAC",51.18,0,51.18,8592765006622,1,8592765006622,81,28592765006626,"8536201090",0.24]
[100662,"Ex9CL-H 2P 25A A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=100mA, typ A","NAC",71.680000000000007,0,71.680000000000007,8592765006639,1,8592765006639,81,28592765006633,"8536201090",0.24]
[100663,"Ex9CL-H 2P 25A A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=25A, IΔn=300mA, typ A","NAC",71.680000000000007,0,71.680000000000007,8592765006646,1,8592765006646,81,28592765006640,"8536201090",0.24]
[100664,"Ex9CL-H 2P 40A A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=30mA, typ A","NAC",61.73,0,61.73,8592765006653,1,8592765006653,81,28592765006657,"8536201090",0.24]
[100665,"Ex9CL-H 2P 40A A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=100mA, typ A","NAC",77.260000000000005,0,77.260000000000005,8592765006660,1,8592765006660,81,28592765006664,"8536201090",0.24]
[100666,"Ex9CL-H 2P 40A A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=40A, IΔn=300mA, typ A","NAC",77.260000000000005,0,77.260000000000005,8592765006677,1,8592765006677,81,28592765006671,"8536201090",0.24]
[100667,"Ex9CL-H 2P 63A A 30mA  ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=30mA, typ A","NAC",86.71,0,86.71,8592765006684,1,8592765006684,81,28592765006688,"8536201090",0.24]
[100668,"Ex9CL-H 2P 63A A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, typ A","NAC",88.54,0,88.54,8592765006691,1,8592765006691,81,28592765006695,"8536201090",0.24]
[100669,"Ex9CL-H 2P 63A A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, typ A","NAC",88.54,0,88.54,8592765006707,1,8592765006707,81,28592765006701,"8536201090",0.24]
[100670,"Ex9CL-H 4P 25A A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=30mA, typ A","NAC",57.46,0,57.46,8592765006714,1,8592765006714,45,28592765006718,"8536201090",0.48]
[100671,"Ex9CL-H 4P 25A A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=100mA, typ A","NAC",77.19,0,77.19,8592765006721,1,8592765006721,45,28592765006725,"8536201090",0.48]
[100672,"Ex9CL-H 4P 25A A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=25A, IΔn=300mA, typ A","NAC",77.19,0,77.19,8592765006738,1,8592765006738,45,28592765006732,"8536201090",0.48]
[100673,"Ex9CL-H 4P 40A A 30mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=30mA, typ A","NAC",71.22,0,71.22,8592765006745,1,8592765006745,45,28592765006749,"8536201090",0.48]
[100674,"Ex9CL-H 4P 40A A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=100mA, typ A","NAC",78.05,0,78.05,8592765006752,1,8592765006752,45,28592765006756,"8536201090",0.48]
[100675,"Ex9CL-H 4P 40A A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=40A, IΔn=300mA, typ A","NAC",78.05,{"$f":"NAC","v":0},78.05,8592765006769,1,8592765006769,45,28592765006763,"8536201090",0.48]
[100676,"Ex9CL-H 4P 63A A 30mA  ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=30mA, typ A","NAC",91.45,0,91.45,8592765006776,1,8592765006776,45,28592765006770,"8536201090",0.48]
[100677,"Ex9CL-H 4P 63A A 100mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, typ A","NAC",91.45,0,91.45,8592765006783,1,8592765006783,45,28592765006787,"8536201090",0.48]
[100678,"Ex9CL-H 4P 63A A 300mA ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, typ A","NAC",91.45,0,91.45,8592765006790,1,8592765006790,45,28592765006794,"8536201090",0.48]
[100715,"Ex9CL-100 2P 63A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, typ S+AC","NAC",105.82,0,105.82,8592765007162,1,8592765007162,81,28592765007166,"8536201090",0.24]
[100716,"Ex9CL-100 2P 63A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, typ S+AC","NAC",105.82,0,105.82,8592765007179,1,8592765007179,81,28592765007173,"8536201090",0.24]
[100717,"Ex9CL-100 2P 80A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=80A, IΔn=100mA, typ S+AC","NAC",156.93,0,156.93,8592765007186,1,8592765007186,81,28592765007180,"8536209090",0.24]
[100718,"Ex9CL-100 2P 80A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=80A, IΔn=300mA, typ S+AC","NAC",156.93,0,156.93,8592765007193,1,8592765007193,81,28592765007197,"8536209090",0.24]
[100719,"Ex9CL-100 2P 100A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=100A, IΔn=100mA, typ S+AC","NAC",212.3,0,212.3,8592765007209,1,8592765007209,81,28592765007203,"8536209090",0.24]
[100720,"Ex9CL-100 2P 100A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=100A, IΔn=300mA, typ S+AC","NAC",212.3,0,212.3,8592765007216,1,8592765007216,81,28592765007210,"8536209090",0.24]
[100721,"Ex9CL-100 4P 63A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, typ S+AC","NAC",116.95,0,116.95,8592765007223,1,8592765007223,45,28592765007227,"8536201090",0.48]
[100722,"Ex9CL-100 4P 63A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, typ S+AC","NAC",116.95,0,116.95,8592765007230,1,8592765007230,45,28592765007234,"8536201090",0.48]
[100723,"Ex9CL-100 4P 80A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=80A, IΔn=100mA, typ S+AC","NAC",169.23,0,169.23,8592765007247,1,8592765007247,45,28592765007241,"8536209090",0.48]
[100724,"Ex9CL-100 4P 80A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=80A, IΔn=300mA, typ S+AC","NAC",169.23,0,169.23,8592765007254,1,8592765007254,45,28592765007258,"8536209090",0.48]
[100725,"Ex9CL-100 4P 100A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=100A, IΔn=100mA, typ S+AC","NAC",234.13,0,234.13,8592765007261,1,8592765007261,45,28592765007265,"8536209090",0.48]
[100726,"Ex9CL-100 4P 100A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=100A, IΔn=300mA, typ S+AC","NAC",234.13,0,234.13,8592765007278,1,8592765007278,45,28592765007272,"8536209090",0.48]
[100727,"Ex9CL-100 2P 63A A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=100mA, typ S+A","NAC",116.44,0,116.44,8592765007285,1,8592765007285,81,28592765007289,"8536201090",0.24]
[100728,"Ex9CL-100 2P 63A A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=63A, IΔn=300mA, typ S+A","NAC",116.44,0,116.44,8592765007292,1,8592765007292,81,28592765007296,"8536201090",0.24]
[100729,"Ex9CL-100 2P 80A A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=80A, IΔn=100mA, typ S+A","NAC",172.67,0,172.67,8592765007308,1,8592765007308,81,28592765007302,"8536209090",0.24]
[100730,"Ex9CL-100 2P 80A A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=80A, IΔn=300mA, typ S+A","NAC",172.67,0,172.67,8592765007315,1,8592765007315,81,28592765007319,"8536209090",0.24]
[100731,"Ex9CL-100 2P 100A A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=100A, IΔn=100mA, typ S+A","NAC",233.52,0,233.52,8592765007322,1,8592765007322,81,28592765007326,"8536209090",0.24]
[100732,"Ex9CL-100 2P 100A A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 2-pole, In=100A, IΔn=300mA, typ S+A","NAC",233.52,0,233.52,8592765007339,1,8592765007339,81,28592765007333,"8536209090",0.24]
[100733,"Ex9CL-100 4P 63A A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=100mA, typ S+A","NAC",128.68,0,128.68,8592765007346,1,8592765007346,45,28592765007340,"8536201090",0.48]
[100734,"Ex9CL-100 4P 63A A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=63A, IΔn=300mA, typ S+A","NAC",128.68,0,128.68,8592765007353,1,8592765007353,45,28592765007357,"8536201090",0.48]
[100735,"Ex9CL-100 4P 80A A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=80A, IΔn=100mA, typ S+A","NAC",186.21,0,186.21,8592765007360,1,8592765007360,45,28592765007364,"8536209090",0.48]
[100736,"Ex9CL-100 4P 80A A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=80A, IΔn=300mA, typ S+A","NAC",186.21,0,186.21,8592765007377,1,8592765007377,45,28592765007371,"8536209090",0.48]
[100737,"Ex9CL-100 4P 100A A 100mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=100A, IΔn=100mA, typ S+A","NAC",257.54000000000002,0,257.54000000000002,8592765007384,1,8592765007384,45,28592765007388,"8536209090",0.48]
[100738,"Ex9CL-100 4P 100A A 300mA S ","Residual Current Circuit Breaker, Icn=10kA, 4-pole, In=100A, IΔn=300mA, typ S+A","NAC",257.54000000000002,0,257.54000000000002,8592765007391,1,8592765007391,45,28592765007395,"8536209090",0.48]
[101445,"YS31","Sticker with information on the regular monthly testing","NAC",1.37,0,1.37,null,null,null,null,null,"8538909999"]
[]
["Residual Current Breakers with Overload protection Ex9BL-H, 10 kA",null,null,null,null,null,null,"","","","","",null,""]
[107381,"Ex9BL-H 1P+N B6 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=6A, IΔn=30mA, typ AC","NAE",46.97,{"$f":"NAE","v":0},{"$f":"E1421*(1-F1421)","v":46.97},8592765073822,6,18592765073829,72,28592765073826,"8536201090",0.24]
[107382,"Ex9BL-H 1P+N B10 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=10A, IΔn=30mA, typ AC","NAE",50.67,{"$f":"NAE","v":0},50.67,8592765073839,6,18592765073836,72,28592765073833,"8536201090",0.24]
[107383,"Ex9BL-H 1P+N B13 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=13A, IΔn=30mA, typ AC","NAE",50.67,0,50.67,8592765073846,6,18592765073843,72,28592765073840,"8536201090",0.24]
[107384,"Ex9BL-H 1P+N B16 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=16A, IΔn=30mA, typ AC","NAE",42.29,0,42.29,8592765073853,6,18592765073850,72,28592765073857,"8536201090",0.24]
[107385,"Ex9BL-H 1P+N B20 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=20A, IΔn=30mA, typ AC","NAE",46,0,46,8592765073860,6,18592765073867,72,28592765073864,"8536201090",0.24]
[107386,"Ex9BL-H 1P+N B25 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=25A, IΔn=30mA, typ AC","NAE",49.83,0,49.83,8592765073877,6,18592765073874,72,28592765073871,"8536201090",0.24]
[107387,"Ex9BL-H 1P+N B32 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=32A, IΔn=30mA, typ AC","NAE",54.56,0,54.56,8592765073884,6,18592765073881,72,28592765073888,"8536201090",0.25]
[107388,"Ex9BL-H 1P+N B40 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=40A, IΔn=30mA, typ AC","NAE",57.66,0,57.66,8592765073891,6,18592765073898,72,28592765073895,"8536201090",0.25]
[107391,"Ex9BL-H 1P+N C6 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=6A, IΔn=30mA, typ AC","NAE",46.97,0,46.97,8592765073921,6,18592765073928,72,28592765073925,"8536201090",0.24]
[107392,"Ex9BL-H 1P+N C10 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=10A, IΔn=30mA, typ AC","NAE",50.67,0,50.67,8592765073938,6,18592765073935,72,28592765073932,"8536201090",0.24]
[107393,"Ex9BL-H 1P+N C13 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=13A, IΔn=30mA, typ AC","NAE",50.67,0,50.67,8592765073945,6,18592765073942,72,28592765073949,"8536201090",0.24]
[107394,"Ex9BL-H 1P+N C16 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=16A, IΔn=30mA, typ AC","NAE",42.29,0,42.29,8592765073952,6,18592765073959,72,28592765073956,"8536201090",0.24]
[107395,"Ex9BL-H 1P+N C20 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=20A, IΔn=30mA, typ AC","NAE",46,0,46,8592765073969,6,18592765073966,72,28592765073963,"8536201090",0.24]
[107396,"Ex9BL-H 1P+N C25 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=25A, IΔn=30mA, typ AC","NAE",49.83,0,49.83,8592765073976,6,18592765073973,72,28592765073970,"8536201090",0.24]
[107397,"Ex9BL-H 1P+N C32 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=32A, IΔn=30mA, typ AC","NAE",54.56,0,54.56,8592765073983,6,18592765073980,72,28592765073987,"8536201090",0.25]
[107398,"Ex9BL-H 1P+N C40 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=40A, IΔn=30mA, typ AC","NAE",57.66,0,57.66,8592765073990,6,18592765073997,72,28592765073994,"8536201090",0.25]
[107401,"Ex9BL-H 1P+N B6 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=6A, IΔn=30mA, typ A","NAE",68.67,0,68.67,8592765074027,6,18592765074024,72,28592765074021,"8536201090",0.24]
[107402,"Ex9BL-H 1P+N B10 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=10A, IΔn=30mA, typ A","NAE",68.91,0,68.91,8592765074034,6,18592765074031,72,28592765074038,"8536201090",0.24]
[107403,"Ex9BL-H 1P+N B13 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=13A, IΔn=30mA, typ A","NAE",68.91,0,68.91,8592765074041,6,18592765074048,72,28592765074045,"8536201090",0.24]
[107404,"Ex9BL-H 1P+N B16 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=16A, IΔn=30mA, typ A","NAE",57.1,0,57.1,8592765074058,6,18592765074055,72,28592765074052,"8536201090",0.24]
[107405,"Ex9BL-H 1P+N B20 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=20A, IΔn=30mA, typ A","NAE",67.260000000000005,0,67.260000000000005,8592765074065,6,18592765074062,72,28592765074069,"8536201090",0.24]
[107406,"Ex9BL-H 1P+N B25 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=25A, IΔn=30mA, typ A","NAE",70.67,0,70.67,8592765074072,6,18592765074079,72,28592765074076,"8536201090",0.24]
[107407,"Ex9BL-H 1P+N B32 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=32A, IΔn=30mA, typ A","NAE",75.260000000000005,0,75.260000000000005,8592765074089,6,18592765074086,72,28592765074083,"8536201090",0.25]
[107408,"Ex9BL-H 1P+N B40 A 30mA","RCBO, Icn=10kA, 1+Npole, char. B, In=40A, IΔn=30mA, typ A","NAE",77.569999999999993,0,77.569999999999993,8592765074096,6,18592765074093,72,28592765074090,"8536201090",0.25]
[107411,"Ex9BL-H 1P+N C6 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=6A, IΔn=30mA, typ A","NAE",68.67,0,68.67,8592765074126,6,18592765074123,72,28592765074120,"8536201090",0.24]
[107412,"Ex9BL-H 1P+N C10 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=10A, IΔn=30mA, typ A","NAE",68.91,0,68.91,8592765074133,6,18592765074130,72,28592765074137,"8536201090",0.24]
[107413,"Ex9BL-H 1P+N C13 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=13A, IΔn=30mA, typ A","NAE",68.91,0,68.91,8592765074140,6,18592765074147,72,28592765074144,"8536201090",0.24]
[107414,"Ex9BL-H 1P+N C16 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=16A, IΔn=30mA, typ A","NAE",57.1,0,57.1,8592765074157,6,18592765074154,72,28592765074151,"8536201090",0.24]
[107415,"Ex9BL-H 1P+N C20 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=20A, IΔn=30mA, typ A","NAE",67.260000000000005,0,67.260000000000005,8592765074164,6,18592765074161,72,28592765074168,"8536201090",0.24]
[107416,"Ex9BL-H 1P+N C25 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=25A, IΔn=30mA, typ A","NAE",70.67,0,70.67,8592765074171,6,18592765074178,72,28592765074175,"8536201090",0.24]
[107417,"Ex9BL-H 1P+N C32 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=32A, IΔn=30mA, typ A","NAE",75.260000000000005,0,75.260000000000005,8592765074188,6,18592765074185,72,28592765074182,"8536201090",0.25]
[107418,"Ex9BL-H 1P+N C40 A 30mA","RCBO, Icn=10kA, 1+Npole, char. C, In=40A, IΔn=30mA, typ A","NAE",77.569999999999993,0,77.569999999999993,8592765074195,6,18592765074192,72,28592765074199,"8536201090",0.25]
[107461,"Ex9BL-H 1P+N B6 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=6A, IΔn=100mA, typ AC","NAE",47.88,0,47.88,8592765074621,6,18592765074628,72,28592765074625,"8536201090",0.24]
[107462,"Ex9BL-H 1P+N B10 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=10A, IΔn=100mA, typ AC","NAE",51.66,0,51.66,8592765074638,6,18592765074635,72,28592765074632,"8536201090",0.24]
[107463,"Ex9BL-H 1P+N B13 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=13A, IΔn=100mA, typ AC","NAE",51.66,0,51.66,8592765074645,6,18592765074642,72,28592765074649,"8536201090",0.24]
[107464,"Ex9BL-H 1P+N B16 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=16A, IΔn=100mA, typ AC","NAE",43.13,0,43.13,8592765074652,6,18592765074659,72,28592765074656,"8536201090",0.24]
[107465,"Ex9BL-H 1P+N B20 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=20A, IΔn=100mA, typ AC","NAE",46.89,0,46.89,8592765074669,6,18592765074666,72,28592765074663,"8536201090",0.24]
[107466,"Ex9BL-H 1P+N B25 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=25A, IΔn=100mA, typ AC","NAE",50.8,0,50.8,8592765074676,6,18592765074673,72,28592765074670,"8536201090",0.24]
[107467,"Ex9BL-H 1P+N B32 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=32A, IΔn=100mA, typ AC","NAE",55.61,0,55.61,8592765074683,6,18592765074680,72,28592765074687,"8536201090",0.25]
[107468,"Ex9BL-H 1P+N B40 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=40A, IΔn=100mA, typ AC","NAE",58.76,0,58.76,8592765074690,6,18592765074697,72,28592765074694,"8536201090",0.25]
[107471,"Ex9BL-H 1P+N C6  100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=6A, IΔn=100mA, typ AC","NAE",47.88,0,47.88,8592765074720,6,18592765074727,72,28592765074724,"8536201090",0.24]
[107472,"Ex9BL-H 1P+N C10 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=10A, IΔn=100mA, typ AC","NAE",51.66,0,51.66,8592765074737,6,18592765074734,72,28592765074731,"8536201090",0.24]
[107473,"Ex9BL-H 1P+N C13 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=13A, IΔn=100mA, typ AC","NAE",51.66,0,51.66,8592765074744,6,18592765074741,72,28592765074748,"8536201090",0.24]
[107474,"Ex9BL-H 1P+N C16 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=16A, IΔn=100mA, typ AC","NAE",43.13,0,43.13,8592765074751,6,18592765074758,72,28592765074755,"8536201090",0.24]
[107475,"Ex9BL-H 1P+N C20 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=20A, IΔn=100mA, typ AC","NAE",46.89,0,46.89,8592765074768,6,18592765074765,72,28592765074762,"8536201090",0.24]
[107476,"Ex9BL-H 1P+N C25 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=25A, IΔn=100mA, typ AC","NAE",50.8,0,50.8,8592765074775,6,18592765074772,72,28592765074779,"8536201090",0.24]
[107477,"Ex9BL-H 1P+N C32 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=32A, IΔn=100mA, typ AC","NAE",55.61,0,55.61,8592765074782,6,18592765074789,72,28592765074786,"8536201090",0.25]
[107478,"Ex9BL-H 1P+N C40 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=40A, IΔn=100mA, typ AC","NAE",58.76,0,58.76,8592765074799,6,18592765074796,72,28592765074793,"8536201090",0.25]
[107481,"Ex9BL-H 1P+N B6 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=6A, IΔn=100mA, typ A","NAE",133.37,0,133.37,8592765074829,6,18592765074826,72,28592765074823,"8536201090",0.24]
[107482,"Ex9BL-H 1P+N B10 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=10A, IΔn=100mA, typ A","NAE",133.79,0,133.79,8592765074836,6,18592765074833,72,28592765074830,"8536201090",0.24]
[107483,"Ex9BL-H 1P+N B13 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=13A, IΔn=100mA, typ A","NAE",133.79,0,133.79,8592765074843,6,18592765074840,72,28592765074847,"8536201090",0.24]
[107484,"Ex9BL-H 1P+N B16 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=16A, IΔn=100mA, typ A","NAE",110.85,0,110.85,8592765074850,6,18592765074857,72,28592765074854,"8536201090",0.24]
[107485,"Ex9BL-H 1P+N B20 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=20A, IΔn=100mA, typ A","NAE",130.58000000000001,0,130.58000000000001,8592765074867,6,18592765074864,72,28592765074861,"8536201090",0.24]
[107486,"Ex9BL-H 1P+N B25 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=25A, IΔn=100mA, typ A","NAE",137.22999999999999,0,137.22999999999999,8592765074874,6,18592765074871,72,28592765074878,"8536201090",0.24]
[107487,"Ex9BL-H 1P+N B32 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=32A, IΔn=100mA, typ A","NAE",146.16,0,146.16,8592765074881,6,18592765074888,72,28592765074885,"8536201090",0.25]
[107488,"Ex9BL-H 1P+N B40 A 100mA","RCBO, Icn=10kA, 1+Npole, char. B, In=40A, IΔn=100mA, typ A","NAE",150.62,0,150.62,8592765074898,6,18592765074895,72,28592765074892,"8536201090",0.25]
[107491,"Ex9BL-H 1P+N C6  A 100mA ","RCBO, Icn=10kA, 1+Npole, char. C, In=6A, IΔn=100mA, typ A","NAE",133.37,0,133.37,8592765074928,6,18592765074925,72,28592765074922,"8536201090",0.24]
[107492,"Ex9BL-H 1P+N C10 A 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=10A, IΔn=100mA, typ A","NAE",133.79,0,133.79,8592765074935,6,18592765074932,72,28592765074939,"8536201090",0.24]
[107493,"Ex9BL-H 1P+N C13 A 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=13A, IΔn=100mA, typ A","NAE",133.79,0,133.79,8592765074942,6,18592765074949,72,28592765074946,"8536201090",0.24]
[107494,"Ex9BL-H 1P+N C16 A 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=16A, IΔn=100mA, typ A","NAE",110.85,0,110.85,8592765074959,6,18592765074956,72,28592765074953,"8536201090",0.24]
[107495,"Ex9BL-H 1P+N C20 A 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=20A, IΔn=100mA, typ A","NAE",130.58000000000001,0,130.58000000000001,8592765074966,6,18592765074963,72,28592765074960,"8536201090",0.24]
[107496,"Ex9BL-H 1P+N C25 A 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=25A, IΔn=100mA, typ A","NAE",137.22999999999999,0,137.22999999999999,8592765074973,6,18592765074970,72,28592765074977,"8536201090",0.24]
[107497,"Ex9BL-H 1P+N C32 A 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=32A, IΔn=100mA, typ A","NAE",146.16,0,146.16,8592765074980,6,18592765074987,72,28592765074984,"8536201090",0.25]
[107498,"Ex9BL-H 1P+N C40 A 100mA","RCBO, Icn=10kA, 1+Npole, char. C, In=40A, IΔn=100mA, typ A","NAE",150.62,0,150.62,8592765074997,6,18592765074994,72,28592765074991,"8536201090",0.25]
[107541,"Ex9BL-H 1P+N B6 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=6A, IΔn=300mA, typ AC","NAE",47.88,0,{"$f":"E1485*(1-F1485)","v":47.88},8592765075420,6,18592765075427,72,28592765075424,"8536201090",0.24]
[107542,"Ex9BL-H 1P+N B10 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=10A, IΔn=300mA, typ AC","NAE",51.66,{"$f":"NAE","v":0},51.66,8592765075437,6,18592765075434,72,28592765075431,"8536201090",0.24]
[107543,"Ex9BL-H 1P+N B13 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=13A, IΔn=300mA, typ AC","NAE",51.66,0,51.66,8592765075444,6,18592765075441,72,28592765075448,"8536201090",0.24]
[107544,"Ex9BL-H 1P+N B16 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=16A, IΔn=300mA, typ AC","NAE",43.13,0,43.13,8592765075451,6,18592765075458,72,28592765075455,"8536201090",0.24]
[107545,"Ex9BL-H 1P+N B20 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=20A, IΔn=300mA, typ AC","NAE",46.89,0,46.89,8592765075468,6,18592765075465,72,28592765075462,"8536201090",0.24]
[107546,"Ex9BL-H 1P+N B25 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=25A, IΔn=300mA, typ AC","NAE",50.8,0,50.8,8592765075475,6,18592765075472,72,28592765075479,"8536201090",0.24]
[107547,"Ex9BL-H 1P+N B32 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=32A, IΔn=300mA, typ AC","NAE",55.61,0,55.61,8592765075482,6,18592765075489,72,28592765075486,"8536201090",0.25]
[107548,"Ex9BL-H 1P+N B40 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=40A, IΔn=300mA, typ AC","NAE",58.76,0,58.76,8592765075499,6,18592765075496,72,28592765075493,"8536201090",0.25]
[107551,"Ex9BL-H 1P+N C6  300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=6A, IΔn=300mA, typ AC","NAE",47.88,0,47.88,8592765075529,6,18592765075526,72,28592765075523,"8536201090",0.24]
[107552,"Ex9BL-H 1P+N C10 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=10A, IΔn=300mA, typ AC","NAE",51.66,0,51.66,8592765075536,6,18592765075533,72,28592765075530,"8536201090",0.24]
[107553,"Ex9BL-H 1P+N C13 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=13A, IΔn=300mA, typ AC","NAE",51.66,0,51.66,8592765075543,6,18592765075540,72,28592765075547,"8536201090",0.24]
[107554,"Ex9BL-H 1P+N C16 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=16A, IΔn=300mA, typ AC","NAE",43.13,0,43.13,8592765075550,6,18592765075557,72,28592765075554,"8536201090",0.24]
[107555,"Ex9BL-H 1P+N C20 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=20A, IΔn=300mA, typ AC","NAE",46.89,0,46.89,8592765075567,6,18592765075564,72,28592765075561,"8536201090",0.24]
[107556,"Ex9BL-H 1P+N C25 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=25A, IΔn=300mA, typ AC","NAE",50.8,0,50.8,8592765075574,6,18592765075571,72,28592765075578,"8536201090",0.24]
[107557,"Ex9BL-H 1P+N C32 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=32A, IΔn=300mA, typ AC","NAE",55.61,0,55.61,8592765075581,6,18592765075588,72,28592765075585,"8536201090",0.25]
[107558,"Ex9BL-H 1P+N C40 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=40A, IΔn=300mA, typ AC","NAE",58.76,0,58.76,8592765075598,6,18592765075595,72,28592765075592,"8536201090",0.25]
[107561,"Ex9BL-H 1P+N B6 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=6A, IΔn=300mA, typ A","NAE",133.37,0,133.37,8592765075628,6,18592765075625,72,28592765075622,"8536201090",0.24]
[107562,"Ex9BL-H 1P+N B10 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=10A, IΔn=300mA, typ A","NAE",133.79,0,133.79,8592765075635,6,18592765075632,72,28592765075639,"8536201090",0.24]
[107563,"Ex9BL-H 1P+N B13 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=13A, IΔn=300mA, typ A","NAE",133.79,0,133.79,8592765075642,6,18592765075649,72,28592765075646,"8536201090",0.24]
[107564,"Ex9BL-H 1P+N B16 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=16A, IΔn=300mA, typ A","NAE",110.85,0,110.85,8592765075659,6,18592765075656,72,28592765075653,"8536201090",0.24]
[107565,"Ex9BL-H 1P+N B20 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=20A, IΔn=300mA, typ A","NAE",130.58000000000001,0,130.58000000000001,8592765075666,6,18592765075663,72,28592765075660,"8536201090",0.24]
[107566,"Ex9BL-H 1P+N B25 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=25A, IΔn=300mA, typ A","NAE",137.22999999999999,0,137.22999999999999,8592765075673,6,18592765075670,72,28592765075677,"8536201090",0.24]
[107567,"Ex9BL-H 1P+N B32 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=32A, IΔn=300mA, typ A","NAE",146.16,0,146.16,8592765075680,6,18592765075687,72,28592765075684,"8536201090",0.25]
[107568,"Ex9BL-H 1P+N B40 A 300mA","RCBO, Icn=10kA, 1+Npole, char. B, In=40A, IΔn=300mA, typ A","NAE",150.62,0,150.62,8592765075697,6,18592765075694,72,28592765075691,"8536201090",0.25]
[107571,"Ex9BL-H 1P+N C6  A 300mA ","RCBO, Icn=10kA, 1+Npole, char. C, In=6A, IΔn=300mA, typ A","NAE",133.37,0,133.37,8592765075727,6,18592765075724,72,28592765075721,"8536201090",0.24]
[107572,"Ex9BL-H 1P+N C10 A 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=10A, IΔn=300mA, typ A","NAE",133.79,0,133.79,8592765075734,6,18592765075731,72,28592765075738,"8536201090",0.24]
[107573,"Ex9BL-H 1P+N C13 A 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=13A, IΔn=300mA, typ A","NAE",133.79,0,133.79,8592765075741,6,18592765075748,72,28592765075745,"8536201090",0.24]
[107574,"Ex9BL-H 1P+N C16 A 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=16A, IΔn=300mA, typ A","NAE",110.85,0,110.85,8592765075758,6,18592765075755,72,28592765075752,"8536201090",0.24]
[107575,"Ex9BL-H 1P+N C20 A 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=20A, IΔn=300mA, typ A","NAE",130.58000000000001,0,130.58000000000001,8592765075765,6,18592765075762,72,28592765075769,"8536201090",0.24]
[107576,"Ex9BL-H 1P+N C25 A 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=25A, IΔn=300mA, typ A","NAE",137.22999999999999,0,137.22999999999999,8592765075772,6,18592765075779,72,28592765075776,"8536201090",0.24]
[107577,"Ex9BL-H 1P+N C32 A 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=32A, IΔn=300mA, typ A","NAE",146.16,0,146.16,8592765075789,6,18592765075786,72,28592765075783,"8536201090",0.25]
[107578,"Ex9BL-H 1P+N C40 A 300mA","RCBO, Icn=10kA, 1+Npole, char. C, In=40A, IΔn=300mA, typ A","NAE",150.62,0,150.62,8592765075796,6,18592765075793,72,28592765075790,"8536201090",0.25]
[]
["Residual Current Breakers with Overload protection Ex9BL-N, 6 kA"]
[107619,"Ex9BL-N 1P+N B6 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=30mA, typ AC","NAF",35.6,{"$f":"NAF","v":0},{"$f":"E1519*(1-F1519)","v":35.6},8592765076205,6,18592765076202,72,28592765076209,"8536201090",0.24]
[107620,"Ex9BL-N 1P+N B10 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=30mA, typ AC","NAF",32.94,{"$f":"NAF","v":0},32.94,8592765076212,6,18592765076219,72,28592765076216,"8536201090",0.24]
[107621,"Ex9BL-N 1P+N B13 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=13A, IΔn=30mA, typ AC","NAF",32.94,0,32.94,8592765076229,6,18592765076226,72,28592765076223,"8536201090",0.24]
[107622,"Ex9BL-N 1P+N B16 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=30mA, typ AC","NAF",32.94,0,32.94,8592765076236,6,18592765076233,72,28592765076230,"8536201090",0.24]
[107623,"Ex9BL-N 1P+N B20 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=30mA, typ AC","NAF",35.6,0,35.6,8592765076243,6,18592765076240,72,28592765076247,"8536201090",0.24]
[107624,"Ex9BL-N 1P+N B25 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=30mA, typ AC","NAF",38.450000000000003,0,38.450000000000003,8592765076250,6,18592765076257,72,28592765076254,"8536201090",0.24]
[107625,"Ex9BL-N 1P+N B32 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=30mA, typ AC","NAF",41.35,0,41.35,8592765076267,6,18592765076264,72,28592765076261,"8536201090",0.25]
[107626,"Ex9BL-N 1P+N B40 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=30mA, typ AC","NAF",43.69,0,43.69,8592765076274,6,18592765076271,72,28592765076278,"8536201090",0.25]
[107627,"Ex9BL-N 1P+N C6 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=30mA, typ AC","NAF",35.6,0,35.6,8592765076281,6,18592765076288,72,28592765076285,"8536201090",0.24]
[107628,"Ex9BL-N 1P+N C10 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=30mA, typ AC","NAF",32.94,0,32.94,8592765076298,6,18592765076295,72,28592765076292,"8536201090",0.24]
[107629,"Ex9BL-N 1P+N C13 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=13A, IΔn=30mA, typ AC","NAF",32.94,0,32.94,8592765076304,6,18592765076301,72,28592765076308,"8536201090",0.24]
[107630,"Ex9BL-N 1P+N C16 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=30mA, typ AC","NAF",32.94,0,32.94,8592765076311,6,18592765076318,72,28592765076315,"8536201090",0.24]
[107631,"Ex9BL-N 1P+N C20 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=30mA, typ AC","NAF",34.409999999999997,0,34.409999999999997,8592765076328,6,18592765076325,72,28592765076322,"8536201090",0.24]
[107632,"Ex9BL-N 1P+N C25 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=30mA, typ AC","NAF",34.409999999999997,0,34.409999999999997,8592765076335,6,18592765076332,72,28592765076339,"8536201090",0.24]
[107633,"Ex9BL-N 1P+N C32 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=30mA, typ AC","NAF",34.4,0,34.4,8592765076342,6,18592765076349,72,28592765076346,"8536201090",0.25]
[107634,"Ex9BL-N 1P+N C40 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=30mA, typ AC","NAF",38.78,0,38.78,8592765076359,6,18592765076356,72,28592765076353,"8536201090",0.25]
[107635,"Ex9BL-N 1P+N B6 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=30mA, typ A","NAF",52,0,52,8592765076366,6,18592765076363,72,28592765076360,"8536201090",0.24]
[107636,"Ex9BL-N 1P+N B10 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=30mA, typ A","NAF",44.77,0,44.77,8592765076373,6,18592765076370,72,28592765076377,"8536201090",0.24]
[107637,"Ex9BL-N 1P+N B13 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=13A, IΔn=30mA, typ A","NAF",44.77,0,44.77,8592765076380,6,18592765076387,72,28592765076384,"8536201090",0.24]
[107638,"Ex9BL-N 1P+N B16 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=30mA, typ A","NAF",44.77,0,44.77,8592765076397,6,18592765076394,72,28592765076391,"8536201090",0.24]
[107639,"Ex9BL-N 1P+N B20 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=30mA, typ A","NAF",52,0,52,8592765076403,6,18592765076400,72,28592765076407,"8536201090",0.24]
[107640,"Ex9BL-N 1P+N B25 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=30mA, typ A","NAF",54.54,0,54.54,8592765076410,6,18592765076417,72,28592765076414,"8536201090",0.24]
[107641,"Ex9BL-N 1P+N B32 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=30mA, typ A","NAF",57.05,0,57.05,8592765076427,6,18592765076424,72,28592765076421,"8536201090",0.25]
[107642,"Ex9BL-N 1P+N B40 A 30mA","RCBO, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=30mA, typ A","NAF",58.78,0,58.78,8592765076434,6,18592765076431,72,28592765076438,"8536201090",0.25]
[107643,"Ex9BL-N 1P+N C6 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=30mA, typ A","NAF",52,0,52,8592765076441,6,18592765076448,72,28592765076445,"8536201090",0.24]
[107644,"Ex9BL-N 1P+N C10 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=30mA, typ A","NAF",44.77,0,44.77,8592765076458,6,18592765076455,72,28592765076452,"8536201090",0.24]
[107645,"Ex9BL-N 1P+N C13 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=13A, IΔn=30mA, typ A","NAF",44.77,0,44.77,8592765076465,6,18592765076462,72,28592765076469,"8536201090",0.24]
[107646,"Ex9BL-N 1P+N C16 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=30mA, typ A","NAF",44.77,0,44.77,8592765076472,6,18592765076479,72,28592765076476,"8536201090",0.24]
[107647,"Ex9BL-N 1P+N C20 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=30mA, typ A","NAF",52,0,52,8592765076489,6,18592765076486,72,28592765076483,"8536201090",0.24]
[107648,"Ex9BL-N 1P+N C25 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=30mA, typ A","NAF",54.54,0,54.54,8592765076496,6,18592765076493,72,28592765076490,"8536201090",0.24]
[107649,"Ex9BL-N 1P+N C32 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=30mA, typ A","NAF",57.05,0,57.05,8592765076502,6,18592765076509,72,28592765076506,"8536201090",0.25]
[107650,"Ex9BL-N 1P+N C40 A 30mA","RCBO, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=30mA, typ A","NAF",58.78,0,58.78,8592765076519,6,18592765076516,72,28592765076513,"8536201090",0.25]
[107651,"Ex9BL-N 1P+N B6 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=100mA, typ AC","NAF",36.65,0,36.65,8592765076526,6,18592765076523,72,28592765076520,"8536201090",0.24]
[107652,"Ex9BL-N 1P+N B10 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=100mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076533,6,18592765076530,72,28592765076537,"8536201090",0.24]
[107653,"Ex9BL-N 1P+N B13 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=13A, IΔn=100mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076540,6,18592765076547,72,28592765076544,"8536201090",0.24]
[107654,"Ex9BL-N 1P+N B16 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=100mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076557,6,18592765076554,72,28592765076551,"8536201090",0.24]
[107655,"Ex9BL-N 1P+N B20 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=100mA, typ AC","NAF",36.65,0,36.65,8592765076564,6,18592765076561,72,28592765076568,"8536201090",0.24]
[107656,"Ex9BL-N 1P+N B25 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=100mA, typ AC","NAF",39.57,0,39.57,8592765076571,6,18592765076578,72,28592765076575,"8536201090",0.24]
[107657,"Ex9BL-N 1P+N B32 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=100mA, typ AC","NAF",42.57,0,42.57,8592765076588,6,18592765076585,72,28592765076582,"8536201090",0.25]
[107658,"Ex9BL-N 1P+N B40 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=100mA, typ AC","NAF",44.98,0,44.98,8592765076595,6,18592765076592,72,28592765076599,"8536201090",0.25]
[107659,"Ex9BL-N 1P+N C6  100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=100mA, typ AC","NAF",36.65,0,36.65,8592765076601,6,18592765076608,72,28592765076605,"8536201090",0.24]
[107660,"Ex9BL-N 1P+N C10 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=100mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076618,6,18592765076615,72,28592765076612,"8536201090",0.24]
[107661,"Ex9BL-N 1P+N C13 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=13A, IΔn=100mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076625,6,18592765076622,72,28592765076629,"8536201090",0.24]
[107662,"Ex9BL-N 1P+N C16 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=100mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076632,6,18592765076639,72,28592765076636,"8536201090",0.24]
[107663,"Ex9BL-N 1P+N C20 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=100mA, typ AC","NAF",36.65,0,36.65,8592765076649,6,18592765076646,72,28592765076643,"8536201090",0.24]
[107664,"Ex9BL-N 1P+N C25 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=100mA, typ AC","NAF",39.57,0,39.57,8592765076656,6,18592765076653,72,28592765076650,"8536201090",0.24]
[107665,"Ex9BL-N 1P+N C32 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=100mA, typ AC","NAF",42.57,0,42.57,8592765076663,6,18592765076660,72,28592765076667,"8536201090",0.25]
[107666,"Ex9BL-N 1P+N C40  100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=100mA, typ AC","NAF",44.98,0,44.98,8592765076670,6,18592765076677,72,28592765076674,"8536201090",0.25]
[107667,"Ex9BL-N 1P+N B6 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=100mA, typ A","NAF",53.55,0,53.55,8592765076687,6,18592765076684,72,28592765076681,"8536201090",0.24]
[107668,"Ex9BL-N 1P+N B10 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=100mA, typ A","NAF",46.1,0,46.1,8592765076694,6,18592765076691,72,28592765076698,"8536201090",0.24]
[107669,"Ex9BL-N 1P+N B13 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=13A, IΔn=100mA, typ A","NAF",46.1,0,46.1,8592765076700,6,18592765076707,72,28592765076704,"8536201090",0.24]
[107670,"Ex9BL-N 1P+N B16 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=100mA, typ A","NAF",46.1,0,46.1,8592765076717,6,18592765076714,72,28592765076711,"8536201090",0.24]
[107671,"Ex9BL-N 1P+N B20 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=100mA, typ A","NAF",53.55,0,53.55,8592765076724,6,18592765076721,72,28592765076728,"8536201090",0.24]
[107672,"Ex9BL-N 1P+N B25 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=100mA, typ A","NAF",56.14,0,56.14,8592765076731,6,18592765076738,72,28592765076735,"8536201090",0.24]
[107673,"Ex9BL-N 1P+N B32 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=100mA, typ A","NAF",58.73,0,58.73,8592765076748,6,18592765076745,72,28592765076742,"8536201090",0.25]
[107674,"Ex9BL-N 1P+N B40 A 100mA","RCBO, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=100mA, typ A","NAF",60.5,0,60.5,8592765076755,6,18592765076752,72,28592765076759,"8536201090",0.25]
[107675,"Ex9BL-N 1P+N C6  A 100mA ","RCBO, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=100mA, typ A","NAF",53.55,0,53.55,8592765076762,6,18592765076769,72,28592765076766,"8536201090",0.24]
[107676,"Ex9BL-N 1P+N C10 A 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=100mA, typ A","NAF",46.1,0,46.1,8592765076779,6,18592765076776,72,28592765076773,"8536201090",0.24]
[107677,"Ex9BL-N 1P+N C13 A 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=13A, IΔn=100mA, typ A","NAF",46.1,0,46.1,8592765076786,6,18592765076783,72,28592765076780,"8536201090",0.24]
[107678,"Ex9BL-N 1P+N C16 A 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=100mA, typ A","NAF",46.1,0,46.1,8592765076793,6,18592765076790,72,28592765076797,"8536201090",0.24]
[107679,"Ex9BL-N 1P+N C20 A 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=100mA, typ A","NAF",53.55,0,53.55,8592765076809,6,18592765076806,72,28592765076803,"8536201090",0.24]
[107680,"Ex9BL-N 1P+N C25 A 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=100mA, typ A","NAF",56.14,0,56.14,8592765076816,6,18592765076813,72,28592765076810,"8536201090",0.24]
[107681,"Ex9BL-N 1P+N C32 A 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=100mA, typ A","NAF",58.73,0,58.73,8592765076823,6,18592765076820,72,28592765076827,"8536201090",0.25]
[107682,"Ex9BL-N 1P+N C40 A 100mA","RCBO, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=100mA, typ A","NAF",60.5,0,60.5,8592765076830,6,18592765076837,72,28592765076834,"8536201090",0.25]
[107683,"Ex9BL-N 1P+N B6 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=300mA, typ AC","NAF",36.65,0,{"$f":"E1583*(1-F1583)","v":36.65},8592765076847,6,18592765076844,72,28592765076841,"8536201090",0.24]
[107684,"Ex9BL-N 1P+N B10 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=300mA, typ AC","NAF",33.909999999999997,{"$f":"NAF","v":0},33.909999999999997,8592765076854,6,18592765076851,72,28592765076858,"8536201090",0.24]
[107685,"Ex9BL-N 1P+N B13 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=13A, IΔn=300mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076861,6,18592765076868,72,28592765076865,"8536201090",0.24]
[107686,"Ex9BL-N 1P+N B16 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=300mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076878,6,18592765076875,72,28592765076872,"8536201090",0.24]
[107687,"Ex9BL-N 1P+N B20 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=300mA, typ AC","NAF",36.65,0,36.65,8592765076885,6,18592765076882,72,28592765076889,"8536201090",0.24]
[107688,"Ex9BL-N 1P+N B25 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=300mA, typ AC","NAF",39.57,0,39.57,8592765076892,6,18592765076899,72,28592765076896,"8536201090",0.24]
[107689,"Ex9BL-N 1P+N B32 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=300mA, typ AC","NAF",42.57,0,42.57,8592765076908,6,18592765076905,72,28592765076902,"8536201090",0.25]
[107690,"Ex9BL-N 1P+N B40 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=300mA, typ AC","NAF",44.98,0,44.98,8592765076915,6,18592765076912,72,28592765076919,"8536201090",0.25]
[107691,"Ex9BL-N 1P+N C6  300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=300mA, typ AC","NAF",36.65,0,36.65,8592765076922,6,18592765076929,72,28592765076926,"8536201090",0.24]
[107692,"Ex9BL-N 1P+N C10 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=300mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076939,6,18592765076936,72,28592765076933,"8536201090",0.24]
[107693,"Ex9BL-N 1P+N C13 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=13A, IΔn=300mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076946,6,18592765076943,72,28592765076940,"8536201090",0.24]
[107694,"Ex9BL-N 1P+N C16 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=300mA, typ AC","NAF",33.909999999999997,0,33.909999999999997,8592765076953,6,18592765076950,72,28592765076957,"8536201090",0.24]
[107695,"Ex9BL-N 1P+N C20 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=300mA, typ AC","NAF",36.65,0,36.65,8592765076960,6,18592765076967,72,28592765076964,"8536201090",0.24]
[107696,"Ex9BL-N 1P+N C25 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=300mA, typ AC","NAF",39.57,0,39.57,8592765076977,6,18592765076974,72,28592765076971,"8536201090",0.24]
[107697,"Ex9BL-N 1P+N C32 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=300mA, typ AC","NAF",42.57,0,42.57,8592765076984,6,18592765076981,72,28592765076988,"8536201090",0.25]
[107698,"Ex9BL-N 1P+N C40 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=300mA, typ AC","NAF",44.98,0,44.98,8592765076991,6,18592765076998,72,28592765076995,"8536201090",0.25]
[107699,"Ex9BL-N 1P+N B6 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=300mA, typ A","NAF",53.55,0,53.55,8592765077004,6,18592765077001,72,28592765077008,"8536201090",0.24]
[107700,"Ex9BL-N 1P+N B10 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=300mA, typ A","NAF",46.1,0,46.1,8592765077011,6,18592765077018,72,28592765077015,"8536201090",0.24]
[107701,"Ex9BL-N 1P+N B13 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=13A, IΔn=300mA, typ A","NAF",46.1,0,46.1,8592765077028,6,18592765077025,72,28592765077022,"8536201090",0.24]
[107702,"Ex9BL-N 1P+N B16 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=300mA, typ A","NAF",46.1,0,46.1,8592765077035,6,18592765077032,72,28592765077039,"8536201090",0.24]
[107703,"Ex9BL-N 1P+N B20 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=300mA, typ A","NAF",53.55,0,53.55,8592765077042,6,18592765077049,72,28592765077046,"8536201090",0.24]
[107704,"Ex9BL-N 1P+N B25 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=300mA, typ A","NAF",56.14,0,56.14,8592765077059,6,18592765077056,72,28592765077053,"8536201090",0.24]
[107705,"Ex9BL-N 1P+N B32 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=300mA, typ A","NAF",58.73,0,58.73,8592765077066,6,18592765077063,72,28592765077060,"8536201090",0.25]
[107706,"Ex9BL-N 1P+N B40 A 300mA","RCBO, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=300mA, typ A","NAF",60.5,0,60.5,8592765077073,6,18592765077070,72,28592765077077,"8536201090",0.25]
[107707,"Ex9BL-N 1P+N C6 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=300mA, typ A","NAF",53.55,0,53.55,8592765077080,6,18592765077087,72,28592765077084,"8536201090",0.24]
[107708,"Ex9BL-N 1P+N C10 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=300mA, typ A","NAF",46.1,0,46.1,8592765077097,6,18592765077094,72,28592765077091,"8536201090",0.24]
[107709,"Ex9BL-N 1P+N C13 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=13A, IΔn=300mA, typ A","NAF",46.1,0,46.1,8592765077103,6,18592765077100,72,28592765077107,"8536201090",0.24]
[107710,"Ex9BL-N 1P+N C16 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=300mA, typ A","NAF",46.1,0,46.1,8592765077110,6,18592765077117,72,28592765077114,"8536201090",0.24]
[107711,"Ex9BL-N 1P+N C20 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=300mA, typ A","NAF",53.55,0,53.55,8592765077127,6,18592765077124,72,28592765077121,"8536201090",0.24]
[107712,"Ex9BL-N 1P+N C25 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=300mA, typ A","NAF",56.14,0,56.14,8592765077134,6,18592765077131,72,28592765077138,"8536201090",0.24]
[107713,"Ex9BL-N 1P+N C32 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=300mA, typ A","NAF",58.73,0,58.73,8592765077141,6,18592765077148,72,28592765077145,"8536201090",0.25]
[107714,"Ex9BL-N 1P+N C40 A 300mA","RCBO, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=300mA, typ A","NAF",60.5,0,60.5,8592765077158,6,18592765077155,72,28592765077152,"8536201090",0.25]
[]
["One-module Residual Current circuit Breakers with Overload protection Ex9NLE, 6kA"]
[111146,"Ex9NLE EL 1PN B6 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},{"$f":"E1617*(1-F1617)","v":24.57},8592765111463,12,18592765111460,144,28592765111467,8536200000,0.121]
[111147,"Ex9NLE EL 1PN B10 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111470,12,18592765111477,144,28592765111474,8536200000,0.121]
[111148,"Ex9NLE EL 1PN B16 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111487,12,18592765111484,144,28592765111481,8536200000,0.121]
[111149,"Ex9NLE EL 1PN B20 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111494,12,18592765111491,144,28592765111498,8536200000,0.121]
[111150,"Ex9NLE EL 1PN B25 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111500,12,18592765111507,144,28592765111504,8536200000,0.121]
[111151,"Ex9NLE EL 1PN B32 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111517,12,18592765111514,144,28592765111511,8536200000,0.121]
[111152,"Ex9NLE EL 1PN B40 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111524,12,18592765111521,144,28592765111528,8536200000,0.121]
[111153,"Ex9NLE EL 1PN C6 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111531,12,18592765111538,144,28592765111535,8536200000,0.121]
[111154,"Ex9NLE EL 1PN C10 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111548,12,18592765111545,144,28592765111542,8536200000,0.121]
[111155,"Ex9NLE EL 1PN C16 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111555,12,18592765111552,144,28592765111559,8536200000,0.121]
[111156,"Ex9NLE EL 1PN C20 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111562,12,18592765111569,144,28592765111566,8536200000,0.121]
[111157,"Ex9NLE EL 1PN C25 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111579,12,18592765111576,144,28592765111573,8536200000,0.121]
[111158,"Ex9NLE EL 1PN C32 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111586,12,18592765111583,144,28592765111580,8536200000,0.121]
[111159,"Ex9NLE EL 1PN C40 30mA","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=30mA, typ AC","NAAA",24.57,{"$f":"NAAA","v":0},24.57,8592765111593,12,18592765111590,144,28592765111597,8536200000,0.121]
[111160,"Ex9NLE EL 1PN B6 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=6A, IΔn=30mA, typ A","NAAA",24,{"$f":"NAAA","v":0},24,8592765111609,12,18592765111606,144,28592765111603,8536200000,0.121]
[111161,"Ex9NLE EL 1PN B10 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=10A, IΔn=30mA, typ A","NAAA",22.86,{"$f":"NAAA","v":0},22.86,8592765111616,12,18592765111613,144,28592765111610,8536200000,0.121]
[111162,"Ex9NLE EL 1PN B16 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=16A, IΔn=30mA, typ A","NAAA",22.29,{"$f":"NAAA","v":0},22.29,8592765111623,12,18592765111620,144,28592765111627,8536200000,0.121]
[111163,"Ex9NLE EL 1PN B20 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=20A, IΔn=30mA, typ A","NAAA",22.29,{"$f":"NAAA","v":0},22.29,8592765111630,12,18592765111637,144,28592765111634,8536200000,0.121]
[111164,"Ex9NLE EL 1PN B25 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=25A, IΔn=30mA, typ A","NAAA",22.29,{"$f":"NAAA","v":0},22.29,8592765111647,12,18592765111644,144,28592765111641,8536200000,0.121]
[111165,"Ex9NLE EL 1PN B32 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=32A, IΔn=30mA, typ A","NAAA",23.43,{"$f":"NAAA","v":0},23.43,8592765111654,12,18592765111651,144,28592765111658,8536200000,0.121]
[111166,"Ex9NLE EL 1PN B40 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. B, In=40A, IΔn=30mA, typ A","NAAA",23.71,{"$f":"NAAA","v":0},23.71,8592765111661,12,18592765111668,144,28592765111665,8536200000,0.121]
[111167,"Ex9NLE EL 1PN C6 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=6A, IΔn=30mA, typ A","NAAA",24,{"$f":"NAAA","v":0},24,8592765111678,12,18592765111675,144,28592765111672,8536200000,0.121]
[111168,"Ex9NLE EL 1PN C10 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=10A, IΔn=30mA, typ A","NAAA",22.86,{"$f":"NAAA","v":0},22.86,8592765111685,12,18592765111682,144,28592765111689,8536200000,0.121]
[111169,"Ex9NLE EL 1PN C16 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=16A, IΔn=30mA, typ A","NAAA",22.29,{"$f":"NAAA","v":0},22.29,8592765111692,12,18592765111699,144,28592765111696,8536200000,0.121]
[111170,"Ex9NLE EL 1PN C20 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=20A, IΔn=30mA, typ A","NAAA",22.29,{"$f":"NAAA","v":0},22.29,8592765111708,12,18592765111705,144,28592765111702,8536200000,0.121]
[111171,"Ex9NLE EL 1PN C25 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=25A, IΔn=30mA, typ A","NAAA",22.29,{"$f":"NAAA","v":0},22.29,8592765111715,12,18592765111712,144,28592765111719,8536200000,0.121]
[111172,"Ex9NLE EL 1PN C32 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=32A, IΔn=30mA, typ A","NAAA",23.43,{"$f":"NAAA","v":0},23.43,8592765111722,12,18592765111729,144,28592765111726,8536200000,0.121]
[111173,"Ex9NLE EL 1PN C40 30mA A","Electronic RCBO, 1 module, Icn=6kA, 1+Npole, char. C, In=40A, IΔn=30mA, typ A","NAAA",23.71,{"$f":"NAAA","v":0},23.71,8592765111739,12,18592765111736,144,28592765111733,8536200000,0.121]
[]
["RCD add-on blocks Ex9LE"]
[100557,"Ex9LE 10mA 1PN 40A","RCD add-on block for Ex9B, 1+Npole, In=40A, IΔn=10mA","NAG",77.34,{"$f":"NAG","v":0},{"$f":"E1647*(1-F1647)","v":77.34},8592765005588,1,8592765005588,54,28592765005582,"8536201090",0.14000000000000001]
[100558,"Ex9LE 10mA 2P 40A","RCD add-on block for Ex9B, 2-pole, In=40A, IΔn=10mA","NAG",77.67,0,77.67,8592765005595,1,8592765005595,45,28592765005599,"8536201090",0.14000000000000001]
[100559,"Ex9LE 10mA 3P 40A","RCD add-on block for Ex9B, 3-pole, In=40A, IΔn=10mA","NAG",68.39,0,68.39,8592765005601,1,8592765005601,27,28592765005605,"8536201090",0.2]
[100560,"Ex9LE 10mA 3PN 40A","RCD add-on block for Ex9B, 3+Npole, In=40A, IΔn=10mA","NAG",59.6,0,59.6,8592765005618,1,8592765005618,27,28592765005612,"8536201090",0.2]
[100561,"Ex9LE 10mA 4P 40A","RCD add-on block for Ex9B, 4-pole, In=40A, IΔn=10mA","NAG",59.92,0,59.92,8592765005625,1,8592765005625,24,28592765005629,"8536201090",0.2]
[100562,"Ex9LE 10mA 1PN 63A","RCD add-on block for Ex9B, 1+Npole, In=63A, IΔn=10mA","NAG",81.14,0,81.14,8592765005632,1,8592765005632,54,28592765005636,"8536201090",0.14000000000000001]
[100563,"Ex9LE 10mA 2P 63A","RCD add-on block for Ex9B, 2-pole, In=63A, IΔn=10mA","NAG",81.56,0,81.56,8592765005649,1,8592765005649,45,28592765005643,"8536201090",0.14000000000000001]
[100564,"Ex9LE 10mA 3P 63A","RCD add-on block for Ex9B, 3-pole, In=63A, IΔn=10mA","NAG",71.75,0,71.75,8592765005656,1,8592765005656,27,28592765005650,"8536201090",0.2]
[100565,"Ex9LE 10mA 3PN 63A","RCD add-on block for Ex9B, 3+Npole, In=63A, IΔn=10mA","NAG",62.54,0,62.54,8592765005663,1,8592765005663,27,28592765005667,"8536201090",0.2]
[100566,"Ex9LE 10mA 4P 63A","RCD add-on block for Ex9B, 4-pole, In=63A, IΔn=10mA","NAG",62.88,0,62.88,8592765005670,1,8592765005670,24,28592765005674,"8536201090",0.2]
[100567,"Ex9LE 30mA 1PN 40A","RCD add-on block for Ex9B, 1+Npole, In=40A, IΔn=30mA","NAG",70.069999999999993,0,70.069999999999993,8592765005687,1,8592765005687,54,28592765005681,"8536201090",0.14000000000000001]
[100568,"Ex9LE 30mA 2P 40A","RCD add-on block for Ex9B, 2-pole, In=40A, IΔn=30mA","NAG",70.83,0,70.83,8592765005694,1,8592765005694,45,28592765005698,"8536201090",0.14000000000000001]
[100569,"Ex9LE 30mA 3P 40A","RCD add-on block for Ex9B, 3-pole, In=40A, IΔn=30mA","NAG",61.11,0,61.11,8592765005700,1,8592765005700,27,28592765005704,"8536201090",0.2]
[100570,"Ex9LE 30mA 3PN 40A","RCD add-on block for Ex9B, 3+Npole, In=40A, IΔn=30mA","NAG",52.14,0,52.14,8592765005717,1,8592765005717,27,28592765005711,"8536201090",0.2]
[100571,"Ex9LE 30mA 4P 40A","RCD add-on block for Ex9B, 4-pole, In=40A, IΔn=30mA","NAG",53.17,0,53.17,8592765005724,1,8592765005724,24,28592765005728,"8536201090",0.2]
[100572,"Ex9LE 30mA 1PN 63A","RCD add-on block for Ex9B, 1+Npole, In=63A, IΔn=30mA","NAG",73.53,0,73.53,8592765005731,1,8592765005731,54,28592765005735,"8536201090",0.14000000000000001]
[100573,"Ex9LE 30mA 2P 63A","RCD add-on block for Ex9B, 2-pole, In=63A, IΔn=30mA","NAG",74.290000000000006,0,74.290000000000006,8592765005748,1,8592765005748,45,28592765005742,"8536201090",0.14000000000000001]
[100574,"Ex9LE 30mA 3P 63A","RCD add-on block for Ex9B, 3-pole, In=63A, IΔn=30mA","NAG",64.150000000000006,0,64.150000000000006,8592765005755,1,8592765005755,27,28592765005759,"8536201090",0.2]
[100575,"Ex9LE 30mA 3PN 63A","RCD add-on block for Ex9B, 3+Npole, In=63A, IΔn=30mA","NAG",54.68,0,54.68,8592765005762,1,8592765005762,27,28592765005766,"8536201090",0.2]
[100576,"Ex9LE 30mA 4P 63A","RCD add-on block for Ex9B, 4-pole, In=63A, IΔn=30mA","NAG",56.71,0,56.71,8592765005779,1,8592765005779,24,28592765005773,"8536201090",0.2]
[100577,"Ex9LE 100mA 1PN 40A","RCD add-on block for Ex9B, 1+Npole, In=40A, IΔn=100mA","NAG",65.489999999999995,0,65.489999999999995,8592765005786,1,8592765005786,54,28592765005780,"8536201090",0.14000000000000001]
[100578,"Ex9LE 100mA 2P 40A","RCD add-on block for Ex9B, 2-pole, In=40A, IΔn=100mA","NAG",67.02,0,67.02,8592765005793,1,8592765005793,45,28592765005797,"8536201090",0.14000000000000001]
[100579,"Ex9LE 100mA 3P 40A","RCD add-on block for Ex9B, 3-pole, In=40A, IΔn=100mA","NAG",56.56,0,56.56,8592765005809,1,8592765005809,27,28592765005803,"8536201090",0.2]
[100580,"Ex9LE 100mA 3PN 40A","RCD add-on block for Ex9B, 3+Npole, In=40A, IΔn=100mA","NAG",47.49,0,47.49,8592765005816,1,8592765005816,27,28592765005810,"8536201090",0.2]
[100581,"Ex9LE 100mA 4P 40A","RCD add-on block for Ex9B, 4-pole, In=40A, IΔn=100mA","NAG",48.68,0,48.68,8592765005823,1,8592765005823,24,28592765005827,"8536201090",0.2]
[100582,"Ex9LE 100mA 1PN 63A","RCD add-on block for Ex9B, 1+Npole, In=63A, IΔn=100mA","NAG",68.7,0,68.7,8592765005830,1,8592765005830,54,28592765005834,"8536201090",0.14000000000000001]
[100583,"Ex9LE 100mA 2P 63A","RCD add-on block for Ex9B, 2-pole, In=63A, IΔn=100mA","NAG",70.319999999999993,0,70.319999999999993,8592765005847,1,8592765005847,45,28592765005841,"8536201090",0.14000000000000001]
[100584,"Ex9LE 100mA 3P 63A","RCD add-on block for Ex9B, 3-pole, In=63A, IΔn=100mA","NAG",59.34,0,59.34,8592765005854,1,8592765005854,27,28592765005858,"8536201090",0.2]
[100585,"Ex9LE 100mA 3PN 63A","RCD add-on block for Ex9B, 3+Npole, In=63A, IΔn=100mA","NAG",49.88,0,49.88,8592765005861,1,8592765005861,27,28592765005865,"8536201090",0.2]
[100586,"Ex9LE 100mA 4P 63A","RCD add-on block for Ex9B, 4-pole, In=63A, IΔn=100mA","NAG",51.05,0,51.05,8592765005878,1,8592765005878,24,28592765005872,"8536201090",0.2]
[100587,"Ex9LE 300mA 1PN 40A","RCD add-on block for Ex9B, 1+Npole, In=40A, IΔn=300mA","NAG",61.02,0,61.02,8592765005885,1,8592765005885,54,28592765005889,"8536201090",0.14000000000000001]
[100588,"Ex9LE 300mA 2P 40A","RCD add-on block for Ex9B, 2-pole, In=40A, IΔn=300mA","NAG",61.94,0,61.94,8592765005892,1,8592765005892,45,28592765005896,"8536201090",0.14000000000000001]
[100589,"Ex9LE 300mA 3P 40A","RCD add-on block for Ex9B, 3-pole, In=40A, IΔn=300mA","NAG",51.98,0,51.98,8592765005908,1,8592765005908,27,28592765005902,"8536201090",0.2]
[100590,"Ex9LE 300mA 3PN 40A","RCD add-on block for Ex9B, 3+Npole, In=40A, IΔn=300mA","NAG",42.94,0,42.94,8592765005915,1,8592765005915,27,28592765005919,"8536201090",0.2]
[100591,"Ex9LE 300mA 4P 40A","RCD add-on block for Ex9B, 4-pole, In=40A, IΔn=300mA","NAG",43.87,0,43.87,8592765005922,1,8592765005922,24,28592765005926,"8536201090",0.2]
[100592,"Ex9LE 300mA 1PN 63A","RCD add-on block for Ex9B, 1+Npole, In=63A, IΔn=300mA","NAG",64.069999999999993,0,64.069999999999993,8592765005939,1,8592765005939,54,28592765005933,"8536201090",0.14000000000000001]
[100593,"Ex9LE 300mA 2P 63A","RCD add-on block for Ex9B, 2-pole, In=63A, IΔn=300mA","NAG",64.98,0,64.98,8592765005946,1,8592765005946,45,28592765005940,"8536201090",0.14000000000000001]
[100594,"Ex9LE 300mA 3P 63A","RCD add-on block for Ex9B, 3-pole, In=63A, IΔn=300mA","NAG",54.52,0,54.52,8592765005953,1,8592765005953,27,28592765005957,"8536201090",0.2]
[100595,"Ex9LE 300mA 3PN 63A","RCD add-on block for Ex9B, 3+Npole, In=63A, IΔn=300mA","NAG",45.04,0,45.04,8592765005960,1,8592765005960,27,28592765005964,"8536201090",0.2]
[100596,"Ex9LE 300mA 4P 63A","RCD add-on block for Ex9B, 4-pole, In=63A, IΔn=300mA","NAG",46.06,0,46.06,8592765005977,1,8592765005977,24,28592765005971,"8536201090",0.2]
[]
["Energy meter Ex9EM",null,null,null,null,null,null,"","","","","",null,""]
[107281,"Ex9EM 1P 1M 80A MO MT","Energy Meter 1-pole, 1-module, 80 A, ModBus-communication, Multi-tariff, LCD display","NAZ",68.739999999999995,{"$f":"NAZ","v":0},{"$f":"E1689*(1-F1689)","v":68.739999999999995},8592765072818,10,18592765072815,120,28592765072812,"9028301100",0.11799999999999999]
[107282,"Ex9EM 1P 1M 45A 1T","Energy Meter 1-pole, 1-module, 45 A, 1-tariff, LCD display","NAZ",48.18,{"$f":"NAZ","v":0},{"$f":"E1690*(1-F1690)","v":48.18},8592765072825,10,18592765072822,120,28592765072829,"9028301100",7.0000000000000007E-2]
[107283,"Ex9EM 1P 1M 45A 1T MCH","Energy Meter 1-pole, 1-module, 45 A, 1-tariff, Mechanical display","NAZ",48.18,0,48.18,8592765072832,10,18592765072839,120,28592765072836,"9028301100",8.7999999999999995E-2]
[107284,"Ex9EM 3P 4M CT 1T","Energy Meter 3-pole, 4-module, current transformer, 1-tariff, LCD display","NAZ",152.82,0,152.82,8592765072849,1,18592765072846,45,28592765072843,"9028301900",0.27800000000000002]
[107285,"Ex9EM 3P 4M 80A 1T","Energy Meter 3-pole, 4-module, 80 A, 1-tariff, LCD display","NAZ",132.72999999999999,0,132.72999999999999,8592765072856,1,18592765072853,45,28592765072850,"9028301900",0.36599999999999999]
[107286,"Ex9EM 1P 1M 32A 1T","Energy Meter 1-pole, 1-module, 32 A, 1-tariff, LCD display","NAZ",41.47,0,41.47,8592765072863,10,18592765072860,120,28592765072867,"9028301100",7.0000000000000007E-2]
[107287,"Ex9EMS 1P 1M 45A 1T","Smart energy meter 1-pole, 1-module, 45 A, 1-tariff, LCD display","NAZ",88.5,0,88.5,8592765072870,1,18592765072877,60,28592765072874,"9028301100",0.08]
[107288,"Ex9EMS 1P 1M 45A 2T","Smart energy meter 1-pole, 1-module, 45 A, 2-tariff, LCD display","NAZ",91.38,0,91.38,8592765072887,1,18592765072884,60,28592765072881,"9028301100",0.08]
[107289,"Ex9EMS 1P 1M 45A MB 2T","Smart energy meter 1-pole, 1-module, 45 A, Mbus-communication, 2-tariff, LCD display","NAZ",112.17,0,112.17,8592765072894,1,18592765072891,60,28592765072898,"9028301100",0.08]
[107290,"Ex9EMS 1P 1M 45A MO 2T","Smart energy meter 1-pole, 1-module, 45 A, ModBus-communication, 2-tariff, LCD display","NAZ",100.69,0,100.69,8592765072900,1,18592765072907,60,28592765072904,"9028301100",0.08]
[107291,"Ex9EMS 1P 2M 100A 1T","Smart energy meter 1-pole, 2-module, 100 A, 1-tariff, LCD display","NAZ",98.15,0,98.15,8592765072917,1,18592765072914,48,28592765072911,"9028301100",0.16]
[107292,"Ex9EMS 1P 2M 100A 2T","Smart energy meter 1-pole, 2-module, 100 A, 2-tariff, LCD display","NAZ",98.27,0,98.27,8592765072924,1,18592765072921,48,28592765072928,"9028301100",0.16]
[107293,"Ex9EMS 1P 2M 100A MB 2T","Smart energy meter 1-pole, 2-module, 100 A, Mbus-communication, 2-tariff, LCD display","NAZ",101.89,0,101.89,8592765072931,1,18592765072938,48,28592765072935,"9028301100",0.16]
[107294,"Ex9EMS 1P 2M 100A MO 2T","Smart energy meter 1-pole, 2-module, 100 A, ModBus-communication, 2-tariff, LCD display","NAZ",121.25,0,121.25,8592765072948,1,18592765072945,48,28592765072942,"9028301100",0.16]
[107295,"Ex9EMS 3P 4M 100A 2T","Smart energy meter 3-pole, 4-module, 100 A, 2-tariff, LCD display","NAZ",202.32,0,202.32,8592765072955,1,18592765072952,36,28592765072959,"9028301900",0.16]
[107296,"Ex9EMS 3P 4M 100A MB 2T","Smart energy meter 3-pole, 4-module, 100 A, Mbus-communication, 2-tariff, LCD display","NAZ",237.92,0,237.92,8592765072962,1,18592765072969,36,28592765072966,"9028301900",0.16]
[107297,"Ex9EMS 3P 4M 100A MO 2T","Smart energy meter 3-pole, 4-module, 100 A, ModBus-communication, 2-tariff, LCD display","NAZ",231.51,0,231.51,8592765072979,1,18592765072976,36,28592765072973,"9028301900",0.39]
[107298,"Ex9EMS 3P 4M CT 2T","Smart energy meter 3-pole, 4-module, current transformer, 2-tariff, LCD display","NAZ",208.18,0,208.18,8592765072986,1,18592765072983,36,28592765072980,"9028301900",0.39]
[107299,"Ex9EMS 3P 4M CT MB 2T","Smart energy meter 3-pole, 4-module, current transformer, Mbus-communication, 2-tariff, LCD display","NAZ",240.39,0,240.39,8592765072993,1,18592765072990,36,28592765072997,"9028301900",0.39]
[107300,"Ex9EMS 3P 4M CT MO 2T","Smart energy meter 3-pole, 4-module, current transformer, ModBus-communication, 2-tariff, LCD display","NAZ",247.86,0,247.86,8592765073006,1,18592765073003,36,28592765073000,"9028301900",0.39]
[107301,"CT 5/100A SC","Current Transformer 5/100A, solid core","NAZ",27.95,0,27.95,8592765073013,1,18592765073010,100,28592765073017,"8504901900",0.25]
[107302,"CT 5/150A SC","Current Transfromer 5/150A, solid core","NAZ",27.95,0,27.95,8592765073020,1,18592765073027,100,28592765073024,"8504901900",0.25]
[107303,"CT 5/200A SC","Current Transfromer 5/200A, solid core","NAZ",27.95,0,27.95,8592765073037,1,18592765073034,100,28592765073031,"8504901900",0.25]
[107304,"CT 5/250A SC","Current Transfromer 5/250A, solid core","NAZ",27.95,0,27.95,8592765073044,1,18592765073041,100,28592765073048,"8504901900",0.25]
[107305,"CT 5/300A SC","Current Transfromer 5/300A, solid core","NAZ",27.95,0,27.95,8592765073051,1,18592765073058,100,28592765073055,"8504901900",0.25]
[107306,"CT 5/400A SC","Current Transfromer 5/400A, solid core","NAZ",27.95,0,27.95,8592765073068,1,18592765073065,60,28592765073062,"8504901900",0.35]
[107307,"CT 5/500A SC","Current Transfromer 5/500A, solid core","NAZ",37.99,0,37.99,8592765073075,1,18592765073072,60,28592765073079,"8504901900",0.35]
[107308,"CT 5/600A SC","Current Transfromer 5/600A, solid core","NAZ",39.51,0,39.51,8592765073082,1,18592765073089,60,28592765073086,"8504901900",0.35]
[107309,"CT 5/1000A SC","Current Transfromer 5/1000A, solid core","NAZ",39.51,0,39.51,8592765073099,1,18592765073096,30,28592765073093,"8504901900",0.59]
[107310,"CT 5/100A","Current Transfromer 5/100A, split core","NAZ",48.13,0,48.13,8592765073105,1,18592765073102,48,28592765073109,"8504901900",0.25]
[107311,"CT 5/150A","Current Transfromer 5/150A, split core","NAZ",48.13,0,48.13,8592765073112,1,18592765073119,48,28592765073116,"8504901900",0.25]
[107312,"CT 5/200A","Current Transfromer 5/200A, split core","NAZ",48.13,0,48.13,8592765073129,1,18592765073126,48,28592765073123,"8504901900",0.25]
[107313,"CT 5/250A","Current Transfromer 5/250A, split core","NAZ",48.13,0,48.13,8592765073136,1,18592765073133,48,28592765073130,"8504901900",0.25]
[107314,"CT 5/300A","Current Transfromer 5/300A, split core","NAZ",48.13,0,48.13,8592765073143,1,18592765073140,48,28592765073147,"8504901900",0.25]
[107315,"CT 5/400A","Current Transfromer 5/400A, split core","NAZ",98.95,0,98.95,8592765073150,1,18592765073157,39,28592765073154,"8504901900",0.42]
[107316,"CT 5/600A","Current Transfromer 5/600A, split core","NAZ",98.95,0,98.95,8592765073167,1,18592765073164,39,28592765073161,"8504901900",0.42]
[109855,"IR USB","IR connecting cable","NAZ",100.64,{"$f":"NAZ","v":0},{"$f":"E1725*(1-F1725)","v":100.64},8592765098559,10,18592765098556,100,28592765098553,"8544429090",8.4000000000000005E-2]
[109856,"IR BR 1M","Bracket for IR cable 1M","NAZ",14.81,{"$f":"NAZ","v":0},{"$f":"E1726*(1-F1726)","v":14.81},8592765098566,64,18592765098563,512,28592765098560,"90289010",8.0000000000000002E-3]
[109857,"IR BR 2M","Bracket for IR cable 2M","NAZ",20.85,{"$f":"NAZ","v":0},20.85,8592765098573,40,18592765098570,320,28592765098577,"90289010",1.2E-2]
[109858,"IR BR 4M","Bracket for IR cable 4M","NAZ",20.85,{"$f":"NAZ","v":0},20.85,8592765098580,24,18592765098587,192,28592765098584,"90289010",1.6E-2]
[]
["Installation relays and contactors Ex9CH"]
[107010,"Ex9CH20 10 24V 50/60Hz","Installation relay, 20 A, coil 24V, 1 NO contact","NAS",20.74,{"$f":"NAS","v":0},{"$f":"E1731*(1-F1731)","v":20.74},8592765070111,2,18592765070118,162,28592765070115,"8536419089",0.1]
[107011,"Ex9CH20 10 230V 50/60Hz","Installation relay, 20 A, coil 230V, 1 NO contact","NAS",17.21,{"$f":"NAS","v":0},17.21,8592765070128,2,18592765070125,162,28592765070122,"8536490099",0.1]
[107013,"Ex9CH20 01 24V 50/60Hz","Installation relay, 20 A, coil 24V, 1 NC contact","NAS",20.74,0,20.74,8592765070142,2,18592765070149,162,28592765070146,"8536419089",0.1]
[107014,"Ex9CH20 01 230V 50/60Hz","Installation relay, 20 A, coil 230V, 1 NC contact","NAS",17.21,0,17.21,8592765070159,2,18592765070156,162,28592765070153,"8536490099",0.1]
[102401,"Ex9CH20 11 24V 50/60Hz","Installation relay, 20 A, coil 24 V,  1 NC + 1 NO  contact","NAS",23.45,0,23.45,8592765024022,2,18592765024029,162,28592765024026,"8536419089",0.12]
[102402,"Ex9CH20 11 220/230V 50/60Hz","Installation relay, 20 A, coil 220/230 V,  1 NC + 1 NO  contact","NAS",16.27,0,16.27,8592765024039,2,18592765024036,162,28592765024033,"8536490099",0.12]
[102403,"Ex9CH20 11 240V 50/60Hz","Installation relay, 20 A, coil 240 V,  1 NC + 1 NO  contact","NAS",19.920000000000002,0,19.920000000000002,8592765024046,2,18592765024043,162,28592765024040,"8536490099",0.12]
[102398,"Ex9CH20 20 24V 50/60Hz","Installation relay, 20 A, coil 24 V, 2 NO  contact","NAS",23.45,0,23.45,8592765023995,2,18592765023992,162,28592765023999,"8536419089",0.12]
[102399,"Ex9CH20 20 220/230V 50/60Hz","Installation relay, 20 A, coil 220/230 V, 2 NO  contact","NAS",16.27,0,16.27,8592765024008,2,18592765024005,162,28592765024002,"8536490099",0.12]
[102400,"Ex9CH20 20 240V 50/60Hz","Installation relay, 20 A, coil 240 V, 2 NO  contact","NAS",19.920000000000002,0,19.920000000000002,8592765024015,2,18592765024012,162,28592765024019,"8536490099",0.12]
[102404,"Ex9CH20 02 24V 50/60Hz","Installation relay, 20 A, coil 24 V, 2 NC  contact","NAS",23.45,0,23.45,8592765024053,2,18592765024050,162,28592765024057,"8536419089",0.12]
[102405,"Ex9CH20 02 220/230V 50/60Hz","Installation relay, 20 A, coil 220/230 V, 2 NC  contact","NAS",17.510000000000002,0,17.510000000000002,8592765024060,2,18592765024067,162,28592765024064,"8536490099",0.12]
[102406,"Ex9CH20 02 240V 50/60Hz","Installation relay, 20 A, coil 240 V, 2 NC  contact","NAS",23.45,0,23.45,8592765024077,2,18592765024074,162,28592765024071,"8536490099",0.12]
[102409,"Ex9CH20 22 24V 50/60Hz","Installation relay, 20 A, coil 24 V,  2 NC + 2 NO  contact","NAS",30.87,0,30.87,8592765024107,1,8592765024107,81,28592765024101,"8536419089",0.21]
[102410,"Ex9CH20 22 220/230V 50/60Hz","Installation relay, 20 A, coil 220/230 V,  2 NC + 2 NO  contact","NAS",25.88,0,25.88,8592765024114,1,8592765024114,81,28592765024118,"8536490099",0.21]
[107317,"Ex9CH20 31 24V 50/60Hz","Installation relay, 20 A, coil 24 V,  3 NO + 1 NC  contact","NAS",31.82,0,31.82,8592765073174,1,8592765073174,81,28592765073178,"8536419089",0.24]
[107318,"Ex9CH20 31 230V 50/60Hz","Installation relay, 20 A, coil 230 V,  3 NO + 1 NC  contact","NAS",26.91,0,26.91,8592765073181,1,8592765073181,81,28592765073185,"8536490099",0.24]
[102407,"Ex9CH20 40 24V 50/60Hz","Installation relay, 20 A, coil 24 V, 4 NO  contact","NAS",30.87,0,30.87,8592765024084,1,18592765024081,81,28592765024088,"8536419089",0.21]
[102408,"Ex9CH20 40 230V 50/60Hz","Installation relay, 20 A, coil 230 V, 4 NO  contact","NAS",25.88,0,25.88,8592765024091,1,8592765024091,81,28592765024095,"8536490099",0.21]
[107321,"Ex9CH25 11 24V 50/60Hz","Installation contactor, 25 A, coil 24 V,  1 NC + 1 NO  contact","NAS",25.47,0,25.47,8592765073211,2,18592765073218,108,28592765073215,"8536419089",0.14000000000000001]
[107322,"Ex9CH25 11 230V 50/60Hz","Installation contactor, 25 A, coil 230 V,  1 NC + 1 NO  contact","NAS",21.95,0,21.95,8592765073228,2,18592765073225,108,28592765073222,"8536490099",0.14000000000000001]
[107319,"Ex9CH25 20 24V 50/60Hz","Installation contactor, 25 A, coil 24V, 2 NO contacts","NAS",25.47,0,25.47,8592765073198,2,18592765073195,108,28592765073192,"8536419089",0.14000000000000001]
[107320,"Ex9CH25 20 230V 50/60Hz","Installation contactor, 25 A, coil 230V, 2 NO contacts","NAS",21.95,0,21.95,8592765073204,2,18592765073201,108,28592765073208,"8536490099",0.14000000000000001]
[107016,"Ex9CH25 02 24V 50/60Hz","Installation contactor, 25 A, coil 24V, 2 NC contacts","NAS",25.47,0,25.47,8592765070173,2,18592765070170,162,28592765070177,"8536419089",0.12]
[107017,"Ex9CH25 02 230V 50/60Hz","Installation contactor, 25 A, coil 230V, 2 NC contacts","NAS",21.95,0,21.95,8592765070180,2,18592765070187,162,28592765070184,"8536490099",0.12]
[102413,"Ex9CH25 22 24V 50/60Hz","Installation contactor, 25 A, coil 24 V,  2 NC + 2 NO  contact","NAS",33.86,0,33.86,8592765024145,1,8592765024145,81,28592765024149,"8536419089",0.21]
[102414,"Ex9CH25 22 220/230V 50/60Hz","Installation contactor, 25 A, coil 220/230 V,  2 NC + 2 NO  contact","NAS",27.87,0,27.87,8592765024152,1,8592765024152,81,28592765024156,"8536490099",0.21]
[107019,"Ex9CH25 31 24V 50/60Hz","Installation contactor, 25 A, coil 24V, 3 NO + 1 NC contacts","NAS",35.840000000000003,0,35.840000000000003,8592765070203,1,8592765070203,81,28592765070207,"8536419089",0.21]
[107020,"Ex9CH25 31 230V 50/60Hz","Installation contactor, 25 A, coil 230V, 3 NO + 1 NC contacts","NAS",24.88,0,24.88,8592765070210,1,8592765070210,81,28592765070214,"8536490099",0.21]
[102411,"Ex9CH25 40 24V 50/60Hz","Installation contactor, 25 A, coil 24 V, 4 NO  contact","NAS",35.840000000000003,0,35.840000000000003,8592765024121,1,8592765024121,81,28592765024125,"8536419089",0.21]
[102412,"Ex9CH25 40 230V 50/60Hz","Installation contactor, 25 A, coil 230 V, 4 NO  contact","NAS",24.88,0,24.88,8592765024138,1,8592765024138,81,28592765024132,"8536490099",0.21]
[102417,"Ex9CH40 11 24V 50/60Hz","Installation contactor, 40 A, coil 24 V,  1 NC + 1 NO  contact","NAS",55.34,0,55.34,8592765024183,1,8592765024183,81,28592765024187,"8536419089",0.22]
[102418,"Ex9CH40 11 220/230V 50/60Hz","Installation contactor, 40 A, coil 220/230 V,  1 NC + 1 NO  contact","NAS",48.84,0,48.84,8592765024190,1,8592765024190,81,28592765024194,"8536490099",0.22]
[102415,"Ex9CH40 20 24V 50/60Hz","Installation contactor, 40 A, coil 24 V, 2 NO  contact","NAS",55.34,0,55.34,8592765024169,1,8592765024169,81,28592765024163,"8536419089",0.22]
[102416,"Ex9CH40 20 220/230V 50/60Hz","Installation contactor, 40 A, coil 220/230 V, 2 NO  contact","NAS",37.54,0,37.54,8592765024176,1,8592765024176,81,28592765024170,"8536490099",0.22]
[107023,"Ex9CH40 02 24V 50/60Hz","Installation contactor, 40 A, coil 24V, 2 NC contacts","NAS",55.34,0,55.34,8592765070241,1,8592765070241,81,28592765070245,"8536419089",0.22]
[107024,"Ex9CH40 02 230V 50/60Hz","Installation contactor, 40 A, coil 230V, 2 NC contacts","NAS",48.84,0,48.84,8592765070258,1,8592765070258,81,28592765070252,"8536490099",0.22]
[107323,"Ex9CH40 22 24V 50/60Hz","Installation contactor, 40 A, coil 24 V, 2 NO + 2 NC contact","NAS",58.6,0,58.6,8592765073235,1,8592765073235,54,28592765073239,"8536419089",0.44]
[107324,"Ex9CH40 22 230V 50/60Hz","Installation contactor, 40 A, coil 230 V, 2 NO + 2 NC contact","NAS",52.09,0,52.09,8592765073242,1,8592765073242,54,28592765073246,"8536490099",0.44]
[107021,"Ex9CH40 31 24V 50/60Hz","Installation contactor, 40 A, coil 24V, 3 NO + 1 NC contacts","NAS",61.85,0,61.85,8592765070227,1,8592765070227,54,28592765070221,"8536419089",0.4]
[107022,"Ex9CH40 31 230V 50/60Hz","Installation contactor, 40 A, coil 230V, 3 NO + 1 NC contacts","NAS",55.34,0,55.34,8592765070234,1,8592765070234,54,28592765070238,"8536490099",0.4]
[102419,"Ex9CH40 40 24V 50/60Hz","Installation contactor, 40 A, coil 24 V, 4 NO  contact","NAS",61.85,0,61.85,8592765024206,1,8592765024206,54,28592765024200,"8536419089",0.4]
[102420,"Ex9CH40 40 220/230V 50/60Hz","Installation contactor, 40 A, coil 220/230 V, 4 NO  contact","NAS",49.19,0,49.19,8592765024213,1,8592765024213,54,28592765024217,"8536490099",0.4]
[102421,"Ex9CH40 40 240V 50/60Hz","Installation contactor, 40 A, coil 240 V, 4 NO  contact","NAS",55.34,0,55.34,8592765024220,1,8592765024220,54,28592765024224,"8536490099",0.4]
[102424,"Ex9CH63 11 24V 50/60Hz","Installation contactor, 63 A, coil 24 V,  1 NC + 1 NO  contact","NAS",84.65,0,84.65,8592765024251,1,8592765024251,81,28592765024255,"8536419089",0.22]
[102425,"Ex9CH63 11 220/230V 50/60Hz","Installation contactor, 63 A, coil 220/230 V,  1 NC + 1 NO  contact","NAS",74.87,0,74.87,8592765024268,1,8592765024268,81,28592765024262,"8536490099",0.22]
[102422,"Ex9CH63 20 24V 50/60Hz","Installation contactor, 63 A, coil 24 V, 2 NO  contact","NAS",84.65,0,84.65,8592765024237,1,8592765024237,81,28592765024231,"8536419089",0.22]
[102423,"Ex9CH63 20 220/230V 50/60Hz","Installation contactor, 63 A, coil 220/230 V, 2 NO  contact","NAS",51.94,0,51.94,8592765024244,1,8592765024244,81,28592765024248,"8536490099",0.22]
[107025,"Ex9CH63 02 24V 50/60Hz","Installation contactor, 63 A, coil 24V, 2 NC contacts","NAS",84.65,0,84.65,8592765070265,1,8592765070265,81,28592765070269,"8536419089",0.22]
[107026,"Ex9CH63 02 230V 50/60Hz","Installation contactor, 63 A, coil 230V, 2 NC contacts","NAS",74.87,0,74.87,8592765070272,1,8592765070272,81,28592765070276,"8536490099",0.22]
[107325,"Ex9CH63 22 24V 50/60Hz","Installation contactor, 63 A, coil 24V, 2 NO + 2 NC contacts","NAS",79.760000000000005,0,79.760000000000005,8592765073259,1,8592765073259,54,28592765073253,"8536419089",0.44]
[107326,"Ex9CH63 22 230V 50/60Hz","Installation contactor, 63 A, coil 230V, 2 NO + 2 NC contacts","NAS",69.989999999999995,0,69.989999999999995,8592765073266,1,8592765073266,54,28592765073260,"8536490099",0.44]
[107027,"Ex9CH63 31 24V 50/60Hz","Installation contactor, 63 A, coil 24V, 3 NO + 1 NC contacts","NAS",74.87,0,74.87,8592765070289,1,8592765070289,54,28592765070283,"8536419089",0.4]
[107028,"Ex9CH63 31 230V 50/60Hz","Installation contactor, 63 A, coil 230V, 3 NO + 1 NC contacts","NAS",65.11,0,65.11,8592765070296,1,8592765070296,54,28592765070290,"8536490099",0.4]
[102426,"Ex9CH63 40 24V 50/60Hz","Installation contactor, 63 A, coil 24 V, 4 NO  contact","NAS",74.87,0,74.87,8592765024275,1,8592765024275,54,28592765024279,"8536419089",0.4]
[102427,"Ex9CH63 40 220/230V 50/60Hz","Installation contactor, 63 A, coil 220/230 V, 4 NO  contact","NAS",52.41,0,52.41,8592765024282,1,8592765024282,54,28592765024286,"8536490099",0.4]
[102428,"Ex9CH63 40 240V 50/60Hz","Installation contactor, 63 A, coil 240 V, 4 NO  contact","NAS",65.11,0,65.11,8592765024299,1,8592765024299,54,28592765024293,"8536490099",0.4]
[107956,"Ex9CH20 SP","Distance block/separator between Ex9CH devices, width 0.5 MU","NAS",3.09,0,3.09,8592765079572,1,8592765079572,0,28592765079576,"8536490099",0.02]
[]
["Impulse relays Ex9JU"]
[110260,"Ex9JU-16/1P AC220V","Impulse relay, 16 A, coil 220V AC, 1-pole","NAS",12.5,{"$f":"NAS","v":0},{"$f":"E1791*(1-F1791)","v":12.5},8592765102607,12,18592765102604,180,28592765102601,"8536419089",0.105]
[110261,"Ex9JU-16/1P AC230V","Impulse relay, 16 A, coil 230V AC, 1-pole","NAS",12.5,{"$f":"NAS","v":0},12.5,8592765102614,12,18592765102611,180,28592765102618,"8536419089",0.105]
[110262,"Ex9JU-16/2P AC24V","Impulse relay, 16 A, coil 24V AC, 2-pole","NAS",13.5,0,13.5,8592765102621,12,18592765102628,180,28592765102625,"8536419089",0.111]
[110263,"Ex9JU-16/2P AC220V","Impulse relay, 16 A, coil 220V AC, 2-pole","NAS",13.5,0,13.5,8592765102638,12,18592765102635,180,28592765102632,"8536419089",0.111]
[110264,"Ex9JU-16/2P AC230V","Impulse relay, 16 A, coil 230V AC, 2-pole","NAS",13.5,0,13.5,8592765102645,12,18592765102642,180,28592765102649,"8536419089",0.111]
[110265,"Ex9JU-16/3P AC24V","Impulse relay, 16 A, coil 24V AC, 3-pole","NAS",19.8,0,19.8,8592765102652,6,18592765102659,90,28592765102656,"8536419089",0.215]
[110266,"Ex9JU-16/3P AC220V","Impulse relay, 16 A, coil 220V AC, 3-pole","NAS",19.8,0,19.8,8592765102669,6,18592765102666,90,28592765102663,"8536419089",0.215]
[110267,"Ex9JU-16/3P AC230V","Impulse relay, 16 A, coil 230V AC, 3-pole","NAS",19.8,0,19.8,8592765102676,6,18592765102673,90,28592765102670,"8536419089",0.215]
[110268,"Ex9JU-16/4P AC24V","Impulse relay, 16 A, coil 24V AC, 4-pole","NAS",32.200000000000003,0,32.200000000000003,8592765102683,6,18592765102680,90,28592765102687,"8536419089",0.222]
[110269,"Ex9JU-16/4P AC220V","Impulse relay, 16 A, coil 220V AC, 4-pole","NAS",32.200000000000003,0,32.200000000000003,8592765102690,6,18592765102697,90,28592765102694,"8536419089",0.222]
[110270,"Ex9JU-16/4P AC230V","Impulse relay, 16 A, coil 230V AC, 4-pole","NAS",32.200000000000003,0,32.200000000000003,8592765102706,6,18592765102703,90,28592765102700,"8536419089",0.222]
[110271,"Ex9JU-32/1P AC220V","Impulse relay, 32 A, coil 220V AC, 1-pole","NAS",8.25,0,8.25,8592765102713,12,18592765102710,180,28592765102717,"8536419089",0.111]
[110272,"Ex9JU-32/1P AC230V","Impulse relay, 32 A, coil 230V AC, 1-pole","NAS",8.25,0,8.25,8592765102720,12,18592765102727,180,28592765102724,"8536419089",0.111]
[110273,"Ex9JU-32/2P AC24V","Impulse relay, 32 A, coil 24V AC, 2-pole","NAS",14.15,0,14.15,8592765102737,6,18592765102734,90,28592765102731,"8536419089",0.219]
[110274,"Ex9JU-32/2P AC220V","Impulse relay, 32 A, coil 220V AC, 2-pole","NAS",14.15,0,14.15,8592765102744,6,18592765102741,90,28592765102748,"8536419089",0.219]
[110275,"Ex9JU-32/2P AC230V","Impulse relay, 32 A, coil 230V AC, 2-pole","NAS",14.15,0,14.15,8592765102751,6,18592765102758,90,28592765102755,"8536419089",0.219]
[110276,"Ex9JU-32/3P AC24V","Impulse relay, 32 A, coil 24V AC, 3-pole","NAS",21.6,0,21.6,8592765102768,4,18592765102765,60,28592765102762,"8536419089",0.32700000000000001]
[110277,"Ex9JU-32/3P AC220V","Impulse relay, 32 A, coil 220V AC, 3-pole","NAS",21.6,0,21.6,8592765102775,4,18592765102772,60,28592765102779,"8536419089",0.32700000000000001]
[110278,"Ex9JU-32/3P AC230V","Impulse relay, 32 A, coil 230V AC, 3-pole","NAS",21.6,0,21.6,8592765102782,4,18592765102789,60,28592765102786,"8536419089",0.32700000000000001]
[110279,"Ex9JU-32/4P AC24V","Impulse relay, 32 A, coil 24V AC, 4-pole","NAS",27.12,0,27.12,8592765102799,3,18592765102796,45,28592765102793,"8536419089",0.435]
[110280,"Ex9JU-32/4P AC220V","Impulse relay, 32 A, coil 220V AC, 4-pole","NAS",27.12,0,27.12,8592765102805,3,18592765102802,45,28592765102809,"8536419089",0.435]
[110281,"Ex9JU-32/4P AC230V","Impulse relay, 32 A, coil 230V AC, 4-pole","NAS",27.12,0,27.12,8592765102812,3,18592765102819,45,28592765102816,"8536419089",0.435]
[110282,"Ex9JU-16/1P DC24V","Impulse relay, 16 A, coil 24V DC, 1-pole","NAS",8.82,0,8.82,8592765102829,12,18592765102826,180,28592765102823,"8536419089",0.105]
[110283,"Ex9JU-16/1P DC127V","Impulse relay, 16 A, coil 127V DC, 1-pole","NAS",8.82,0,8.82,8592765102836,12,18592765102833,180,28592765102830,"8536419089",0.105]
[110284,"Ex9JU-16/2P DC24V","Impulse relay, 16 A, coil 24V DC, 2-pole","NAS",10.68,0,10.68,8592765102843,12,18592765102840,180,28592765102847,"8536419089",0.111]
[110285,"Ex9JU-16/3P DC24V","Impulse relay, 16 A, coil 24V DC, 3-pole","NAS",18.559999999999999,0,18.559999999999999,8592765102850,6,18592765102857,90,28592765102854,"8536419089",0.215]
[110286,"Ex9JU-16/4P DC24V","Impulse relay, 16 A, coil 24V DC, 4-pole","NAS",19.079999999999998,0,19.079999999999998,8592765102867,6,18592765102864,90,28592765102861,"8536419089",0.222]
[110287,"Ex9JU-32/1P DC24V","Impulse relay, 32 A, coil 24V DC, 1-pole","NAS",10.58,0,10.58,8592765102874,12,18592765102871,180,28592765102878,"8536419089",0.111]
[110288,"Ex9JU-32/2P DC24V","Impulse relay, 32 A, coil 24V DC, 2-pole","NAS",12.82,0,12.82,8592765102881,6,18592765102888,90,28592765102885,"8536419089",0.219]
[110289,"Ex9JU-32/3P DC24V","Impulse relay, 32 A, coil 24V DC, 3-pole","NAS",24,0,24,8592765102898,4,18592765102895,60,28592765102892,"8536419089",0.32700000000000001]
[110290,"Ex9JU-32/4P DC24V","Impulse relay, 32 A, coil 24V DC, 4-pole","NAS",26.9,0,26.9,8592765102904,3,18592765102901,45,28592765102908,"8536419089",0.435]
[]
["Surge protection devices Ex9UE, class 1+2 (B+C) 25kA, plug-in module design with signalization"]
[105503,"Ex9UE1+2 25 3P 280","Surge protection device, class 1+2 (B+C), Iimp=25 kA, Uc=280 VAC, 3-pole","NAR",529.02,{"$f":"NAR","v":0},{"$f":"E1824*(1-F1824)","v":529.02},8592765055040,1,8592765055040,27,28592765055044,"8536309090","0.78"]
[105504,"Ex9UE1+2 25R 3P 280","Surge protection device, class 1+2 (B+C), Iimp=25 kA, Uc=280 VAC, 3-pole, with remote-signal contact","NAR",539.29,{"$f":"NAR","v":0},539.29,8592765055057,1,8592765055057,27,28592765055051,"8536309090","0.78"]
[105505,"Ex9UE1+2 25 3PN 280","Surge protection device, class 1+2 (B+C), Iimp=25 kA, Uc=280 VAC, 3+Npole","NAR",727.17,0,727.17,8592765055064,1,8592765055064,18,28592765055068,"8536309090","1.00"]
[105506,"Ex9UE1+2 25R 3PN 280","Surge protection device, class 1+2 (B+C), Iimp=25 kA, Uc=280 VAC, 3+Npole, with remote-signal contact","NAR",737.43,0,737.43,8592765055071,1,8592765055071,18,28592765055075,"8536309090","1.00"]
[105507,"Ex9UE1+2 25 4P 280","Surge protection device, class 1+2 (B+C), Iimp=25 kA, Uc=280 VAC, 4-pole","NAR",682.13,0,682.13,8592765055088,1,8592765055088,18,28592765055082,"8536309090","1.08"]
[105508,"Ex9UE1+2 25R 4P 280","Surge protection device, class 1+2 (B+C), Iimp=25 kA, Uc=280 VAC, 4-pole, with remote-signal contact","NAR",692.56,0,692.56,8592765055095,1,8592765055095,18,28592765055099,"8536309090","1.08"]
[105495,"Ex9UE1+2 25 1P 280 M","Surge protection device, class 1+2 (B+C), Iimp=25 kA, Uc=280 VAC, plug-in module only","NAR",131.30000000000001,0,131.30000000000001,8592765054968,1,8592765054968,81,28592765054962,"8536309090"]
[105496,"Ex9UE1+2 100 NPE M","Surge protection device, class 1+2 (B+C), Iimp=100 kA, NPE plug-in module only","NAR",213.16,0,213.16,8592765054975,1,8592765054975,81,28592765054979,"8536309090"]
[]
["Surge protection devices Ex9UE, class 1 (B)"]
[107115,"Ex9UE1 35 1P 350","Surge protection device, class 1 (B), Iimp=35 kA, Uc=385 VAC, 1-pole","NAR",253.85,{"$f":"NAR","v":0},{"$f":"E1834*(1-F1834)","v":253.85},8592765071163,1,8592765071163,81,28592765071167,"8536309090","0.17"]
[107119,"Ex9UE1 100 NPE","Surge protection device, class 1 (B), Iimp=100 kA, NPE","NAR",293.31,0,293.31,8592765071200,1,8592765071200,45,28592765071204,"8536309090","0.29"]
[]
["Surge protection devices Ex9UE, class 1+2 (B+C), plug-in module design with signalization"]
[103330,"Ex9UE1+2 12.5 1P 275 M","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, plug-in module only","NAR",69.540000000000006,{"$f":"NAR","v":0},{"$f":"E1838*(1-F1838)","v":69.540000000000006},8592765033314,1,8592765033314,null,28592765033318,"8536309090",0.12]
[103331,"Ex9UE1+2 NPE M","Surge protection device, class 1+2 (B+C), Iimp=50 kA, NPE plug-in module only","NAR",222.11,{"$f":"NAR","v":0},222.11,8592765033321,1,8592765033321,null,28592765033325,"8536309090",0.12]
[103332,"Ex9UE1+2 12.5 1P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 1-pole","NAR",97.92,0,97.92,8592765033338,1,8592765033338,96,28592765033332,"8536309090",0.15]
[103333,"Ex9UE1+2 12.5R  1P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 1-pole, with remote-signal contact","NAR",128.85,0,128.85,8592765033345,1,8592765033345,96,28592765033349,"8536309090",0.15]
[103334,"Ex9UE1+2 12.5 1PN 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 1+Npole","NAR",314.74,0,314.74,8592765033352,1,8592765033352,60,28592765033356,"8536309090",0.3]
[103335,"Ex9UE1+2 12.5R  1PN 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 1+Npole, with remote-signal contact","NAR",344.11,0,344.11,8592765033369,1,8592765033369,60,28592765033363,"8536309090",0.3]
[103336,"Ex9UE1+2 12.5 2P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 2-pole","NAR",205.84,0,205.84,8592765033376,1,8592765033376,60,28592765033370,"8536309090",0.3]
[103337,"Ex9UE1+2 12.5R  2P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 2-pole, with remote-signal contact","NAR",236.77,0,236.77,8592765033383,1,8592765033383,60,28592765033387,"8536309090",0.3]
[103338,"Ex9UE1+2 12.5 3P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 3-pole","NAR",131.5,0,131.5,8592765033390,1,8592765033390,54,28592765033394,"8536309090",0.45]
[103339,"Ex9UE1+2 12.5R  3P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 3-pole, with remote-signal contact","NAR",301.75,0,301.75,8592765033406,1,8592765033406,54,28592765033400,"8536309090",0.45]
[103340,"Ex9UE1+2 12.5 3PN 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 3+Npole","NAR",525.69000000000005,0,525.69000000000005,8592765033413,1,8592765033413,45,28592765033417,"8536309090",0.6]
[103341,"Ex9UE1+2 12.5R  3PN 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 3+Npole, with remote-signal contact","NAR",553.51,0,553.51,8592765033420,1,8592765033420,45,28592765033424,"8536309090",0.6]
[103342,"Ex9UE1+2 12.5 4P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 4-pole","NAR",315.98,0,315.98,8592765033437,1,8592765033437,45,28592765033431,"8536309090",0.6]
[103343,"Ex9UE1+2 12.5R  4P 275","Surge protection device, class 1+2 (B+C), Iimp=12,5 kA, Uc=275 VAC, 4-pole, with remote-signal contact","NAR",362.38,0,362.38,8592765033444,1,8592765033444,45,28592765033448,"8536309090",0.6]
[]
["Surge protection devices Ex9UE, class 2 (C), plug-in module design with signalization"]
[103344,"Ex9UE2 20 1P 275 M","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, plug-in module only","NAR",38.99,{"$f":"NAR","v":0},{"$f":"E1854*(1-F1854)","v":38.99},8592765033451,1,8592765033451,null,28592765033455,"8536309090",0.08]
[103752,"Ex9UE2 20 1P 320 M","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, plug-in module only","NAR",39.53,0,39.53,8592765037534,1,8592765037534,null,28592765037538,"8536309090",0.08]
[103753,"Ex9UE2 20 1P 385 M","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, plug-in module only","NAR",40.54,0,40.54,8592765037541,1,8592765037541,null,28592765037545,"8536309090",0.1]
[103345,"Ex9UE2 20 1P 440 M","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, plug-in module only","NAR",41.2,0,{"$f":"E1857*(1-F1857)","v":41.2},8592765033468,1,8592765033468,null,28592765033462,"8536309090",0.1]
[103346,"Ex9UE2 40 NPE M","Surge protection device, class 2 (C), In=40 kA, NPE plug-in module only","NAR",94.1,0,{"$f":"E1858*(1-F1858)","v":94.1},8592765033475,1,8592765033475,null,28592765033479,"8536309090",0.08]
[103347,"Ex9UE2 20 1P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 1-pole","NAR",35.380000000000003,0,35.380000000000003,8592765033482,1,8592765033482,96,28592765033486,"8536309090",0.11]
[103348,"Ex9UE2 20R 1P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 1-pole, with remote-signal contact","NAR",66.31,0,66.31,8592765033499,1,8592765033499,96,28592765033493,"8536309090",0.11]
[103349,"Ex9UE2 20 1PN 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 1+Npole","NAR",110.5,0,110.5,8592765033505,1,8592765033505,60,28592765033509,"8536309090",0.22]
[103350,"Ex9UE2 20R 1PN 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 1+Npole, with remote-signal contact","NAR",141.43,0,141.43,8592765033512,1,8592765033512,60,28592765033516,"8536309090",0.22]
[103351,"Ex9UE2 20 2P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 2-pole","NAR",94.7,0,94.7,8592765033529,1,8592765033529,60,28592765033523,"8536309090",0.22]
[103352,"Ex9UE2 20R 2P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 2-pole, with remote-signal contact","NAR",125.61,0,125.61,8592765033536,1,8592765033536,60,28592765033530,"8536309090",0.22]
[103353,"Ex9UE2 20 3P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 3-pole","NAR",58.81,0,58.81,8592765033543,1,8592765033543,54,28592765033547,"8536309090",0.33]
[103354,"Ex9UE2 20R 3P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 3-pole, with remote-signal contact","NAR",151.74,0,151.74,8592765033550,1,8592765033550,54,28592765033554,"8536309090",0.33]
[103355,"Ex9UE2 20 3PN 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 3+Npole","NAR",178.16,0,178.16,8592765033567,1,8592765033567,45,28592765033561,"8536309090",0.44]
[103356,"Ex9UE2 20R 3PN 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 3+Npole, with remote-signal contact","NAR",207.55,0,207.55,8592765033574,1,8592765033574,45,28592765033578,"8536309090",0.44]
[103357,"Ex9UE2 20 4P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 4-pole","NAR",123.97,0,123.97,8592765033581,1,8592765033581,45,28592765033585,"8536309090",0.44]
[103358,"Ex9UE2 20R 4P 275","Surge protection device, class 2 (C), In=20 kA, Uc=275 VAC, 4-pole, with remote-signal contact","NAR",166.93,0,166.93,8592765033598,1,8592765033598,45,28592765033592,"8536309090",0.44]
[103754,"Ex9UE2 20 1P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 1-pole","NAR",38.15,0,38.15,8592765037558,1,8592765037558,96,28592765037552,"8536309090",0.11]
[103755,"Ex9UE2 20R 1P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 1-pole, with remote-signal contact","NAR",67.540000000000006,0,67.540000000000006,8592765037565,1,8592765037565,96,28592765037569,"8536309090",0.11]
[103756,"Ex9UE2 20 1PN 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 1+Npole","NAR",115.83,0,115.83,8592765037572,1,8592765037572,60,28592765037576,"8536309090",0.22]
[103757,"Ex9UE2 20R 1PN 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 1+Npole, with remote-signal contact","NAR",146.76,0,146.76,8592765037589,1,8592765037589,60,28592765037583,"8536309090",0.22]
[103758,"Ex9UE2 20 2P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 2-pole","NAR",100.1,0,100.1,8592765037596,1,8592765037596,60,28592765037590,"8536309090",0.22]
[103759,"Ex9UE2 20R 2P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 2-pole, with remote-signal contact","NAR",131.02000000000001,0,131.02000000000001,8592765037602,1,8592765037602,60,28592765037606,"8536309090",0.22]
[103760,"Ex9UE2 20 3P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 3-pole","NAR",128.32,0,128.32,8592765037619,1,8592765037619,54,28592765037613,"8536309090",0.33]
[103761,"Ex9UE2 20R 3P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 3-pole, with remote-signal contact","NAR",157.87,0,157.87,8592765037626,1,8592765037626,54,28592765037620,"8536309090",0.33]
[103762,"Ex9UE2 20 3PN 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 3+Npole","NAR",193.17,0,193.17,8592765037633,1,8592765037633,45,28592765037637,"8536309090",0.44]
[103763,"Ex9UE2 20R 3PN 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 3+Npole, with remote-signal contact","NAR",222.92,0,222.92,8592765037640,1,8592765037640,45,28592765037644,"8536309090",0.44]
[103764,"Ex9UE2 20 4P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 4-pole","NAR",144.11000000000001,0,144.11000000000001,8592765037657,1,8592765037657,45,28592765037651,"8536309090",0.44]
[103765,"Ex9UE2 20R 4P 320","Surge protection device, class 2 (C), In=20 kA, Uc=320 VAC, 4-pole, with remote-signal contact","NAR",175.04,0,175.04,8592765037664,1,8592765037664,45,28592765037668,"8536309090",0.44]
[103766,"Ex9UE2 20 1P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 1-pole","NAR",43.16,0,43.16,8592765037671,1,8592765037671,96,28592765037675,"8536309090",0.11]
[103767,"Ex9UE2 20R 1P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 1-pole, with remote-signal contact","NAR",69.739999999999995,0,69.739999999999995,8592765037688,1,8592765037688,96,28592765037682,"8536309090",0.11]
[103768,"Ex9UE2 20 1PN 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 1+Npole","NAR",125.43,0,125.43,8592765037695,1,8592765037695,60,28592765037699,"8536309090",0.22]
[103769,"Ex9UE2 20R 1PN 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 1+Npole, with remote-signal contact","NAR",156.36000000000001,0,156.36000000000001,8592765037701,1,8592765037701,60,28592765037705,"8536309090",0.22]
[103770,"Ex9UE2 20 2P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 2-pole","NAR",109.84,0,109.84,8592765037718,1,8592765037718,60,28592765037712,"8536309090",0.22]
[103771,"Ex9UE2 20R 2P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 2-pole, with remote-signal contact","NAR",140.77000000000001,0,140.77000000000001,8592765037725,1,8592765037725,60,28592765037729,"8536309090",0.22]
[103772,"Ex9UE2 20 3P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 3-pole","NAR",138.51,0,138.51,8592765037732,1,8592765037732,54,28592765037736,"8536309090",0.33]
[103773,"Ex9UE2 20R 3P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 3-pole, with remote-signal contact","NAR",168.89,0,168.89,8592765037749,1,8592765037749,54,28592765037743,"8536309090",0.33]
[103774,"Ex9UE2 20 3PN 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 3+Npole","NAR",220.14,0,220.14,8592765037756,1,8592765037756,45,28592765037750,"8536309090",0.44]
[103775,"Ex9UE2 20R 3PN 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 3+Npole, with remote-signal contact","NAR",250.61,0,250.61,8592765037763,1,8592765037763,45,28592765037767,"8536309090",0.44]
[103776,"Ex9UE2 20 4P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 4-pole","NAR",158.66999999999999,0,158.66999999999999,8592765037770,1,8592765037770,45,28592765037774,"8536309090",0.44]
[103777,"Ex9UE2 20R 4P 385","Surge protection device, class 2 (C), In=20 kA, Uc=385 VAC, 4-pole, with remote-signal contact","NAR",189.6,0,189.6,8592765037787,1,8592765037787,45,28592765037781,"8536309090",0.44]
[103359,"Ex9UE2 20 1P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 1-pole","NAR",46.48,0,46.48,8592765033604,1,8592765033604,96,28592765033608,"8536309090",0.11]
[103360,"Ex9UE2 20R 1P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 1-pole, with remote-signal contact","NAR",71.22,0,71.22,8592765033611,1,8592765033611,96,28592765033615,"8536309090",0.11]
[103361,"Ex9UE2 20 1PN 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 1+Npole","NAR",131.84,0,131.84,8592765033628,1,8592765033628,60,28592765033622,"8536309090",0.22]
[103362,"Ex9UE2 20R 1PN 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 1+Npole, with remote-signal contact","NAR",162.77000000000001,0,162.77000000000001,8592765033635,1,8592765033635,60,28592765033639,"8536309090",0.22]
[103363,"Ex9UE2 20 2P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 2-pole","NAR",116.35,0,116.35,8592765033642,1,8592765033642,60,28592765033646,"8536309090",0.22]
[103364,"Ex9UE2 20R 2P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 2-pole, with remote-signal contact","NAR",147.28,0,147.28,8592765033659,1,8592765033659,60,28592765033653,"8536309090",0.22]
[103365,"Ex9UE2 20 3P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 3-pole","NAR",145.29,0,145.29,8592765033666,1,8592765033666,54,28592765033660,"8536309090",0.33]
[103366,"Ex9UE2 20R 3P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 3-pole, with remote-signal contact","NAR",176.22,0,176.22,8592765033673,1,8592765033673,54,28592765033677,"8536309090",0.33]
[103367,"Ex9UE2 20 3PN 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 3+Npole","NAR",238.15,0,238.15,8592765033680,1,8592765033680,45,28592765033684,"8536309090",0.44]
[103368,"Ex9UE2 20R 3PN 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 3+Npole, with remote-signal contact","NAR",269.07,0,269.07,8592765033697,1,8592765033697,45,28592765033691,"8536309090",0.44]
[103369,"Ex9UE2 20 4P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 4-pole","NAR",168.38,0,168.38,8592765033703,1,8592765033703,45,28592765033707,"8536309090",0.44]
[103370,"Ex9UE2 20R 4P 440","Surge protection device, class 2 (C), In=20 kA, Uc=440 VAC, 4-pole, with remote-signal contact","NAR",199.32,0,199.32,8592765033710,1,8592765033710,45,28592765033714,"8536309090",0.44]
[]
["Surge protection devices Ex9UE, class 3 (D), plug-in module design with signalization"]
[106858,"Ex9UE3 10 275","Surge protection device, class 3 (D), In=10 kA, Uc=275 VAC, 1+Npole","NAR",41.96,{"$f":"NAR","v":0},{"$f":"E1909*(1-F1909)","v":41.96},8592765068590,1,8592765068590,60,28592765068594,"8536309090",0.08]
[106857,"Ex9UE3 10R 275","Surge protection device, class 3 (D), In=10 kA, Uc=275 VAC, 1+Npole, with remote-signal contact","NAR",49.5,{"$f":"NAR","v":0},{"$f":"E1910*(1-F1910)","v":49.5},8592765068583,1,8592765068583,60,28592765068587,"8536309090",0.08]
[106859,"Ex9UE3 10 275M","Surge protection device, class 3 (D), In=10 kA, Uc=275 VAC, plug-in module only","NAR",32.86,{"$f":"NAR","v":0},{"$f":"E1911*(1-F1911)","v":32.86},8592765068606,1,8592765068606,null,28592765068600,"8536309090",0.03]
[]
["Modular Isolators Ex9I125"]
[102304,"Ex9I125 1P 16A","Isolator, width 1 module, 1-pole, 16A","NAH",5.44,{"$f":"NAH","v":0},{"$f":"E1914*(1-F1914)","v":5.44},8592765023056,12,18592765023053,144,28592765023050,"8536508090",0.09]
[102305,"Ex9I125 1P 25A ","Isolator, width 1 module, 1-pole, 25A","NAH",6.04,0,6.04,8592765023063,12,18592765023060,144,28592765023067,"8536508090",0.09]
[100862,"Ex9I125 1P 32A","Isolator, width 1 module, 1-pole, 32A","NAH",6.37,{"$f":"NAH","v":0},6.37,8592765008633,12,18592765008630,144,28592765008637,"8536508090",0.09]
[100863,"Ex9I125 1P 40A ","Isolator, width 1 module, 1-pole, 40A","NAH",8.26,0,8.26,8592765008640,12,18592765008647,144,28592765008644,"8536508090",0.09]
[100864,"Ex9I125 1P 63A","Isolator, width 1 module, 1-pole, 63A","NAH",9.2100000000000009,0,9.2100000000000009,8592765008657,12,18592765008654,144,28592765008651,"8536508090",0.09]
[100865,"Ex9I125 1P 80A","Isolator, width 1 module, 1-pole, 80A","NAH",11.67,0,11.67,8592765008664,12,18592765008661,144,28592765008668,"8536508090",0.09]
[100866,"Ex9I125 1P 100A ","Isolator, width 1 module, 1-pole, 100A","NAH",13.86,0,13.86,8592765008671,12,18592765008678,144,28592765008675,"8536508090",0.09]
[100867,"Ex9I125 1P 125A ","Isolator, width 1 module, 1-pole, 125A","NAH",14.22,0,14.22,8592765008688,12,18592765008685,144,28592765008682,"8536508090",0.09]
[102306,"Ex9I125 2P 16A ","Isolator, width 2 modules, 2-pole, 16A","NAH",12.26,{"$f":"NAH","v":0},12.26,8592765023070,6,18592765023077,72,28592765023074,"8536508090",0.18]
[102307,"Ex9I125 2P 25A ","Isolator, width 2 modules, 2-pole, 25A","NAH",12.44,0,12.44,8592765023087,6,18592765023084,72,28592765023081,"8536508090",0.18]
[100868,"Ex9I125 2P 32A ","Isolator, width 2 modules, 2-pole, 32A","NAH",12.68,0,12.68,8592765008695,6,18592765008692,72,28592765008699,"8536508090",0.18]
[100869,"Ex9I125 2P 40A ","Isolator, width 2 modules, 2-pole, 40A","NAH",15.16,0,15.16,8592765008701,6,18592765008708,72,28592765008705,"8536508090",0.18]
[100870,"Ex9I125 2P 63A ","Isolator, width 2 modules, 2-pole, 63A","NAH",15.8,0,15.8,8592765008718,6,18592765008715,72,28592765008712,"8536508090",0.18]
[100871,"Ex9I125 2P 80A ","Isolator, width 2 modules, 2-pole, 80A","NAH",20.059999999999999,0,20.059999999999999,8592765008725,6,18592765008722,72,28592765008729,"8536508090",0.18]
[100872,"Ex9I125 2P 100A ","Isolator, width 2 modules, 2-pole, 100A","NAH",23.69,0,23.69,8592765008732,6,18592765008739,72,28592765008736,"8536508090",0.18]
[100873,"Ex9I125 2P 125A ","Isolator, width 2 modules, 2-pole, 125A","NAH",25.39,0,25.39,8592765008749,6,18592765008746,72,28592765008743,"8536508090",0.18]
[102308,"Ex9I125 3P 16A ","Isolator, width 3 modules, 3-pole, 16A","NAH",11.98,{"$f":"NAH","v":0},11.98,8592765023094,4,18592765023091,48,28592765023098,"8536508090",0.27]
[102309,"Ex9I125 3P 25A","Isolator, width 3 modules, 3-pole, 25A","NAH",12.13,0,12.13,8592765023100,4,18592765023107,48,28592765023104,"8536508090",0.27]
[100874,"Ex9I125 3P 32A ","Isolator, width 3 modules, 3-pole, 32A","NAH",12.36,0,12.36,8592765008756,4,18592765008753,48,28592765008750,"8536508090",0.27]
[100875,"Ex9I125 3P 40A","Isolator, width 3 modules, 3-pole, 40A","NAH",12.51,0,12.51,8592765008763,4,18592765008760,48,28592765008767,"8536508090",0.27]
[100876,"Ex9I125 3P 63A ","Isolator, width 3 modules, 3-pole, 63A","NAH",18.93,0,18.93,8592765008770,4,18592765008777,48,28592765008774,"8536508090",0.27]
[100877,"Ex9I125 3P 80A","Isolator, width 3 modules, 3-pole, 80A","NAH",21.66,0,21.66,8592765008787,4,18592765008784,48,28592765008781,"8536508090",0.27]
[100878,"Ex9I125 3P 100A ","Isolator, width 3 modules, 3-pole, 100A","NAH",33.54,0,33.54,8592765008794,4,18592765008791,48,28592765008798,"8536508090",0.27]
[100879,"Ex9I125 3P 125A ","Isolator, width 3 modules, 3-pole, 125A","NAH",35.56,0,35.56,8592765008800,4,18592765008807,48,28592765008804,"8536508090",0.27]
[102310,"Ex9I125 4P 16A ","Isolator, width 4 modules, 4-pole, 16A","NAH",26.03,{"$f":"NAH","v":0},26.03,8592765023117,3,18592765023114,36,28592765023111,"8536508090",0.36]
[102311,"Ex9I125 4P 25A","Isolator, width 4 modules, 4-pole, 25A","NAH",26.2,0,26.2,8592765023124,3,18592765023121,36,28592765023128,"8536508090",0.36]
[100880,"Ex9I125 4P 32A ","Isolator, width 4 modules, 4-pole, 32A","NAH",26.6,0,26.6,8592765008817,3,18592765008814,36,28592765008811,"8536508090",0.36]
[100881,"Ex9I125 4P 40A ","Isolator, width 4 modules, 4-pole, 40A","NAH",27.89,0,27.89,8592765008824,3,18592765008821,36,28592765008828,"8536508090",0.36]
[100882,"Ex9I125 4P 63A ","Isolator, width 4 modules, 4-pole, 63A","NAH",31.99,0,31.99,8592765008831,3,18592765008838,36,28592765008835,"8536508090",0.36]
[100883,"Ex9I125 4P 80A ","Isolator, width 4 modules, 4-pole, 80A","NAH",40.840000000000003,0,40.840000000000003,8592765008848,3,18592765008845,36,28592765008842,"8536508090",0.36]
[100884,"Ex9I125 4P 100A","Isolator, width 4 modules, 4-pole, 100A","NAH",47.44,0,47.44,8592765008855,3,18592765008852,36,28592765008859,"8536508090",0.36]
[100885,"Ex9I125 4P 125A","Isolator, width 4 modules, 4-pole, 125A","NAH",53.89,0,53.89,8592765008862,3,18592765008869,36,28592765008866,"8536508090",0.36]
[]
["Single-module Isolators Ex9I40"]
[102296,"Ex9I40 1P 16A","Isolator, width 1 module, 1-pole, 16A","NAH",5.44,{"$f":"NAH","v":0},{"$f":"E1948*(1-F1948)","v":5.44},8592765022974,12,18592765022971,144,28592765022978,"8536508090",0.06]
[102297,"Ex9I40 1P 25A ","Isolator, width 1 module, 1-pole, 25A","NAH",6.04,0,6.04,8592765022981,12,18592765022988,144,28592765022985,"8536508090",0.06]
[101387,"Ex9I40 1P 32A","Isolator, width 1 module, 1-pole, 32A","NAH",6.37,0,6.37,8592765013880,12,18592765013887,144,28592765013884,"8536508090",0.06]
[101388,"Ex9I40 1P 40A ","Isolator, width 1 module, 1-pole, 40A","NAH",8.26,0,8.26,8592765013897,12,18592765013894,144,28592765013891,"8536508090",0.06]
[102298,"Ex9I40 2P 16A ","Isolator, width 1 module, 2-pole, 16A","NAH",11.97,0,11.97,8592765022998,12,18592765022995,144,28592765022992,"8536508090",0.06]
[102299,"Ex9I40 2P 25A ","Isolator, width 1 module, 2-pole, 25A","NAH",12.79,0,12.79,8592765023001,12,18592765023008,144,28592765023005,"8536508090",0.06]
[101389,"Ex9I40 2P 32A ","Isolator, width 1 module, 2-pole, 32A","NAH",13.57,0,13.57,8592765013903,12,18592765013900,144,28592765013907,"8536508090",0.06]
[101390,"Ex9I40 2P 40A ","Isolator, width 1 module, 2-pole, 40A","NAH",16.14,0,16.14,8592765013910,12,18592765013917,144,28592765013914,"8536508090",0.06]
[102300,"Ex9I40 3P 16A ","Isolator, width 1 module, 3-pole, 16A","NAH",12.92,0,12.92,8592765023018,12,18592765023015,144,28592765023012,"8536508090",0.06]
[102301,"Ex9I40 3P 25A","Isolator, width 1 module, 3-pole, 25A","NAH",13.18,0,13.18,8592765023025,12,18592765023022,144,28592765023029,"8536508090",0.06]
[101391,"Ex9I40 3P 32A ","Isolator, width 1 module, 3-pole, 32A","NAH",13.41,0,13.41,8592765013927,12,18592765013924,144,28592765013921,"8536508090",0.06]
[101392,"Ex9I40 3P 40A","Isolator, width 1 module, 3-pole, 40A","NAH",13.57,0,13.57,8592765013934,12,18592765013931,144,28592765013938,"8536508090",0.06]
[102302,"Ex9I40 4P 16A ","Isolator, width 1 module, 4-pole, 16A","NAH",25.85,0,25.85,8592765023032,12,18592765023039,144,28592765023036,"8536508090",0.06]
[102303,"Ex9I40 4P 25A","Isolator, width 1 module, 4-pole, 25A","NAH",27.08,0,27.08,8592765023049,12,18592765023046,144,28592765023043,"8536508090",0.06]
[101393,"Ex9I40 4P 32A ","Isolator, width 1 module, 4-pole, 32A","NAH",28.54,0,28.54,8592765013941,12,18592765013948,144,28592765013945,"8536508090",0.06]
[101394,"Ex9I40 4P 40A","Isolator, width 1 module, 4-pole, 40A","NAH",30.18,0,30.18,8592765013958,12,18592765013955,144,28592765013952,"8536508090",0.06]
[]
["Modular Isolators Ex9BI, with possibility use of accessories"]
[102378,"Ex9BI 1P 16A","Isolator, width 1 module, 1-pole, 16A","NAH",5.71,{"$f":"NAH","v":0},{"$f":"E1966*(1-F1966)","v":5.71},8592765023797,12,18592765023794,144,28592765023791,"8536508090",0.09]
[102379,"Ex9BI 1P 25A","Isolator, width 1 module, 1-pole, 25A","NAH",6.33,0,6.33,8592765023803,12,18592765023800,144,28592765023807,"8536508090",0.09]
[102380,"Ex9BI 1P 32A","Isolator, width 1 module, 1-pole, 32A","NAH",6.7,0,6.7,8592765023810,12,18592765023817,144,28592765023814,"8536508090",0.09]
[102381,"Ex9BI 1P 40A","Isolator, width 1 module, 1-pole, 40A","NAH",8.66,0,8.66,8592765023827,12,18592765023824,144,28592765023821,"8536508090",0.09]
[102382,"Ex9BI 1P 63A","Isolator, width 1 module, 1-pole, 63A","NAH",9.67,0,9.67,8592765023834,12,18592765023831,144,28592765023838,"8536508090",0.09]
[102383,"Ex9BI 2P 16A","Isolator, width 2 modules, 2-pole, 16A","NAH",12.85,0,12.85,8592765023841,6,18592765023848,72,28592765023845,"8536508090",0.18]
[102384,"Ex9BI 2P 25A","Isolator, width 2 modules, 2-pole, 25A","NAH",13.07,0,13.07,8592765023858,6,18592765023855,72,28592765023852,"8536508090",0.18]
[102385,"Ex9BI 2P 32A","Isolator, width 2 modules, 2-pole, 32A","NAH",13.31,0,13.31,8592765023865,6,18592765023862,72,28592765023869,"8536508090",0.18]
[102386,"Ex9BI 2P 40A","Isolator, width 2 modules, 2-pole, 40A","NAH",15.93,0,15.93,8592765023872,6,18592765023879,72,28592765023876,"8536508090",0.18]
[102387,"Ex9BI 2P 63A","Isolator, width 2 modules, 2-pole, 63A","NAH",16.57,0,16.57,8592765023889,6,18592765023886,72,28592765023883,"8536508090",0.18]
[102388,"Ex9BI 3P 16A","Isolator, width 3 modules, 3-pole, 16A","NAH",12.58,0,12.58,8592765023896,4,18592765023893,48,28592765023890,"8536508090",0.27]
[102389,"Ex9BI 3P 25A","Isolator, width 3 modules, 3-pole, 25A","NAH",12.73,0,12.73,8592765023902,4,18592765023909,48,28592765023906,"8536508090",0.27]
[102390,"Ex9BI 3P 32A","Isolator, width 3 modules, 3-pole, 32A","NAH",12.97,0,12.97,8592765023919,4,18592765023916,48,28592765023913,"8536508090",0.27]
[102391,"Ex9BI 3P 40A","Isolator, width 3 modules, 3-pole, 40A","NAH",13.15,0,13.15,8592765023926,4,18592765023923,48,28592765023920,"8536508090",0.27]
[102392,"Ex9BI 3P 63A","Isolator, width 3 modules, 3-pole, 63A","NAH",19.87,0,19.87,8592765023933,4,18592765023930,48,28592765023937,"8536508090",0.27]
[102393,"Ex9BI 4P 16A","Isolator, width 4 modules, 4-pole, 16A","NAH",27.33,0,27.33,8592765023940,3,18592765023947,36,28592765023944,"8536508090",0.36]
[102394,"Ex9BI 4P 25A","Isolator, width 4 modules, 4-pole, 25A","NAH",27.5,0,27.5,8592765023957,3,18592765023954,36,28592765023951,"8536508090",0.36]
[102395,"Ex9BI 4P 32A","Isolator, width 4 modules, 4-pole, 32A","NAH",27.94,0,27.94,8592765023964,3,18592765023961,36,28592765023968,"8536508090",0.36]
[102396,"Ex9BI 4P 40A","Isolator, width 4 modules, 4-pole, 40A","NAH",29.29,0,29.29,8592765023971,3,18592765023978,36,28592765023975,"8536508090",0.36]
[102397,"Ex9BI 4P 63A","Isolator, width 4 modules, 4-pole, 63A","NAH",33.590000000000003,0,33.590000000000003,8592765023988,3,18592765023985,36,28592765023982,"8536508090",0.36]
[]
["Digital Timers Ex9TD"]
[110554,"Ex9DTS 1CO 230V","Instalation Timer Digital, weekly and daily program, 1channels with CO contact, Voltage 230V","NAX",127.62,{"$f":"NAX","v":0},{"$f":"E1988*(1-F1988)","v":127.62},8592765105547,1,8592765105547,1,null,"9107000090",0.13]
[110555,"Ex9DTS 2CO 230V","Instalation Timer Digital, weekly and daily program, 2channels with CO contact, Voltage 230V","NAX",149.15,0,{"$f":"E1989*(1-F1989)","v":149.15},8592765105554,1,8592765105554,1,null,"9107000090",0.14299999999999999]
[110556,"Ex9DTSC 1CO 230V","Instalation Timer Digital, yearly, monthly, weekly and daily program, Comfort functions, 1channel with CO contact, Voltage 230V","NAX",188.7,0,188.7,8592765105561,1,8592765105561,1,null,"9107000090",0.14299999999999999]
[110557,"Ex9DTSC 2CO 230V","Instalation Timer Digital, yearly, monthly, weekly and daily program, Comfort functions, 2channels with CO contact, Voltage 230V","NAX",225.19,0,225.19,8592765105578,1,8592765105578,1,null,"9107000090",0.14299999999999999]
[]
["Analogue Timers Ex9TA"]
[103514,"Ex9TAMS 1NO 230V","Instalation Timer Analogue, Mini, daily program, Synchronouos, 1channel with NO contact, Voltage 230V","NAX",59.13,{"$f":"NAX","v":0},{"$f":"E1994*(1-F1994)","v":59.13},8592765035158,1,8592765035158,null,28592765035152,"9107000090",0.1]
[103515,"Ex9TAMQ 1NO 230V","Instalation Timer Analogue, Mini, daily program, Quartz, 1channel with NO contact, Voltage 230V","NAX",82.4,0,82.4,8592765035165,1,8592765035165,null,28592765035169,"9107000090",0.11]
[103516,"Ex9TAQ 1CO 230V","Instalation Timer Analogue, daily program, Quartz, 1channel with CO contact, Voltage 230V","NAX",90.69,0,90.69,8592765035172,1,8592765035172,null,28592765035176,"9107000090","0.18"]
[]
["Instalation Staircase Switch Ex9SS"]
[110558,"Ex9SSB 230V","Instalation Staircase Switch, Basic functions, Voltage 230V","NAX",66.19,{"$f":"NAX","v":0},{"$f":"E1999*(1-F1999)","v":66.19},8592765105585,1,8592765105585,1,null,"9107000090",6.2E-2]
[110559,"Ex9SSP 230V","Instalation Staircase Switch, Programable functions, Voltage 230V","NAX",96,{"$f":"NAX","v":0},96,8592765105592,1,8592765105592,1,null,"9107000090",6.5000000000000002E-2]
[]
["Light intensity switches Ex9L"]
[110560,"Ex9LAS 1CO 230V","Installation Light intensity switch, Analogue, 1channel with CO contact, Voltage 230V","NAX",108.98,{"$f":"NAX","v":0},{"$f":"E2003*(1-F2003)","v":108.98},8592765105608,1,8592765105608,1,null,"9107000090",7.4999999999999997E-2]
[110561,"Ex9LDS 1CO 230V","Installation Light intensity switch, Digital, 1channel with CO contacts, Voltage 230V","NAX",234.81,{"$f":"NAX","v":0},{"$f":"E2004*(1-F2004)","v":234.81},8592765105615,1,8592765105615,1,null,"9107000090",0.127]
[]
["Change-over switches Ex9BT"]
[102656,"Ex9BT2 10 16A","Change-over switch, 16 A, 1 NO contact","NAU",8.77,{"$f":"NAU","v":0},{"$f":"E2007*(1-F2007)","v":8.77},8592765026576,12,18592765026573,144,28592765026570,"8536508090",1.02]
[102657,"Ex9BT2 20 16A","Change-over switch, 16 A, 2 NO contacts","NAU",12.18,{"$f":"NAU","v":0},12.18,8592765026583,12,18592765026580,144,28592765026587,"8536508090",1.02]
[102658,"Ex9BT2 30 16A","Change-over switch, 16 A, 3 NO contacts","NAU",19.41,0,19.41,8592765026590,12,18592765026597,144,28592765026594,"8536508090",1.02]
[102659,"Ex9BT2 40 16A","Change-over switch, 16 A, 4 NO contacts","NAU",23.75,0,23.75,8592765026606,12,18592765026603,144,28592765026600,"8536508090",1.02]
[102660,"Ex9BT2 01 16A","Change-over switch, 16 A, 1 NC contact","NAU",8.77,0,8.77,8592765026613,12,18592765026610,144,28592765026617,"8536508090",1.02]
[102661,"Ex9BT2 02 16A","Change-over switch, 16 A, 2 NC, contacts","NAU",12.18,0,12.18,8592765026620,12,18592765026627,144,28592765026624,"8536508090",1.02]
[102662,"Ex9BT2 03 16A","Change-over switch, 16 A, 3 NC contacts","NAU",19.41,0,19.41,8592765026637,12,18592765026634,144,28592765026631,"8536508090",1.02]
[102663,"Ex9BT2 04 16A","Change-over switch, 16 A, 4 NC contacts","NAU",23.75,0,23.75,8592765026644,12,18592765026641,144,28592765026648,"8536508090",1.02]
[102664,"Ex9BT2 11 16A","Change-over switch, 16 A, 1 NO + 1 NC contact","NAU",12.08,0,12.08,8592765026651,12,18592765026658,144,28592765026655,"8536508090",1.02]
[102665,"Ex9BT2 22 16A","Change-over switch, 16 A, 2 NO + 2 NC contacts","NAU",27.91,0,27.91,8592765026668,12,18592765026665,144,28592765026662,"8536508090",1.02]
[102666,"Ex9BT2 13 16A","Change-over switch, 16 A, 1 NO + 3 NC contacts","NAU",27.91,0,27.91,8592765026675,12,18592765026672,144,28592765026679,"8536508090",1.02]
[102667,"Ex9BT2 31 16A","Change-over switch, 16 A, 3 NO + 1 NC contacts","NAU",28.34,0,28.34,8592765026682,12,18592765026689,144,28592765026686,"8536508090",1.02]
[102668,"Ex9BT2 1CO 16A","Change-over switch, 16 A, 1 CO contact","NAU",11.45,0,11.45,8592765026699,12,18592765026696,144,28592765026693,"8536508090",1.02]
[102669,"Ex9BT2 2CO 16A","Change-over switch, 16 A, 2 CO contacts","NAU",25.18,0,25.18,8592765026705,6,18592765026702,72,28592765026709,"8536508090",1.02]
[102670,"Ex9BT2 20 32A","Change-over switch, 32 A, 2 NO contacts","NAU",18.170000000000002,0,18.170000000000002,8592765026712,6,18592765026719,72,28592765026716,"8536508090",1.02]
[102671,"Ex9BT2 40 32A","Change-over switch, 32 A, 4 NO contacts","NAU",28.51,0,28.51,8592765026729,6,18592765026726,72,28592765026723,"8536508090",1.02]
[102672,"Ex9BT2 02 32A","Change-over switch, 32 A, 2 NC, contacts","NAU",18.170000000000002,0,18.170000000000002,8592765026736,6,18592765026733,72,28592765026730,"8536508090",1.02]
[102673,"Ex9BT2 04 32A","Change-over switch, 32 A, 4 NC contacts","NAU",28.51,0,28.51,8592765026743,6,18592765026740,72,28592765026747,"8536508090",1.02]
[102674,"Ex9BT2 20 16A LED230VAC/DC","Change-over switch, 16 A, 2 NO contacts, with LED 230 V AC/DC","NAU",19.12,0,19.12,8592765026750,6,18592765026757,72,28592765026754,"8536508090",0.92]
[102675,"Ex9BT2 20 16A LED48VAC/DC","Change-over switch, 16 A, 2 NO contacts, with LED 48 V AC/DC","NAU",19.12,0,19.12,8592765026767,6,18592765026764,72,28592765026761,"8536508090",0.92]
[102676,"Ex9BT2 02 16A LED230VAC/DC","Change-over switch, 16 A, 2 NC, contacts, with LED 230 V AC/DC","NAU",19.12,0,19.12,8592765026774,6,18592765026771,72,28592765026778,"8536508090",0.92]
[102677,"Ex9BT2 02 16A LED48VAC/DC","Change-over switch, 16 A, 2 NC, contacts, with LED 48 V AC/DC","NAU",19.12,0,19.12,8592765026781,6,18592765026788,72,28592765026785,"8536508090",0.92]
[102678,"Ex9BT2 1CO 16A LED230VAC/DC","Change-over switch, 16 A, 1 CO contact, with LED 230 V AC/DC","NAU",19.38,0,19.38,8592765026798,6,18592765026795,72,28592765026792,"8536508090",0.92]
[102679,"Ex9BT2 1CO 16A LED48VAC/DC","Change-over switch, 16 A, 1 CO contact, with LED 48 V AC/DC","NAU",19.38,0,19.38,8592765026804,6,18592765026801,72,28592765026808,"8536508090",0.92]
[102680,"Ex9BT3 1CO 16A","3-position change-over switch (I-0-II), 16 A, 1 CO contact","NAU",21.32,{"$f":"NAU","v":0},{"$f":"E2031*(1-F2031)","v":21.32},8592765026811,12,18592765026818,144,28592765026815,"8536508090",0.09]
[102681,"Ex9BT3 1CO 32A","3-position change-over switch (I-0-II), 32 A, 1 CO contact","NAU",25.59,{"$f":"NAU","v":0},{"$f":"E2032*(1-F2032)","v":25.59},8592765026828,12,18592765026825,144,28592765026822,"8536508090",0.09]
[102682,"Ex9BT3 2CO 16A","3-position change-over switch (I-0-II), 16 A, 2 CO contacts","NAU",27.4,0,27.4,8592765026835,12,18592765026832,144,28592765026839,"8536508090",0.09]
[102683,"Ex9BT3 2CO 32A","3-position change-over switch (I-0-II), 32 A, 2 CO contacts","NAU",32.89,0,32.89,8592765026842,12,18592765026849,144,28592765026846,"8536508090",0.09]
[]
["Signal Lamps Ex9PD, Ex9PDe"]
[102429,"Ex9PD1r 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 red LED","NAU",9.81,{"$f":"NAU","v":0},{"$f":"E2037*(1-F2037)","v":9.81},8592765024305,2,18592765024302,162,28592765024309,"8531807000",0.09]
[102430,"Ex9PD1r 12V AC/DC","Signal lamp, 12V AC/DC, 1 red LED","NAU",9.81,0,{"$f":"E2038*(1-F2038)","v":9.81},8592765024312,2,18592765024319,162,28592765024316,"8531807000",0.09]
[102431,"Ex9PD1r 24V AC/DC","Signal lamp, 24V AC/DC, 1 red LED","NAU",9.81,0,9.81,8592765024329,2,18592765024326,162,28592765024323,"8531807000",0.09]
[102432,"Ex9PD1r 110V AC/DC","Signal lamp, 110V AC/DC, 1 red LED","NAU",9.81,0,9.81,8592765024336,2,18592765024333,162,28592765024330,"8531807000",0.09]
[102433,"Ex9PD1r 230V AC/DC","Signal lamp, 230V AC/DC, 1 red LED","NAU",9.81,0,9.81,8592765024343,2,18592765024340,162,28592765024347,"8531807000",0.09]
[102434,"Ex9PD1y 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 yellow LED","NAU",9.81,0,9.81,8592765024350,2,18592765024357,162,28592765024354,"8531807000",0.09]
[102435,"Ex9PD1y 12V AC/DC","Signal lamp, 12V AC/DC, 1 yellow LED","NAU",9.81,0,9.81,8592765024367,2,18592765024364,162,28592765024361,"8531807000",0.09]
[102436,"Ex9PD1y 24V AC/DC","Signal lamp, 24V AC/DC, 1 yellow LED","NAU",9.81,0,9.81,8592765024374,2,18592765024371,162,28592765024378,"8531807000",0.09]
[102437,"Ex9PD1y 110V AC/DC","Signal lamp, 110V AC/DC, 1 yellow LED","NAU",9.81,0,9.81,8592765024381,2,18592765024388,162,28592765024385,"8531807000",0.09]
[102438,"Ex9PD1y 230V AC/DC","Signal lamp, 230V AC/DC, 1 yellow LED","NAU",9.81,0,9.81,8592765024398,2,18592765024395,162,28592765024392,"8531807000",0.09]
[102439,"Ex9PD1g 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 green LED","NAU",9.81,0,9.81,8592765024404,2,18592765024401,162,28592765024408,"8531807000",0.09]
[102440,"Ex9PD1g 12V AC/DC","Signal lamp, 12V AC/DC, 1 green LED","NAU",9.81,0,9.81,8592765024411,2,18592765024418,162,28592765024415,"8531807000",0.09]
[102441,"Ex9PD1g 24V AC/DC","Signal lamp, 24V AC/DC, 1 green LED","NAU",9.81,0,9.81,8592765024428,2,18592765024425,162,28592765024422,"8531807000",0.09]
[102442,"Ex9PD1g 110V AC/DC","Signal lamp, 110V AC/DC, 1 green LED","NAU",9.81,0,9.81,8592765024435,2,18592765024432,162,28592765024439,"8531807000",0.09]
[102443,"Ex9PD1g 230V AC/DC","Signal lamp, 230V AC/DC, 1 green LED","NAU",9.81,0,9.81,8592765024442,2,18592765024449,162,28592765024446,"8531807000",0.09]
[102444,"Ex9PD1b 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 blue LED","NAU",9.81,0,9.81,8592765024459,2,18592765024456,162,28592765024453,"8531807000",0.09]
[102445,"Ex9PD1b 12V AC/DC","Signal lamp, 12V AC/DC, 1 blue LED","NAU",9.81,0,9.81,8592765024466,2,18592765024463,162,28592765024460,"8531807000",0.09]
[102446,"Ex9PD1b 24V AC/DC","Signal lamp, 24V AC/DC, 1 blue LED","NAU",9.81,0,9.81,8592765024473,2,18592765024470,162,28592765024477,"8531807000",0.09]
[102447,"Ex9PD1b 110V AC/DC","Signal lamp, 110V AC/DC, 1 blue LED","NAU",9.81,0,9.81,8592765024480,2,18592765024487,162,28592765024484,"8531807000",0.09]
[102448,"Ex9PD1b 230V AC/DC","Signal lamp, 230V AC/DC, 1 blue LED","NAU",9.81,0,9.81,8592765024497,2,18592765024494,162,28592765024491,"8531807000",0.09]
[102449,"Ex9PD1w 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 white LED","NAU",9.81,0,9.81,8592765024503,2,18592765024500,162,28592765024507,"8531807000",0.09]
[102450,"Ex9PD1w 12V AC/DC","Signal lamp, 12V AC/DC, 1 white LED","NAU",9.81,0,9.81,8592765024510,2,18592765024517,162,28592765024514,"8531807000",0.09]
[102451,"Ex9PD1w 24V AC/DC","Signal lamp, 24V AC/DC, 1 white LED","NAU",9.81,0,9.81,8592765024527,2,18592765024524,162,28592765024521,"8531807000",0.09]
[102452,"Ex9PD1w 110V AC/DC","Signal lamp, 110V AC/DC, 1 white LED","NAU",9.81,0,9.81,8592765024534,2,18592765024531,162,28592765024538,"8531807000",0.09]
[102453,"Ex9PD1w 230V AC/DC","Signal lamp, 230V AC/DC, 1 white LED","NAU",9.81,0,9.81,8592765024541,2,18592765024548,162,28592765024545,"8531807000",0.09]
[102454,"Ex9PD2gg 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 2 green LED ","NAU",20.239999999999998,0,20.239999999999998,8592765024558,2,18592765024555,162,28592765024552,"8531807000",0.1]
[102455,"Ex9PD2gg 12V AC/DC","Signal lamp, 12V AC/DC, 2 green LED ","NAU",20.239999999999998,0,20.239999999999998,8592765024565,2,18592765024562,162,28592765024569,"8531807000",0.1]
[102456,"Ex9PD2gg 24V AC/DC","Signal lamp, 24V AC/DC, 2 green LED ","NAU",20.239999999999998,0,20.239999999999998,8592765024572,2,18592765024579,162,28592765024576,"8531807000",0.1]
[102457,"Ex9PD2gg 110V AC/DC","Signal lamp, 110V AC/DC, 2 green LED ","NAU",20.239999999999998,0,20.239999999999998,8592765024589,2,18592765024586,162,28592765024583,"8531807000",0.1]
[102458,"Ex9PD2gg 230V AC/DC","Signal lamp, 230V AC/DC, 2 green LED ","NAU",20.239999999999998,0,20.239999999999998,8592765024596,2,18592765024593,162,28592765024590,"8531807000",0.1]
[102459,"Ex9PD2gr 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 green LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024602,2,18592765024609,162,28592765024606,"8531807000",0.1]
[102460,"Ex9PD2gr 12V AC/DC","Signal lamp, 12V AC/DC, 1 green LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024619,2,18592765024616,162,28592765024613,"8531807000",0.1]
[102461,"Ex9PD2gr 24V AC/DC","Signal lamp, 24V AC/DC, 1 green LED and 1 red  LED","NAU",20.239999999999998,{"$f":"NAU","v":0},20.239999999999998,8592765024626,2,18592765024623,162,28592765024620,"8531807000",0.1]
[102462,"Ex9PD2gr 110V AC/DC","Signal lamp, 110V AC/DC, 1 green LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024633,2,18592765024630,162,28592765024637,"8531807000",0.1]
[102463,"Ex9PD2gr 230V AC/DC","Signal lamp, 230V AC/DC, 1 green LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024640,2,18592765024647,162,28592765024644,"8531807000",0.1]
[102464,"Ex9PD2gy 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 green LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024657,2,18592765024654,162,28592765024651,"8531807000",0.1]
[102465,"Ex9PD2gy 12V AC/DC","Signal lamp, 12V AC/DC, 1 green LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024664,2,18592765024661,162,28592765024668,"8531807000",0.1]
[102466,"Ex9PD2gy 24V AC/DC","Signal lamp, 24V AC/DC, 1 green LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024671,2,18592765024678,162,28592765024675,"8531807000",0.1]
[102467,"Ex9PD2gy 110V AC/DC","Signal lamp, 110V AC/DC, 1 green LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024688,2,18592765024685,162,28592765024682,"8531807000",0.1]
[102468,"Ex9PD2gy 230V AC/DC","Signal lamp, 230V AC/DC, 1 green LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024695,2,18592765024692,162,28592765024699,"8531807000",0.1]
[102469,"Ex9PD2gb 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 green LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024701,2,18592765024708,162,28592765024705,"8531807000",0.1]
[102470,"Ex9PD2gb 12V AC/DC","Signal lamp, 12V AC/DC, 1 green LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024718,2,18592765024715,162,28592765024712,"8531807000",0.1]
[102471,"Ex9PD2gb 24V AC/DC","Signal lamp, 24V AC/DC, 1 green LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024725,2,18592765024722,162,28592765024729,"8531807000",0.1]
[102472,"Ex9PD2gb 110V AC/DC","Signal lamp, 110V AC/DC, 1 green LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024732,2,18592765024739,162,28592765024736,"8531807000",0.1]
[102473,"Ex9PD2gb 230V AC/DC","Signal lamp, 230V AC/DC, 1 green LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024749,2,18592765024746,162,28592765024743,"8531807000",0.1]
[102474,"Ex9PD2gw 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 green LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024756,2,18592765024753,162,28592765024750,"8531807000",0.1]
[102475,"Ex9PD2gw 12V AC/DC","Signal lamp, 12V AC/DC, 1 green LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024763,2,18592765024760,162,28592765024767,"8531807000",0.1]
[102476,"Ex9PD2gw 24V AC/DC","Signal lamp, 24V AC/DC, 1 green LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024770,2,18592765024777,162,28592765024774,"8531807000",0.1]
[102477,"Ex9PD2gw 110V AC/DC","Signal lamp, 110V AC/DC, 1 green LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024787,2,18592765024784,162,28592765024781,"8531807000",0.1]
[102478,"Ex9PD2gw 230V AC/DC","Signal lamp, 230V AC/DC, 1 green LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024794,2,18592765024791,162,28592765024798,"8531807000",0.1]
[102479,"Ex9PD2rr 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 red LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024800,2,18592765024807,162,28592765024804,"8531807000",0.1]
[102480,"Ex9PD2rr 12V AC/DC","Signal lamp, 12V AC/DC, 1 red LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024817,2,18592765024814,162,28592765024811,"8531807000",0.1]
[102481,"Ex9PD2rr 24V AC/DC","Signal lamp, 24V AC/DC, 1 red LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024824,2,18592765024821,162,28592765024828,"8531807000",0.1]
[102482,"Ex9PD2rr 110V AC/DC","Signal lamp, 110V AC/DC, 1 red LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024831,2,18592765024838,162,28592765024835,"8531807000",0.1]
[102483,"Ex9PD2rr 230V AC/DC","Signal lamp, 230V AC/DC, 1 red LED and 1 red  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024848,2,18592765024845,162,28592765024842,"8531807000",0.1]
[102484,"Ex9PD2ry 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 red LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024855,2,18592765024852,162,28592765024859,"8531807000",0.1]
[102485,"Ex9PD2ry 12V AC/DC","Signal lamp, 12V AC/DC, 1 red LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024862,2,18592765024869,162,28592765024866,"8531807000",0.1]
[102486,"Ex9PD2ry 24V AC/DC","Signal lamp, 24V AC/DC, 1 red LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024879,2,18592765024876,162,28592765024873,"8531807000",0.1]
[102487,"Ex9PD2ry 110V AC/DC","Signal lamp, 110V AC/DC, 1 red LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024886,2,18592765024883,162,28592765024880,"8531807000",0.1]
[102488,"Ex9PD2ry 230V AC/DC","Signal lamp, 230V AC/DC, 1 red LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024893,2,18592765024890,162,28592765024897,"8531807000",0.1]
[102489,"Ex9PD2rb 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 red LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024909,2,18592765024906,162,28592765024903,"8531807000",0.1]
[102490,"Ex9PD2rb 12V AC/DC","Signal lamp, 12V AC/DC, 1 red LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024916,2,18592765024913,162,28592765024910,"8531807000",0.1]
[102491,"Ex9PD2rb 24V AC/DC","Signal lamp, 24V AC/DC, 1 red LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024923,2,18592765024920,162,28592765024927,"8531807000",0.1]
[102492,"Ex9PD2rb 110V AC/DC","Signal lamp, 110V AC/DC, 1 red LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024930,2,18592765024937,162,28592765024934,"8531807000",0.1]
[102493,"Ex9PD2rb 230V AC/DC","Signal lamp, 230V AC/DC, 1 red LED and 1 blue  LED","NAU",20.239999999999998,{"$f":"NAU","v":0},20.239999999999998,8592765024947,2,18592765024944,162,28592765024941,"8531807000",0.1]
[102494,"Ex9PD2rw 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 red LED and 1 white  LED","NAU",20.239999999999998,0,{"$f":"E2102*(1-F2102)","v":20.239999999999998},8592765024954,2,18592765024951,162,28592765024958,"8531807000",0.1]
[102495,"Ex9PD2rw 12V AC/DC","Signal lamp, 12V AC/DC, 1 red LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024961,2,18592765024968,162,28592765024965,"8531807000",0.1]
[102496,"Ex9PD2rw 24V AC/DC","Signal lamp, 24V AC/DC, 1 red LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024978,2,18592765024975,162,28592765024972,"8531807000",0.1]
[102497,"Ex9PD2rw 110V AC/DC","Signal lamp, 110V AC/DC, 1 red LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024985,2,18592765024982,162,28592765024989,"8531807000",0.1]
[102498,"Ex9PD2rw 230V AC/DC","Signal lamp, 230V AC/DC, 1 red LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765024992,2,18592765024999,162,28592765024996,"8531807000",0.1]
[102499,"Ex9PD2yy 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 yellow LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025005,2,18592765025002,162,28592765025009,"8531807000",0.1]
[102500,"Ex9PD2yy 12V AC/DC","Signal lamp, 12V AC/DC, 1 yellow LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025012,2,18592765025019,162,28592765025016,"8531807000",0.1]
[102501,"Ex9PD2yy 24V AC/DC","Signal lamp, 24V AC/DC, 1 yellow LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025029,2,18592765025026,162,28592765025023,"8531807000",0.1]
[102502,"Ex9PD2yy 110V AC/DC","Signal lamp, 110V AC/DC, 1 yellow LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025036,2,18592765025033,162,28592765025030,"8531807000",0.1]
[102503,"Ex9PD2yy 230V AC/DC","Signal lamp, 230V AC/DC, 1 yellow LED and 1 yellow  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025043,2,18592765025040,162,28592765025047,"8531807000",0.1]
[102504,"Ex9PD2yb 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 yellow LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025050,2,18592765025057,162,28592765025054,"8531807000",0.1]
[102505,"Ex9PD2yb 12V AC/DC","Signal lamp, 12V AC/DC, 1 yellow LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025067,2,18592765025064,162,28592765025061,"8531807000",0.1]
[102506,"Ex9PD2yb 24V AC/DC","Signal lamp, 24V AC/DC, 1 yellow LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025074,2,18592765025071,162,28592765025078,"8531807000",0.1]
[102507,"Ex9PD2yb 110V AC/DC","Signal lamp, 110V AC/DC, 1 yellow LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025081,2,18592765025088,162,28592765025085,"8531807000",0.1]
[102508,"Ex9PD2yb 230V AC/DC","Signal lamp, 230V AC/DC, 1 yellow LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025098,2,18592765025095,162,28592765025092,"8531807000",0.1]
[102509,"Ex9PD2yw 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 yellow LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025104,2,18592765025101,162,28592765025108,"8531807000",0.1]
[102510,"Ex9PD2yw 12V AC/DC","Signal lamp, 12V AC/DC, 1 yellow LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025111,2,18592765025118,162,28592765025115,"8531807000",0.1]
[102511,"Ex9PD2yw 24V AC/DC","Signal lamp, 24V AC/DC, 1 yellow LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025128,2,18592765025125,162,28592765025122,"8531807000",0.1]
[102512,"Ex9PD2yw 110V AC/DC","Signal lamp, 110V AC/DC, 1 yellow LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025135,2,18592765025132,162,28592765025139,"8531807000",0.1]
[102513,"Ex9PD2yw 230V AC/DC","Signal lamp, 230V AC/DC, 1 yellow LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025142,2,18592765025149,162,28592765025146,"8531807000",0.1]
[102514,"Ex9PD2bb 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 blue LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025159,2,18592765025156,162,28592765025153,"8531807000",0.1]
[102515,"Ex9PD2bb 12V AC/DC","Signal lamp, 12V AC/DC, 1 blue LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025166,2,18592765025163,162,28592765025160,"8531807000",0.1]
[102516,"Ex9PD2bb 24V AC/DC","Signal lamp, 24V AC/DC, 1 blue LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025173,2,18592765025170,162,28592765025177,"8531807000",0.1]
[102517,"Ex9PD2bb 110V AC/DC","Signal lamp, 110V AC/DC, 1 blue LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025180,2,18592765025187,162,28592765025184,"8531807000",0.1]
[102518,"Ex9PD2bb 230V AC/DC","Signal lamp, 230V AC/DC, 1 blue LED and 1 blue  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025197,2,18592765025194,162,28592765025191,"8531807000",0.1]
[102519,"Ex9PD2bw 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 blue LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025203,2,18592765025200,162,28592765025207,"8531807000",0.1]
[102520,"Ex9PD2bw 12V AC/DC","Signal lamp, 12V AC/DC, 1 blue LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025210,2,18592765025217,162,28592765025214,"8531807000",0.1]
[102521,"Ex9PD2bw 24V AC/DC","Signal lamp, 24V AC/DC, 1 blue LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025227,2,18592765025224,162,28592765025221,"8531807000",0.1]
[102522,"Ex9PD2bw 110V AC/DC","Signal lamp, 110V AC/DC, 1 blue LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025234,2,18592765025231,162,28592765025238,"8531807000",0.1]
[102523,"Ex9PD2bw 230V AC/DC","Signal lamp, 230V AC/DC, 1 blue LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025241,2,18592765025248,162,28592765025245,"8531807000",0.1]
[102524,"Ex9PD2ww 6.3V AC/DC","Signal lamp, 6,3V AC/DC, 1 white LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025258,2,18592765025255,162,28592765025252,"8531807000",0.1]
[102525,"Ex9PD2ww 12V AC/DC","Signal lamp, 12V AC/DC, 1 white LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025265,2,18592765025262,162,28592765025269,"8531807000",0.1]
[102526,"Ex9PD2ww 24V AC/DC","Signal lamp, 24V AC/DC, 1 white LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025272,2,18592765025279,162,28592765025276,"8531807000",0.1]
[102527,"Ex9PD2ww 110V AC/DC","Signal lamp, 110V AC/DC, 1 white LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025289,2,18592765025286,162,28592765025283,"8531807000",0.1]
[102528,"Ex9PD2ww 230V AC/DC","Signal lamp, 230V AC/DC, 1 white LED and 1 white  LED","NAU",20.239999999999998,0,20.239999999999998,8592765025296,2,18592765025293,162,28592765025290,"8531807000",0.1]
[106307,"Ex9PD1e 24V AC/DC","Signal lamp, 24V AC/DC, 1 dual-color LED, red/green","NAU",20.39,{"$f":"NAU","v":0},20.39,8592765063083,2,18592765063080,162,28592765063087,"8531807000",0.1]
[106308,"Ex9PD1e 48V AC/DC","Signal lamp, 48V AC/DC, 1 dual-color LED, red/green","NAU",20.39,{"$f":"NAU","v":0},20.39,8592765063090,2,18592765063097,162,28592765063094,"8531807000",0.1]
[106309,"Ex9PD1e 230V AC/DC","Signal lamp, 230V AC/DC, 1 dual-color LED, red/green","NAU",20.39,0,20.39,8592765063106,2,18592765063103,162,28592765063100,"8531807000",0.1]
[106310,"Ex9PD2e 24V AC/DC","Signal lamp, 24V AC/DC, 2 dual-color LEDs, red/green","NAU",31.43,0,31.43,8592765063113,2,18592765063110,162,28592765063117,"8531807000",0.1]
[106311,"Ex9PD2e 48V AC/DC","Signal lamp, 48V AC/DC, 2 dual-color LEDs, red/green","NAU",31.43,0,31.43,8592765063120,2,18592765063127,162,28592765063124,"8531807000",0.1]
[106312,"Ex9PD2e 230V AC/DC","Signal lamp, 230V AC/DC, 2 dual-color LEDs, red/green","NAU",31.43,0,31.43,8592765063137,2,18592765063134,162,28592765063131,"8531807000",0.1]
[106313,"Ex9PD3e 230/400V AC/DC","Signal lamp, 230/400V AC/DC, 3 red LEDs","NAU",33.11,0,33.11,8592765063144,2,18592765063141,162,28592765063148,"8531807000",0.1]
[]
["Din-rail bell, Ex9HB "]
[111415,"Ex9HB AC12V","DIN Rail Bell AC12V","NAU",7.14,{"$f":"NAU","v":0},{"$f":"E2146*(1-F2146)","v":7.14},8592765114150,12,18592765114157,192,28592765114154,8531804090,7.1999999999999995E-2]
[111416,"Ex9HB AC230V ","DIN Rail Bell AC230V","NAU",7.43,{"$f":"NAU","v":0},{"$f":"E2147*(1-F2147)","v":7.43},8592765114167,12,18592765114164,192,28592765114161,8531804090,6.9000000000000006E-2]
[]
["Moulded Case Circuit Breakers Ex9M"]
[100886,"Ex9M1S TM AC16 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=16A, 3-pole","NCA",106.4,{"$f":"NCA","v":0},{"$f":"E2150*(1-F2150)","v":106.4},8592765008879,1,8592765008879,8,28592765008873,"8536201090",1.2]
[100887,"Ex9M1S TM AC20 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=20A, 3-pole","NCA",106.4,0,106.4,8592765008886,1,8592765008886,8,28592765008880,"8536201090",1.2]
[100888,"Ex9M1S TM AC25 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=25A, 3-pole","NCA",106.4,0,106.4,8592765008893,1,8592765008893,8,28592765008897,"8536201090",1.2]
[100889,"Ex9M1S TM AC32 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=32A, 3-pole","NCA",106.4,0,106.4,8592765008909,1,8592765008909,8,28592765008903,"8536201090",1.2]
[100890,"Ex9M1S TM AC40 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=40A, 3-pole","NCA",95.91,0,95.91,8592765008916,1,8592765008916,8,28592765008910,"8536201090",1.2]
[100891,"Ex9M1S TM AC50 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=50A, 3-pole","NCA",106.4,0,106.4,8592765008923,1,8592765008923,8,28592765008927,"8536201090",1.2]
[100892,"Ex9M1S TM AC63 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=63A, 3-pole","NCA",100.75,0,100.75,8592765008930,1,8592765008930,8,28592765008934,"8536201090",1.2]
[100893,"Ex9M1S TM AC80 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=80A, 3-pole","NCA",107.11,0,107.11,8592765008947,1,8592765008947,8,28592765008941,"8536209090",1.2]
[100894,"Ex9M1S TM AC100 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=100A, 3-pole","NCA",110.81,0,110.81,8592765008954,1,8592765008954,8,28592765008958,"8536209090",1.2]
[100895,"Ex9M1S TM AC125 3P","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=125A, 3-pole","NCA",111.8,0,111.8,8592765008961,1,8592765008961,8,28592765008965,"8536209090",1.2]
[100896,"Ex9M1N TM AC16 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=16A, 3-pole","NCA",167.1,0,167.1,8592765008978,1,8592765008978,8,28592765008972,"8536201090",1.2]
[100897,"Ex9M1N TM AC20 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=20A, 3-pole","NCA",167.1,0,167.1,8592765008985,1,8592765008985,8,28592765008989,"8536201090",1.2]
[100898,"Ex9M1N TM AC25 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=25A, 3-pole","NCA",167.1,0,167.1,8592765008992,1,8592765008992,8,28592765008996,"8536201090",1.2]
[100899,"Ex9M1N TM AC32 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=32A, 3-pole","NCA",167.1,0,167.1,8592765009005,1,8592765009005,8,28592765009009,"8536201090",1.2]
[100900,"Ex9M1N TM AC40 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=40A, 3-pole","NCA",167.1,0,167.1,8592765009012,1,8592765009012,8,28592765009016,"8536201090",1.2]
[100901,"Ex9M1N TM AC50 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=50A, 3-pole","NCA",167.1,0,167.1,8592765009029,1,8592765009029,8,28592765009023,"8536201090",1.2]
[100902,"Ex9M1N TM AC63 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=63A, 3-pole","NCA",197.22,0,197.22,8592765009036,1,8592765009036,8,28592765009030,"8536201090",1.2]
[100903,"Ex9M1N TM AC80 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=80A, 3-pole","NCA",197.22,0,197.22,8592765009043,1,8592765009043,8,28592765009047,"8536209090",1.2]
[100904,"Ex9M1N TM AC100 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=100A, 3-pole","NCA",202.54,0,202.54,8592765009050,1,8592765009050,8,28592765009054,"8536209090",1.2]
[100905,"Ex9M1N TM AC125 3P","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=125A, 3-pole","NCA",371.24,0,371.24,8592765009067,1,8592765009067,8,28592765009061,"8536209090",1.2]
[100926,"Ex9M1H TM AC16 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=16A, 3-pole","NCA",198.88,0,198.88,8592765009272,1,8592765009272,8,28592765009276,"8536201090",1.2]
[100927,"Ex9M1H TM AC20 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=20A, 3-pole","NCA",198.88,0,198.88,8592765009289,1,8592765009289,8,28592765009283,"8536201090",1.2]
[100928,"Ex9M1H TM AC25 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=25A, 3-pole","NCA",198.88,0,198.88,8592765009296,1,8592765009296,8,28592765009290,"8536201090",1.2]
[100929,"Ex9M1H TM AC32 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=32A, 3-pole","NCA",198.88,0,198.88,8592765009302,1,8592765009302,8,28592765009306,"8536201090",1.2]
[100930,"Ex9M1H TM AC40 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=40A, 3-pole","NCA",198.88,0,198.88,8592765009319,1,8592765009319,8,28592765009313,"8536201090",1.2]
[100931,"Ex9M1H TM AC50 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=50A, 3-pole","NCA",198.88,0,198.88,8592765009326,1,8592765009326,8,28592765009320,"8536201090",1.2]
[100932,"Ex9M1H TM AC63 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=63A, 3-pole","NCA",233.58,0,233.58,8592765009333,1,8592765009333,8,28592765009337,"8536201090",1.2]
[100933,"Ex9M1H TM AC80 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=80A, 3-pole","NCA",233.58,0,233.58,8592765009340,1,8592765009340,8,28592765009344,"8536209090",1.2]
[100934,"Ex9M1H TM AC100 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=100A, 3-pole","NCA",241.17,0,241.17,8592765009357,1,8592765009357,8,28592765009351,"8536209090",1.2]
[100935,"Ex9M1H TM AC125 3P","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=125A, 3-pole","NCA",404.09,0,404.09,8592765009364,1,8592765009364,8,28592765009368,"8536209090",1.2]
[100946,"Ex9M1P TM AC16 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=16A, 3-pole","NCA",275.29000000000002,0,275.29000000000002,8592765009470,1,8592765009470,8,28592765009474,"8536201090",1.2]
[100947,"Ex9M1P TM AC20 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=20A, 3-pole","NCA",275.29000000000002,0,275.29000000000002,8592765009487,1,8592765009487,8,28592765009481,"8536201090",1.2]
[100948,"Ex9M1P TM AC25 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=25A, 3-pole","NCA",275.29000000000002,{"$f":"NCA","v":0},275.29000000000002,8592765009494,1,8592765009494,8,28592765009498,"8536201090",1.2]
[100949,"Ex9M1P TM AC32 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=32A, 3-pole","NCA",275.29000000000002,0,275.29000000000002,8592765009500,1,8592765009500,8,28592765009504,"8536201090",1.2]
[100950,"Ex9M1P TM AC40 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=40A, 3-pole","NCA",275.29000000000002,0,275.29000000000002,8592765009517,1,8592765009517,8,28592765009511,"8536201090",1.2]
[100951,"Ex9M1P TM AC50 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=50A, 3-pole","NCA",275.29000000000002,0,275.29000000000002,8592765009524,1,8592765009524,8,28592765009528,"8536201090",1.2]
[100952,"Ex9M1P TM AC63 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=63A, 3-pole","NCA",317.45999999999998,0,317.45999999999998,8592765009531,1,8592765009531,8,28592765009535,"8536201090",1.2]
[100953,"Ex9M1P TM AC80 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=80A, 3-pole","NCA",317.45999999999998,0,317.45999999999998,8592765009548,1,8592765009548,8,28592765009542,"8536209090",1.2]
[100954,"Ex9M1P TM AC100 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=100A, 3-pole","NCA",340.88,0,340.88,8592765009555,1,8592765009555,8,28592765009559,"8536209090",1.2]
[100955,"Ex9M1P TM AC125 3P","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=125A, 3-pole","NCA",454.15,0,454.15,8592765009562,1,8592765009562,8,28592765009566,"8536209090",1.2]
[101293,"Ex9M2S TM AC125 3P","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=125A, 3-pole","NCA",209.46,0,209.46,8592765012944,1,8592765012944,4,28592765012948,"8536209090",1.7]
[101294,"Ex9M2S TM AC160 3P","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=160A, 3-pole","NCA",158.5,0,158.5,8592765012951,1,8592765012951,4,28592765012955,"8536209090",1.7]
[101295,"Ex9M2S TM AC180 3P","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=180A, 3-pole","NCA",259.16000000000003,0,259.16000000000003,8592765012968,1,8592765012968,4,28592765012962,"8536209090",1.7]
[101296,"Ex9M2S TM AC200 3P","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=200A, 3-pole","NCA",196.54,0,196.54,8592765012975,1,8592765012975,4,28592765012979,"8536209090",1.7]
[101297,"Ex9M2S TM AC225 3P","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=225A, 3-pole","NCA",301.26,0,301.26,8592765012982,1,8592765012982,4,28592765012986,"8536209090",1.7]
[101298,"Ex9M2S TM AC250 3P","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=250A, 3-pole","NCA",211.05,0,211.05,8592765012999,1,8592765012999,4,28592765012993,"8536209090",1.7]
[101299,"Ex9M2N TM AC125 3P","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=125A, 3-pole","NCA",363.32,0,363.32,8592765013002,1,8592765013002,4,28592765013006,"8536209090",1.7]
[101300,"Ex9M2N TM AC160 3P","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=160A, 3-pole","NCA",497.28,0,497.28,8592765013019,1,8592765013019,4,28592765013013,"8536209090",1.7]
[101301,"Ex9M2N TM AC180 3P","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=180A, 3-pole","NCA",546.09,0,{"$f":"E2198*(1-F2198)","v":546.09},8592765013026,1,8592765013026,4,28592765013020,"8536209090",1.7]
[101302,"Ex9M2N TM AC200 3P","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=200A, 3-pole","NCA",589.75,0,589.75,8592765013033,1,8592765013033,4,28592765013037,"8536209090",1.7]
[101303,"Ex9M2N TM AC225 3P","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=225A, 3-pole","NCA",640.72,0,640.72,8592765013040,1,8592765013040,4,28592765013044,"8536209090",1.7]
[101304,"Ex9M2N TM AC250 3P","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=250A, 3-pole","NCA",686.93,0,686.93,8592765013057,1,8592765013057,4,28592765013051,"8536209090",1.7]
[101317,"Ex9M2H TM AC125 3P","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=125A, 3-pole","NCA",388.89,0,388.89,8592765013187,1,8592765013187,4,28592765013181,"8536209090",1.7]
[101318,"Ex9M2H TM AC160 3P","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=160A, 3-pole","NCA",526.1,0,526.1,8592765013194,1,8592765013194,4,28592765013198,"8536209090",1.7]
[101319,"Ex9M2H TM AC180 3P","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=180A, 3-pole","NCA",546.09,0,546.09,8592765013200,1,8592765013200,4,28592765013204,"8536209090",1.7]
[101320,"Ex9M2H TM AC200 3P","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=200A, 3-pole","NCA",622.36,0,622.36,8592765013217,1,8592765013217,4,28592765013211,"8536209090",1.7]
[101321,"Ex9M2H TM AC225 3P","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=225A, 3-pole","NCA",640.72,0,640.72,8592765013224,1,8592765013224,4,28592765013228,"8536209090",1.7]
[101322,"Ex9M2H TM AC250 3P","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=250A, 3-pole","NCA",724.2,0,724.2,8592765013231,1,8592765013231,4,28592765013235,"8536209090",1.7]
[101329,"Ex9M2P TM AC125 3P","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=125A, 3-pole","NCA",421.56,0,421.56,8592765013309,1,8592765013309,4,28592765013303,"8536209090",1.7]
[101330,"Ex9M2P TM AC160 3P","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=160A, 3-pole","NCA",551.83000000000004,0,551.83000000000004,8592765013316,1,8592765013316,4,28592765013310,"8536209090",1.7]
[101331,"Ex9M2P TM AC180 3P","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=180A, 3-pole","NCA",599.16,0,599.16,8592765013323,1,8592765013323,4,28592765013327,"8536209090",1.7]
[101332,"Ex9M2P TM AC200 3P","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=200A, 3-pole","NCA",644.85,0,644.85,8592765013330,1,8592765013330,4,28592765013334,"8536209090",1.7]
[101333,"Ex9M2P TM AC225 3P","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=225A, 3-pole","NCA",705.87,0,705.87,8592765013347,1,8592765013347,4,28592765013341,"8536209090",1.7]
[101334,"Ex9M2P TM AC250 3P","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=250A, 3-pole","NCA",762.26,0,762.26,8592765013354,1,8592765013354,4,28592765013358,"8536209090",1.7]
[101454,"Ex9M3S TM AC250 3P","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=250A, 3-pole","NCA",443.57,0,443.57,8592765014559,1,8592765014559,null,28592765014553,"8536209090",5]
[101455,"Ex9M3S TM AC315 3P","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=315A, 3-pole","NCA",532.82000000000005,0,532.82000000000005,8592765014566,1,8592765014566,null,28592765014560,"8536209090",5]
[101456,"Ex9M3S TM AC350 3P","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=350A, 3-pole","NCA",552.44000000000005,0,552.44000000000005,8592765014573,1,8592765014573,null,28592765014577,"8536209090",5]
[101457,"Ex9M3S TM AC400 3P","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=400A, 3-pole","NCA",443.57,0,443.57,8592765014580,1,8592765014580,null,28592765014584,"8536209090",5]
[101458,"Ex9M3N TM AC250 3P","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=250A, 3-pole","NCA",522.24,0,522.24,8592765014597,1,8592765014597,null,28592765014591,"8536209090",5]
[101459,"Ex9M3N TM AC315 3P","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=315A, 3-pole","NCA",564.51,0,564.51,8592765014603,1,8592765014603,null,28592765014607,"8536209090",5]
[101460,"Ex9M3N TM AC350 3P","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=350A, 3-pole","NCA",578.1,0,578.1,8592765014610,1,8592765014610,null,28592765014614,"8536209090",5]
[101461,"Ex9M3N TM AC400 3P","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=400A, 3-pole","NCA",591.67999999999995,0,591.67999999999995,8592765014627,1,8592765014627,null,28592765014621,"8536209090",5]
[101470,"Ex9M3H TM AC250 3P","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=250A, 3-pole","NCA",972.25,0,972.25,8592765014719,1,8592765014719,null,28592765014713,"8536209090",5]
[101471,"Ex9M3H TM AC315 3P","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=315A, 3-pole","NCA",989.7,0,989.7,8592765014726,1,8592765014726,null,28592765014720,"8536209090",5]
[101472,"Ex9M3H TM AC350 3P","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=350A, 3-pole","NCA",1006.24,0,1006.24,8592765014733,1,8592765014733,null,28592765014737,"8536209090",5]
[101473,"Ex9M3H TM AC400 3P","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=400A, 3-pole","NCA",1046.01,0,1046.01,8592765014740,1,8592765014740,null,28592765014744,"8536209090",5]
[101478,"Ex9M3P TM AC250 3P","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=250A, 3-pole","NCA",1088.8499999999999,0,1088.8499999999999,8592765014795,1,8592765014795,null,28592765014799,"8536209090",5]
[101479,"Ex9M3P TM AC315 3P","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=315A, 3-pole","NCA",1108.3699999999999,0,1108.3699999999999,8592765014801,1,8592765014801,null,28592765014805,"8536209090",5]
[101480,"Ex9M3P TM AC350 3P","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=350A, 3-pole","NCA",1126.96,0,1126.96,8592765014818,1,8592765014818,null,28592765014812,"8536209090",5]
[101481,"Ex9M3P TM AC400 3P","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=400A, 3-pole","NCA",1171.49,0,1171.49,8592765014825,1,8592765014825,null,28592765014829,"8536209090",5]
[103373,"Ex9M4S TM AC400 3P","Circuit Breaker, frame size M4, Icu=Ics=36kA, In=400A, 3-pole","NCA",703.65,{"$f":"NCA","v":0},{"$f":"E2230*(1-F2230)","v":703.65},8592765033741,1,8592765033741,null,28592765033745,"8536209090",10.199999999999999]
[103374,"Ex9M4S TM AC500 3P","Circuit Breaker, frame size M4, Icu=Ics=36kA, In=500A, 3-pole","NCA",811.92,{"$f":"NCA","v":0},{"$f":"E2231*(1-F2231)","v":811.92},8592765033758,1,8592765033758,null,28592765033752,"8536209090",10.199999999999999]
[103375,"Ex9M4S TM AC630 3P","Circuit Breaker, frame size M4, Icu=Ics=36kA, In=630A, 3-pole","NCA",926.35,{"$f":"NCA","v":0},{"$f":"E2232*(1-F2232)","v":926.35},8592765033765,1,8592765033765,null,28592765033769,"8536209090",10.199999999999999]
[103376,"Ex9M4N TM AC400 3P","Circuit Breaker, frame size M4, Icu=Ics=50kA, In=400A, 3-pole","NCA",685.13,0,{"$f":"E2233*(1-F2233)","v":685.13},8592765033772,1,8592765033772,null,28592765033776,"8536209090",10.199999999999999]
[103377,"Ex9M4N TM AC500 3P","Circuit Breaker, frame size M4, Icu=Ics=50kA, In=500A, 3-pole","NCA",805.93,0,805.93,8592765033789,1,8592765033789,null,28592765033783,"8536209090",10.199999999999999]
[103378,"Ex9M4N TM AC630 3P","Circuit Breaker, frame size M4, Icu=Ics=50kA, In=630A, 3-pole","NCA",899.14,0,899.14,8592765033796,1,8592765033796,null,28592765033790,"8536209090",10.199999999999999]
[103385,"Ex9M4H TM AC400 3P","Circuit Breaker, frame size M4, Icu=Ics=100kA, In=400A, 3-pole","NCA",1390.3,0,1390.3,8592765033864,1,8592765033864,null,28592765033868,"8536209090",10.199999999999999]
[103386,"Ex9M4H TM AC500 3P","Circuit Breaker, frame size M4, Icu=Ics=100kA, In=500A, 3-pole","NCA",1503.2,0,1503.2,8592765033871,1,8592765033871,null,28592765033875,"8536209090",10.199999999999999]
[103387,"Ex9M4H TM AC630 3P","Circuit Breaker, frame size M4, Icu=Ics=100kA, In=630A, 3-pole","NCA",1637.74,0,1637.74,8592765033888,1,8592765033888,null,28592765033882,"8536209090",10.199999999999999]
[103391,"Ex9M4P TM AC400 3P","Circuit Breaker, frame size M4, Icu=Ics=150kA, In=400A, 3-pole","NCA",1577.43,0,1577.43,8592765033925,1,8592765033925,null,28592765033929,"8536209090",10.199999999999999]
[103392,"Ex9M4P TM AC500 3P","Circuit Breaker, frame size M4, Icu=Ics=150kA, In=500A, 3-pole","NCA",1849.61,0,1849.61,8592765033932,1,8592765033932,null,28592765033936,"8536209090",10.199999999999999]
[103393,"Ex9M4P TM AC630 3P","Circuit Breaker, frame size M4, Icu=Ics=150kA, In=630A, 3-pole","NCA",2126.44,0,2126.44,8592765033949,1,8592765033949,null,28592765033943,"8536209090",10.199999999999999]
[103394,"Ex9M5S TM AC630 3P","Circuit Breaker, frame size M5, Icu=Ics=36kA, In=630A, 3-pole","NCA",1187.71,0,1187.71,8592765033956,1,8592765033956,null,28592765033950,"8536209090",10.199999999999999]
[103395,"Ex9M5S TM AC700 3P","Circuit Breaker, frame size M5, Icu=Ics=36kA, In=700A, 3-pole","NCA",1322.25,0,1322.25,8592765033963,1,8592765033963,null,28592765033967,"8536209090",10.199999999999999]
[103396,"Ex9M5S TM AC800 3P","Circuit Breaker, frame size M5, Icu=Ics=36kA, In=800A, 3-pole","NCA",1422.78,0,1422.78,8592765033970,1,8592765033970,null,28592765033974,"8536209090",10.199999999999999]
[103397,"Ex9M5N TM AC630 3P","Circuit Breaker, frame size M5, Icu=Ics=50kA, In=630A, 3-pole","NCA",1252.67,0,1252.67,8592765033987,1,8592765033987,null,28592765033981,"8536209090",10.199999999999999]
[103398,"Ex9M5N TM AC700 3P","Circuit Breaker, frame size M5, Icu=Ics=50kA, In=700A, 3-pole","NCA",1300.98,0,1300.98,8592765033994,1,8592765033994,null,28592765033998,"8536209090",10.199999999999999]
[103399,"Ex9M5N TM AC800 3P","Circuit Breaker, frame size M5, Icu=Ics=50kA, In=800A, 3-pole","NCA",1356.84,0,1356.84,8592765034007,1,8592765034007,null,28592765034001,"8536209090",10.199999999999999]
[103406,"Ex9M5H TM AC630 3P","Circuit Breaker, frame size M5, Icu=Ics=100kA, In=630A, 3-pole","NCA",2333.67,0,2333.67,8592765034076,1,8592765034076,null,28592765034070,"8536209090",10.199999999999999]
[103407,"Ex9M5H TM AC700 3P","Circuit Breaker, frame size M5, Icu=Ics=100kA, In=700A, 3-pole","NCA",2700.2,0,2700.2,8592765034083,1,8592765034083,null,28592765034087,"8536209090",10.199999999999999]
[103408,"Ex9M5H TM AC800 3P","Circuit Breaker, frame size M5, Icu=Ics=100kA, In=800A, 3-pole","NCA",3088.37,0,3088.37,8592765034090,1,8592765034090,null,28592765034094,"8536209090",10.199999999999999]
[103412,"Ex9M5P TM AC630 3P","Circuit Breaker, frame size M5, Icu=Ics=150kA, In=630A, 3-pole","NCA",2728.03,0,2728.03,8592765034137,1,8592765034137,null,28592765034131,"8536209090",10.199999999999999]
[103413,"Ex9M5P TM AC700 3P","Circuit Breaker, frame size M5, Icu=Ics=150kA, In=700A, 3-pole","NCA",3243.02,0,3243.02,8592765034144,1,8592765034144,null,28592765034148,"8536209090",10.199999999999999]
[103414,"Ex9M5P TM AC800 3P","Circuit Breaker, frame size M5, Icu=Ics=150kA, In=800A, 3-pole","NCA",3728.61,0,3728.61,8592765034151,1,8592765034151,null,28592765034155,"8536209090",10.199999999999999]
[]
["Molded Case Circuit Breakers with electronic tripping unit Ex9M6"]
[110340,"Ex9M6N SU20L 800 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 3-pole","NCF",1139.0899999999999,{"$f":"NCF","v":0},{"$f":"E2256*(1-F2256)","v":1139.0899999999999},8592765103406,1,18592765103403,1,28592765103400,"8536209090",12.5]
[110341,"Ex9M6N SU20L 1000 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 3-pole","NCF",1564.88,{"$f":"NCF","v":0},{"$f":"E2257*(1-F2257)","v":1564.88},8592765103413,1,18592765103410,1,28592765103417,"8536209090",12.5]
[110342,"Ex9M6N SU20L 1250 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 3-pole","NCF",1841.03,0,1841.03,8592765103420,1,18592765103427,1,28592765103424,"8536209090",12.5]
[110343,"Ex9M6N SU20L 1600 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 3-pole","NCF",2023.11,0,2023.11,8592765103437,1,18592765103434,1,28592765103431,"8536209090",12.5]
[110344,"Ex9M6N SU20L 800 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 4-pole with protected N-pole","NCF",2588.12,0,2588.12,8592765103444,1,18592765103441,1,28592765103448,"8536209090",16.5]
[110345,"Ex9M6N SU20L 1000 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 4-pole with protected N-pole","NCF",2941.05,0,2941.05,8592765103451,1,18592765103458,1,28592765103455,"8536209090",16.5]
[110346,"Ex9M6N SU20L 1250 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 4-pole with protected N-pole","NCF",3460.05,0,3460.05,8592765103468,1,18592765103465,1,28592765103462,"8536209090",16.5]
[110347,"Ex9M6N SU20L 1600 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 4-pole with protected N-pole","NCF",3802.26,0,3802.26,8592765103475,1,18592765103472,1,28592765103479,"8536209090",16.5]
[110348,"Ex9M6Q SU20L 800 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 3-pole","NCF",1567.62,0,1567.62,8592765103482,1,18592765103489,1,28592765103486,"8536209090",12.5]
[110349,"Ex9M6Q SU20L 1000 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 3-pole","NCF",1931.39,0,1931.39,8592765103499,1,18592765103496,1,28592765103493,"8536209090",12.5]
[110350,"Ex9M6Q SU20L 1250 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 3-pole","NCF",2135.7399999999998,0,2135.7399999999998,8592765103505,1,18592765103502,1,28592765103509,"8536209090",12.5]
[110351,"Ex9M6Q SU20L 1600 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 3-pole","NCF",3290.03,0,3290.03,8592765103512,1,18592765103519,1,28592765103516,"8536209090",12.5]
[110352,"Ex9M6Q SU20L 800 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 4-pole with protected N-pole","NCF",3290.41,0,3290.41,8592765103529,1,18592765103526,1,28592765103523,"8536209090",16.5]
[110353,"Ex9M6Q SU20L 1000 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 4-pole with protected N-pole","NCF",3739.1,0,3739.1,8592765103536,1,18592765103533,1,28592765103530,"8536209090",16.5]
[110354,"Ex9M6Q SU20L 1250 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 4-pole with protected N-pole","NCF",4398.9399999999996,0,4398.9399999999996,8592765103543,1,18592765103540,1,28592765103547,"8536209090",16.5]
[110355,"Ex9M6Q SU20L 1600 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 4-pole with protected N-pole","NCF",4834,0,4834,8592765103550,1,18592765103557,1,28592765103554,"8536209090",16.5]
[110356,"Ex9M6H SU20L 800 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 3-pole","NCF",3101.82,0,3101.82,8592765103567,1,18592765103564,1,28592765103561,"8536209090",12.5]
[110357,"Ex9M6H SU20L 1000 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 3-pole","NCF",3524.8,0,3524.8,8592765103574,1,18592765103571,1,28592765103578,"8536209090",12.5]
[110358,"Ex9M6H SU20L 1250 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 3-pole","NCF",4146.82,0,4146.82,8592765103581,1,18592765103588,1,28592765103585,"8536209090",12.5]
[110359,"Ex9M6H SU20L 1600 3P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 3-pole","NCF",4556.9399999999996,0,4556.9399999999996,8592765103598,1,18592765103595,1,28592765103592,"8536209090",12.5]
[110360,"Ex9M6H SU20L 800 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 4-pole with protected N-pole","NCF",3992.69,0,3992.69,8592765103604,1,18592765103601,1,28592765103608,"8536209090",16.5]
[110361,"Ex9M6H SU20L 1000 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 4-pole with protected N-pole","NCF",4537.1499999999996,0,4537.1499999999996,8592765103611,1,18592765103618,1,28592765103615,"8536209090",16.5]
[110362,"Ex9M6H SU20L 1250 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 4-pole with protected N-pole","NCF",5337.82,0,5337.82,8592765103628,1,18592765103625,1,28592765103622,"8536209090",16.5]
[110363,"Ex9M6H SU20L 1600 4P","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 4-pole with protected N-pole","NCF",5865.74,0,5865.74,8592765103635,1,18592765103632,1,28592765103639,"8536209090",16.5]
[110364,"Ex9M6N SU20L 800 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 3-pole, with MOD AC230","NCF",2011.5,0,2011.5,8592765103642,1,18592765103649,1,28592765103646,"8536209090",14.5]
[110365,"Ex9M6N SU20L 1000 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 3-pole, with MOD AC230","NCF",2199.29,0,2199.29,8592765103659,1,18592765103656,1,28592765103653,"8536209090",14.5]
[110366,"Ex9M6N SU20L 1250 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 3-pole, with MOD AC230","NCF",2475.44,0,2475.44,8592765103666,1,18592765103663,1,28592765103660,"8536209090",14.5]
[110367,"Ex9M6N SU20L 1600 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 3-pole, with MOD AC230","NCF",2657.52,0,2657.52,8592765103673,1,18592765103670,1,28592765103677,"8536209090",14.5]
[110368,"Ex9M6N SU20L 800 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 4-pole with protected N-pole, with MOD AC230","NCF",3222.53,0,3222.53,8592765103680,1,18592765103687,1,28592765103684,"8536209090",18.5]
[110369,"Ex9M6N SU20L 1000 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 4-pole with protected N-pole, with MOD AC230","NCF",3575.46,0,3575.46,8592765103697,1,18592765103694,1,28592765103691,"8536209090",18.5]
[110370,"Ex9M6N SU20L 1250 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 4-pole with protected N-pole, with MOD AC230","NCF",4094.46,0,4094.46,8592765103703,1,18592765103700,1,28592765103707,"8536209090",18.5]
[110371,"Ex9M6N SU20L 1600 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 4-pole with protected N-pole, with MOD AC230","NCF",4436.67,0,4436.67,8592765103710,1,18592765103717,1,28592765103714,"8536209090",18.5]
[110372,"Ex9M6N SU20L 800 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 3-pole, with MOD AC400","NCF",2182.11,0,2182.11,8592765103727,1,18592765103724,1,28592765103721,"8536209090",14.5]
[110373,"Ex9M6N SU20L 1000 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 3-pole, with MOD AC400","NCF",2369.9,0,2369.9,8592765103734,1,18592765103731,1,28592765103738,"8536209090",14.5]
[110374,"Ex9M6N SU20L 1250 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 3-pole, with MOD AC400","NCF",2646.05,0,2646.05,8592765103741,1,18592765103748,1,28592765103745,"8536209090",14.5]
[110375,"Ex9M6N SU20L 1600 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 3-pole, with MOD AC400","NCF",2828.13,0,2828.13,8592765103758,1,18592765103755,1,28592765103752,"8536209090",14.5]
[110376,"Ex9M6N SU20L 800 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 4-pole with protected N-pole, with MOD AC400","NCF",3393.14,0,3393.14,8592765103765,1,18592765103762,1,28592765103769,"8536209090",18.5]
[110377,"Ex9M6N SU20L 1000 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 4-pole with protected N-pole, with MOD AC400","NCF",3746.07,0,3746.07,8592765103772,1,18592765103779,1,28592765103776,"8536209090",18.5]
[110378,"Ex9M6N SU20L 1250 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 4-pole with protected N-pole, with MOD AC400","NCF",4265.07,0,4265.07,8592765103789,1,18592765103786,1,28592765103783,"8536209090",18.5]
[110379,"Ex9M6N SU20L 1600 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 4-pole with protected N-pole, with MOD AC400","NCF",4607.28,0,4607.28,8592765103796,1,18592765103793,1,28592765103790,"8536209090",18.5]
[110380,"Ex9M6N SU20L 800 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 3-pole, with MOD DC110","NCF",2287.27,0,2287.27,8592765103802,1,18592765103809,1,28592765103806,"8536209090",14.5]
[110381,"Ex9M6N SU20L 1000 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 3-pole, with MOD DC110","NCF",2475.06,0,2475.06,8592765103819,1,18592765103816,1,28592765103813,"8536209090",14.5]
[110382,"Ex9M6N SU20L 1250 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 3-pole, with MOD DC110","NCF",2751.21,0,2751.21,8592765103826,1,18592765103823,1,28592765103820,"8536209090",14.5]
[110383,"Ex9M6N SU20L 1600 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 3-pole, with MOD DC110","NCF",2933.29,0,2933.29,8592765103833,1,18592765103830,1,28592765103837,"8536209090",14.5]
[110384,"Ex9M6N SU20L 800 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 4-pole with protected N-pole, with MOD DC110","NCF",3498.3,0,3498.3,8592765103840,1,18592765103847,1,28592765103844,"8536209090",18.5]
[110385,"Ex9M6N SU20L 1000 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 4-pole with protected N-pole, with MOD DC110","NCF",3851.23,0,3851.23,8592765103857,1,18592765103854,1,28592765103851,"8536209090",18.5]
[110386,"Ex9M6N SU20L 1250 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 4-pole with protected N-pole, with MOD DC110","NCF",4370.2299999999996,0,4370.2299999999996,8592765103864,1,18592765103861,1,28592765103868,"8536209090",18.5]
[110387,"Ex9M6N SU20L 1600 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 4-pole with protected N-pole, with MOD DC110","NCF",4712.4399999999996,0,4712.4399999999996,8592765103871,1,18592765103878,1,28592765103875,"8536209090",18.5]
[110388,"Ex9M6N SU20L 800 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 3-pole, with MOD DC220","NCF",2287.27,0,2287.27,8592765103888,1,18592765103885,1,28592765103882,"8536209090",14.5]
[110389,"Ex9M6N SU20L 1000 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 3-pole, with MOD DC220","NCF",2475.06,0,2475.06,8592765103895,1,18592765103892,1,28592765103899,"8536209090",14.5]
[110390,"Ex9M6N SU20L 1250 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 3-pole, with MOD DC220","NCF",2751.21,0,2751.21,8592765103901,1,18592765103908,1,28592765103905,"8536209090",14.5]
[110391,"Ex9M6N SU20L 1600 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 3-pole, with MOD DC220","NCF",2933.29,0,2933.29,8592765103918,1,18592765103915,1,28592765103912,"8536209090",14.5]
[110392,"Ex9M6N SU20L 800 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=800A, 4-pole with protected N-pole, with MOD DC220","NCF",3498.3,0,3498.3,8592765103925,1,18592765103922,1,28592765103929,"8536209090",18.5]
[110393,"Ex9M6N SU20L 1000 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1000A, 4-pole with protected N-pole, with MOD DC220","NCF",3851.23,0,3851.23,8592765103932,1,18592765103939,1,28592765103936,"8536209090",18.5]
[110394,"Ex9M6N SU20L 1250 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1250A, 4-pole with protected N-pole, with MOD DC220","NCF",4370.2299999999996,0,4370.2299999999996,8592765103949,1,18592765103946,1,28592765103943,"8536209090",18.5]
[110395,"Ex9M6N SU20L 1600 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=65kA, In=1600A, 4-pole with protected N-pole, with MOD DC220","NCF",4712.4399999999996,0,4712.4399999999996,8592765103956,1,18592765103953,1,28592765103950,"8536209090",18.5]
[110396,"Ex9M6Q SU20L 800 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 3-pole, with MOD AC230","NCF",2402.79,0,2402.79,8592765103963,1,18592765103960,1,28592765103967,"8536209090",14.5]
[110397,"Ex9M6Q SU20L 1000 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 3-pole, with MOD AC230","NCF",2772.36,0,2772.36,8592765103970,1,18592765103977,1,28592765103974,"8536209090",14.5]
[110398,"Ex9M6Q SU20L 1250 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 3-pole, with MOD AC230","NCF",2984.08,0,2984.08,8592765103987,1,18592765103984,1,28592765103981,"8536209090",14.5]
[110399,"Ex9M6Q SU20L 1600 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 3-pole, with MOD AC230","NCF",3924.44,0,3924.44,8592765103994,1,18592765103991,1,28592765103998,"8536209090",14.5]
[110400,"Ex9M6Q SU20L 800 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 4-pole with protected N-pole, with MOD AC230","NCF",3924.82,0,3924.82,8592765104007,1,18592765104004,1,28592765104001,"8536209090",18.5]
[110401,"Ex9M6Q SU20L 1000 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 4-pole with protected N-pole, with MOD AC230","NCF",4373.51,0,4373.51,8592765104014,1,18592765104011,1,28592765104018,"8536209090",18.5]
[110402,"Ex9M6Q SU20L 1250 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 4-pole with protected N-pole, with MOD AC230","NCF",5033.3500000000004,0,5033.3500000000004,8592765104021,1,18592765104028,1,28592765104025,"8536209090",18.5]
[110403,"Ex9M6Q SU20L 1600 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 4-pole with protected N-pole, with MOD AC230","NCF",5468.41,0,5468.41,8592765104038,1,18592765104035,1,28592765104032,"8536209090",18.5]
[110404,"Ex9M6Q SU20L 800 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 3-pole, with MOD AC400","NCF",3044.48,0,3044.48,8592765104045,1,18592765104042,1,28592765104049,"8536209090",14.5]
[110405,"Ex9M6Q SU20L 1000 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 3-pole, with MOD AC400","NCF",3349.86,{"$f":"NCF","v":0},{"$f":"E2321*(1-F2321)","v":3349.86},8592765104052,1,18592765104059,1,28592765104056,"8536209090",14.5]
[110406,"Ex9M6Q SU20L 1250 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 3-pole, with MOD AC400","NCF",3798.94,0,3798.94,8592765104069,1,18592765104066,1,28592765104063,"8536209090",14.5]
[110407,"Ex9M6Q SU20L 1600 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 3-pole, with MOD AC400","NCF",4095.05,0,4095.05,8592765104076,1,18592765104073,1,28592765104070,"8536209090",14.5]
[110408,"Ex9M6Q SU20L 800 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 4-pole with protected N-pole, with MOD AC400","NCF",4095.43,0,4095.43,8592765104083,1,18592765104080,1,28592765104087,"8536209090",18.5]
[110409,"Ex9M6Q SU20L 1000 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 4-pole with protected N-pole, with MOD AC400","NCF",4544.12,0,4544.12,8592765104090,1,18592765104097,1,28592765104094,"8536209090",18.5]
[110410,"Ex9M6Q SU20L 1250 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 4-pole with protected N-pole, with MOD AC400","NCF",5203.96,0,5203.96,8592765104106,1,18592765104103,1,28592765104100,"8536209090",18.5]
[110411,"Ex9M6Q SU20L 1600 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 4-pole with protected N-pole, with MOD AC400","NCF",5639.02,0,5639.02,8592765104113,1,18592765104110,1,28592765104117,"8536209090",18.5]
[110412,"Ex9M6Q SU20L 800 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 3-pole, with MOD DC110","NCF",3149.64,0,3149.64,8592765104120,1,18592765104127,1,28592765104124,"8536209090",14.5]
[110413,"Ex9M6Q SU20L 1000 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 3-pole, with MOD DC110","NCF",3455.02,0,3455.02,8592765104137,1,18592765104134,1,28592765104131,"8536209090",14.5]
[110414,"Ex9M6Q SU20L 1250 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 3-pole, with MOD DC110","NCF",3904.1,0,3904.1,8592765104144,1,18592765104141,1,28592765104148,"8536209090",14.5]
[110415,"Ex9M6Q SU20L 1600 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 3-pole, with MOD DC110","NCF",4200.21,0,4200.21,8592765104151,1,18592765104158,1,28592765104155,"8536209090",14.5]
[110416,"Ex9M6Q SU20L 800 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 4-pole with protected N-pole, with MOD DC110","NCF",4200.59,0,4200.59,8592765104168,1,18592765104165,1,28592765104162,"8536209090",18.5]
[110417,"Ex9M6Q SU20L 1000 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 4-pole with protected N-pole, with MOD DC110","NCF",4649.28,0,4649.28,8592765104175,1,18592765104172,1,28592765104179,"8536209090",18.5]
[110418,"Ex9M6Q SU20L 1250 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 4-pole with protected N-pole, with MOD DC110","NCF",5309.12,0,5309.12,8592765104182,1,18592765104189,1,28592765104186,"8536209090",18.5]
[110419,"Ex9M6Q SU20L 1600 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 4-pole with protected N-pole, with MOD DC110","NCF",5744.18,0,5744.18,8592765104199,1,18592765104196,1,28592765104193,"8536209090",18.5]
[110420,"Ex9M6Q SU20L 800 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 3-pole, with MOD DC220","NCF",3149.64,0,3149.64,8592765104205,1,18592765104202,1,28592765104209,"8536209090",14.5]
[110421,"Ex9M6Q SU20L 1000 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 3-pole, with MOD DC220","NCF",3455.02,0,3455.02,8592765104212,1,18592765104219,1,28592765104216,"8536209090",14.5]
[110422,"Ex9M6Q SU20L 1250 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 3-pole, with MOD DC220","NCF",3904.1,0,3904.1,8592765104229,1,18592765104226,1,28592765104223,"8536209090",14.5]
[110423,"Ex9M6Q SU20L 1600 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 3-pole, with MOD DC220","NCF",4200.21,0,4200.21,8592765104236,1,18592765104233,1,28592765104230,"8536209090",14.5]
[110424,"Ex9M6Q SU20L 800 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=800A, 4-pole with protected N-pole, with MOD DC220","NCF",4200.59,0,4200.59,8592765104243,1,18592765104240,1,28592765104247,"8536209090",18.5]
[110425,"Ex9M6Q SU20L 1000 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1000A, 4-pole with protected N-pole, with MOD DC220","NCF",4649.28,0,4649.28,8592765104250,1,18592765104257,1,28592765104254,"8536209090",18.5]
[110426,"Ex9M6Q SU20L 1250 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1250A, 4-pole with protected N-pole, with MOD DC220","NCF",5309.12,0,5309.12,8592765104267,1,18592765104264,1,28592765104261,"8536209090",18.5]
[110427,"Ex9M6Q SU20L 1600 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=85kA, In=1600A, 4-pole with protected N-pole, with MOD DC220","NCF",5744.18,0,5744.18,8592765104274,1,18592765104271,1,28592765104278,"8536209090",18.5]
[110428,"Ex9M6H SU20L 800 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 3-pole, with MOD AC230","NCF",3736.23,0,3736.23,8592765104281,1,18592765104288,1,28592765104285,"8536209090",14.5]
[110429,"Ex9M6H SU20L 1000 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 3-pole, with MOD AC230","NCF",4159.21,0,4159.21,8592765104298,1,18592765104295,1,28592765104292,"8536209090",14.5]
[110430,"Ex9M6H SU20L 1250 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 3-pole, with MOD AC230","NCF",4781.2299999999996,0,4781.2299999999996,8592765104304,1,18592765104301,1,28592765104308,"8536209090",14.5]
[110431,"Ex9M6H SU20L 1600 3P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 3-pole, with MOD AC230","NCF",5191.3500000000004,0,5191.3500000000004,8592765104311,1,18592765104318,1,28592765104315,"8536209090",14.5]
[110432,"Ex9M6H SU20L 800 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 4-pole with protected N-pole, with MOD AC230","NCF",4627.1000000000004,0,4627.1000000000004,8592765104328,1,18592765104325,1,28592765104322,"8536209090",18.5]
[110433,"Ex9M6H SU20L 1000 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 4-pole with protected N-pole, with MOD AC230","NCF",5171.5600000000004,0,5171.5600000000004,8592765104335,1,18592765104332,1,28592765104339,"8536209090",18.5]
[110434,"Ex9M6H SU20L 1250 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 4-pole with protected N-pole, with MOD AC230","NCF",5972.23,0,5972.23,8592765104342,1,18592765104349,1,28592765104346,"8536209090",18.5]
[110435,"Ex9M6H SU20L 1600 4P MOD AC230","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 4-pole with protected N-pole, with MOD AC230","NCF",6500.15,0,6500.15,8592765104359,1,18592765104356,1,28592765104353,"8536209090",18.5]
[110436,"Ex9M6H SU20L 800 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 3-pole, with MOD AC400","NCF",3906.84,0,3906.84,8592765104366,1,18592765104363,1,28592765104360,"8536209090",14.5]
[110437,"Ex9M6H SU20L 1000 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 3-pole, with MOD AC400","NCF",4329.82,0,4329.82,8592765104373,1,18592765104370,1,28592765104377,"8536209090",14.5]
[110438,"Ex9M6H SU20L 1250 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 3-pole, with MOD AC400","NCF",4951.84,0,4951.84,8592765104380,1,18592765104387,1,28592765104384,"8536209090",14.5]
[110439,"Ex9M6H SU20L 1600 3P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 3-pole, with MOD AC400","NCF",5361.96,0,5361.96,8592765104397,1,18592765104394,1,28592765104391,"8536209090",14.5]
[110440,"Ex9M6H SU20L 800 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 4-pole with protected N-pole, with MOD AC400","NCF",4797.71,0,4797.71,8592765104403,1,18592765104400,1,28592765104407,"8536209090",18.5]
[110441,"Ex9M6H SU20L 1000 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 4-pole with protected N-pole, with MOD AC400","NCF",5342.17,0,5342.17,8592765104410,1,18592765104417,1,28592765104414,"8536209090",18.5]
[110442,"Ex9M6H SU20L 1250 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 4-pole with protected N-pole, with MOD AC400","NCF",6142.84,0,6142.84,8592765104427,1,18592765104424,1,28592765104421,"8536209090",18.5]
[110443,"Ex9M6H SU20L 1600 4P MOD AC400","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 4-pole with protected N-pole, with MOD AC400","NCF",6670.76,0,6670.76,8592765104434,1,18592765104431,1,28592765104438,"8536209090",18.5]
[110444,"Ex9M6H SU20L 800 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 3-pole, with MOD DC110","NCF",4012,0,4012,8592765104441,1,18592765104448,1,28592765104445,"8536209090",14.5]
[110445,"Ex9M6H SU20L 1000 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 3-pole, with MOD DC110","NCF",4434.9799999999996,0,4434.9799999999996,8592765104458,1,18592765104455,1,28592765104452,"8536209090",14.5]
[110446,"Ex9M6H SU20L 1250 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 3-pole, with MOD DC110","NCF",5057,0,5057,8592765104465,1,18592765104462,1,28592765104469,"8536209090",14.5]
[110447,"Ex9M6H SU20L 1600 3P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 3-pole, with MOD DC110","NCF",5467.12,0,5467.12,8592765104472,1,18592765104479,1,28592765104476,"8536209090",14.5]
[110448,"Ex9M6H SU20L 800 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 4-pole with protected N-pole, with MOD DC110","NCF",4902.87,0,4902.87,8592765104489,1,18592765104486,1,28592765104483,"8536209090",18.5]
[110449,"Ex9M6H SU20L 1000 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 4-pole with protected N-pole, with MOD DC110","NCF",5447.33,0,5447.33,8592765104496,1,18592765104493,1,28592765104490,"8536209090",18.5]
[110450,"Ex9M6H SU20L 1250 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 4-pole with protected N-pole, with MOD DC110","NCF",6248,0,6248,8592765104502,1,18592765104509,1,28592765104506,"8536209090",18.5]
[110451,"Ex9M6H SU20L 1600 4P MOD DC110","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 4-pole with protected N-pole, with MOD DC110","NCF",6775.92,0,6775.92,8592765104519,1,18592765104516,1,28592765104513,"8536209090",18.5]
[110452,"Ex9M6H SU20L 800 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 3-pole, with MOD DC220","NCF",4012,0,4012,8592765104526,1,18592765104523,1,28592765104520,"8536209090",14.5]
[110453,"Ex9M6H SU20L 1000 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 3-pole, with MOD DC220","NCF",4434.9799999999996,0,4434.9799999999996,8592765104533,1,18592765104530,1,28592765104537,"8536209090",14.5]
[110454,"Ex9M6H SU20L 1250 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 3-pole, with MOD DC220","NCF",5057,0,5057,8592765104540,1,18592765104547,1,28592765104544,"8536209090",14.5]
[110455,"Ex9M6H SU20L 1600 3P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 3-pole, with MOD DC220","NCF",5467.12,0,5467.12,8592765104557,1,18592765104554,1,28592765104551,"8536209090",14.5]
[110456,"Ex9M6H SU20L 800 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=800A, 4-pole with protected N-pole, with MOD DC220","NCF",4902.87,0,4902.87,8592765104564,1,18592765104561,1,28592765104568,"8536209090",18.5]
[110457,"Ex9M6H SU20L 1000 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1000A, 4-pole with protected N-pole, with MOD DC220","NCF",5447.33,0,5447.33,8592765104571,1,18592765104578,1,28592765104575,"8536209090",18.5]
[110458,"Ex9M6H SU20L 1250 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1250A, 4-pole with protected N-pole, with MOD DC220","NCF",6248,0,6248,8592765104588,1,18592765104585,1,28592765104582,"8536209090",18.5]
[110459,"Ex9M6H SU20L 1600 4P MOD DC220","Circuit Breaker, frame size M6, SU20L, Icu=Ics=100kA, In=1600A, 4-pole with protected N-pole, with MOD DC220","NCF",6775.92,0,6775.92,8592765104595,1,18592765104592,1,28592765104599,"8536209090",18.5]
[]
["Moulded Case Circuit Breakers Ex9M 4P"]
[103062,"Ex9M1S TM AC16 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=16A, 4-pole with protected N-pole","NCA",247.18,{"$f":"NCA","v":0},{"$f":"E2378*(1-F2378)","v":247.18},8592765030634,1,8592765030634,null,28592765030638,"8536201090",1.7]
[103063,"Ex9M1S TM AC20 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=20A, 4-pole with protected N-pole","NCA",247.18,0,{"$f":"E2379*(1-F2379)","v":247.18},8592765030641,1,8592765030641,null,28592765030645,"8536201090",1.7]
[103064,"Ex9M1S TM AC25 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=25A, 4-pole with protected N-pole","NCA",247.18,0,247.18,8592765030658,1,8592765030658,null,28592765030652,"8536201090",1.7]
[103065,"Ex9M1S TM AC32 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=32A, 4-pole with protected N-pole","NCA",247.18,0,247.18,8592765030665,1,8592765030665,null,28592765030669,"8536201090",1.7]
[103066,"Ex9M1S TM AC40 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=40A, 4-pole with protected N-pole","NCA",247.18,0,247.18,8592765030672,1,8592765030672,null,28592765030676,"8536201090",1.7]
[103067,"Ex9M1S TM AC50 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=50A, 4-pole with protected N-pole","NCA",247.18,0,247.18,8592765030689,1,8592765030689,null,28592765030683,"8536201090",1.7]
[103068,"Ex9M1S TM AC63 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=63A, 4-pole with protected N-pole","NCA",279.38,0,279.38,8592765030696,1,8592765030696,null,28592765030690,"8536201090",1.7]
[103069,"Ex9M1S TM AC80 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=80A, 4-pole with protected N-pole","NCA",279.38,0,279.38,8592765030702,1,8592765030702,null,28592765030706,"8536209090",1.7]
[103070,"Ex9M1S TM AC100 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=100A, 4-pole with protected N-pole","NCA",356.59,0,356.59,8592765030719,1,8592765030719,null,28592765030713,"8536209090",1.7]
[103071,"Ex9M1S TM AC125 4P4T","Circuit Breaker, frame size M1, Icu=Ics=36kA, In=125A, 4-pole with protected N-pole","NCA",493.38,0,493.38,8592765030726,1,8592765030726,null,28592765030720,"8536209090",1.7]
[103072,"Ex9M1N TM AC16 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=16A, 4-pole with protected N-pole","NCA",321.81,0,321.81,8592765030733,1,8592765030733,null,28592765030737,"8536201090",1.7]
[103073,"Ex9M1N TM AC20 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=20A, 4-pole with protected N-pole","NCA",321.81,0,321.81,8592765030740,1,8592765030740,null,28592765030744,"8536201090",1.7]
[103074,"Ex9M1N TM AC25 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=25A, 4-pole with protected N-pole","NCA",321.81,0,321.81,8592765030757,1,8592765030757,null,28592765030751,"8536201090",1.7]
[103075,"Ex9M1N TM AC32 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=32A, 4-pole with protected N-pole","NCA",321.81,0,321.81,8592765030764,1,8592765030764,null,28592765030768,"8536201090",1.7]
[103076,"Ex9M1N TM AC40 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=40A, 4-pole with protected N-pole","NCA",321.81,0,321.81,8592765030771,1,8592765030771,null,28592765030775,"8536201090",1.7]
[103077,"Ex9M1N TM AC50 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=50A, 4-pole with protected N-pole","NCA",321.81,0,321.81,8592765030788,1,8592765030788,null,28592765030782,"8536201090",1.7]
[103078,"Ex9M1N TM AC63 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=63A, 4-pole with protected N-pole","NCA",343.66,0,343.66,8592765030795,1,8592765030795,null,28592765030799,"8536201090",1.7]
[103079,"Ex9M1N TM AC80 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=80A, 4-pole with protected N-pole","NCA",379.76,0,379.76,8592765030801,1,8592765030801,null,28592765030805,"8536209090",1.7]
[103080,"Ex9M1N TM AC100 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=100A, 4-pole with protected N-pole","NCA",389.99,0,389.99,8592765030818,1,8592765030818,null,28592765030812,"8536209090",1.7]
[103081,"Ex9M1N TM AC125 4P4T","Circuit Breaker, frame size M1, Icu=Ics=50kA, In=125A, 4-pole with protected N-pole","NCA",714.76,0,714.76,8592765030825,1,8592765030825,null,28592765030829,"8536209090",1.7]
[103102,"Ex9M1H TM AC16 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=16A, 4-pole with protected N-pole","NCA",382.93,0,382.93,8592765031037,1,8592765031037,null,28592765031031,"8536201090",1.7]
[103103,"Ex9M1H TM AC20 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=20A, 4-pole with protected N-pole","NCA",382.93,0,382.93,8592765031044,1,8592765031044,null,28592765031048,"8536201090",1.7]
[103104,"Ex9M1H TM AC25 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=25A, 4-pole with protected N-pole","NCA",382.93,0,382.93,8592765031051,1,8592765031051,null,28592765031055,"8536201090",1.7]
[103105,"Ex9M1H TM AC32 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=32A, 4-pole with protected N-pole","NCA",382.93,0,382.93,8592765031068,1,8592765031068,null,28592765031062,"8536201090",1.7]
[103106,"Ex9M1H TM AC40 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=40A, 4-pole with protected N-pole","NCA",382.93,0,382.93,8592765031075,1,8592765031075,null,28592765031079,"8536201090",1.7]
[103107,"Ex9M1H TM AC50 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=50A, 4-pole with protected N-pole","NCA",382.93,0,382.93,8592765031082,1,8592765031082,null,28592765031086,"8536201090",1.7]
[103108,"Ex9M1H TM AC63 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=63A, 4-pole with protected N-pole","NCA",397.94,0,397.94,8592765031099,1,8592765031099,null,28592765031093,"8536201090",1.7]
[103109,"Ex9M1H TM AC80 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=80A, 4-pole with protected N-pole","NCA",449.81,0,449.81,8592765031105,1,8592765031105,null,28592765031109,"8536209090",1.7]
[103110,"Ex9M1H TM AC100 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=100A, 4-pole with protected N-pole","NCA",530.70000000000005,0,530.70000000000005,8592765031112,1,8592765031112,null,28592765031116,"8536209090",1.7]
[103111,"Ex9M1H TM AC125 4P4T","Circuit Breaker, frame size M1, Icu=Ics=100kA, In=125A, 4-pole with protected N-pole","NCA",889.09,0,889.09,8592765031129,1,8592765031129,null,28592765031123,"8536209090",1.7]
[103122,"Ex9M1P TM AC16 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=16A, 4-pole with protected N-pole","NCA",529.96,0,529.96,8592765031235,1,8592765031235,null,28592765031239,"8536201090",1.7]
[103123,"Ex9M1P TM AC20 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=20A, 4-pole with protected N-pole","NCA",529.96,0,529.96,8592765031242,1,8592765031242,null,28592765031246,"8536201090",1.7]
[103124,"Ex9M1P TM AC25 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=25A, 4-pole with protected N-pole","NCA",529.96,0,529.96,8592765031259,1,8592765031259,null,28592765031253,"8536201090",1.7]
[103125,"Ex9M1P TM AC32 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=32A, 4-pole with protected N-pole","NCA",529.96,0,529.96,8592765031266,1,8592765031266,null,28592765031260,"8536201090",1.7]
[103126,"Ex9M1P TM AC40 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=40A, 4-pole with protected N-pole","NCA",529.96,0,529.96,8592765031273,1,8592765031273,null,28592765031277,"8536201090",1.7]
[103127,"Ex9M1P TM AC50 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=50A, 4-pole with protected N-pole","NCA",529.96,0,529.96,8592765031280,1,8592765031280,null,28592765031284,"8536201090",1.7]
[103128,"Ex9M1P TM AC63 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=63A, 4-pole with protected N-pole","NCA",611.21,0,611.21,8592765031297,1,8592765031297,null,28592765031291,"8536201090",1.7]
[103129,"Ex9M1P TM AC80 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=80A, 4-pole with protected N-pole","NCA",611.21,0,611.21,8592765031303,1,8592765031303,null,28592765031307,"8536209090",1.7]
[103130,"Ex9M1P TM AC100 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=100A, 4-pole with protected N-pole","NCA",656.27,0,656.27,8592765031310,1,8592765031310,null,28592765031314,"8536209090",1.7]
[103131,"Ex9M1P TM AC125 4P4T","Circuit Breaker, frame size M1, Icu=Ics=150kA, In=125A, 4-pole with protected N-pole","NCA",874.35,0,874.35,8592765031327,1,8592765031327,null,28592765031321,"8536209090",1.7]
[103132,"Ex9M2S TM AC125 4P4T","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=125A, 4-pole with protected N-pole","NCA",555.61,0,555.61,8592765031334,1,8592765031334,null,28592765031338,"8536209090",2.2000000000000002]
[103133,"Ex9M2S TM AC160 4P4T","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=160A, 4-pole with protected N-pole","NCA",617.61,0,617.61,8592765031341,1,8592765031341,null,28592765031345,"8536209090",2.2000000000000002]
[103134,"Ex9M2S TM AC180 4P4T","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=180A, 4-pole with protected N-pole","NCA",687.44,0,687.44,8592765031358,1,8592765031358,null,28592765031352,"8536209090",2.2000000000000002]
[103135,"Ex9M2S TM AC200 4P4T","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=200A, 4-pole with protected N-pole","NCA",759.08,0,759.08,8592765031365,1,8592765031365,null,28592765031369,"8536209090",2.2000000000000002]
[103136,"Ex9M2S TM AC225 4P4T","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=225A, 4-pole with protected N-pole","NCA",799.1,0,799.1,8592765031372,1,8592765031372,null,28592765031376,"8536209090",2.2000000000000002]
[103137,"Ex9M2S TM AC250 4P4T","Circuit Breaker, frame size M2, Icu=Ics=36kA, In=250A, 4-pole with protected N-pole","NCA",841.69,0,841.69,8592765031389,1,8592765031389,null,28592765031383,"8536209090",2.2000000000000002]
[103138,"Ex9M2N TM AC125 4P4T","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=125A, 4-pole with protected N-pole","NCA",617.32000000000005,0,617.32000000000005,8592765031396,1,8592765031396,null,28592765031390,"8536209090",2.2000000000000002]
[103139,"Ex9M2N TM AC160 4P4T","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=160A, 4-pole with protected N-pole","NCA",844.85,0,844.85,8592765031402,1,8592765031402,null,28592765031406,"8536209090",2.2000000000000002]
[103140,"Ex9M2N TM AC180 4P4T","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=180A, 4-pole with protected N-pole","NCA",927.76,0,927.76,8592765031419,1,8592765031419,null,28592765031413,"8536209090",2.2000000000000002]
[103141,"Ex9M2N TM AC200 4P4T","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=200A, 4-pole with protected N-pole","NCA",1001.81,0,1001.81,8592765031426,1,8592765031426,null,28592765031420,"8536209090",2.2000000000000002]
[103142,"Ex9M2N TM AC225 4P4T","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=225A, 4-pole with protected N-pole","NCA",1088.4100000000001,0,1088.4100000000001,8592765031433,1,8592765031433,null,28592765031437,"8536209090",2.2000000000000002]
[103143,"Ex9M2N TM AC250 4P4T","Circuit Breaker, frame size M2, Icu=Ics=50kA, In=250A, 4-pole with protected N-pole","NCA",1166.9100000000001,0,1166.9100000000001,8592765031440,1,8592765031440,null,28592765031444,"8536209090",2.2000000000000002]
[103156,"Ex9M2H TM AC125 4P4T","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=125A, 4-pole with protected N-pole","NCA",660.72,0,660.72,8592765031570,1,8592765031570,null,28592765031574,"8536209090",2.2000000000000002]
[103157,"Ex9M2H TM AC160 4P4T","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=160A, 4-pole with protected N-pole","NCA",893.75,0,893.75,8592765031587,1,8592765031587,null,28592765031581,"8536209090",2.2000000000000002]
[103158,"Ex9M2H TM AC180 4P4T","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=180A, 4-pole with protected N-pole","NCA",927.76,0,927.76,8592765031594,1,8592765031594,null,28592765031598,"8536209090",2.2000000000000002]
[103159,"Ex9M2H TM AC200 4P4T","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=200A, 4-pole with protected N-pole","NCA",1057.3399999999999,0,1057.3399999999999,8592765031600,1,8592765031600,null,28592765031604,"8536209090",2.2000000000000002]
[103160,"Ex9M2H TM AC225 4P4T","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=225A, 4-pole with protected N-pole","NCA",1088.4100000000001,0,1088.4100000000001,8592765031617,1,8592765031617,null,28592765031611,"8536209090",2.2000000000000002]
[103161,"Ex9M2H TM AC250 4P4T","Circuit Breaker, frame size M2, Icu=Ics=100kA, In=250A, 4-pole with protected N-pole","NCA",1230.3399999999999,0,1230.3399999999999,8592765031624,1,8592765031624,null,28592765031628,"8536209090",2.2000000000000002]
[103168,"Ex9M2P TM AC125 4P4T","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=125A, 4-pole with protected N-pole","NCA",716.1,0,716.1,8592765031693,1,8592765031693,null,28592765031697,"8536209090",2.2000000000000002]
[103169,"Ex9M2P TM AC160 4P4T","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=160A, 4-pole with protected N-pole","NCA",937.48,0,937.48,8592765031709,1,8592765031709,null,28592765031703,"8536209090",2.2000000000000002]
[103170,"Ex9M2P TM AC180 4P4T","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=180A, 4-pole with protected N-pole","NCA",1017.92,0,1017.92,8592765031716,1,8592765031716,null,28592765031710,"8536209090",2.2000000000000002]
[103171,"Ex9M2P TM AC200 4P4T","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=200A, 4-pole with protected N-pole","NCA",1095.49,0,1095.49,8592765031723,1,8592765031723,null,28592765031727,"8536209090",2.2000000000000002]
[103172,"Ex9M2P TM AC225 4P4T","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=225A, 4-pole with protected N-pole","NCA",1199.1099999999999,0,1199.1099999999999,8592765031730,1,8592765031730,null,28592765031734,"8536209090",2.2000000000000002]
[103173,"Ex9M2P TM AC250 4P4T","Circuit Breaker, frame size M2, Icu=Ics=150kA, In=250A, 4-pole with protected N-pole","NCA",1294.8900000000001,0,1294.8900000000001,8592765031747,1,8592765031747,null,28592765031741,"8536209090",2.2000000000000002]
[103174,"Ex9M3S TM AC250 4P4T","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=250A, 4-pole with protected N-pole","NCA",1136.3399999999999,{"$f":"NCA","v":0},1136.3399999999999,8592765031754,1,8592765031754,null,28592765031758,"8536209090",6.6]
[103175,"Ex9M3S TM AC315 4P4T","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=315A, 4-pole with protected N-pole","NCA",1217.6099999999999,0,{"$f":"E2443*(1-F2443)","v":1217.6099999999999},8592765031761,1,8592765031761,null,28592765031765,"8536209090",6.6]
[103176,"Ex9M3S TM AC350 4P4T","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=350A, 4-pole with protected N-pole","NCA",1276.3,0,1276.3,8592765031778,1,8592765031778,null,28592765031772,"8536209090",6.6]
[103177,"Ex9M3S TM AC400 4P4T","Circuit Breaker, frame size M3, Icu=Ics=36kA, In=400A, 4-pole with protected N-pole","NCA",1300.24,0,1300.24,8592765031785,1,8592765031785,null,28592765031789,"8536209090",6.6]
[103178,"Ex9M3N TM AC250 4P4T","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=250A, 4-pole with protected N-pole","NCA",1202.42,0,1202.42,8592765031792,1,8592765031792,null,28592765031796,"8536209090",6.6]
[103179,"Ex9M3N TM AC315 4P4T","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=315A, 4-pole with protected N-pole","NCA",1273.3,0,1273.3,8592765031808,1,8592765031808,null,28592765031802,"8536209090",6.6]
[103180,"Ex9M3N TM AC350 4P4T","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=350A, 4-pole with protected N-pole","NCA",1341.47,0,1341.47,8592765031815,1,8592765031815,null,28592765031819,"8536209090",6.6]
[103181,"Ex9M3N TM AC400 4P4T","Circuit Breaker, frame size M3, Icu=Ics=50kA, In=400A, 4-pole with protected N-pole","NCA",1363.74,0,1363.74,8592765031822,1,8592765031822,null,28592765031826,"8536209090",6.6]
[103190,"Ex9M3H TM AC250 4P4T","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=250A, 4-pole with protected N-pole","NCA",1758.13,0,1758.13,8592765031914,1,8592765031914,null,28592765031918,"8536209090",6.6]
[103191,"Ex9M3H TM AC315 4P4T","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=315A, 4-pole with protected N-pole","NCA",1790.69,0,1790.69,8592765031921,1,8592765031921,null,28592765031925,"8536209090",6.6]
[103192,"Ex9M3H TM AC350 4P4T","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=350A, 4-pole with protected N-pole","NCA",1819.62,0,1819.62,8592765031938,1,8592765031938,null,28592765031932,"8536209090",6.6]
[103193,"Ex9M3H TM AC400 4P4T","Circuit Breaker, frame size M3, Icu=Ics=100kA, In=400A, 4-pole with protected N-pole","NCA",1891.99,0,1891.99,8592765031945,1,8592765031945,null,28592765031949,"8536209090",6.6]
[103198,"Ex9M3P TM AC250 4P4T","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=250A, 4-pole with protected N-pole","NCA",1967.94,0,1967.94,8592765031990,1,8592765031990,null,28592765031994,"8536209090",6.6]
[103199,"Ex9M3P TM AC315 4P4T","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=315A, 4-pole with protected N-pole","NCA",2004.11,0,2004.11,8592765032003,1,8592765032003,null,28592765032007,"8536209090",6.6]
[103200,"Ex9M3P TM AC350 4P4T","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=350A, 4-pole with protected N-pole","NCA",2036.69,0,2036.69,8592765032010,1,8592765032010,null,28592765032014,"8536209090",6.6]
[103201,"Ex9M3P TM AC400 4P4T","Circuit Breaker, frame size M3, Icu=Ics=150kA, In=400A, 4-pole with protected N-pole","NCA",2119.87,0,2119.87,8592765032027,1,8592765032027,null,28592765032021,"8536209090",6.6]
[103415,"Ex9M4S TM AC400 4P4T","Circuit Breaker, frame size M4, Icu=Ics=36kA, In=400A, 4-pole with protected N-pole","NCA",1619.18,{"$f":"NCA","v":0},{"$f":"E2458*(1-F2458)","v":1619.18},8592765034168,1,8592765034168,null,28592765034162,"8536209090",13.5]
[103416,"Ex9M4S TM AC500 4P4T","Circuit Breaker, frame size M4, Icu=Ics=36kA, In=500A, 4-pole with protected N-pole","NCA",1868.18,0,{"$f":"E2459*(1-F2459)","v":1868.18},8592765034175,1,8592765034175,null,28592765034179,"8536209090",13.5]
[103417,"Ex9M4S TM AC630 4P4T","Circuit Breaker, frame size M4, Icu=Ics=36kA, In=630A, 4-pole with protected N-pole","NCA",2131.08,0,2131.08,8592765034182,1,8592765034182,null,28592765034186,"8536209090",13.5]
[103418,"Ex9M4N TM AC400 4P4T","Circuit Breaker, frame size M4, Icu=Ics=50kA, In=400A, 4-pole with protected N-pole","NCA",1639.29,0,1639.29,8592765034199,1,8592765034199,null,28592765034193,"8536209090",13.5]
[103419,"Ex9M4N TM AC500 4P4T","Circuit Breaker, frame size M4, Icu=Ics=50kA, In=500A, 4-pole with protected N-pole","NCA",1888.29,0,1888.29,8592765034205,1,8592765034205,null,28592765034209,"8536209090",13.5]
[103420,"Ex9M4N TM AC630 4P4T","Circuit Breaker, frame size M4, Icu=Ics=50kA, In=630A, 4-pole with protected N-pole","NCA",2177.4699999999998,0,2177.4699999999998,8592765034212,1,8592765034212,null,28592765034216,"8536209090",13.5]
[103427,"Ex9M4H TM AC400 4P4T","Circuit Breaker, frame size M4, Icu=Ics=100kA, In=400A, 4-pole with protected N-pole","NCA",2919.8,0,2919.8,8592765034281,1,8592765034281,null,28592765034285,"8536209090",13.5]
[103428,"Ex9M4H TM AC500 4P4T","Circuit Breaker, frame size M4, Icu=Ics=100kA, In=500A, 4-pole with protected N-pole","NCA",3156.41,0,3156.41,8592765034298,1,8592765034298,null,28592765034292,"8536209090",13.5]
[103429,"Ex9M4H TM AC630 4P4T","Circuit Breaker, frame size M4, Icu=Ics=100kA, In=630A, 4-pole with protected N-pole","NCA",3439.42,0,3439.42,8592765034304,1,8592765034304,null,28592765034308,"8536209090",13.5]
[103433,"Ex9M4P TM AC400 4P4T","Circuit Breaker, frame size M4, Icu=Ics=150kA, In=400A, 4-pole with protected N-pole","NCA",2366.15,0,2366.15,8592765034342,1,8592765034342,null,28592765034346,"8536209090",13.5]
[103434,"Ex9M4P TM AC500 4P4T","Circuit Breaker, frame size M4, Icu=Ics=150kA, In=500A, 4-pole with protected N-pole","NCA",2774.43,0,2774.43,8592765034359,1,8592765034359,null,28592765034353,"8536209090",13.5]
[103435,"Ex9M4P TM AC630 4P4T","Circuit Breaker, frame size M4, Icu=Ics=150kA, In=630A, 4-pole with protected N-pole","NCA",3190.43,0,3190.43,8592765034366,1,8592765034366,null,28592765034360,"8536209090",13.5]
[103436,"Ex9M5S TM AC630 4P4T","Circuit Breaker, frame size M5, Icu=Ics=36kA, In=630A, 4-pole with protected N-pole","NCA",1861.99,0,1861.99,8592765034373,1,8592765034373,null,28592765034377,"8536209090",13.5]
[103437,"Ex9M5S TM AC700 4P4T","Circuit Breaker, frame size M5, Icu=Ics=36kA, In=700A, 4-pole with protected N-pole","NCA",2148.1,0,2148.1,8592765034380,1,8592765034380,null,28592765034384,"8536209090",13.5]
[103438,"Ex9M5S TM AC800 4P4T","Circuit Breaker, frame size M5, Icu=Ics=36kA, In=800A, 4-pole with protected N-pole","NCA",2451.21,0,2451.21,8592765034397,1,8592765034397,null,28592765034391,"8536209090",13.5]
[103439,"Ex9M5N TM AC630 4P4T","Circuit Breaker, frame size M5, Icu=Ics=50kA, In=630A, 4-pole with protected N-pole","NCA",1885.19,0,1885.19,8592765034403,1,8592765034403,null,28592765034407,"8536209090",13.5]
[103440,"Ex9M5N TM AC700 4P4T","Circuit Breaker, frame size M5, Icu=Ics=50kA, In=700A, 4-pole with protected N-pole","NCA",2171.29,0,2171.29,8592765034410,1,8592765034410,null,28592765034414,"8536209090",13.5]
[103441,"Ex9M5N TM AC800 4P4T","Circuit Breaker, frame size M5, Icu=Ics=50kA, In=800A, 4-pole with protected N-pole","NCA",2503.79,0,2503.79,8592765034427,1,8592765034427,null,28592765034421,"8536209090",13.5]
[103448,"Ex9M5H TM AC630 4P4T","Circuit Breaker, frame size M5, Icu=Ics=100kA, In=630A, 4-pole with protected N-pole","NCA",3357.45,0,3357.45,8592765034496,1,8592765034496,null,28592765034490,"8536209090",13.5]
[103449,"Ex9M5H TM AC700 4P4T","Circuit Breaker, frame size M5, Icu=Ics=100kA, In=700A, 4-pole with protected N-pole","NCA",3629.64,0,3629.64,8592765034502,1,8592765034502,null,28592765034506,"8536209090",13.5]
[103450,"Ex9M5H TM AC800 4P4T","Circuit Breaker, frame size M5, Icu=Ics=100kA, In=800A, 4-pole with protected N-pole","NCA",3955.95,0,3955.95,8592765034519,1,8592765034519,null,28592765034513,"8536209090",13.5]
[103454,"Ex9M5P TM AC630 4P4T","Circuit Breaker, frame size M5, Icu=Ics=150kA, In=630A, 4-pole with protected N-pole","NCA",2721.84,0,2721.84,8592765034557,1,8592765034557,null,28592765034551,"8536209090",13.5]
[103455,"Ex9M5P TM AC700 4P4T","Circuit Breaker, frame size M5, Icu=Ics=150kA, In=700A, 4-pole with protected N-pole","NCA",3190.43,0,3190.43,8592765034564,1,8592765034564,null,28592765034568,"8536209090",13.5]
[103456,"Ex9M5P TM AC800 4P4T","Circuit Breaker, frame size M5, Icu=Ics=150kA, In=800A, 4-pole with protected N-pole","NCA",3668.3,0,3668.3,8592765034571,1,8592765034571,null,28592765034575,"8536209090",13.5]
[]
["DC Moulded Case Circuit Breakers Ex9MD"]
[101768,"Ex9MD1B TM DC16 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=16A, 3-pole","NCB",319.26,{"$f":"NCB","v":0},{"$f":"E2484*(1-F2484)","v":319.26},8592765017697,1,8592765017697,null,28592765017691,"8536201090",1.2]
[101769,"Ex9MD1B TM DC20 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=20A, 3-pole","NCB",319.26,0,319.26,8592765017703,1,8592765017703,null,28592765017707,"8536201090",1.2]
[101770,"Ex9MD1B TM DC25 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=25A, 3-pole","NCB",321.94,0,321.94,8592765017710,1,8592765017710,null,28592765017714,"8536201090",1.2]
[101771,"Ex9MD1B TM DC32 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=32A, 3-pole","NCB",324.61,0,324.61,8592765017727,1,8592765017727,null,28592765017721,"8536201090",1.2]
[101772,"Ex9MD1B TM DC40 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=40A, 3-pole","NCB",332.66,0,332.66,8592765017734,1,8592765017734,null,28592765017738,"8536201090",1.2]
[101773,"Ex9MD1B TM DC50 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=50A, 3-pole","NCB",343.39,0,343.39,8592765017741,1,8592765017741,null,28592765017745,"8536201090",1.2]
[101774,"Ex9MD1B TM DC63 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=63A, 3-pole","NCB",362.17,0,362.17,8592765017758,1,8592765017758,null,28592765017752,"8536201090",1.2]
[101775,"Ex9MD1B TM DC80 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=80A, 3-pole","NCB",380.97,0,380.97,8592765017765,1,8592765017765,null,28592765017769,"8536209090",1.2]
[101776,"Ex9MD1B TM DC100 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=100A, 3-pole","NCB",426.55,0,426.55,8592765017772,1,8592765017772,null,28592765017776,"8536209090",1.2]
[101777,"Ex9MD1B TM DC125 3P","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=125A, 3-pole","NCB",482.91,0,482.91,8592765017789,1,8592765017789,null,28592765017783,"8536209090",1.2]
[101778,"Ex9MD1S TM DC16 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=16A, 3-pole","NCB",378.28,0,378.28,8592765017796,1,8592765017796,null,28592765017790,"8536201090",1.2]
[101779,"Ex9MD1S TM DC20 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=20A, 3-pole","NCB",380.97,0,380.97,8592765017802,1,8592765017802,null,28592765017806,"8536201090",1.2]
[101780,"Ex9MD1S TM DC25 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=25A, 3-pole","NCB",383.63,0,383.63,8592765017819,1,8592765017819,null,28592765017813,"8536201090",1.2]
[101781,"Ex9MD1S TM DC32 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=32A, 3-pole","NCB",388.99,0,388.99,8592765017826,1,8592765017826,null,28592765017820,"8536201090",1.2]
[101782,"Ex9MD1S TM DC40 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=40A, 3-pole","NCB",394.36,0,394.36,8592765017833,1,8592765017833,null,28592765017837,"8536201090",1.2]
[101783,"Ex9MD1S TM DC50 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=50A, 3-pole","NCB",407.79,0,407.79,8592765017840,1,8592765017840,null,28592765017844,"8536201090",1.2]
[101784,"Ex9MD1S TM DC63 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=63A, 3-pole","NCB",423.88,0,423.88,8592765017857,1,8592765017857,null,28592765017851,"8536201090",1.2]
[101785,"Ex9MD1S TM DC80 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=80A, 3-pole","NCB",453.38,0,453.38,8592765017864,1,8592765017864,null,28592765017868,"8536209090",1.2]
[101786,"Ex9MD1S TM DC100 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=100A, 3-pole","NCB",490.94,0,490.94,8592765017871,1,8592765017871,null,28592765017875,"8536209090",1.2]
[101787,"Ex9MD1S TM DC125 3P","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=125A, 3-pole","NCB",549.98,0,549.98,8592765017888,1,8592765017888,null,28592765017882,"8536209090",1.2]
[101788,"Ex9MD1N TM DC16 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=16A, 3-pole","NCB",469.48,0,469.48,8592765017895,1,8592765017895,null,28592765017899,"8536201090",1.2]
[101789,"Ex9MD1N TM DC20 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=20A, 3-pole","NCB",472.18,0,472.18,8592765017901,1,8592765017901,null,28592765017905,"8536201090",1.2]
[101790,"Ex9MD1N TM DC25 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=25A, 3-pole","NCB",477.53,0,477.53,8592765017918,1,8592765017918,null,28592765017912,"8536201090",1.2]
[101791,"Ex9MD1N TM DC32 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=32A, 3-pole","NCB",485.57,0,485.57,8592765017925,1,8592765017925,null,28592765017929,"8536201090",1.2]
[101792,"Ex9MD1N TM DC40 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=40A, 3-pole","NCB",496.31,0,496.31,8592765017932,1,8592765017932,null,28592765017936,"8536201090",1.2]
[101793,"Ex9MD1N TM DC50 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=50A, 3-pole","NCB",509.73,0,509.73,8592765017949,1,8592765017949,null,28592765017943,"8536201090",1.2]
[101794,"Ex9MD1N TM DC63 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=63A, 3-pole","NCB",525.83000000000004,0,525.83000000000004,8592765017956,1,8592765017956,null,28592765017950,"8536201090",1.2]
[101795,"Ex9MD1N TM DC80 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=80A, 3-pole","NCB",544.6,0,544.6,8592765017963,1,8592765017963,null,28592765017967,"8536209090",1.2]
[101796,"Ex9MD1N TM DC100 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=100A, 3-pole","NCB",568.75,0,568.75,8592765017970,1,8592765017970,null,28592765017974,"8536209090",1.2]
[101797,"Ex9MD1N TM DC125 3P","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=125A, 3-pole","NCB",641.19000000000005,0,641.19000000000005,8592765017987,1,8592765017987,null,28592765017981,"8536209090",1.2]
[101818,"Ex9MD1H TM DC16 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=16A, 3-pole","NCB",670.69,0,670.69,8592765018199,1,8592765018199,null,28592765018193,"8536201090",1.2]
[101819,"Ex9MD1H TM DC20 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=20A, 3-pole","NCB",676.07,0,676.07,8592765018205,1,8592765018205,null,28592765018209,"8536201090",1.2]
[101820,"Ex9MD1H TM DC25 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=25A, 3-pole","NCB",684.11,{"$f":"NCB","v":0},684.11,8592765018212,1,8592765018212,null,28592765018216,"8536201090",1.2]
[101821,"Ex9MD1H TM DC32 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=32A, 3-pole","NCB",694.84,0,694.84,8592765018229,1,8592765018229,null,28592765018223,"8536201090",1.2]
[101822,"Ex9MD1H TM DC40 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=40A, 3-pole","NCB",708.24,0,708.24,8592765018236,1,8592765018236,null,28592765018230,"8536201090",1.2]
[101823,"Ex9MD1H TM DC50 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=50A, 3-pole","NCB",721.67,0,721.67,8592765018243,1,8592765018243,null,28592765018247,"8536201090",1.2]
[101824,"Ex9MD1H TM DC63 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=63A, 3-pole","NCB",740.44,0,740.44,8592765018250,1,8592765018250,null,28592765018254,"8536201090",1.2]
[101825,"Ex9MD1H TM DC80 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=80A, 3-pole","NCB",767.28,0,767.28,8592765018267,1,8592765018267,null,28592765018261,"8536209090",1.2]
[101826,"Ex9MD1H TM DC100 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=100A, 3-pole","NCB",807.51,0,807.51,8592765018274,1,8592765018274,null,28592765018278,"8536209090",1.2]
[101827,"Ex9MD1H TM DC125 3P","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=125A, 3-pole","NCB",898.73,0,898.73,8592765018281,1,8592765018281,null,28592765018285,"8536209090",1.2]
[101828,"Ex9MD1B TM DC16 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=16A, 4-pole ","NCB",399.72,0,399.72,8592765018298,1,8592765018298,null,28592765018292,"8536201090",1.7]
[101829,"Ex9MD1B TM DC20 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=20A, 4-pole ","NCB",405.1,0,405.1,8592765018304,1,8592765018304,null,28592765018308,"8536201090",1.7]
[101830,"Ex9MD1B TM DC25 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=25A, 4-pole ","NCB",418.51,0,418.51,8592765018311,1,8592765018311,null,28592765018315,"8536201090",1.7]
[101831,"Ex9MD1B TM DC32 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=32A, 4-pole ","NCB",426.55,0,426.55,8592765018328,1,8592765018328,null,28592765018322,"8536201090",1.7]
[101832,"Ex9MD1B TM DC40 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=40A, 4-pole ","NCB",437.29,0,437.29,8592765018335,1,8592765018335,null,28592765018339,"8536201090",1.7]
[101833,"Ex9MD1B TM DC50 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=50A, 4-pole ","NCB",450.7,0,450.7,8592765018342,1,8592765018342,null,28592765018346,"8536201090",1.7]
[101834,"Ex9MD1B TM DC63 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=63A, 4-pole ","NCB",477.53,0,477.53,8592765018359,1,8592765018359,null,28592765018353,"8536201090",1.7]
[101835,"Ex9MD1B TM DC80 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=80A, 4-pole ","NCB",496.31,0,496.31,8592765018366,1,8592765018366,null,28592765018360,"8536209090",1.7]
[101836,"Ex9MD1B TM DC100 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=100A, 4-pole ","NCB",512.41,0,512.41,8592765018373,1,8592765018373,null,28592765018377,"8536209090",1.7]
[101837,"Ex9MD1B TM DC125 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=25kA, In=125A, 4-pole ","NCB",541.91,0,541.91,8592765018380,1,8592765018380,null,28592765018384,"8536209090",1.7]
[101838,"Ex9MD1S TM DC16 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=16A, 4-pole ","NCB",504.35,0,504.35,8592765018397,1,8592765018397,null,28592765018391,"8536201090",1.7]
[101839,"Ex9MD1S TM DC20 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=20A, 4-pole ","NCB",509.73,0,509.73,8592765018403,1,8592765018403,null,28592765018407,"8536201090",1.7]
[101840,"Ex9MD1S TM DC25 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=25A, 4-pole ","NCB",517.78,0,517.78,8592765018410,1,8592765018410,null,28592765018414,"8536201090",1.7]
[101841,"Ex9MD1S TM DC32 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=32A, 4-pole ","NCB",525.83000000000004,0,525.83000000000004,8592765018427,1,8592765018427,null,28592765018421,"8536201090",1.7]
[101842,"Ex9MD1S TM DC40 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=40A, 4-pole ","NCB",539.24,0,539.24,8592765018434,1,8592765018434,null,28592765018438,"8536201090",1.7]
[101843,"Ex9MD1S TM DC50 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=50A, 4-pole ","NCB",552.65,0,552.65,8592765018441,1,8592765018441,null,28592765018445,"8536201090",1.7]
[101844,"Ex9MD1S TM DC63 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=63A, 4-pole ","NCB",574.12,0,574.12,8592765018458,1,8592765018458,null,28592765018452,"8536201090",1.7]
[101845,"Ex9MD1S TM DC80 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=80A, 4-pole ","NCB",606.29999999999995,0,606.29999999999995,8592765018465,1,8592765018465,null,28592765018469,"8536209090",1.7]
[101846,"Ex9MD1S TM DC100 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=100A, 4-pole ","NCB",630.45000000000005,0,630.45000000000005,8592765018472,1,8592765018472,null,28592765018476,"8536209090",1.7]
[101847,"Ex9MD1S TM DC125 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=36kA, In=125A, 4-pole ","NCB",649.22,0,649.22,8592765018489,1,8592765018489,null,28592765018483,"8536209090",1.7]
[101848,"Ex9MD1N TM DC16 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=16A, 4-pole ","NCB",649.22,0,649.22,8592765018496,1,8592765018496,null,28592765018490,"8536201090",1.7]
[101849,"Ex9MD1N TM DC20 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=20A, 4-pole ","NCB",654.59,0,654.59,8592765018502,1,8592765018502,null,28592765018506,"8536201090",1.7]
[101850,"Ex9MD1N TM DC25 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=25A, 4-pole ","NCB",659.95,0,659.95,8592765018519,1,8592765018519,null,28592765018513,"8536201090",1.7]
[101851,"Ex9MD1N TM DC32 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=32A, 4-pole ","NCB",670.69,0,670.69,8592765018526,1,8592765018526,null,28592765018520,"8536201090",1.7]
[101852,"Ex9MD1N TM DC40 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=40A, 4-pole ","NCB",684.11,{"$f":"NCB","v":0},{"$f":"E2548*(1-F2548)","v":684.11},8592765018533,1,8592765018533,null,28592765018537,"8536201090",1.7]
[101853,"Ex9MD1N TM DC50 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=50A, 4-pole ","NCB",702.89,0,702.89,8592765018540,1,8592765018540,null,28592765018544,"8536201090",1.7]
[101854,"Ex9MD1N TM DC63 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=63A, 4-pole ","NCB",732.4,0,732.4,8592765018557,1,8592765018557,null,28592765018551,"8536201090",1.7]
[101855,"Ex9MD1N TM DC80 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=80A, 4-pole ","NCB",769.96,0,769.96,8592765018564,1,8592765018564,null,28592765018568,"8536209090",1.7]
[101856,"Ex9MD1N TM DC100 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=100A, 4-pole ","NCB",810.2,0,810.2,8592765018571,1,8592765018571,null,28592765018575,"8536209090",1.7]
[101857,"Ex9MD1N TM DC125 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=50kA, In=125A, 4-pole ","NCB",912.14,0,912.14,8592765018588,1,8592765018588,null,28592765018582,"8536209090",1.7]
[101878,"Ex9MD1H TM DC16 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=16A, 4-pole ","NCB",930.93,0,930.93,8592765018793,1,8592765018793,null,28592765018797,"8536201090",1.7]
[101879,"Ex9MD1H TM DC20 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=20A, 4-pole ","NCB",936.28,0,936.28,8592765018809,1,8592765018809,null,28592765018803,"8536201090",1.7]
[101880,"Ex9MD1H TM DC25 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=25A, 4-pole ","NCB",944.33,0,944.33,8592765018816,1,8592765018816,null,28592765018810,"8536201090",1.7]
[101881,"Ex9MD1H TM DC32 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=32A, 4-pole ","NCB",955.06,0,955.06,8592765018823,1,8592765018823,null,28592765018827,"8536201090",1.7]
[101882,"Ex9MD1H TM DC40 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=40A, 4-pole ","NCB",968.48,0,968.48,8592765018830,1,8592765018830,null,28592765018834,"8536201090",1.7]
[101883,"Ex9MD1H TM DC50 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=50A, 4-pole ","NCB",987.27,0,987.27,8592765018847,1,8592765018847,null,28592765018841,"8536201090",1.7]
[101884,"Ex9MD1H TM DC63 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=63A, 4-pole ","NCB",1011.4,0,1011.4,8592765018854,1,8592765018854,null,28592765018858,"8536201090",1.7]
[101885,"Ex9MD1H TM DC80 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=80A, 4-pole ","NCB",1040.92,0,1040.92,8592765018861,1,8592765018861,null,28592765018865,"8536209090",1.7]
[101886,"Ex9MD1H TM DC100 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=100A, 4-pole ","NCB",1099.94,0,1099.94,8592765018878,1,8592765018878,null,28592765018872,"8536209090",1.7]
[101887,"Ex9MD1H TM DC125 4P4T","DC Circuit Breaker, frame size M1, Icu=Ics=100kA, In=125A, 4-pole ","NCB",1193.8399999999999,0,1193.8399999999999,8592765018885,1,8592765018885,null,28592765018889,"8536209090",1.7]
[101888,"Ex9MD2B TM DC125 3P","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=125A, 3-pole","NCB",351.44,0,351.44,8592765018892,1,8592765018892,null,28592765018896,"8536209090",1.7]
[101889,"Ex9MD2B TM DC160 3P","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=160A, 3-pole","NCB",418.51,0,418.51,8592765018908,1,8592765018908,null,28592765018902,"8536209090",1.7]
[101890,"Ex9MD2B TM DC180 3P","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=180A, 3-pole","NCB",402.41,0,402.41,8592765018915,1,8592765018915,null,28592765018919,"8536209090",1.7]
[101891,"Ex9MD2B TM DC200 3P","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=200A, 3-pole","NCB",442.66,0,442.66,8592765018922,1,8592765018922,null,28592765018926,"8536209090",1.7]
[101892,"Ex9MD2B TM DC225 3P","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=225A, 3-pole","NCB",458.75,0,458.75,8592765018939,1,8592765018939,null,28592765018933,"8536209090",1.7]
[101893,"Ex9MD2B TM DC250 3P","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=250A, 3-pole","NCB",480.21,0,480.21,8592765018946,1,8592765018946,null,28592765018940,"8536209090",1.7]
[101894,"Ex9MD2S TM DC125 3P","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=125A, 3-pole","NCB",402.41,0,402.41,8592765018953,1,8592765018953,null,28592765018957,"8536209090",1.7]
[101895,"Ex9MD2S TM DC160 3P","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=160A, 3-pole","NCB",458.75,0,458.75,8592765018960,1,8592765018960,null,28592765018964,"8536209090",1.7]
[101896,"Ex9MD2S TM DC180 3P","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=180A, 3-pole","NCB",474.84,0,474.84,8592765018977,1,8592765018977,null,28592765018971,"8536209090",1.7]
[101897,"Ex9MD2S TM DC200 3P","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=200A, 3-pole","NCB",490.94,0,490.94,8592765018984,1,8592765018984,null,28592765018988,"8536209090",1.7]
[101898,"Ex9MD2S TM DC225 3P","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=225A, 3-pole","NCB",509.73,0,509.73,8592765018991,1,8592765018991,null,28592765018995,"8536209090",1.7]
[101899,"Ex9MD2S TM DC250 3P","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=250A, 3-pole","NCB",531.19000000000005,0,531.19000000000005,8592765019004,1,8592765019004,null,28592765019008,"8536209090",1.7]
[101900,"Ex9MD2N TM DC125 3P","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=125A, 3-pole","NCB",501.66,0,501.66,8592765019011,1,8592765019011,null,28592765019015,"8536209090",1.7]
[101901,"Ex9MD2N TM DC160 3P","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=160A, 3-pole","NCB",560.71,0,560.71,8592765019028,1,8592765019028,null,28592765019022,"8536209090",1.7]
[101902,"Ex9MD2N TM DC180 3P","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=180A, 3-pole","NCB",576.79999999999995,0,576.79999999999995,8592765019035,1,8592765019035,null,28592765019039,"8536209090",1.7]
[101903,"Ex9MD2N TM DC200 3P","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=200A, 3-pole","NCB",592.89,0,592.89,8592765019042,1,8592765019042,null,28592765019046,"8536209090",1.7]
[101904,"Ex9MD2N TM DC225 3P","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=225A, 3-pole","NCB",614.36,{"$f":"NCB","v":0},614.36,8592765019059,1,8592765019059,null,28592765019053,"8536209090",1.7]
[101905,"Ex9MD2N TM DC250 3P","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=250A, 3-pole","NCB",635.83000000000004,0,635.83000000000004,8592765019066,1,8592765019066,null,28592765019060,"8536209090",1.7]
[101918,"Ex9MD2H TM DC125 3P","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=125A, 3-pole","NCB",710.93,0,710.93,8592765019196,1,8592765019196,null,28592765019190,"8536209090",1.7]
[101919,"Ex9MD2H TM DC160 3P","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=160A, 3-pole","NCB",748.49,0,748.49,8592765019202,1,8592765019202,null,28592765019206,"8536209090",1.7]
[101920,"Ex9MD2H TM DC180 3P","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=180A, 3-pole","NCB",772.64,0,772.64,8592765019219,1,8592765019219,null,28592765019213,"8536209090",1.7]
[101921,"Ex9MD2H TM DC200 3P","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=200A, 3-pole","NCB",791.41,0,791.41,8592765019226,1,8592765019226,null,28592765019220,"8536209090",1.7]
[101922,"Ex9MD2H TM DC225 3P","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=225A, 3-pole","NCB",812.88,0,812.88,8592765019233,1,8592765019233,null,28592765019237,"8536209090",1.7]
[101923,"Ex9MD2H TM DC250 3P","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=250A, 3-pole","NCB",834.34,0,834.34,8592765019240,1,8592765019240,null,28592765019244,"8536209090",1.7]
[101924,"Ex9MD2B TM DC125 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=125A, 4-pole ","NCB",477.53,0,477.53,8592765019257,1,8592765019257,null,28592765019251,"8536209090",2.2000000000000002]
[101925,"Ex9MD2B TM DC160 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=160A, 4-pole ","NCB",560.71,0,560.71,8592765019264,1,8592765019264,null,28592765019268,"8536209090",2.2000000000000002]
[101926,"Ex9MD2B TM DC180 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=180A, 4-pole ","NCB",574.12,0,574.12,8592765019271,1,8592765019271,null,28592765019275,"8536209090",2.2000000000000002]
[101927,"Ex9MD2B TM DC200 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=200A, 4-pole ","NCB",590.20000000000005,0,590.20000000000005,8592765019288,1,8592765019288,null,28592765019282,"8536209090",2.2000000000000002]
[101928,"Ex9MD2B TM DC225 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=225A, 4-pole ","NCB",611.67999999999995,0,611.67999999999995,8592765019295,1,8592765019295,null,28592765019299,"8536209090",2.2000000000000002]
[101929,"Ex9MD2B TM DC250 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=25kA, In=250A, 4-pole ","NCB",635.83000000000004,0,635.83000000000004,8592765019301,1,8592765019301,null,28592765019305,"8536209090",2.2000000000000002]
[101930,"Ex9MD2S TM DC125 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=125A, 4-pole ","NCB",587.53,0,587.53,8592765019318,1,8592765019318,null,28592765019312,"8536209090",2.2000000000000002]
[101931,"Ex9MD2S TM DC160 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=160A, 4-pole ","NCB",635.83000000000004,0,635.83000000000004,8592765019325,1,8592765019325,null,28592765019329,"8536209090",2.2000000000000002]
[101932,"Ex9MD2S TM DC180 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=180A, 4-pole ","NCB",649.22,0,649.22,8592765019332,1,8592765019332,null,28592765019336,"8536209090",2.2000000000000002]
[101933,"Ex9MD2S TM DC200 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=200A, 4-pole ","NCB",662.65,0,662.65,8592765019349,1,8592765019349,null,28592765019343,"8536209090",2.2000000000000002]
[101934,"Ex9MD2S TM DC225 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=225A, 4-pole ","NCB",678.74,0,678.74,8592765019356,1,8592765019356,null,28592765019350,"8536209090",2.2000000000000002]
[101935,"Ex9MD2S TM DC250 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=36kA, In=250A, 4-pole ","NCB",702.89,0,702.89,8592765019363,1,8592765019363,null,28592765019367,"8536209090",2.2000000000000002]
[101936,"Ex9MD2N TM DC125 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=125A, 4-pole ","NCB",743.12,0,743.12,8592765019370,1,8592765019370,null,28592765019374,"8536209090",2.2000000000000002]
[101937,"Ex9MD2N TM DC160 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=160A, 4-pole ","NCB",780.69,0,780.69,8592765019387,1,8592765019387,null,28592765019381,"8536209090",2.2000000000000002]
[101938,"Ex9MD2N TM DC180 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=180A, 4-pole ","NCB",796.78,0,796.78,8592765019394,1,8592765019394,null,28592765019398,"8536209090",2.2000000000000002]
[101939,"Ex9MD2N TM DC200 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=200A, 4-pole ","NCB",826.29,0,826.29,8592765019400,1,8592765019400,null,28592765019404,"8536209090",2.2000000000000002]
[101940,"Ex9MD2N TM DC225 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=225A, 4-pole ","NCB",855.81,0,855.81,8592765019417,1,8592765019417,null,28592765019411,"8536209090",2.2000000000000002]
[101941,"Ex9MD2N TM DC250 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=50kA, In=250A, 4-pole ","NCB",898.73,0,898.73,8592765019424,1,8592765019424,null,28592765019428,"8536209090",2.2000000000000002]
[101954,"Ex9MD2H TM DC125 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=125A, 4-pole ","NCB",1040.92,0,1040.92,8592765019554,1,8592765019554,null,28592765019558,"8536209090",2.2000000000000002]
[101955,"Ex9MD2H TM DC160 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=160A, 4-pole ","NCB",1057,0,1057,8592765019561,1,8592765019561,null,28592765019565,"8536209090",2.2000000000000002]
[101956,"Ex9MD2H TM DC180 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=180A, 4-pole ","NCB",1070.44,0,1070.44,8592765019578,1,8592765019578,null,28592765019572,"8536209090",2.2000000000000002]
[101957,"Ex9MD2H TM DC200 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=200A, 4-pole ","NCB",1102.6300000000001,0,1102.6300000000001,8592765019585,1,8592765019585,null,28592765019589,"8536209090",2.2000000000000002]
[101958,"Ex9MD2H TM DC225 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=225A, 4-pole ","NCB",1134.83,0,1134.83,8592765019592,1,8592765019592,null,28592765019596,"8536209090",2.2000000000000002]
[101959,"Ex9MD2H TM DC250 4P4T","DC Circuit Breaker, frame size M2, Icu=Ics=100kA, In=250A, 4-pole ","NCB",1185.8,0,1185.8,8592765019608,1,8592765019608,null,28592765019602,"8536209090",2.2000000000000002]
[101960,"Ex9MD3B TM DC250 3P","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=250A, 3-pole","NCB",464.12,{"$f":"NCB","v":0},{"$f":"E2612*(1-F2612)","v":464.12},8592765019615,1,8592765019615,null,28592765019619,"8536209090",5]
[101961,"Ex9MD3B TM DC315 3P","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=315A, 3-pole","NCB",482.91,0,482.91,8592765019622,1,8592765019622,null,28592765019626,"8536209090",5]
[101962,"Ex9MD3B TM DC350 3P","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=350A, 3-pole","NCB",507.04,0,507.04,8592765019639,1,8592765019639,null,28592765019633,"8536209090",5]
[101963,"Ex9MD3B TM DC400 3P","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=400A, 3-pole","NCB",533.89,0,533.89,8592765019646,1,8592765019646,null,28592765019640,"8536209090",5]
[101964,"Ex9MD3S TM DC250 3P","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=250A, 3-pole","NCB",525.83000000000004,0,525.83000000000004,8592765019653,1,8592765019653,null,28592765019657,"8536209090",5]
[101965,"Ex9MD3S TM DC315 3P","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=315A, 3-pole","NCB",560.71,0,560.71,8592765019660,1,8592765019660,null,28592765019664,"8536209090",5]
[101966,"Ex9MD3S TM DC350 3P","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=350A, 3-pole","NCB",598.25,0,598.25,8592765019677,1,8592765019677,null,28592765019671,"8536209090",5]
[101967,"Ex9MD3S TM DC400 3P","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=400A, 3-pole","NCB",646.54999999999995,0,646.54999999999995,8592765019684,1,8592765019684,null,28592765019688,"8536209090",5]
[101968,"Ex9MD3N TM DC250 3P","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=250A, 3-pole","NCB",635.83000000000004,0,635.83000000000004,8592765019691,1,8592765019691,null,28592765019695,"8536209090",5]
[101969,"Ex9MD3N TM DC315 3P","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=315A, 3-pole","NCB",713.61,0,713.61,8592765019707,1,8592765019707,null,28592765019701,"8536209090",5]
[101970,"Ex9MD3N TM DC350 3P","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=350A, 3-pole","NCB",759.22,0,759.22,8592765019714,1,8592765019714,null,28592765019718,"8536209090",5]
[101971,"Ex9MD3N TM DC400 3P","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=400A, 3-pole","NCB",831.66,0,831.66,8592765019721,1,8592765019721,null,28592765019725,"8536209090",5]
[101980,"Ex9MD3H TM DC250 3P","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=250A, 3-pole","NCB",837.03,0,837.03,8592765019813,1,8592765019813,null,28592765019817,"8536209090",5]
[101981,"Ex9MD3H TM DC315 3P","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=315A, 3-pole","NCB",906.79,0,906.79,8592765019820,1,8592765019820,null,28592765019824,"8536209090",5]
[101982,"Ex9MD3H TM DC350 3P","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=350A, 3-pole","NCB",947.01,0,947.01,8592765019837,1,8592765019837,null,28592765019831,"8536209090",5]
[101983,"Ex9MD3H TM DC400 3P","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=400A, 3-pole","NCB",995.3,0,995.3,8592765019844,1,8592765019844,null,28592765019848,"8536209090",5]
[101984,"Ex9MD3B TM DC250 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=250A, 4-pole ","NCB",649.22,0,649.22,8592765019851,1,8592765019851,null,28592765019855,"8536209090",6.6]
[101985,"Ex9MD3B TM DC315 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=315A, 4-pole ","NCB",748.49,0,748.49,8592765019868,1,8592765019868,null,28592765019862,"8536209090",6.6]
[101986,"Ex9MD3B TM DC350 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=350A, 4-pole ","NCB",778.02,0,778.02,8592765019875,1,8592765019875,null,28592765019879,"8536209090",6.6]
[101987,"Ex9MD3B TM DC400 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=25kA, In=400A, 4-pole ","NCB",807.51,0,807.51,8592765019882,1,8592765019882,null,28592765019886,"8536209090",6.6]
[101988,"Ex9MD3S TM DC250 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=250A, 4-pole ","NCB",761.89,0,761.89,8592765019899,1,8592765019899,null,28592765019893,"8536209090",6.6]
[101989,"Ex9MD3S TM DC315 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=315A, 4-pole ","NCB",887.99,0,887.99,8592765019905,1,8592765019905,null,28592765019909,"8536209090",6.6]
[101990,"Ex9MD3S TM DC350 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=350A, 4-pole ","NCB",920.19,0,920.19,8592765019912,1,8592765019912,null,28592765019916,"8536209090",6.6]
[101991,"Ex9MD3S TM DC400 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=36kA, In=400A, 4-pole ","NCB",963.1,0,963.1,8592765019929,1,8592765019929,null,28592765019923,"8536209090",6.6]
[101992,"Ex9MD3N TM DC250 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=250A, 4-pole ","NCB",914.82,0,914.82,8592765019936,1,8592765019936,null,28592765019930,"8536209090",6.6]
[101993,"Ex9MD3N TM DC315 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=315A, 4-pole ","NCB",1067.74,0,1067.74,8592765019943,1,8592765019943,null,28592765019947,"8536209090",6.6]
[101994,"Ex9MD3N TM DC350 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=350A, 4-pole ","NCB",1097.26,0,1097.26,8592765019950,1,8592765019950,null,28592765019954,"8536209090",6.6]
[101995,"Ex9MD3N TM DC400 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=50kA, In=400A, 4-pole ","NCB",1132.1199999999999,0,1132.1199999999999,8592765019967,1,8592765019967,null,28592765019961,"8536209090",6.6]
[102004,"Ex9MD3H TM DC250 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=250A, 4-pole ","NCB",1204.56,0,1204.56,8592765020055,1,8592765020055,null,28592765020059,"8536209090",6.6]
[102005,"Ex9MD3H TM DC315 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=315A, 4-pole ","NCB",1287.74,0,1287.74,8592765020062,1,8592765020062,null,28592765020066,"8536209090",6.6]
[102006,"Ex9MD3H TM DC350 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=350A, 4-pole ","NCB",1319.92,0,1319.92,8592765020079,1,8592765020079,null,28592765020073,"8536209090",6.6]
[102007,"Ex9MD3H TM DC400 4P4T","DC Circuit Breaker, frame size M3, Icu=Ics=100kA, In=400A, 4-pole ","NCB",1360.17,0,1360.17,8592765020086,1,8592765020086,null,28592765020080,"8536209090",6.6]
[103932,"Ex9MD4B TM DC400 3P","DC Circuit Breaker, frame size M4, Icu=Ics=25kA, In=400A, 3-pole","NCB",1058.24,{"$f":"NCB","v":0},{"$f":"E2644*(1-F2644)","v":1058.24},8592765039330,1,8592765039330,1,28592765039334,"8536209090",10.199999999999999]
[103933,"Ex9MD4B TM DC500 3P","DC Circuit Breaker, frame size M4, Icu=Ics=25kA, In=500A, 3-pole","NCB",1137.26,0,{"$f":"E2645*(1-F2645)","v":1137.26},8592765039347,1,8592765039347,1,28592765039341,"8536209090",10.199999999999999]
[103934,"Ex9MD4B TM DC630 3P","DC Circuit Breaker, frame size M4, Icu=Ics=25kA, In=630A, 3-pole","NCB",1240.3399999999999,0,1240.3399999999999,8592765039354,1,8592765039354,1,28592765039358,"8536209090",10.199999999999999]
[103935,"Ex9MD4S TM DC400 3P","DC Circuit Breaker, frame size M4, Icu=Ics=36kA, In=400A, 3-pole","NCB",1175.05,0,1175.05,8592765039361,1,8592765039361,1,28592765039365,"8536209090",10.199999999999999]
[103936,"Ex9MD4S TM DC500 3P","DC Circuit Breaker, frame size M4, Icu=Ics=36kA, In=500A, 3-pole","NCB",1274.69,0,1274.69,8592765039378,1,8592765039378,1,28592765039372,"8536209090",10.199999999999999]
[103937,"Ex9MD4S TM DC630 3P","DC Circuit Breaker, frame size M4, Icu=Ics=36kA, In=630A, 3-pole","NCB",1362.14,0,1362.14,8592765039385,1,8592765039385,1,28592765039389,"8536209090",10.199999999999999]
[103938,"Ex9MD4N TM DC400 3P","DC Circuit Breaker, frame size M4, Icu=Ics=50kA, In=400A, 3-pole","NCB",1298.75,0,1298.75,8592765039392,1,8592765039392,1,28592765039396,"8536209090",10.199999999999999]
[103939,"Ex9MD4N TM DC500 3P","DC Circuit Breaker, frame size M4, Icu=Ics=50kA, In=500A, 3-pole","NCB",1381.21,0,1381.21,8592765039408,1,8592765039408,1,28592765039402,"8536209090",10.199999999999999]
[103940,"Ex9MD4N TM DC630 3P","DC Circuit Breaker, frame size M4, Icu=Ics=50kA, In=630A, 3-pole","NCB",1452.61,0,1452.61,8592765039415,1,8592765039415,1,28592765039419,"8536209090",10.199999999999999]
[103947,"Ex9MD4H TM DC400 3P","DC Circuit Breaker, frame size M4, Icu=Ics=100kA, In=400A, 3-pole","NCB",1370.89,0,1370.89,8592765039484,1,8592765039484,1,28592765039488,"8536209090",10.199999999999999]
[103948,"Ex9MD4H TM DC500 3P","DC Circuit Breaker, frame size M4, Icu=Ics=100kA, In=500A, 3-pole","NCB",1446.48,0,1446.48,8592765039491,1,8592765039491,1,28592765039495,"8536209090",10.199999999999999]
[103949,"Ex9MD4H TM DC630 3P","DC Circuit Breaker, frame size M4, Icu=Ics=100kA, In=630A, 3-pole","NCB",1530.82,0,1530.82,8592765039507,1,8592765039507,1,28592765039501,"8536209090",10.199999999999999]
[103950,"Ex9MD4B TM DC400 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=25kA, In=400A, 4-pole","NCB",1425.87,0,1425.87,8592765039514,1,8592765039514,1,28592765039518,"8536209090",13.5]
[103951,"Ex9MD4B TM DC500 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=25kA, In=500A, 4-pole","NCB",1559.87,0,1559.87,8592765039521,1,8592765039521,1,28592765039525,"8536209090",13.5]
[103952,"Ex9MD4B TM DC630 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=25kA, In=630A, 4-pole","NCB",1659.51,0,1659.51,8592765039538,1,8592765039538,1,28592765039532,"8536209090",13.5]
[103953,"Ex9MD4S TM DC400 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=36kA, In=400A, 4-pole","NCB",1607.96,0,1607.96,8592765039545,1,8592765039545,1,28592765039549,"8536209090",13.5]
[103954,"Ex9MD4S TM DC500 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=36kA, In=500A, 4-pole","NCB",1673.25,0,1673.25,8592765039552,1,8592765039552,1,28592765039556,"8536209090",13.5]
[103955,"Ex9MD4S TM DC630 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=36kA, In=630A, 4-pole","NCB",1770.88,0,1770.88,8592765039569,1,8592765039569,1,28592765039563,"8536209090",13.5]
[103956,"Ex9MD4N TM DC400 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=50kA, In=400A, 4-pole","NCB",1714.49,0,1714.49,8592765039576,1,8592765039576,1,28592765039570,"8536209090",13.5]
[103957,"Ex9MD4N TM DC500 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=50kA, In=500A, 4-pole","NCB",1803.82,0,1803.82,8592765039583,1,8592765039583,1,28592765039587,"8536209090",13.5]
[103958,"Ex9MD4N TM DC630 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=50kA, In=630A, 4-pole","NCB",1888.46,0,1888.46,8592765039590,1,8592765039590,1,28592765039594,"8536209090",13.5]
[103965,"Ex9MD4H TM DC400 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=100kA, In=400A, 4-pole","NCB",1834.74,0,1834.74,8592765039668,1,8592765039668,1,28592765039662,"8536209090",13.5]
[103966,"Ex9MD4H TM DC500 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=100kA, In=500A, 4-pole","NCB",1896.58,0,1896.58,8592765039675,1,8592765039675,1,28592765039679,"8536209090",13.5]
[103967,"Ex9MD4H TM DC630 4P4T","DC Circuit Breaker, frame size M4, Icu=Ics=100kA, In=630A, 4-pole","NCB",1989.97,0,1989.97,8592765039682,1,8592765039682,1,28592765039686,"8536209090",13.5]
[103968,"Ex9MD5B TM DC630 3P","DC Circuit Breaker, frame size M5, Icu=Ics=25kA, In=630A, 3-pole","NCB",1979.04,0,1979.04,8592765039699,1,8592765039699,1,28592765039693,"8536209090",10.199999999999999]
[103969,"Ex9MD5B TM DC700 3P","DC Circuit Breaker, frame size M5, Icu=Ics=25kA, In=700A, 3-pole","NCB",2192.06,0,2192.06,8592765039705,1,8592765039705,1,28592765039709,"8536209090",10.199999999999999]
[103970,"Ex9MD5B TM DC800 3P","DC Circuit Breaker, frame size M5, Icu=Ics=25kA, In=800A, 3-pole","NCB",2360.41,0,2360.41,8592765039712,1,8592765039712,1,28592765039716,"8536209090",10.199999999999999]
[103971,"Ex9MD5S TM DC630 3P","DC Circuit Breaker, frame size M5, Icu=Ics=36kA, In=630A, 3-pole","NCB",2243.61,0,2243.61,8592765039729,1,8592765039729,1,28592765039723,"8536209090",10.199999999999999]
[103972,"Ex9MD5S TM DC700 3P","DC Circuit Breaker, frame size M5, Icu=Ics=36kA, In=700A, 3-pole","NCB",2367.29,0,2367.29,8592765039736,1,8592765039736,1,28592765039730,"8536209090",10.199999999999999]
[103973,"Ex9MD5S TM DC800 3P","DC Circuit Breaker, frame size M5, Icu=Ics=36kA, In=800A, 3-pole","NCB",2530.96,0,2530.96,8592765039743,1,8592765039743,1,28592765039747,"8536209090",10.199999999999999]
[103974,"Ex9MD5N TM DC630 3P","DC Circuit Breaker, frame size M5, Icu=Ics=50kA, In=630A, 3-pole","NCB",2398.21,0,2398.21,8592765039750,1,8592765039750,1,28592765039754,"8536209090",10.199999999999999]
[103975,"Ex9MD5N TM DC700 3P","DC Circuit Breaker, frame size M5, Icu=Ics=50kA, In=700A, 3-pole","NCB",2508.15,0,2508.15,8592765039767,1,8592765039767,1,28592765039761,"8536209090",10.199999999999999]
[103976,"Ex9MD5N TM DC800 3P","DC Circuit Breaker, frame size M5, Icu=Ics=50kA, In=800A, 3-pole","NCB",2623.91,0,2623.91,8592765039774,1,8592765039774,1,28592765039778,"8536209090",10.199999999999999]
[103983,"Ex9MD5H TM DC630 3P","DC Circuit Breaker, frame size M5, Icu=Ics=100kA, In=630A, 3-pole","NCB",2587.1799999999998,0,2587.1799999999998,8592765039842,1,8592765039842,1,28592765039846,"8536209090",10.199999999999999]
[103984,"Ex9MD5H TM DC700 3P","DC Circuit Breaker, frame size M5, Icu=Ics=100kA, In=700A, 3-pole","NCB",2752.1,0,2752.1,8592765039859,1,8592765039859,1,28592765039853,"8536209090",10.199999999999999]
[103985,"Ex9MD5H TM DC800 3P","DC Circuit Breaker, frame size M5, Icu=Ics=100kA, In=800A, 3-pole","NCB",2892.47,0,2892.47,8592765039866,1,8592765039866,1,28592765039860,"8536209090",10.199999999999999]
[103986,"Ex9MD5B TM DC630 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=25kA, In=630A, 4-pole","NCB",2972,0,2972,8592765039873,1,8592765039873,1,28592765039877,"8536209090",13.5]
[103987,"Ex9MD5B TM DC700 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=25kA, In=700A, 4-pole","NCB",2999.47,0,2999.47,8592765039880,1,8592765039880,1,28592765039884,"8536209090",13.5]
[103988,"Ex9MD5B TM DC800 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=25kA, In=800A, 4-pole","NCB",3102.55,0,3102.55,8592765039897,1,8592765039897,1,28592765039891,"8536209090",13.5]
[103989,"Ex9MD5S TM DC630 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=36kA, In=630A, 4-pole","NCB",3164.4,0,3164.4,8592765039903,1,8592765039903,1,28592765039907,"8536209090",13.5]
[103990,"Ex9MD5S TM DC700 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=36kA, In=700A, 4-pole","NCB",3246.87,0,3246.87,8592765039910,1,8592765039910,1,28592765039914,"8536209090",13.5]
[103991,"Ex9MD5S TM DC800 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=36kA, In=800A, 4-pole","NCB",3290.09,0,3290.09,8592765039927,1,8592765039927,1,28592765039921,"8536209090",13.5]
[103992,"Ex9MD5N TM DC630 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=50kA, In=630A, 4-pole","NCB",3325.88,0,3325.88,8592765039934,1,8592765039934,1,28592765039938,"8536209090",13.5]
[103993,"Ex9MD5N TM DC700 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=50kA, In=700A, 4-pole","NCB",3349.93,0,3349.93,8592765039941,1,8592765039941,1,28592765039945,"8536209090",13.5]
[103994,"Ex9MD5N TM DC800 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=50kA, In=800A, 4-pole","NCB",3410.96,0,3410.96,8592765039958,1,8592765039958,1,28592765039952,"8536209090",13.5]
[104001,"Ex9MD5H TM DC630 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=100kA, In=630A, 4-pole","NCB",3294.97,0,3294.97,8592765040022,1,8592765040022,1,28592765040026,"8536209090",13.5]
[104002,"Ex9MD5H TM DC700 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=100kA, In=700A, 4-pole","NCB",3432.39,0,3432.39,8592765040039,1,8592765040039,1,28592765040033,"8536209090",13.5]
[104003,"Ex9MD5H TM DC800 4P4T","DC Circuit Breaker, frame size M5, Icu=Ics=100kA, In=800A, 4-pole","NCB",3760.21,0,3760.21,8592765040046,1,8592765040046,1,28592765040040,"8536209090",13.5]
[]
["AC Switch disconnectors Ex9MSD"]
[103044,"Ex9M1SD AC63 3P","AC Switch disconnector, frame size M1, In=63 A, 3-pole, AC type","NCD",84.08,{"$f":"NCD","v":0},{"$f":"E2694*(1-F2694)","v":84.08},8592765030450,1,8592765030450,null,28592765030454,"8536508090",1]
[103045,"Ex9M1SD AC100 3P","AC Switch disconnector, frame size M1, In=100 A, 3-pole, AC type","NCD",104.34,0,{"$f":"E2695*(1-F2695)","v":104.34},8592765030467,1,8592765030467,null,28592765030461,"8536209090",1]
[103046,"Ex9M1SD AC125 3P","AC Switch disconnector, frame size M1, In=125 A, 3-pole, AC type","NCD",140.74,0,140.74,8592765030474,1,8592765030474,null,28592765030478,"8536209090",1]
[103047,"Ex9M1SD AC63 4P","AC Switch disconnector, frame size M1, In=63 A, 4-pole, AC type","NCD",112.11,0,112.11,8592765030481,1,8592765030481,null,28592765030485,"8536508090",1.5]
[103048,"Ex9M1SD AC100 4P","AC Switch disconnector, frame size M1, In=100 A, 4-pole, AC type","NCD",139.09,0,139.09,8592765030498,1,8592765030498,null,28592765030492,"8536209090",1.5]
[103049,"Ex9M1SD AC125 4P","AC Switch disconnector, frame size M1, In=125 A, 4-pole, AC type","NCD",187.67,0,187.67,8592765030504,1,8592765030504,null,28592765030508,"8536209090",1.5]
[103050,"Ex9M2SD AC125 3P","AC Switch disconnector, frame size M2, In=125 A, 3-pole, AC type","NCD",161.84,0,161.84,8592765030511,1,8592765030511,null,28592765030515,"8536209090",1.5]
[103051,"Ex9M2SD AC160 3P","AC Switch disconnector, frame size M2, In=160 A, 3-pole, AC type","NCD",179.75,0,179.75,8592765030528,1,8592765030528,null,28592765030522,"8536209090",1.5]
[103052,"Ex9M2SD AC200 3P","AC Switch disconnector, frame size M2, In=200 A, 3-pole, AC type","NCD",207.52,0,207.52,8592765030535,1,8592765030535,null,28592765030539,"8536209090",1.5]
[103053,"Ex9M2SD AC250 3P","AC Switch disconnector, frame size M2, In=250 A, 3-pole, AC type","NCD",259.63,0,259.63,8592765030542,1,8592765030542,null,28592765030546,"8536209090",1.5]
[103054,"Ex9M2SD AC125 4P","AC Switch disconnector, frame size M2, In=125 A, 4-pole, AC type","NCD",215.79,0,215.79,8592765030559,1,8592765030559,null,28592765030553,"8536209090",2]
[103055,"Ex9M2SD AC160 4P","AC Switch disconnector, frame size M2, In=160 A, 4-pole, AC type","NCD",239.65,0,239.65,8592765030566,1,8592765030566,null,28592765030560,"8536209090",2]
[103056,"Ex9M2SD AC200 4P","AC Switch disconnector, frame size M2, In=200 A, 4-pole, AC type","NCD",276.7,0,276.7,8592765030573,1,8592765030573,null,28592765030577,"8536209090",2]
[103057,"Ex9M2SD AC250 4P","AC Switch disconnector, frame size M2, In=250 A, 4-pole, AC type","NCD",346.15,0,346.15,8592765030580,1,8592765030580,null,28592765030584,"8536209090",2]
[103058,"Ex9M3SD AC250 3P","AC Switch disconnector, frame size M3, In=250 A, 3-pole, AC type","NCD",320.86,0,320.86,8592765030597,1,8592765030597,null,28592765030591,"8536209090",4.5]
[103059,"Ex9M3SD AC400 3P","AC Switch disconnector, frame size M3, In=400 A, 3-pole, AC type","NCD",367.13,0,367.13,8592765030603,1,8592765030603,null,28592765030607,"8536209090",4.5]
[103060,"Ex9M3SD AC250 4P","AC Switch disconnector, frame size M3, In=250 A, 4-pole, AC type","NCD",427.8,0,427.8,8592765030610,1,8592765030610,null,28592765030614,"8536209090",6]
[103061,"Ex9M3SD AC400 4P","AC Switch disconnector, frame size M3, In=400 A, 4-pole, AC type","NCD",489.54,0,489.54,8592765030627,1,8592765030627,null,28592765030621,"8536209090",6]
[104016,"Ex9M4SD AC630 3P","AC Switch disconnector, frame size M4, In=630 A, 3-pole, AC type","NCD",454.97,{"$f":"NCD","v":0},{"$f":"E2712*(1-F2712)","v":454.97},8592765040176,1,8592765040176,null,28592765040170,"8536209090",10.199999999999999]
[104017,"Ex9M4SD AC630 4P","AC Switch disconnector, frame size M4, In=630 A, 4-pole, AC type","NCD",606.65,{"$f":"NCD","v":0},{"$f":"E2713*(1-F2713)","v":606.65},8592765040183,1,8592765040183,null,28592765040187,"8536209090",13.5]
[104018,"Ex9M5SD AC800 3P","AC Switch disconnector, frame size M5, In=800 A, 3-pole, AC type","NCD",859.74,{"$f":"NCD","v":0},859.74,8592765040190,1,8592765040190,null,28592765040194,"8536209090",10.199999999999999]
[104019,"Ex9M5SD AC800 4P","AC Switch disconnector, frame size M5, In=800 A, 4-pole, AC type","NCD",1146.32,{"$f":"NCD","v":0},1146.32,8592765040206,1,8592765040206,null,28592765040200,"8536209090",13.5]
[110478,"Ex9M6SD AC800 3P","AC Switch disconnector, frame size M6, In=800 A, 3-pole, AC type","NCD",874.32,{"$f":"NCF","v":0},{"$f":"E2716*(1-F2716)","v":874.32},8592765104786,1,18592765104783,1,28592765104780,"8536209090",14]
[110479,"Ex9M6SD AC1000 3P","AC Switch disconnector, frame size M6, In=1000 A, 3-pole, AC type","NCD",940.13,0,{"$f":"E2717*(1-F2717)","v":940.13},8592765104793,1,18592765104790,1,28592765104797,"8536209090",14]
[110480,"Ex9M6SD AC1250 3P","AC Switch disconnector, frame size M6, In=1250 A, 3-pole, AC type","NCD",1033.1099999999999,0,1033.1099999999999,8592765104809,1,18592765104806,1,28592765104803,"8536209090",14]
[110481,"Ex9M6SD AC1600 3P","AC Switch disconnector, frame size M6, In=1600 A, 3-pole, AC type","NCD",1087.48,0,1087.48,8592765104816,1,18592765104813,1,28592765104810,"8536209090",14]
[110482,"Ex9M6SD AC800 4P","AC Switch disconnector, frame size M6, In=800 A, 4-pole, AC type","NCD",1150.92,0,1150.92,8592765104823,1,18592765104820,1,28592765104827,"8536209090",18.5]
[110483,"Ex9M6SD AC1000 4P","AC Switch disconnector, frame size M6, In=1000 A, 4-pole, AC type","NCD",1237.55,0,1237.55,8592765104830,1,18592765104837,1,28592765104834,"8536209090",18.5]
[110484,"Ex9M6SD AC1250 4P","AC Switch disconnector, frame size M6, In=1250 A, 4-pole, AC type","NCD",1359.94,0,1359.94,8592765104847,1,18592765104844,1,28592765104841,"8536209090",18.5]
[110485,"Ex9M6SD AC1600 4P","AC Switch disconnector, frame size M6, In=1600 A, 4-pole, AC type","NCD",1431.52,0,1431.52,8592765104854,1,18592765104851,1,28592765104858,"8536209090",18.5]
[]
["DC Switch disconnectors Ex9MSD"]
[102008,"Ex9M1SD DC63 3P","DC Switch disconnector, frame size M1, In=63 A, 3-pole, DC type","NCE",253.32,{"$f":"NCE","v":0},{"$f":"E2726*(1-F2726)","v":253.32},8592765020093,1,8592765020093,null,28592765020097,"8536201090",1]
[102009,"Ex9M1SD DC100 3P","DC Switch disconnector, frame size M1, In=100 A, 3-pole, DC type","NCE",285.47000000000003,0,{"$f":"E2727*(1-F2727)","v":285.47000000000003},8592765020109,1,8592765020109,null,28592765020103,"8536209090",1]
[102010,"Ex9M1SD DC125 3P","DC Switch disconnector, frame size M1, In=125 A, 3-pole, DC type","NCE",302.12,0,302.12,8592765020116,1,8592765020116,null,28592765020110,"8536209090",1]
[102011,"Ex9M1SD DC63 4P","DC Switch disconnector, frame size M1, In=63 A, 4-pole, DC type","NCE",325.47000000000003,0,325.47000000000003,8592765020123,1,8592765020123,null,28592765020127,"8536508090",1.5]
[102012,"Ex9M1SD DC100 4P","DC Switch disconnector, frame size M1, In=100 A, 4-pole, DC type","NCE",351.94,0,351.94,8592765020130,1,8592765020130,null,28592765020134,"8536209090",1.5]
[102013,"Ex9M1SD DC125 4P","DC Switch disconnector, frame size M1, In=125 A, 4-pole, DC type","NCE",371.58,0,371.58,8592765020147,1,8592765020147,null,28592765020141,"8536209090",1.5]
[102014,"Ex9M2SD DC125 3P","DC Switch disconnector, frame size M2, In=125 A, 3-pole, DC type","NCE",389.29,0,389.29,8592765020154,1,8592765020154,null,28592765020158,"8536209090",1.5]
[102015,"Ex9M2SD DC160 3P","DC Switch disconnector, frame size M2, In=160 A, 3-pole, DC type","NCE",399.91,0,399.91,8592765020161,1,8592765020161,null,28592765020165,"8536209090",1.5]
[102016,"Ex9M2SD DC200 3P","DC Switch disconnector, frame size M2, In=200 A, 3-pole, DC type","NCE",905.39,0,905.39,8592765020178,1,8592765020178,null,28592765020172,"8536209090",1.5]
[102017,"Ex9M2SD DC250 3P","DC Switch disconnector, frame size M2, In=250 A, 3-pole, DC type","NCE",966.33,0,966.33,8592765020185,1,8592765020185,null,28592765020189,"8536209090",1.5]
[102018,"Ex9M2SD DC125 4P","DC Switch disconnector, frame size M2, In=125 A, 4-pole, DC type","NCE",396.36,0,396.36,8592765020192,1,8592765020192,null,28592765020196,"8536209090",2]
[102019,"Ex9M2SD DC160 4P","DC Switch disconnector, frame size M2, In=160 A, 4-pole, DC type","NCE",406.97,0,406.97,8592765020208,1,8592765020208,null,28592765020202,"8536209090",2]
[102020,"Ex9M2SD DC200 4P","DC Switch disconnector, frame size M2, In=200 A, 4-pole, DC type","NCE",934.16,0,934.16,8592765020215,1,8592765020215,null,28592765020219,"8536209090",2]
[102021,"Ex9M2SD DC250 4P","DC Switch disconnector, frame size M2, In=250 A, 4-pole, DC type","NCE",1059.44,0,1059.44,8592765020222,1,8592765020222,null,28592765020226,"8536209090",2]
[102022,"Ex9M3SD DC250 3P","DC Switch disconnector, frame size M3, In=250 A, 3-pole, DC type","NCE",1136,0,1136,8592765020239,1,8592765020239,null,28592765020233,"8536209090",4.5]
[102023,"Ex9M3SD DC400 3P","DC Switch disconnector, frame size M3, In=400 A, 3-pole, DC type","NCE",1599.59,0,1599.59,8592765020246,1,8592765020246,null,28592765020240,"8536209090",4.5]
[102024,"Ex9M3SD DC250 4P","DC Switch disconnector, frame size M3, In=250 A, 4-pole, DC type","NCE",1373.1,0,1373.1,8592765020253,1,8592765020253,null,28592765020257,"8536209090",6]
[102025,"Ex9M3SD DC400 4P","DC Switch disconnector, frame size M3, In=400 A, 4-pole, DC type","NCE",2512.62,0,2512.62,8592765020260,1,8592765020260,null,28592765020264,"8536209090",6]
[104008,"Ex9M4SD DC630 3P","DC Switch disconnector, frame size M4, In=630 A, 3-pole, DC type","NCE",2866.51,{"$f":"NCE","v":0},2866.51,8592765040091,1,8592765040091,null,28592765040095,"8536209090",10.199999999999999]
[104009,"Ex9M4SD DC630 4P","DC Switch disconnector, frame size M4, In=630 A, 4-pole, DC type","NCE",3008.07,{"$f":"NCE","v":0},3008.07,8592765040107,1,8592765040107,null,28592765040101,"8536209090",13.5]
[104010,"Ex9M5SD DC800 3P","DC Switch disconnector, frame size M5, In=800 A, 3-pole, DC type","NCE",2608.16,{"$f":"NCE","v":0},2608.16,8592765040114,1,8592765040114,null,28592765040118,"8536209090",10.199999999999999]
[104011,"Ex9M5SD DC800 4P","DC Switch disconnector, frame size M5, In=800 A, 4-pole, DC type","NCE",2636.48,{"$f":"NCE","v":0},2636.48,8592765040121,1,8592765040121,null,28592765040125,"8536209090",13.5]
[110486,"Ex9M6SD DC800 3P","DC Switch disconnector, frame size M6, In=800 A, 3-pole, DC type","NCE",2620.8200000000002,{"$f":"NCF","v":0},2620.8200000000002,8592765104861,1,18592765104868,1,28592765104865,"8536209090",14]
[110487,"Ex9M6SD DC1000 3P","DC Switch disconnector, frame size M6, In=1000 A, 3-pole, DC type","NCE",2818.09,0,2818.09,8592765104878,1,18592765104875,1,28592765104872,"8536209090",14]
[110488,"Ex9M6SD DC1250 3P","DC Switch disconnector, frame size M6, In=1250 A, 3-pole, DC type","NCE",3096.8,0,3096.8,8592765104885,1,18592765104882,1,28592765104889,"8536209090",14]
[110489,"Ex9M6SD DC1600 3P","DC Switch disconnector, frame size M6, In=1600 A, 3-pole, DC type","NCE",3259.79,0,3259.79,8592765104892,1,18592765104899,1,28592765104896,"8536209090",14]
[110490,"Ex9M6SD DC800 4P","DC Switch disconnector, frame size M6, In=800 A, 4-pole, DC type","NCE",2639.99,0,2639.99,8592765104908,1,18592765104905,1,28592765104902,"8536209090",18.5]
[110491,"Ex9M6SD DC1000 4P","DC Switch disconnector, frame size M6, In=1000 A, 4-pole, DC type","NCE",2838.7,0,2838.7,8592765104915,1,18592765104912,1,28592765104919,"8536209090",18.5]
[110492,"Ex9M6SD DC1250 4P","DC Switch disconnector, frame size M6, In=1250 A, 4-pole, DC type","NCE",3119.45,0,3119.45,8592765104922,1,18592765104929,1,28592765104926,"8536209090",18.5]
[110493,"Ex9M6SD DC1600 4P","DC Switch disconnector, frame size M6, In=1600 A, 4-pole, DC type","NCE",3283.63,0,3283.63,8592765104939,1,18592765104936,1,28592765104933,"8536209090",18.5]
[]
["Accessories for Moulded Case Circuit Breakers Ex9M, Ex9MD"]
[101395,"AX21","Auxiliary contact for Ex9M, 1 change over","NCA",2.52,{"$f":"NCA","v":0},{"$f":"E2758*(1-F2758)","v":2.52},8592765013965,1,8592765013965,24,28592765013969,"8536508090",0.2]
[101396,"AL21","Signal contact for Ex9M, 1 change over","NCA",2.52,0,2.52,8592765013972,1,8592765013972,24,28592765013976,"8536508090",0.2]
[106315,"EC 21","Early make aux. contacts for frame size M1 and M2, 1 change over","NCA",30.09,{"$f":"NCA","v":0},30.09,8592765063168,1,18592765063165,null,28592765063162,"8538909999",0.2]
[106317,"EC 23","Early make aux. contacts for frame size M3, M4 and M5, 2 change over","NCA",34.17,0,34.17,8592765063182,1,18592765063189,null,28592765063186,"8538909999",0.4]
[101397,"SHT21 AC48V","Shunt trip release for frame size M1, 48 V AC","NCA",73.69,0,73.69,8592765013989,1,8592765013989,24,28592765013983,"8538909999",0.4]
[101398,"SHT21 AC110V","Shunt trip release for frame size M1, 110 V AC","NCA",73.69,0,73.69,8592765013996,1,8592765013996,24,28592765013990,"8536490099",0.4]
[101399,"SHT21 AC220-240V","Shunt trip release for frame size M1, 220-240 V AC","NCA",29.5,0,29.5,8592765014009,1,8592765014009,24,28592765014003,"8536490099",0.4]
[101400,"SHT21 AC380-415V","Shunt trip release for frame size M1, 380-415 V AC","NCA",46.8,0,46.8,8592765014016,1,8592765014016,24,28592765014010,"8536490099",0.4]
[101401,"SHT21 DC24V","Shunt trip release for frame size M1, 24 V DC","NCA",73.69,0,73.69,8592765014023,1,8592765014023,24,28592765014027,"8536419089",0.4]
[101402,"SHT21 DC48V","Shunt trip release for frame size M1, 48 V DC","NCA",73.69,0,73.69,8592765014030,1,8592765014030,24,28592765014034,"8538909999",0.4]
[101403,"SHT21 DC110V","Shunt trip release for frame size M1, 110 V DC","NCA",73.69,0,73.69,8592765014047,1,8592765014047,24,28592765014041,"8538909999",0.4]
[101405,"SHT21 DC220V","Shunt trip release for frame size M1, 220 V DC","NCA",73.69,0,73.69,8592765014061,1,8592765014061,24,28592765014065,"8538909999",0.4]
[101406,"UVT21 AC220-240V","Undervoltage release for frame size M1, 220-240 V AC","NCA",42.02,0,42.02,8592765014078,1,8592765014078,24,28592765014072,"8536490099",0.76]
[101407,"UVT21 AC380-415V","Undervoltage release for frame size M1, 380-415 V AC","NCA",42.02,0,42.02,8592765014085,1,8592765014085,24,28592765014089,"8536490099",0.18]
[101409,"ERH21","Rotary handle with extension shaft for frame size M1","NCA",39.880000000000003,0,39.880000000000003,8592765014108,1,8592765014108,6,28592765014102,"8538909999",1.36]
[101410,"RHD21","Rotary handle for frame size M1","NCA",28.82,0,28.82,8592765014115,1,8592765014115,36,28592765014119,"8538909999",1.36]
[101411,"MOD21 AC230V","Motor drive for frame size M1, 230 V AC","NCA",258.95,0,258.95,8592765014122,1,8592765014122,8,28592765014126,"8538909999",1.36]
[101412,"MOD21 AC110V","Motor drive for frame size M1, 110 V AC","NCA",294.79000000000002,0,294.79000000000002,8592765014139,1,8592765014139,8,28592765014133,"8538909999",1.36]
[101413,"MOD21 DC220V","Motor drive for frame size M1, 220 V DC","NCA",294.79000000000002,0,294.79000000000002,8592765014146,1,8592765014146,8,28592765014140,"8538909999",1.36]
[101414,"MOD21 DC110V","Motor drive for frame size M1, 110 V DC","NCA",294.79000000000002,0,294.79000000000002,8592765014153,1,8592765014153,8,28592765014157,"8538909999",1.36]
[101415,"MOD21 DC24V","Motor drive for frame size M1, 24 V DC","NCA",294.79000000000002,0,294.79000000000002,8592765014160,1,8592765014160,8,28592765014164,"8538909999",1.36]
[101439,"TCV21 3P","Terminal cover for 3-poles frame size M1, short","NCA",6.87,0,6.87,8592765014405,1,18592765014402,null,28592765014409,"8538909999",0.6]
[101440,"TCE21 3P","Terminal cover for 3-poles frame size M1, long","NCA",8.68,0,8.68,8592765014412,1,18592765014419,null,28592765014416,"8538909999",0.6]
[102372,"TCV21 4P","Terminal cover for 4-poles frame size M1, short","NCA",14.14,0,{"$f":"E2781*(1-F2781)","v":14.14},8592765023735,1,18592765023732,null,28592765023739,"8538909999",0.6]
[102373,"TCE21 4P","Terminal cover for 4-poles frame size M1, long","NCA",18.61,0,18.61,8592765023742,1,18592765023749,null,28592765023746,"8538909999",0.6]
[101441,"PB21 3P","Phase barriers set for 3-poles frame size M1","NCA",8.48,0,8.48,8592765014429,1,18592765014426,null,28592765014423,"4008219000"]
[101416,"SHT22 AC48V","Shunt trip release for frame size from M2, 48 V AC","NCA",73.69,0,73.69,8592765014177,1,8592765014177,24,28592765014171,"8538909999",0.5]
[101417,"SHT22 AC110V","Shunt trip release for frame size from M2, 110 V AC","NCA",73.69,0,73.69,8592765014184,1,8592765014184,24,28592765014188,"8538909999",0.5]
[101418,"SHT22 AC220-240V","Shunt trip release for frame size from M2, 220-240 V AC","NCA",36.119999999999997,0,36.119999999999997,8592765014191,1,8592765014191,24,28592765014195,"8536490099",0.5]
[101419,"SHT22 AC380-415V","Shunt trip release for frame size from M2, 380-415 V AC","NCA",51.62,0,51.62,8592765014207,1,8592765014207,24,28592765014201,"8536490099",0.5]
[101420,"SHT22 DC24V","Shunt trip release for frame size from M2, 24 V DC","NCA",73.69,0,73.69,8592765014214,1,8592765014214,24,28592765014218,"8536419089",0.5]
[101421,"SHT22 DC48V","Shunt trip release for frame size from M2, 48 V DC","NCA",73.69,0,73.69,8592765014221,1,8592765014221,24,28592765014225,"8538909999",0.5]
[101422,"SHT22 DC110V","Shunt trip release for frame size from M2, 110 V DC","NCA",73.69,0,73.69,8592765014238,1,8592765014238,24,28592765014232,"8538909999",0.5]
[101424,"SHT22 DC220V","Shunt trip release for frame size from M2, 220 V DC","NCA",73.69,0,73.69,8592765014252,1,8592765014252,24,28592765014256,"8538909999",0.5]
[101425,"UVT22 AC220-240V","Undervoltage release for frame size from M2, 220-240 V AC","NCA",48.68,0,48.68,8592765014269,1,8592765014269,24,28592765014263,"8536490099",0.5]
[101426,"UVT22 AC380-415V","Undervoltage release for frame size from M2, 380-415 V AC","NCA",48.68,0,48.68,8592765014276,1,8592765014276,24,28592765014270,"8536490099",0.5]
[101428,"ERH22","Rotary handle with extension shaft for frame size M2","NCA",53.46,0,53.46,8592765014290,1,8592765014290,6,28592765014294,"8538909999",0.8]
[101429,"RHD22","Rotary handle for frame size M2","NCA",42.37,0,42.37,8592765014306,1,8592765014306,18,28592765014300,"8538909999",0.34]
[101430,"MOD22 AC230V","Motor drive for frame size M2, 230 V AC","NCA",258.88,0,258.88,8592765014313,1,8592765014313,8,28592765014317,"8538909999",1.36]
[101431,"MOD22 AC110V","Motor drive for frame size M2, 110 V AC","NCA",294.79000000000002,0,294.79000000000002,8592765014320,1,8592765014320,8,28592765014324,"8538909999",1.36]
[101432,"MOD22 DC220V","Motor drive for frame size M2, 220 V DC","NCA",294.79000000000002,0,294.79000000000002,8592765014337,1,8592765014337,8,28592765014331,"8538909999",1.36]
[101433,"MOD22 DC110V","Motor drive for frame size M2, 110 V DC","NCA",294.79000000000002,0,294.79000000000002,8592765014344,1,8592765014344,8,28592765014348,"8538909999",1.36]
[101434,"MOD22 DC24V","Motor drive for frame size M2, 24 V DC","NCA",294.79000000000002,0,294.79000000000002,8592765014351,1,8592765014351,8,28592765014355,"8538909999",1.36]
[101442,"TCV22 3P","Terminal cover for 3-poles frame size M2, short","NCA",9.4700000000000006,0,9.4700000000000006,8592765014436,1,18592765014433,null,28592765014430,"8538909999",0.08]
[101443,"TCE22 3P","Terminal cover for 3-poles frame size M2, long","NCA",11.83,0,11.83,8592765014443,1,18592765014440,null,28592765014447,"8538909999",0.16]
[102374,"TCV22 4P","Terminal cover for 4-poles frame size M2, short","NCA",16.399999999999999,0,16.399999999999999,8592765023759,1,18592765023756,null,28592765023753,"8538909999"]
[102375,"TCE22 4P","Terminal cover for 4-poles frame size M2, long","NCA",21.6,0,21.6,8592765023766,1,18592765023763,null,28592765023760,"8538909999"]
[101444,"PB22 3P","Phase barriers set for 3-poles frame size M2","NCA",8.99,0,8.99,8592765014450,1,18592765014457,null,28592765014454,"4008219000"]
[101482,"ERH23","Rotary handle with extension shaft for frame size M3","NCA",62.84,0,62.84,8592765014832,1,8592765014832,null,28592765014836,"8538909999",1.08]
[101483,"RHD23","Rotary handle for frame size M3","NCA",53.43,0,53.43,8592765014849,1,8592765014849,null,28592765014843,"8538909999",0.72]
[101484,"MOD23 AC230V","Motor drive for frame size M3, 230 V AC","NCA",329.83,0,329.83,8592765014856,1,8592765014856,null,28592765014850,"8538909999",3.46]
[101485,"MOD23 AC110V","Motor drive for frame size M3, 110 V AC","NCA",336.8,0,336.8,8592765014863,1,8592765014863,null,28592765014867,"8538909999",3.46]
[101486,"MOD23 DC220V","Motor drive for frame size M3, 220 V DC","NCA",336.8,0,336.8,8592765014870,1,8592765014870,null,28592765014874,"8538909999",3.46]
[101487,"MOD23 DC110V","Motor drive for frame size M3, 110 V DC","NCA",336.8,0,336.8,8592765014887,1,8592765014887,null,28592765014881,"8538909999",3.46]
[101488,"MOD23 DC24V","Motor drive for frame size M3, 24 V DC","NCA",336.8,0,336.8,8592765014894,1,8592765014894,null,28592765014898,"8538909999",3.46]
[101489,"TCV23 3P","Terminal cover for 3-poles frame size M3, short","NCA",10.59,0,10.59,8592765014900,1,18592765014907,null,28592765014904,"8538909999",0.14000000000000001]
[101490,"TCE23 3P","Terminal cover for 3-poles frame size M3, long","NCA",13.38,0,13.38,8592765014917,1,18592765014914,null,28592765014911,"8538909999",0.36]
[102376,"TCV23 4P","Terminal cover for 4-poles frame size M3, short","NCA",24.23,0,24.23,8592765023773,1,18592765023770,null,28592765023777,"8538909999"]
[102377,"TCE23 4P","Terminal cover for 4-poles frame size M3, long","NCA",32.799999999999997,0,32.799999999999997,8592765023780,1,18592765023787,null,28592765023784,"8538909999"]
[101491,"PB23 3P","Phase barriers set for 3-poles frame size M3","NCA",11.6,{"$f":"NCA","v":0},{"$f":"E2817*(1-F2817)","v":11.6},8592765014924,1,18592765014921,null,28592765014928,"4008219000"]
[103723,"SHT24 AC110V","Shunt trip release for frame size M4 and M5, 110 V AC","NCA",94.66,{"$f":"NCA","v":0},{"$f":"E2818*(1-F2818)","v":94.66},8592765037244,1,18592765037241,24,28592765037248,"8538909999",0.12]
[103724,"SHT24 AC220-240V","Shunt trip release for frame size M4 and M5, 220-240 V AC","NCA",85.53,{"$f":"NCA","v":0},{"$f":"E2819*(1-F2819)","v":85.53},8592765037251,1,18592765037258,24,28592765037255,"8536490099",0.12]
[103725,"SHT24 AC380-415V","Shunt trip release for frame size M4 and M5, 380-415 V AC","NCA",85.53,{"$f":"NCA","v":0},{"$f":"E2820*(1-F2820)","v":85.53},8592765037268,1,18592765037265,24,28592765037262,"8536490099",0.12]
[103727,"SHT24 DC110V","Shunt trip release for frame size M4 and M5, 110 V DC","NCA",94.66,0,{"$f":"E2821*(1-F2821)","v":94.66},8592765037282,1,18592765037289,24,28592765037286,"8538909999",0.12]
[103728,"SHT24 DC220V","Shunt trip release for frame size M4 and M5, 220 V DC","NCA",94.66,0,94.66,8592765037299,1,18592765037296,24,28592765037293,"8538909999",0.12]
[103729,"SHT24 DC24V","Shunt trip release for frame size M4 and M5, 24 V DC","NCA",94.66,0,94.66,8592765037305,1,18592765037302,24,28592765037309,"8536419089",0.12]
[103730,"SHT24 DC48V","Shunt trip release for frame size M4 and M5, 48 V DC","NCA",94.66,0,94.66,8592765037312,1,18592765037319,24,28592765037316,"8538909999",0.12]
[103733,"UVT24 AC110V","Undervoltage release for frame size M4 and M5, 110 V AC","NCA",105.61,0,105.61,8592765037343,1,18592765037340,24,28592765037347,"8538909999",0.12]
[103734,"UVT24 AC220-240V","Undervoltage release for frame size M4 and M5, 220-240 V AC","NCA",100.53,0,100.53,8592765037350,1,18592765037357,24,28592765037354,"8536490099",0.12]
[103735,"UVT24 AC380-415V","Undervoltage release for frame size M4 and M5, 380-415 V AC","NCA",100.53,0,100.53,8592765037367,1,18592765037364,24,28592765037361,"8536490099",0.12]
[103736,"UVT24 DC110V","Undervoltage release for frame size M4 and M5, 110 V AC","NCA",105.61,0,105.61,8592765037374,1,18592765037371,24,28592765037378,"8538909999",0.12]
[103737,"UVT24 DC220V","Undervoltage release for frame size M4 and M5, 220 V DC","NCA",105.61,0,105.61,8592765037381,1,18592765037388,24,28592765037385,"8538909999",0.12]
[103738,"UVT24 DC24V","Undervoltage release for frame size M4 and M5, 24 V DC","NCA",105.61,0,105.61,8592765037398,1,18592765037395,24,28592765037392,"8536419089",0.12]
[103739,"UVT24 DC48V","Undervoltage release for frame size M4 and M5, 48 V DC","NCA",105.61,0,105.61,8592765037404,1,18592765037401,24,28592765037408,"8538909999",0.12]
[103741,"ERH24","Rotary handle with extension shaft for frame size M4 and M5","NCA",100.65,0,100.65,8592765037428,1,18592765037425,null,28592765037422,"8538909999"]
[103742,"RHD24","Rotary handle for frame size M4 and M5","NCA",90.16,0,90.16,8592765037435,1,18592765037432,null,28592765037439,"8538909999",1.6819999999999999]
[103743,"MOD24 AC230V","Motor drive for frame size M4 and M5, 230 V AC","NCA",634.41,0,634.41,8592765037442,1,18592765037449,null,28592765037446,"8538909999",3.72]
[103744,"MOD24 AC110V","Motor drive for frame size M4 and M5, 110 V AC","NCA",910.18,0,910.18,8592765037459,1,18592765037456,null,28592765037453,"8538909999",3.72]
[103745,"MOD24 DC220V","Motor drive for frame size M4 and M5, 220 V DC","NCA",910.18,0,910.18,8592765037466,1,18592765037463,null,28592765037460,"8538909999",3.72]
[103746,"MOD24 DC110V","Motor drive for frame size M4 and M5, 110 V DC","NCA",910.18,0,910.18,8592765037473,1,18592765037470,null,28592765037477,"8538909999",3.72]
[103747,"MOD24 DC24V","Motor drive for frame size M4 and M5, 24 V DC","NCA",910.18,0,910.18,8592765037480,1,18592765037487,null,28592765037484,"8538909999",3.72]
[103748,"TCV24 3P","Terminal cover for 3-poles frame size M4 and M5, short","NCA",17.440000000000001,0,17.440000000000001,8592765037497,1,18592765037494,null,28592765037491,"8538909999"]
[103749,"TCE24 3P","Terminal cover for 3-poles frame size M4 and M5, long","NCA",23.07,0,23.07,8592765037503,1,18592765037500,null,28592765037507,"8538909999",0.32]
[103750,"TCV24 4P","Terminal cover for 4-poles frame size M4 and M5, short","NCA",31.48,0,31.48,8592765037510,1,18592765037517,null,28592765037514,"8538909999"]
[104855,"TCE24 4P","Terminal cover for 4-poles frame size M4 and M5, long","NCA",42.62,0,42.62,8592765048561,1,18592765048568,null,28592765048565,"8538909999"]
[103751,"PB24 3P","Phase barriers set for 3-poles frame size M4 and M5","NCA",15.32,0,15.32,8592765037527,1,18592765037524,null,28592765037521,"4008219000"]
[104856,"PB24 4P","Phase barriers set for 4-poles frame size M4 and M6","NCA",20.100000000000001,0,20.100000000000001,8592765048578,1,18592765048575,null,28592765048572,"4008219000"]
[103705,"MC21","Box terminal for frame size M1, 1x 4-95 mm2, 1 pc.","NCA",3.58,{"$f":"NCA","v":0},3.58,8592765037060,1,18592765037067,null,28592765037064,"8536901000",0.24]
[103707,"MC21 W","Tunnel terminal for frame size M1, 1x 16-95 mm2, 1 pc.","NCA",14.18,{"$f":"NCA","v":0},14.18,8592765037084,1,18592765037081,null,28592765037088,"8536901000",0.2]
[107873,"MCS21","Screw terminal for frame size M1","NCA",3.58,{"$f":"NCA","v":0},{"$f":"E2847*(1-F2847)","v":3.58},8592765078742,1,18592765078749,null,28592765078746,"8536901000",0.02]
[103709,"MC22","Box terminal for frame size M2, 1x 10-120 mm2, 1 pc.","NCA",4.0199999999999996,0,4.0199999999999996,8592765037107,1,18592765037104,null,28592765037101,"8536901000",0.36]
[103869,"MC22 W","Tunnel terminal for frame size M2, 1x 35-120 mm2, 1 pc.","NCA",8.52,0,8.52,8592765038708,1,8592765038708,null,28592765038702,"8536901000"]
[103711,"MC22 W2","Tunnel terminal for frame size M2, 2x 35-120 mm2, 1 pc.","NCA",20.52,0,20.52,8592765037121,1,18592765037128,null,28592765037125,"8536901000",0.5]
[103713,"MC22 W6","Tunnel terminal for frame size M2, 6x 10-35 mm2, 1 pc.","NCA",24.06,0,24.06,8592765037145,1,18592765037142,null,28592765037149,"8536901000",0.1]
[107874,"MCS22","Screw terminal for frame size M2","NCA",4.0199999999999996,{"$f":"NCA","v":0},{"$f":"E2852*(1-F2852)","v":4.0199999999999996},8592765078759,1,18592765078756,null,28592765078753,"8536901000",0.03]
[103715,"MC23","Box terminal for frame size M3, 1x 120-240 mm2, 1 pc.","NCA",17.97,0,17.97,8592765037169,1,18592765037166,null,28592765037163,"8536901000",0.1]
[103717,"MC23 UL","Box terminal for frame size M3, 1x 120-240 mm2, 1 pc., UL version","NCA",27.66,0,27.66,8592765037183,1,18592765037180,null,28592765037187,"8538909999",0.12]
[103719,"MC23 W2","Tunnel terminal for frame size M3, 2x 120-240 mm2, 1 pc.","NCA",27.36,0,27.36,8592765037206,1,18592765037203,null,28592765037200,"8536901000",0.28000000000000003]
[103721,"MC23 W4","Tunnel terminal for frame size M3, 4x 35-95 mm2, 1 pc.","NCA",31.85,0,31.85,8592765037220,1,18592765037227,null,28592765037224,"8536901000",0.18]
[103871,"MC23 W2 UL","Tunnel terminal for frame size M3, 4x 35-95 mm2, 1 pc., UL version","NCA",36.07,0,36.07,8592765038722,1,8592765038722,null,28592765038726,"8538909999",0.24]
[106314,"MC24 W2","Tunnel terminal for frame size M4 and M5, 2x 120-240 mm2, 1 pc.","NCA",23.51,{"$f":"NCA","v":0},23.51,8592765063151,1,18592765063158,null,28592765063155,"8536901000"]
[106321,"WG 10","Mounting depth spacer, 10 mm, 1 set","NCA",6.14,{"$f":"NCA","v":0},6.14,8592765063229,1,18592765063226,5,28592765063223,"4016930090",0.04]
[106362,"WG 13","Mounting depth spacer, 13 mm, 1 set","NCA",7.06,0,7.06,8592765063632,1,18592765063639,5,28592765063636,"4016930090",0.06]
[106319,"DRA21","DIN35 rail adaptor for Ex9M, frame size M1","NCA",12.29,0,12.29,8592765063205,1,18592765063202,5,28592765063209,"7326909890",0.12]
[106320,"DRA22","DIN35 rail adaptor for Ex9M, frame size M2","NCA",14.27,0,14.27,8592765063212,1,18592765063219,5,28592765063216,"7326909890",0.16]
[110189,"ERH2x ES 500mm","Extended shaft for ERH2x","NCA",19.88,{"$f":"NCA","v":0},{"$f":"E2863*(1-F2863)","v":19.88},8592765101891,1,18592765101898,50,28592765101895,"8538909999",0.38]
[110460,"SHT26 DC24V","Shunt trip release for frame size M6, 24 V DC","NCF",94.66,{"$f":"NCF","v":0},94.66,8592765104601,1,18592765104608,null,28592765104605,"8536419089",0.45]
[110461,"SHT26 DC48V","Shunt trip release for frame size M6, 48 V DC","NCF",94.66,0,94.66,8592765104618,1,18592765104615,null,28592765104612,"8536419089",0.45]
[110462,"SHT26 DC110V","Shunt trip release for frame size M6, 110 V DC","NCF",94.66,0,94.66,8592765104625,1,18592765104622,null,28592765104629,"8536490099",0.45]
[110463,"SHT26 DC220V","Shunt trip release for frame size M6, 220 V DC","NCF",94.66,0,94.66,8592765104632,1,18592765104639,null,28592765104636,"8536490099",0.45]
[110464,"SHT26 AC48V","Shunt trip release for frame size M6, 48 V AC","NCF",94.66,0,94.66,8592765104649,1,18592765104646,null,28592765104643,"8536419089",0.45]
[110465,"SHT26 AC110V","Shunt trip release for frame size M6, 110 V AC","NCF",94.66,0,94.66,8592765104656,1,18592765104653,null,28592765104650,"8536490099",0.45]
[110466,"SHT26 AC220-240V","Shunt trip release for frame size M6, 220-240 V AC","NCF",85.53,0,85.53,8592765104663,1,18592765104660,null,28592765104667,"8536490099",0.45]
[110467,"SHT26 AC380-415V","Shunt trip release for frame size M6, 380-415 V AC","NCF",85.53,0,85.53,8592765104670,1,18592765104677,null,28592765104674,"8536490099",0.45]
[110813,"UVT26 DC24V","Undervoltage release for frame size M6, 24 V DC","NCF",122.53,0,{"$f":"E2872*(1-F2872)","v":122.53},8592765108135,1,18592765108132,1,28592765108139,null,0.45]
[110468,"UVT26 AC220-240V","Undervoltage release for frame size M6, 220-240 V AC","NCF",122.53,0,122.53,8592765104687,1,18592765104684,null,28592765104681,"8536209090",0.45]
[110469,"UVT26 AC380-415V","Undervoltage release for frame size M6, 380-415 V AC","NCF",122.53,0,{"$f":"E2874*(1-F2874)","v":122.53},8592765104694,1,18592765104691,null,28592765104698,"8536209090",0.45]
[110694,"JP26 3P 800-1250A","Front connection plate for frame size M6, 3-pole, 800-1250 A","NCF",57.78,0,57.78,8592765106940,1,18592765106947,10,28592765106944,"8538909999",3.5]
[110695,"JP26 3P 1600A","Front connection plate for frame size M6, 3-pole, 1600 A","NCF",113.34,0,113.34,8592765106957,1,18592765106954,10,28592765106951,"8538909999",7.2]
[110696,"JP26 4P 800-1250A","Front connection plate for frame size M6, 4-pole, 800-1250 A","NCF",73.930000000000007,0,73.930000000000007,8592765106964,1,18592765106961,10,28592765106968,"8538909999",4.5]
[110697,"JP26 4P 1600A","Front connection plate for frame size M6, 4-pole, 1600 A","NCF",143.32,0,143.32,8592765106971,1,18592765106978,10,28592765106975,"8538909999",8.4]
[110698,"LHD26","Extended handle for frame size M6","NCF",90.16,0,90.16,8592765106988,1,18592765106985,20,28592765106982,"8538909999",0.1]
[110718,"ERH26","Extended rotary handle for frame size M6","NCF",130.28571428571431,0,{"$f":"E2880*(1-F2880)","v":130.28571428571431},8592765107183,1,18592765107180,null,28592765107187,"8538909999",0.56000000000000005]
[]
["Air Circuit Breakers Ex9A"]
[105025,"+SU30A AC230","Tripping unit SU3.0, variant A, LSI protection with analysis of currents, 230 V AC","NCC",1471.43,{"$f":"NCC","v":0},{"$f":"E2883*(1-F2883)","v":1471.43},8592765050267,1,8592765050267,1,28592765050261,"8536209090"]
[105026,"+SU30A AC400","Tripping unit SU3.0, variant A, LSI protection with analysis of currents, 400 V AC","NCC",1471.43,0,1471.43,8592765050274,1,8592765050274,1,28592765050278,"8536209090"]
[105027,"+SU30A DC24","Tripping unit SU3.0, variant A, LSI protection with analysis of currents, 24 V DC","NCC",1471.43,0,1471.43,8592765050281,1,8592765050281,1,28592765050285,"8536209090"]
[105028,"+SU30D AC230","Tripping unit SU3.0, variant D, LSI protection with analysis of currents and voltages, 230 V AC","NCC",2766.56,0,2766.56,8592765050298,1,8592765050298,1,28592765050292,"8536209090"]
[105029,"+SU30D AC400","Tripping unit SU3.0, variant D, LSI protection with analysis of currents and voltages, 400 V AC","NCC",2766.56,0,2766.56,8592765050304,1,8592765050304,1,28592765050308,"8536209090"]
[105030,"+SU30D DC24","Tripping unit SU3.0, variant D, LSI protection with analysis of currents and voltages, 24 V DC","NCC",2766.56,0,2766.56,8592765050311,1,8592765050311,1,28592765050315,"8536209090"]
[105031,"+SU30P AC230","Tripping unit SU3.0, variant P, LSI protection with analysis of currents, voltages and powers, 230 V AC","NCC",3414.12,0,3414.12,8592765050328,1,8592765050328,1,28592765050322,"8536209090"]
[105032,"+SU30P AC400","Tripping unit SU3.0, variant P, LSI protection with analysis of currents, voltages and powers, 400 V AC","NCC",3414.12,0,3414.12,8592765050335,1,8592765050335,1,28592765050339,"8536209090"]
[105033,"+SU30P DC24","Tripping unit SU3.0, variant P, LSI protection with analysis of currents, voltages and powers, 24 V DC","NCC",3414.12,0,3414.12,8592765050342,1,8592765050342,1,28592765050346,"8536209090"]
[105034,"+SU30H AC230","Tripping unit SU3.0, variant H, LSI protection with complete net analysis, 230 V AC","NCC",4061.7,0,4061.7,8592765050359,1,8592765050359,1,28592765050353,"8536209090"]
[105035,"+SU30H AC400","Tripping unit SU3.0, variant H, LSI protection with complete net analysis, 400 V AC","NCC",4061.7,0,4061.7,8592765050366,1,8592765050366,1,28592765050360,"8536209090"]
[105036,"+SU30H DC24","Tripping unit SU3.0, variant H, LSI protection with complete net analysis, 24 V DC","NCC",4061.7,0,4061.7,8592765050373,1,8592765050373,1,28592765050377,"8536209090"]
[105037,"+SU40A AC230","Tripping unit SU4.0, variant A, LSI+G protection with analysis of currents, 230 V AC","NCC",3474.37,0,3474.37,8592765050380,1,8592765050380,1,28592765050384,"8536209090"]
[105038,"+SU40A AC400","Tripping unit SU4.0, variant A, LSI+G protection with analysis of currents, 400 V AC","NCC",3474.37,0,3474.37,8592765050397,1,8592765050397,1,28592765050391,"8536209090"]
[105039,"+SU40A DC24","Tripping unit SU4.0, variant A, LSI+G protection with analysis of currents, 24 V DC","NCC",3474.37,0,3474.37,8592765050403,1,8592765050403,1,28592765050407,"8536209090"]
[105040,"+SU40D AC230","Tripping unit SU4.0, variant D, LSI+G protection with analysis of currents and voltages, 230 V AC","NCC",3805.1,0,3805.1,8592765050410,1,8592765050410,1,28592765050414,"8536209090"]
[105041,"+SU40D AC400","Tripping unit SU4.0, variant D, LSI+G protection with analysis of currents and voltages, 400 V AC","NCC",3805.1,0,3805.1,8592765050427,1,8592765050427,1,28592765050421,"8536209090"]
[105042,"+SU40D DC24","Tripping unit SU4.0, variant D, LSI+G protection with analysis of currents and voltages, 24 V DC","NCC",3805.1,0,3805.1,8592765050434,1,8592765050434,1,28592765050438,"8536209090"]
[105043,"+SU40P AC230","Tripping unit SU4.0, variant P, LSI+G protection with analysis of currents, voltages and powers, 230 V AC","NCC",3970.44,0,3970.44,8592765050441,1,8592765050441,1,28592765050445,"8536209090"]
[105044,"+SU40P AC400","Tripping unit SU4.0, variant P, LSI+G protection with analysis of currents, voltages and powers, 400 V AC","NCC",3970.44,0,3970.44,8592765050458,1,8592765050458,1,28592765050452,"8536209090"]
[105045,"+SU40P DC24","Tripping unit SU4.0, variant P, LSI+G protection with analysis of currents, voltages and powers, 24 V DC","NCC",3970.44,0,3970.44,8592765050465,1,8592765050465,1,28592765050469,"8536209090"]
[105046,"+SU40H AC230","Tripping unit SU4.0, variant H, LSI+G protection with complete net analysis, 230 V AC","NCC",4135.8100000000004,0,4135.8100000000004,8592765050472,1,8592765050472,1,28592765050476,"8536209090"]
[105047,"+SU40H AC400","Tripping unit SU4.0, variant H, LSI+G protection with complete net analysis, 400 V AC","NCC",4135.8100000000004,0,4135.8100000000004,8592765050489,1,8592765050489,1,28592765050483,"8536209090"]
[105048,"+SU40H DC24","Tripping unit SU4.0, variant H, LSI+G protection with complete net analysis, 24 V DC","NCC",4135.8100000000004,0,4135.8100000000004,8592765050496,1,8592765050496,1,28592765050490,"8536209090"]
[105049,"+SU50A AC230","Tripping unit SU5.0, variant A, LSI+E protection with analysis of currents, 230 V AC","NCC",4169.25,0,4169.25,8592765050502,1,8592765050502,1,28592765050506,"8536209090"]
[105050,"+SU50A AC400","Tripping unit SU5.0, variant A, LSI+E protection with analysis of currents, 400 V AC","NCC",4169.25,0,4169.25,8592765050519,1,8592765050519,1,28592765050513,"8536209090"]
[105051,"+SU50A DC24","Tripping unit SU5.0, variant A, LSI+E protection with analysis of currents, 24 V DC","NCC",4169.25,0,4169.25,8592765050526,1,8592765050526,1,28592765050520,"8536209090"]
[105052,"+SU50D AC230","Tripping unit SU5.0, variant D, LSI+E protection with analysis of currents and voltages, 230 V AC","NCC",4566.1099999999997,0,4566.1099999999997,8592765050533,1,8592765050533,1,28592765050537,"8536209090"]
[105053,"+SU50D AC400","Tripping unit SU5.0, variant D, LSI+E protection with analysis of currents and voltages, 400 V AC","NCC",4566.1099999999997,0,4566.1099999999997,8592765050540,1,8592765050540,1,28592765050544,"8536209090"]
[105054,"+SU50D DC24","Tripping unit SU5.0, variant D, LSI+E protection with analysis of currents and voltages, 24 V DC","NCC",4566.1099999999997,0,4566.1099999999997,8592765050557,1,8592765050557,1,28592765050551,"8536209090"]
[105055,"+SU50P AC230","Tripping unit SU5.0, variant P, LSI+E protection with analysis of currents, voltages and powers, 230 V AC","NCC",4764.54,0,4764.54,8592765050564,1,8592765050564,1,28592765050568,"8536209090"]
[105056,"+SU50P AC400","Tripping unit SU5.0, variant P, LSI+E protection with analysis of currents, voltages and powers, 400 V AC","NCC",4764.54,0,4764.54,8592765050571,1,8592765050571,1,28592765050575,"8536209090"]
[105057,"+SU50P DC24","Tripping unit SU5.0, variant P, LSI+E protection with analysis of currents, voltages and powers, 24 V DC","NCC",4764.54,0,4764.54,8592765050588,1,8592765050588,1,28592765050582,"8536209090"]
[105058,"+SU50H AC230","Tripping unit SU5.0, variant H, LSI+E protection with complete net analysis, 230 V AC","NCC",4962.97,0,4962.97,8592765050595,1,8592765050595,1,28592765050599,"8536209090"]
[105059,"+SU50H AC400","Tripping unit SU5.0, variant H, LSI+E protection with complete net analysis, 400 V AC","NCC",4962.97,0,4962.97,8592765050601,1,8592765050601,1,28592765050605,"8536209090"]
[105060,"+SU50H DC24","Tripping unit SU5.0, variant H, LSI+E protection with complete net analysis, 24 V DC","NCC",4962.97,0,4962.97,8592765050618,1,8592765050618,1,28592765050612,"8536209090"]
[104857,"Ex9A16N 3P D/O 400","Air Circuit Breaker, frame size A16, Icu=55kA, In=400A, 3-pole, Withdrawable ","NCC",1700.75,0,1700.75,8592765048585,1,8592765048585,1,28592765048589,"8536209090",38]
[104858,"Ex9A16N 3P F 400","Air Circuit Breaker, frame size A16, Icu=55kA, In=400A, 3-pole, Fixed ","NCC",1384.74,0,1384.74,8592765048592,1,8592765048592,1,28592765048596,"8536209090",22]
[104859,"Ex9A16N 3P D/O 630","Air Circuit Breaker, frame size A16, Icu=55kA, In=630A, 3-pole, Withdrawable ","NCC",2195.85,0,2195.85,8592765048608,1,8592765048608,1,28592765048602,"8536209090",38]
[104860,"Ex9A16N 3P F 630","Air Circuit Breaker, frame size A16, Icu=55kA, In=630A, 3-pole, Fixed ","NCC",1702.09,0,1702.09,8592765048615,1,8592765048615,1,28592765048619,"8536209090",22]
[104861,"Ex9A16N 3P D/O 800","Air Circuit Breaker, frame size A16, Icu=55kA, In=800A, 3-pole, Withdrawable ","NCC",2380.9699999999998,0,2380.9699999999998,8592765048622,1,8592765048622,1,28592765048626,"8536209090",38]
[104862,"Ex9A16N 3P F 800","Air Circuit Breaker, frame size A16, Icu=55kA, In=800A, 3-pole, Fixed ","NCC",1887.23,0,1887.23,8592765048639,1,8592765048639,1,28592765048633,"8536209090",22]
[104863,"Ex9A16N 3P D/O 1000","Air Circuit Breaker, frame size A16, Icu=55kA, In=1000A, 3-pole, Withdrawable ","NCC",2492.04,0,2492.04,8592765048646,1,8592765048646,1,28592765048640,"8536209090",38]
[104864,"Ex9A16N 3P F 1000","Air Circuit Breaker, frame size A16, Icu=55kA, In=1000A, 3-pole, Fixed ","NCC",1998.33,0,1998.33,8592765048653,1,8592765048653,1,28592765048657,"8536209090",22]
[104865,"Ex9A16N 3P D/O 1250","Air Circuit Breaker, frame size A16, Icu=55kA, In=1250A, 3-pole, Withdrawable ","NCC",3220.3,0,3220.3,8592765048660,1,8592765048660,1,28592765048664,"8536209090",38]
[104866,"Ex9A16N 3P F 1250","Air Circuit Breaker, frame size A16, Icu=55kA, In=1250A, 3-pole, Fixed ","NCC",2726.52,0,2726.52,8592765048677,1,8592765048677,1,28592765048671,"8536209090",22]
[104867,"Ex9A16N 3P D/O 1600","Air Circuit Breaker, frame size A16, Icu=55kA, In=1600A, 3-pole, Withdrawable ","NCC",5577.75,0,5577.75,8592765048684,1,8592765048684,1,28592765048688,"8536209090",38]
[104868,"Ex9A16N 3P F 1600","Air Circuit Breaker, frame size A16, Icu=55kA, In=1600A, 3-pole, Fixed ","NCC",5083.9799999999996,0,5083.9799999999996,8592765048691,1,8592765048691,1,28592765048695,"8536209090",22]
[104869,"Ex9A16N 4P D/O 400","Air Circuit Breaker, frame size A16, Icu=55kA, In=400A, 4-pole, Withdrawable ","NCC",2858.52,0,2858.52,8592765048707,1,8592765048707,1,28592765048701,"8536209090",55]
[104870,"Ex9A16N 4P F 400","Air Circuit Breaker, frame size A16, Icu=55kA, In=400A, 4-pole, Fixed ","NCC",2476.86,0,2476.86,8592765048714,1,8592765048714,1,28592765048718,"8536209090",26.5]
[104871,"Ex9A16N 4P D/O 630","Air Circuit Breaker, frame size A16, Icu=55kA, In=630A, 4-pole, Withdrawable ","NCC",3520.64,0,3520.64,8592765048721,1,8592765048721,1,28592765048725,"8536209090",55]
[104872,"Ex9A16N 4P F 630","Air Circuit Breaker, frame size A16, Icu=55kA, In=630A, 4-pole, Fixed ","NCC",2915.55,0,2915.55,8592765048738,1,8592765048738,1,28592765048732,"8536209090",26.5]
[104873,"Ex9A16N 4P D/O 800","Air Circuit Breaker, frame size A16, Icu=55kA, In=800A, 4-pole, Withdrawable ","NCC",3755.14,0,3755.14,8592765048745,1,8592765048745,1,28592765048749,"8536209090",55]
[104874,"Ex9A16N 4P F 800","Air Circuit Breaker, frame size A16, Icu=55kA, In=800A, 4-pole, Fixed ","NCC",3150.09,0,3150.09,8592765048752,1,8592765048752,1,28592765048756,"8536209090",26.5]
[104875,"Ex9A16N 4P D/O 1000","Air Circuit Breaker, frame size A16, Icu=55kA, In=1000A, 4-pole, Withdrawable ","NCC",4199.47,0,4199.47,8592765048769,1,8592765048769,1,28592765048763,"8536209090",55]
[104876,"Ex9A16N 4P F 1000","Air Circuit Breaker, frame size A16, Icu=55kA, In=1000A, 4-pole, Fixed ","NCC",3594.43,0,3594.43,8592765048776,1,8592765048776,1,28592765048770,"8536209090",26.5]
[104877,"Ex9A16N 4P D/O 1250","Air Circuit Breaker, frame size A16, Icu=55kA, In=1250A, 4-pole, Withdrawable ","NCC",4804.28,0,4804.28,8592765048783,1,8592765048783,1,28592765048787,"8536209090",55]
[104878,"Ex9A16N 4P F 1250","Air Circuit Breaker, frame size A16, Icu=55kA, In=1250A, 4-pole, Fixed ","NCC",4199.21,0,4199.21,8592765048790,1,8592765048790,1,28592765048794,"8536209090",26.5]
[104879,"Ex9A16N 4P D/O 1600","Air Circuit Breaker, frame size A16, Icu=55kA, In=1600A, 4-pole, Withdrawable ","NCC",7346.89,0,7346.89,8592765048806,1,8592765048806,1,28592765048800,"8536209090",55]
[104880,"Ex9A16N 4P F 1600","Air Circuit Breaker, frame size A16, Icu=55kA, In=1600A, 4-pole, Fixed ","NCC",6741.83,0,6741.83,8592765048813,1,8592765048813,1,28592765048817,"8536209090",26.5]
[104881,"Ex9A16Q 3P D/O 400","Air Circuit Breaker, frame size A16, Icu=65kA, In=400A, 3-pole, Withdrawable ","NCC",2209.1,0,2209.1,8592765048820,1,8592765048820,1,28592765048824,"8536209090",38]
[104882,"Ex9A16Q 3P F 400","Air Circuit Breaker, frame size A16, Icu=65kA, In=400A, 3-pole, Fixed ","NCC",1892.94,0,1892.94,8592765048837,1,8592765048837,1,28592765048831,"8536209090",22]
[104883,"Ex9A16Q 3P D/O 630","Air Circuit Breaker, frame size A16, Icu=65kA, In=650A, 3-pole, Withdrawable ","NCC",2760.68,0,2760.68,8592765048844,1,8592765048844,1,28592765048848,"8536209090",38]
[104884,"Ex9A16Q 3P F 630","Air Circuit Breaker, frame size A16, Icu=65kA, In=650A, 3-pole, Fixed ","NCC",2266.75,0,2266.75,8592765048851,1,8592765048851,1,28592765048855,"8536209090",22]
[104885,"Ex9A16Q 3P D/O 800","Air Circuit Breaker, frame size A16, Icu=65kA, In=800A, 3-pole, Withdrawable ","NCC",2946.16,{"$f":"NCC","v":0},{"$f":"E2947*(1-F2947)","v":2946.16},8592765048868,1,8592765048868,1,28592765048862,"8536209090",38]
[104886,"Ex9A16Q 3P F 800","Air Circuit Breaker, frame size A16, Icu=65kA, In=800A, 3-pole, Fixed ","NCC",2452.33,0,2452.33,8592765048875,1,8592765048875,1,28592765048879,"8536209090",22]
[104887,"Ex9A16Q 3P D/O 1000","Air Circuit Breaker, frame size A16, Icu=65kA, In=1000A, 3-pole, Withdrawable ","NCC",3328.97,0,3328.97,8592765048882,1,8592765048882,1,28592765048886,"8536209090",38]
[104888,"Ex9A16Q 3P F 1000","Air Circuit Breaker, frame size A16, Icu=65kA, In=1000A, 3-pole, Fixed ","NCC",2835.26,0,2835.26,8592765048899,1,8592765048899,1,28592765048893,"8536209090",22]
[104889,"Ex9A16Q 3P D/O 1250","Air Circuit Breaker, frame size A16, Icu=65kA, In=1250A, 3-pole, Withdrawable ","NCC",4043.04,0,4043.04,8592765048905,1,8592765048905,1,28592765048909,"8536209090",38]
[104890,"Ex9A16Q 3P F 1250","Air Circuit Breaker, frame size A16, Icu=65kA, In=1250A, 3-pole, Fixed ","NCC",3549.91,0,3549.91,8592765048912,1,8592765048912,1,28592765048916,"8536209090",22]
[104891,"Ex9A16Q 3P D/O 1600","Air Circuit Breaker, frame size A16, Icu=65kA, In=1600A, 3-pole, Withdrawable ","NCC",6176.98,0,6176.98,8592765048929,1,8592765048929,1,28592765048923,"8536209090",38]
[104892,"Ex9A16Q 3P F 1600","Air Circuit Breaker, frame size A16, Icu=65kA, In=1600A, 3-pole, Fixed ","NCC",5683.99,0,5683.99,8592765048936,1,8592765048936,1,28592765048930,"8536209090",22]
[104893,"Ex9A16Q 4P D/O 400","Air Circuit Breaker, frame size A16, Icu=65kA, In=400A, 4-pole, Withdrawable ","NCC",3943.57,0,3943.57,8592765048943,1,8592765048943,1,28592765048947,"8536209090",55]
[104894,"Ex9A16Q 4P F 400","Air Circuit Breaker, frame size A16, Icu=65kA, In=400A, 4-pole, Fixed ","NCC",3561.93,0,3561.93,8592765048950,1,8592765048950,1,28592765048954,"8536209090",26.5]
[104895,"Ex9A16Q 4P D/O 630","Air Circuit Breaker, frame size A16, Icu=65kA, In=650A, 4-pole, Withdrawable ","NCC",4726.28,0,4726.28,8592765048967,1,8592765048967,1,28592765048961,"8536209090",55]
[104896,"Ex9A16Q 4P F 630","Air Circuit Breaker, frame size A16, Icu=65kA, In=650A, 4-pole, Fixed ","NCC",4121.18,0,4121.18,8592765048974,1,8592765048974,1,28592765048978,"8536209090",26.5]
[104897,"Ex9A16Q 4P D/O 800","Air Circuit Breaker, frame size A16, Icu=65kA, In=800A, 4-pole, Withdrawable ","NCC",4824.6499999999996,0,4824.6499999999996,8592765048981,1,8592765048981,1,28592765048985,"8536209090",55]
[104898,"Ex9A16Q 4P F 800","Air Circuit Breaker, frame size A16, Icu=65kA, In=800A, 4-pole, Fixed ","NCC",4219.53,0,4219.53,8592765048998,1,8592765048998,1,28592765048992,"8536209090",26.5]
[104899,"Ex9A16Q 4P D/O 1000","Air Circuit Breaker, frame size A16, Icu=65kA, In=1000A, 4-pole, Withdrawable ","NCC",5219.93,0,5219.93,8592765049001,1,8592765049001,1,28592765049005,"8536209090",55]
[104900,"Ex9A16Q 4P F 1000","Air Circuit Breaker, frame size A16, Icu=65kA, In=1000A, 4-pole, Fixed ","NCC",4614.93,0,4614.93,8592765049018,1,8592765049018,1,28592765049012,"8536209090",26.5]
[104901,"Ex9A16Q 4P D/O 1250","Air Circuit Breaker, frame size A16, Icu=65kA, In=1250A, 4-pole, Withdrawable ","NCC",5946.26,0,5946.26,8592765049025,1,8592765049025,1,28592765049029,"8536209090",55]
[104902,"Ex9A16Q 4P F 1250","Air Circuit Breaker, frame size A16, Icu=65kA, In=1250A, 4-pole, Fixed ","NCC",5341.26,0,5341.26,8592765049032,1,8592765049032,1,28592765049036,"8536209090",26.5]
[104903,"Ex9A16Q 4P D/O 1600","Air Circuit Breaker, frame size A16, Icu=65kA, In=1600A, 4-pole, Withdrawable ","NCC",8290.84,0,8290.84,8592765049049,1,8592765049049,1,28592765049043,"8536209090",55]
[104904,"Ex9A16Q 4P F 1600","Air Circuit Breaker, frame size A16, Icu=65kA, In=1600A, 4-pole, Fixed ","NCC",7686.08,0,7686.08,8592765049056,1,8592765049056,1,28592765049050,"8536209090",26.5]
[104905,"Ex9A32Q 3P D/O 1600","Air Circuit Breaker, frame size A32, Icu=65kA, In=1600A, 3-pole, Withdrawable ","NCC",6237.86,0,6237.86,8592765049063,1,8592765049063,1,28592765049067,"8536209090",98]
[104906,"Ex9A32Q 3P F 1600","Air Circuit Breaker, frame size A32, Icu=65kA, In=1600A, 3-pole, Fixed ","NCC",5960.24,0,5960.24,8592765049070,1,8592765049070,1,28592765049074,"8536209090",52.5]
[104907,"Ex9A32Q 3P D/O 2000","Air Circuit Breaker, frame size A32, Icu=65kA, In=2000A, 3-pole, Withdrawable ","NCC",7631.7,0,7631.7,8592765049087,1,8592765049087,1,28592765049081,"8536209090",98]
[104908,"Ex9A32Q 3P F 2000","Air Circuit Breaker, frame size A32, Icu=65kA, In=2000A, 3-pole, Fixed ","NCC",6917.25,0,6917.25,8592765049094,1,8592765049094,1,28592765049098,"8536209090",52.5]
[104909,"Ex9A32Q 3P D/O 2500","Air Circuit Breaker, frame size A32, Icu=65kA, In=2500A, 3-pole, Withdrawable ","NCC",9417.85,0,9417.85,8592765049100,1,8592765049100,1,28592765049104,"8536209090",98]
[104910,"Ex9A32Q 3P F 2500","Air Circuit Breaker, frame size A32, Icu=65kA, In=2500A, 3-pole, Fixed ","NCC",10243.299999999999,0,10243.299999999999,8592765049117,1,8592765049117,1,28592765049111,"8536209090",52.5]
[104911,"Ex9A32Q 3P D/O 2900","Air Circuit Breaker, frame size A32, Icu=65kA, In=2900A, 3-pole, Withdrawable ","NCC",8586.23,0,8586.23,8592765049124,1,8592765049124,1,28592765049128,"8536209090",98]
[104912,"Ex9A32Q 3P F 2900","Air Circuit Breaker, frame size A32, Icu=65kA, In=2900A, 3-pole, Fixed ","NCC",10301,0,10301,8592765049131,1,8592765049131,1,28592765049135,"8536209090",52.5]
[104913,"Ex9A32Q 3P D/O 3200","Air Circuit Breaker, frame size A32, Icu=65kA, In=3200A, 3-pole, Withdrawable ","NCC",12535.09,0,12535.09,8592765049148,1,8592765049148,1,28592765049142,"8536209090",98]
[104914,"Ex9A32Q 3P F 3200","Air Circuit Breaker, frame size A32, Icu=65kA, In=3200A, 3-pole, Fixed ","NCC",12420.44,0,12420.44,8592765049155,1,8592765049155,1,28592765049159,"8536209090",52.5]
[104915,"Ex9A32Q 4P D/O 1600","Air Circuit Breaker, frame size A32, Icu=65kA, In=1600A, 4-pole, Withdrawable ","NCC",7706.52,0,7706.52,8592765049162,1,8592765049162,1,28592765049166,"8536209090",121]
[104916,"Ex9A32Q 4P F 1600","Air Circuit Breaker, frame size A32, Icu=65kA, In=1600A, 4-pole, Fixed ","NCC",7822.39,0,7822.39,8592765049179,1,8592765049179,1,28592765049173,"8536209090",66.5]
[104917,"Ex9A32Q 4P D/O 2000","Air Circuit Breaker, frame size A32, Icu=65kA, In=2000A, 4-pole, Withdrawable ","NCC",9233.19,0,9233.19,8592765049186,1,8592765049186,1,28592765049180,"8536209090",121]
[104918,"Ex9A32Q 4P F 2000","Air Circuit Breaker, frame size A32, Icu=65kA, In=2000A, 4-pole, Fixed ","NCC",9102.83,0,9102.83,8592765049193,1,8592765049193,1,28592765049197,"8536209090",66.5]
[104919,"Ex9A32Q 4P D/O 2500","Air Circuit Breaker, frame size A32, Icu=65kA, In=2500A, 4-pole, Withdrawable ","NCC",13060.05,0,13060.05,8592765049209,1,8592765049209,1,28592765049203,"8536209090",121]
[104920,"Ex9A32Q 4P F 2500","Air Circuit Breaker, frame size A32, Icu=65kA, In=2500A, 4-pole, Fixed ","NCC",13251.96,0,13251.96,8592765049216,1,8592765049216,1,28592765049210,"8536209090",66.5]
[104921,"Ex9A32Q 4P D/O 2900","Air Circuit Breaker, frame size A32, Icu=65kA, In=2900A, 4-pole, Withdrawable ","NCC",12173.09,0,12173.09,8592765049223,1,8592765049223,1,28592765049227,"8536209090",121]
[104922,"Ex9A32Q 4P F 2900","Air Circuit Breaker, frame size A32, Icu=65kA, In=2900A, 4-pole, Fixed ","NCC",13416.16,0,13416.16,8592765049230,1,8592765049230,1,28592765049234,"8536209090",66.5]
[104923,"Ex9A32Q 4P D/O 3200","Air Circuit Breaker, frame size A32, Icu=65kA, In=3200A, 4-pole, Withdrawable ","NCC",16372.85,0,16372.85,8592765049247,1,8592765049247,1,28592765049241,"8536209090",121]
[104924,"Ex9A32Q 4P F 3200","Air Circuit Breaker, frame size A32, Icu=65kA, In=3200A, 4-pole, Fixed ","NCC",16647.939999999999,0,16647.939999999999,8592765049254,1,8592765049254,1,28592765049258,"8536209090",66.5]
[104925,"Ex9A32R 3P D/O 1600","Air Circuit Breaker, frame size A32, Icu=85kA, In=1600A, 3-pole, Withdrawable ","NCC",6738.71,0,6738.71,8592765049261,1,8592765049261,1,28592765049265,"8536209090",98]
[104926,"Ex9A32R 3P F 1600","Air Circuit Breaker, frame size A32, Icu=85kA, In=1600A, 3-pole, Fixed ","NCC",6465.91,0,6465.91,8592765049278,1,8592765049278,1,28592765049272,"8536209090",52.5]
[104927,"Ex9A32R 3P D/O 2000","Air Circuit Breaker, frame size A32, Icu=85kA, In=2000A, 3-pole, Withdrawable ","NCC",8481.35,0,8481.35,8592765049285,1,8592765049285,1,28592765049289,"8536209090",98]
[104928,"Ex9A32R 3P F 2000","Air Circuit Breaker, frame size A32, Icu=85kA, In=2000A, 3-pole, Fixed ","NCC",7714.99,0,7714.99,8592765049292,1,8592765049292,1,28592765049296,"8536209090",52.5]
[104929,"Ex9A32R 3P D/O 2500","Air Circuit Breaker, frame size A32, Icu=85kA, In=2500A, 3-pole, Withdrawable ","NCC",10351.93,0,10351.93,8592765049308,1,8592765049308,1,28592765049302,"8536209090",98]
[104930,"Ex9A32R 3P F 2500","Air Circuit Breaker, frame size A32, Icu=85kA, In=2500A, 3-pole, Fixed ","NCC",11158.06,0,11158.06,8592765049315,1,8592765049315,1,28592765049319,"8536209090",52.5]
[104931,"Ex9A32R 3P D/O 2900","Air Circuit Breaker, frame size A32, Icu=85kA, In=2900A, 3-pole, Withdrawable ","NCC",9641.44,0,9641.44,8592765049322,1,8592765049322,1,28592765049326,"8536209090",98]
[104932,"Ex9A32R 3P F 2900","Air Circuit Breaker, frame size A32, Icu=85kA, In=2900A, 3-pole, Fixed ","NCC",11919.65,0,11919.65,8592765049339,1,8592765049339,1,28592765049333,"8536209090",52.5]
[104933,"Ex9A32R 3P D/O 3200","Air Circuit Breaker, frame size A32, Icu=85kA, In=3200A, 3-pole, Withdrawable ","NCC",13140.92,0,13140.92,8592765049346,1,8592765049346,1,28592765049340,"8536209090",98]
[104934,"Ex9A32R 3P F 3200","Air Circuit Breaker, frame size A32, Icu=85kA, In=3200A, 3-pole, Fixed ","NCC",13025.03,0,13025.03,8592765049353,1,8592765049353,1,28592765049357,"8536209090",52.5]
[104935,"Ex9A32R 4P D/O 1600","Air Circuit Breaker, frame size A32, Icu=85kA, In=1600A, 4-pole, Withdrawable ","NCC",8237.56,0,8237.56,8592765049360,1,8592765049360,1,28592765049364,"8536209090",121]
[104936,"Ex9A32R 4P F 1600","Air Circuit Breaker, frame size A32, Icu=85kA, In=1600A, 4-pole, Fixed ","NCC",8388.42,0,8388.42,8592765049377,1,8592765049377,1,28592765049371,"8536209090",66.5]
[104937,"Ex9A32R 4P D/O 2000","Air Circuit Breaker, frame size A32, Icu=85kA, In=2000A, 4-pole, Withdrawable ","NCC",10004.32,0,10004.32,8592765049384,1,8592765049384,1,28592765049388,"8536209090",121]
[104938,"Ex9A32R 4P F 2000","Air Circuit Breaker, frame size A32, Icu=85kA, In=2000A, 4-pole, Fixed ","NCC",10034.5,0,10034.5,8592765049391,1,8592765049391,1,28592765049395,"8536209090",66.5]
[104939,"Ex9A32R 4P D/O 2500","Air Circuit Breaker, frame size A32, Icu=85kA, In=2500A, 4-pole, Withdrawable ","NCC",14126.89,0,14126.89,8592765049407,1,8592765049407,1,28592765049401,"8536209090",121]
[104940,"Ex9A32R 4P F 2500","Air Circuit Breaker, frame size A32, Icu=85kA, In=2500A, 4-pole, Fixed ","NCC",14275.37,0,14275.37,8592765049414,1,8592765049414,1,28592765049418,"8536209090",66.5]
[104941,"Ex9A32R 4P D/O 2900","Air Circuit Breaker, frame size A32, Icu=85kA, In=2900A, 4-pole, Withdrawable ","NCC",13235.69,0,13235.69,8592765049421,1,8592765049421,1,28592765049425,"8536209090",121]
[104942,"Ex9A32R 4P F 2900","Air Circuit Breaker, frame size A32, Icu=85kA, In=2900A, 4-pole, Fixed ","NCC",14549.71,0,14549.71,8592765049438,1,8592765049438,1,28592765049432,"8536209090",66.5]
[104943,"Ex9A32R 4P D/O 3200","Air Circuit Breaker, frame size A32, Icu=85kA, In=3200A, 4-pole, Withdrawable ","NCC",17530.189999999999,0,17530.189999999999,8592765049445,1,8592765049445,1,28592765049449,"8536209090",121]
[104944,"Ex9A32R 4P F 3200","Air Circuit Breaker, frame size A32, Icu=85kA, In=3200A, 4-pole, Fixed ","NCC",17716.02,0,17716.02,8592765049452,1,8592765049452,1,28592765049456,"8536209090",66.5]
[104945,"Ex9A32H 3P D/O 1600","Air Circuit Breaker, frame size A32, Icu=100kA, In=1600A, 3-pole, Withdrawable ","NCC",7139.34,0,7139.34,8592765049469,1,8592765049469,1,28592765049463,"8536209090",98]
[104946,"Ex9A32H 3P F 1600","Air Circuit Breaker, frame size A32, Icu=100kA, In=1600A, 3-pole, Fixed ","NCC",6893.13,0,6893.13,8592765049476,1,8592765049476,1,28592765049470,"8536209090",52.5]
[104947,"Ex9A32H 3P D/O 2000","Air Circuit Breaker, frame size A32, Icu=100kA, In=2000A, 3-pole, Withdrawable ","NCC",9215.1,0,9215.1,8592765049483,1,8592765049483,1,28592765049487,"8536209090",98]
[104948,"Ex9A32H 3P F 2000","Air Circuit Breaker, frame size A32, Icu=100kA, In=2000A, 3-pole, Fixed ","NCC",8419.7900000000009,0,8419.7900000000009,8592765049490,1,8592765049490,1,28592765049494,"8536209090",52.5]
[104949,"Ex9A32H 3P D/O 2500","Air Circuit Breaker, frame size A32, Icu=100kA, In=2500A, 3-pole, Withdrawable ","NCC",11133.94,{"$f":"NCC","v":0},{"$f":"E3011*(1-F3011)","v":11133.94},8592765049506,1,8592765049506,1,28592765049500,"8536209090",98]
[104950,"Ex9A32H 3P F 2500","Air Circuit Breaker, frame size A32, Icu=100kA, In=2500A, 3-pole, Fixed ","NCC",11946.15,0,11946.15,8592765049513,1,8592765049513,1,28592765049517,"8536209090",52.5]
[104951,"Ex9A32H 3P D/O 2900","Air Circuit Breaker, frame size A32, Icu=100kA, In=2900A, 3-pole, Withdrawable ","NCC",10416.74,0,10416.74,8592765049520,1,8592765049520,1,28592765049524,"8536209090",98]
[104952,"Ex9A32H 3P F 2900","Air Circuit Breaker, frame size A32, Icu=100kA, In=2900A, 3-pole, Fixed ","NCC",12681.35,0,12681.35,8592765049537,1,8592765049537,1,28592765049531,"8536209090",52.5]
[104953,"Ex9A32H 3P D/O 3200","Air Circuit Breaker, frame size A32, Icu=100kA, In=3200A, 3-pole, Withdrawable ","NCC",13568.15,0,13568.15,8592765049544,1,8592765049544,1,28592765049548,"8536209090",98]
[104954,"Ex9A32H 3P F 3200","Air Circuit Breaker, frame size A32, Icu=100kA, In=3200A, 3-pole, Fixed ","NCC",13486.06,0,13486.06,8592765049551,1,8592765049551,1,28592765049555,"8536209090",52.5]
[104955,"Ex9A32H 4P D/O 1600","Air Circuit Breaker, frame size A32, Icu=100kA, In=1600A, 4-pole, Withdrawable ","NCC",8672.01,0,8672.01,8592765049568,1,8592765049568,1,28592765049562,"8536209090",121]
[104956,"Ex9A32H 4P F 1600","Air Circuit Breaker, frame size A32, Icu=100kA, In=1600A, 4-pole, Fixed ","NCC",8856.67,0,8856.67,8592765049575,1,8592765049575,1,28592765049579,"8536209090",66.5]
[104957,"Ex9A32H 4P D/O 2000","Air Circuit Breaker, frame size A32, Icu=100kA, In=2000A, 4-pole, Withdrawable ","NCC",10662.06,0,10662.06,8592765049582,1,8592765049582,1,28592765049586,"8536209090",121]
[104958,"Ex9A32H 4P F 2000","Air Circuit Breaker, frame size A32, Icu=100kA, In=2000A, 4-pole, Fixed ","NCC",10851.54,0,10851.54,8592765049599,1,8592765049599,1,28592765049593,"8536209090",66.5]
[104959,"Ex9A32H 4P D/O 2500","Air Circuit Breaker, frame size A32, Icu=100kA, In=2500A, 4-pole, Withdrawable ","NCC",15041.68,0,15041.68,8592765049605,1,8592765049605,1,28592765049609,"8536209090",121]
[104960,"Ex9A32H 4P F 2500","Air Circuit Breaker, frame size A32, Icu=100kA, In=2500A, 4-pole, Fixed ","NCC",15141.83,0,15141.83,8592765049612,1,8592765049612,1,28592765049616,"8536209090",66.5]
[104961,"Ex9A32H 4P D/O 2900","Air Circuit Breaker, frame size A32, Icu=100kA, In=2900A, 4-pole, Withdrawable ","NCC",14143.94,0,14143.94,8592765049629,1,8592765049629,1,28592765049623,"8536209090",121]
[104962,"Ex9A32H 4P F 2900","Air Circuit Breaker, frame size A32, Icu=100kA, In=2900A, 4-pole, Fixed ","NCC",15412.41,0,15412.41,8592765049636,1,8592765049636,1,28592765049630,"8536209090",66.5]
[104963,"Ex9A32H 4P D/O 3200","Air Circuit Breaker, frame size A32, Icu=100kA, In=3200A, 4-pole, Withdrawable ","NCC",18501.689999999999,0,18501.689999999999,8592765049643,1,8592765049643,1,28592765049647,"8536209090",121]
[104964,"Ex9A32H 4P F 3200","Air Circuit Breaker, frame size A32, Icu=100kA, In=3200A, 4-pole, Fixed ","NCC",18592.189999999999,0,18592.189999999999,8592765049650,1,8592765049650,1,28592765049654,"8536209090",66.5]
[104965,"Ex9A40Q 3P D/O 2000","Air Circuit Breaker, frame size A40, Icu=65kA, In=2000A, 3-pole, Withdrawable ","NCC",6050.75,0,6050.75,8592765049667,1,8592765049667,1,28592765049661,"8536209090",118]
[104966,"Ex9A40Q 3P F 2000","Air Circuit Breaker, frame size A40, Icu=65kA, In=2000A, 3-pole, Fixed ","NCC",6917.25,0,6917.25,8592765049674,1,8592765049674,1,28592765049678,"8536209090",72.5]
[104967,"Ex9A40Q 3P D/O 2500","Air Circuit Breaker, frame size A40, Icu=65kA, In=2500A, 3-pole, Withdrawable ","NCC",7836.88,0,7836.88,8592765049681,1,8592765049681,1,28592765049685,"8536209090",118]
[104968,"Ex9A40Q 3P F 2500","Air Circuit Breaker, frame size A40, Icu=65kA, In=2500A, 3-pole, Fixed ","NCC",10243.299999999999,0,10243.299999999999,8592765049698,1,8592765049698,1,28592765049692,"8536209090",72.5]
[104969,"Ex9A40Q 3P D/O 2900","Air Circuit Breaker, frame size A40, Icu=65kA, In=2900A, 3-pole, Withdrawable ","NCC",8035.7,0,8035.7,8592765049704,1,8592765049704,1,28592765049708,"8536209090",118]
[104970,"Ex9A40Q 3P F 2900","Air Circuit Breaker, frame size A40, Icu=65kA, In=2900A, 3-pole, Fixed ","NCC",10336.26,0,10336.26,8592765049711,1,8592765049711,1,28592765049715,"8536209090",72.5]
[104971,"Ex9A40Q 3P D/O 3200","Air Circuit Breaker, frame size A40, Icu=65kA, In=3200A, 3-pole, Withdrawable ","NCC",11907.54,0,11907.54,8592765049728,1,8592765049728,1,28592765049722,"8536209090",118]
[104972,"Ex9A40Q 3P F 3200","Air Circuit Breaker, frame size A40, Icu=65kA, In=3200A, 3-pole, Fixed ","NCC",12420.44,0,12420.44,8592765049735,1,8592765049735,1,28592765049739,"8536209090",72.5]
[104973,"Ex9A40Q 3P D/O 4000","Air Circuit Breaker, frame size A40, Icu=65kA, In=4000A, 3-pole, Withdrawable ","NCC",19750.009999999998,0,19750.009999999998,8592765049742,1,8592765049742,1,28592765049746,"8536209090",118]
[104974,"Ex9A40Q 3P F 4000","Air Circuit Breaker, frame size A40, Icu=65kA, In=4000A, 3-pole, Fixed ","NCC",18487.2,0,18487.2,8592765049759,1,8592765049759,1,28592765049753,"8536209090",72.5]
[104975,"Ex9A40Q 4P D/O 2000","Air Circuit Breaker, frame size A40, Icu=65kA, In=2000A, 4-pole, Withdrawable ","NCC",7124.88,0,7124.88,8592765049766,1,8592765049766,1,28592765049760,"8536209090",141]
[104976,"Ex9A40Q 4P F 2000","Air Circuit Breaker, frame size A40, Icu=65kA, In=2000A, 4-pole, Fixed ","NCC",9102.83,0,9102.83,8592765049773,1,8592765049773,1,28592765049777,"8536209090",86.5]
[104977,"Ex9A40Q 4P D/O 2500","Air Circuit Breaker, frame size A40, Icu=65kA, In=2500A, 4-pole, Withdrawable ","NCC",10951.74,0,10951.74,8592765049780,1,8592765049780,1,28592765049784,"8536209090",141]
[104978,"Ex9A40Q 4P F 2500","Air Circuit Breaker, frame size A40, Icu=65kA, In=2500A, 4-pole, Fixed ","NCC",13251.96,0,13251.96,8592765049797,1,8592765049797,1,28592765049791,"8536209090",86.5]
[104979,"Ex9A40Q 4P D/O 2900","Air Circuit Breaker, frame size A40, Icu=65kA, In=2900A, 4-pole, Withdrawable ","NCC",11266.41,0,11266.41,8592765049803,1,8592765049803,1,28592765049807,"8536209090",141]
[104980,"Ex9A40Q 4P F 2900","Air Circuit Breaker, frame size A40, Icu=65kA, In=2900A, 4-pole, Fixed ","NCC",13340.65,0,13340.65,8592765049810,1,8592765049810,1,28592765049814,"8536209090",86.5]
[104981,"Ex9A40Q 4P D/O 3200","Air Circuit Breaker, frame size A40, Icu=65kA, In=3200A, 4-pole, Withdrawable ","NCC",15535.34,0,15535.34,8592765049827,1,8592765049827,1,28592765049821,"8536209090",141]
[104982,"Ex9A40Q 4P F 3200","Air Circuit Breaker, frame size A40, Icu=65kA, In=3200A, 4-pole, Fixed ","NCC",16647.939999999999,0,16647.939999999999,8592765049834,1,8592765049834,1,28592765049838,"8536209090",86.5]
[104983,"Ex9A40Q 4P D/O 4000","Air Circuit Breaker, frame size A40, Icu=65kA, In=4000A, 4-pole, Withdrawable ","NCC",22476.98,0,22476.98,8592765049841,1,8592765049841,1,28592765049845,"8536209090",141]
[104984,"Ex9A40Q 4P F 4000","Air Circuit Breaker, frame size A40, Icu=65kA, In=4000A, 4-pole, Fixed ","NCC",23511.27,0,23511.27,8592765049858,1,8592765049858,1,28592765049852,"8536209090",86.5]
[104985,"Ex9A40R 3P D/O 2000","Air Circuit Breaker, frame size A40, Icu=85kA, In=2000A, 3-pole, Withdrawable ","NCC",6900.38,0,6900.38,8592765049865,1,8592765049865,1,28592765049869,"8536209090",118]
[104986,"Ex9A40R 3P F 2000","Air Circuit Breaker, frame size A40, Icu=85kA, In=2000A, 3-pole, Fixed ","NCC",7714.99,0,7714.99,8592765049872,1,8592765049872,1,28592765049876,"8536209090",72.5]
[104987,"Ex9A40R 3P D/O 2500","Air Circuit Breaker, frame size A40, Icu=85kA, In=2500A, 3-pole, Withdrawable ","NCC",8770.9500000000007,0,8770.9500000000007,8592765049889,1,8592765049889,1,28592765049883,"8536209090",118]
[104988,"Ex9A40R 3P F 2500","Air Circuit Breaker, frame size A40, Icu=85kA, In=2500A, 3-pole, Fixed ","NCC",11158.06,0,11158.06,8592765049896,1,8592765049896,1,28592765049890,"8536209090",72.5]
[104989,"Ex9A40R 3P D/O 2900","Air Circuit Breaker, frame size A40, Icu=85kA, In=2900A, 3-pole, Withdrawable ","NCC",8858.02,0,8858.02,8592765049902,1,8592765049902,1,28592765049906,"8536209090",118]
[104990,"Ex9A40R 3P F 2900","Air Circuit Breaker, frame size A40, Icu=85kA, In=2900A, 3-pole, Fixed ","NCC",11198.43,0,11198.43,8592765049919,1,8592765049919,1,28592765049913,"8536209090",72.5]
[104991,"Ex9A40R 3P D/O 3200","Air Circuit Breaker, frame size A40, Icu=85kA, In=3200A, 3-pole, Withdrawable ","NCC",12513.37,0,12513.37,8592765049926,1,8592765049926,1,28592765049920,"8536209090",118]
[104992,"Ex9A40R 3P F 3200","Air Circuit Breaker, frame size A40, Icu=85kA, In=3200A, 3-pole, Fixed ","NCC",13025.03,0,13025.03,8592765049933,1,8592765049933,1,28592765049937,"8536209090",72.5]
[104993,"Ex9A40R 3P D/O 4000","Air Circuit Breaker, frame size A40, Icu=85kA, In=4000A, 3-pole, Withdrawable ","NCC",18142.03,0,18142.03,8592765049940,1,8592765049940,1,28592765049944,"8536209090",118]
[104994,"Ex9A40R 3P F 4000","Air Circuit Breaker, frame size A40, Icu=85kA, In=4000A, 3-pole, Fixed ","NCC",18843.22,0,18843.22,8592765049957,1,8592765049957,1,28592765049951,"8536209090",72.5]
[104995,"Ex9A40R 4P D/O 2000","Air Circuit Breaker, frame size A40, Icu=85kA, In=2000A, 4-pole, Withdrawable ","NCC",7896.01,0,7896.01,8592765049964,1,8592765049964,1,28592765049968,"8536209090",141]
[104996,"Ex9A40R 4P F 2000","Air Circuit Breaker, frame size A40, Icu=85kA, In=2000A, 4-pole, Fixed ","NCC",10034.5,0,10034.5,8592765049971,1,8592765049971,1,28592765049975,"8536209090",86.5]
[104997,"Ex9A40R 4P D/O 2500","Air Circuit Breaker, frame size A40, Icu=85kA, In=2500A, 4-pole, Withdrawable ","NCC",12018.58,0,12018.58,8592765049988,1,8592765049988,1,28592765049982,"8536209090",141]
[104998,"Ex9A40R 4P F 2500","Air Circuit Breaker, frame size A40, Icu=85kA, In=2500A, 4-pole, Fixed ","NCC",14275.37,0,14275.37,8592765049995,1,8592765049995,1,28592765049999,"8536209090",86.5]
[104999,"Ex9A40R 4P D/O 2900","Air Circuit Breaker, frame size A40, Icu=85kA, In=2900A, 4-pole, Withdrawable ","NCC",12406.53,0,12406.53,8592765050007,1,8592765050007,1,28592765050001,"8536209090",141]
[105000,"Ex9A40R 4P F 2900","Air Circuit Breaker, frame size A40, Icu=85kA, In=2900A, 4-pole, Fixed ","NCC",14524,0,14524,8592765050014,1,8592765050014,1,28592765050018,"8536209090",86.5]
[105001,"Ex9A40R 4P D/O 3200","Air Circuit Breaker, frame size A40, Icu=85kA, In=3200A, 4-pole, Withdrawable ","NCC",16692.669999999998,0,16692.669999999998,8592765050021,1,8592765050021,1,28592765050025,"8536209090",141]
[105002,"Ex9A40R 4P F 3200","Air Circuit Breaker, frame size A40, Icu=85kA, In=3200A, 4-pole, Fixed ","NCC",17716.02,0,17716.02,8592765050038,1,8592765050038,1,28592765050032,"8536209090",86.5]
[105003,"Ex9A40R 4P D/O 4000","Air Circuit Breaker, frame size A40, Icu=85kA, In=4000A, 4-pole, Withdrawable ","NCC",24197.94,0,24197.94,8592765050045,1,8592765050045,1,28592765050049,"8536209090",141]
[105004,"Ex9A40R 4P F 4000","Air Circuit Breaker, frame size A40, Icu=85kA, In=4000A, 4-pole, Fixed ","NCC",24957.01,0,24957.01,8592765050052,1,8592765050052,1,28592765050056,"8536209090",86.5]
[105005,"Ex9A40H 3P D/O 2000","Air Circuit Breaker, frame size A40, Icu=100kA, In=2000A, 3-pole, Withdrawable ","NCC",7634.13,0,7634.13,8592765050069,1,8592765050069,1,28592765050063,"8536209090",118]
[105006,"Ex9A40H 3P F 2000","Air Circuit Breaker, frame size A40, Icu=100kA, In=2000A, 3-pole, Fixed ","NCC",8419.7900000000009,0,8419.7900000000009,8592765050076,1,8592765050076,1,28592765050070,"8536209090",72.5]
[105007,"Ex9A40H 3P D/O 2500","Air Circuit Breaker, frame size A40, Icu=100kA, In=2500A, 3-pole, Withdrawable ","NCC",9552.9599999999991,0,9552.9599999999991,8592765050083,1,8592765050083,1,28592765050087,"8536209090",118]
[105008,"Ex9A40H 3P F 2500","Air Circuit Breaker, frame size A40, Icu=100kA, In=2500A, 3-pole, Fixed ","NCC",11946.15,0,11946.15,8592765050090,1,8592765050090,1,28592765050094,"8536209090",72.5]
[105009,"Ex9A40H 3P D/O 2900","Air Circuit Breaker, frame size A40, Icu=100kA, In=2900A, 3-pole, Withdrawable ","NCC",9630.7099999999991,0,9630.7099999999991,8592765050106,1,8592765050106,1,28592765050100,"8536209090",118]
[105010,"Ex9A40H 3P F 2900","Air Circuit Breaker, frame size A40, Icu=100kA, In=2900A, 3-pole, Fixed ","NCC",12017.9,0,12017.9,8592765050113,1,8592765050113,1,28592765050117,"8536209090",72.5]
[105011,"Ex9A40H 3P D/O 3200","Air Circuit Breaker, frame size A40, Icu=100kA, In=3200A, 3-pole, Withdrawable ","NCC",12940.59,0,12940.59,8592765050120,1,8592765050120,1,28592765050124,"8536209090",118]
[105012,"Ex9A40H 3P F 3200","Air Circuit Breaker, frame size A40, Icu=100kA, In=3200A, 3-pole, Fixed ","NCC",13486.06,0,13486.06,8592765050137,1,8592765050137,1,28592765050131,"8536209090",72.5]
[105013,"Ex9A40H 3P D/O 4000","Air Circuit Breaker, frame size A40, Icu=100kA, In=4000A, 3-pole, Withdrawable ","NCC",18253.080000000002,{"$f":"NCC","v":0},{"$f":"E3075*(1-F3075)","v":18253.080000000002},8592765050144,1,8592765050144,1,28592765050148,"8536209090",118]
[105014,"Ex9A40H 3P F 4000","Air Circuit Breaker, frame size A40, Icu=100kA, In=4000A, 3-pole, Fixed ","NCC",18997.689999999999,0,18997.689999999999,8592765050151,1,8592765050151,1,28592765050155,"8536209090",72.5]
[105015,"Ex9A40H 4P D/O 2000","Air Circuit Breaker, frame size A40, Icu=100kA, In=2000A, 4-pole, Withdrawable ","NCC",8553.74,0,8553.74,8592765050168,1,8592765050168,1,28592765050162,"8536209090",141]
[105016,"Ex9A40H 4P F 2000","Air Circuit Breaker, frame size A40, Icu=100kA, In=2000A, 4-pole, Fixed ","NCC",10851.54,0,10851.54,8592765050175,1,8592765050175,1,28592765050179,"8536209090",86.5]
[105017,"Ex9A40H 4P D/O 2500","Air Circuit Breaker, frame size A40, Icu=100kA, In=2500A, 4-pole, Withdrawable ","NCC",12933.36,0,12933.36,8592765050182,1,8592765050182,1,28592765050186,"8536209090",141]
[105018,"Ex9A40H 4P F 2500","Air Circuit Breaker, frame size A40, Icu=100kA, In=2500A, 4-pole, Fixed ","NCC",15141.83,0,15141.83,8592765050199,1,8592765050199,1,28592765050193,"8536209090",86.5]
[105019,"Ex9A40H 4P D/O 2900","Air Circuit Breaker, frame size A40, Icu=100kA, In=2900A, 4-pole, Withdrawable ","NCC",13184.67,0,13184.67,8592765050205,1,8592765050205,1,28592765050209,"8536209090",141]
[105020,"Ex9A40H 4P F 2900","Air Circuit Breaker, frame size A40, Icu=100kA, In=2900A, 4-pole, Fixed ","NCC",15213.75,0,15213.75,8592765050212,1,8592765050212,1,28592765050216,"8536209090",86.5]
[105021,"Ex9A40H 4P D/O 3200","Air Circuit Breaker, frame size A40, Icu=100kA, In=3200A, 4-pole, Withdrawable ","NCC",17664.18,0,17664.18,8592765050229,1,8592765050229,1,28592765050223,"8536209090",141]
[105022,"Ex9A40H 4P F 3200","Air Circuit Breaker, frame size A40, Icu=100kA, In=3200A, 4-pole, Fixed ","NCC",18592.189999999999,0,18592.189999999999,8592765050236,1,8592765050236,1,28592765050230,"8536209090",86.5]
[105023,"Ex9A40H 4P D/O 4000","Air Circuit Breaker, frame size A40, Icu=100kA, In=4000A, 4-pole, Withdrawable ","NCC",25666.66,0,25666.66,8592765050243,1,8592765050243,1,28592765050247,"8536209090",141]
[105024,"Ex9A40H 4P F 4000","Air Circuit Breaker, frame size A40, Icu=100kA, In=4000A, 4-pole, Fixed ","NCC",26140.95,0,26140.95,8592765050250,1,8592765050250,1,28592765050254,"8536209090",86.5]
[]
["Air Switch Disconnectors Ex9ASD"]
[105063,"Ex9ASD04 3P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=400A, 3-pole, Withdrawable ","NCC",2142.25,{"$f":"NCC","v":0},{"$f":"E3089*(1-F3089)","v":2142.25},8592765050649,1,8592765050649,1,28592765050643,"8536209090",36]
[105064,"Ex9ASD04 3P F","Air Circuit Switch Disconnectors, frame size A16, In=400A, 3-pole, Fixed ","NCC",1737.14,0,1737.14,8592765050656,1,8592765050656,1,28592765050650,"8536209090",20]
[105065,"Ex9ASD06 3P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=600A, 3-pole, Withdrawable ","NCC",2322.5700000000002,0,2322.5700000000002,8592765050663,1,8592765050663,1,28592765050667,"8536209090",36]
[105066,"Ex9ASD06 3P F","Air Circuit Switch Disconnectors, frame size A16, In=600A, 3-pole, Fixed ","NCC",1828.56,0,1828.56,8592765050670,1,8592765050670,1,28592765050674,"8536209090",20]
[105067,"Ex9ASD08 3P D/O","Air Circuit Switch Disconnectors, frame size A16, In=800A, 3-pole, Withdrawable ","NCC",2507.89,0,2507.89,8592765050687,1,8592765050687,1,28592765050681,"8536209090",36]
[105068,"Ex9ASD08 3P F","Air Circuit Switch Disconnectors, frame size A16, In=800A, 3-pole, Fixed ","NCC",2013.87,0,2013.87,8592765050694,1,8592765050694,1,28592765050698,"8536209090",20]
[105069,"Ex9ASD10 3P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=1000A, 3-pole, Withdrawable ","NCC",2619.0700000000002,0,2619.0700000000002,8592765050700,1,8592765050700,1,28592765050704,"8536209090",36]
[105070,"Ex9ASD10 3P F","Air Circuit Switch Disconnectors, frame size A16, In=1000A, 3-pole, Fixed ","NCC",2125.0700000000002,0,2125.0700000000002,8592765050717,1,8592765050717,1,28592765050711,"8536209090",20]
[105071,"Ex9ASD12 3P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=1200A, 3-pole, Withdrawable ","NCC",3348.05,0,3348.05,8592765050724,1,8592765050724,1,28592765050728,"8536209090",36]
[105072,"Ex9ASD12 3P F","Air Circuit Switch Disconnectors, frame size A16, In=1200A, 3-pole, Fixed ","NCC",2854.05,0,2854.05,8592765050731,1,8592765050731,1,28592765050735,"8536209090",20]
[105073,"Ex9ASD16 3P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=1600A, 3-pole, Withdrawable ","NCC",5707.87,0,5707.87,8592765050748,1,8592765050748,1,28592765050742,"8536209090",36]
[105074,"Ex9ASD16 3P F","Air Circuit Switch Disconnectors, frame size A16, In=1600A, 3-pole, Fixed ","NCC",5213.87,0,5213.87,8592765050755,1,8592765050755,1,28592765050759,"8536209090",20]
[107110,"Ex9ASD16b 3P D/O ","Air Circuit Switch Disconnectors, frame size A32, In=1600A, 3-pole, Withdrawable ","NCC",6284.02,0,6284.02,8592765071118,1,8592765071118,1,28592765071112,"8536209090",116]
[107111,"Ex9ASD16b 3P F","Air Circuit Switch Disconnectors, frame size A32, In=1600A, 3-pole, Fixed ","NCC",6210.35,0,6210.35,8592765071125,1,8592765071125,1,28592765071129,"8536209090",70]
[105076,"Ex9ASD20 3P D/O ","Air Circuit Switch Disconnectors, frame size A32, In=2000A, 3-pole, Withdrawable ","NCC",8163.06,0,8163.06,8592765050779,1,8592765050779,1,28592765050773,"8536209090",116]
[105077,"Ex9ASD20 3P F","Air Circuit Switch Disconnectors, frame size A32, In=2000A, 3-pole, Fixed ","NCC",6644.82,0,6644.82,8592765050786,1,8592765050786,1,28592765050780,"8536209090",70]
[105078,"Ex9ASD25 3P D/O","Air Circuit Switch Disconnectors, frame size A32, In=2500A, 3-pole, Withdrawable ","NCC",9390.39,0,9390.39,8592765050793,1,8592765050793,1,28592765050797,"8536209090",116]
[105079,"Ex9ASD25 3P F","Air Circuit Switch Disconnectors, frame size A32, In=2500A, 3-pole, Fixed ","NCC",10668.42,0,10668.42,8592765050809,1,8592765050809,1,28592765050803,"8536209090",70]
[105080,"Ex9ASD29 3P D/O ","Air Circuit Switch Disconnectors, frame size A32, In=2900A, 3-pole, Withdrawable ","NCC",8553.68,0,8553.68,8592765050816,1,8592765050816,1,28592765050810,"8536209090",116]
[105081,"Ex9ASD29 3P F","Air Circuit Switch Disconnectors, frame size A32, In=2900A, 3-pole, Fixed ","NCC",10725.46,0,10725.46,8592765050823,1,8592765050823,1,28592765050827,"8536209090",70]
[105082,"Ex9ASD32 3P D/O","Air Circuit Switch Disconnectors, frame size A32, In=3200A, 3-pole, Withdrawable ","NCC",12389.36,0,12389.36,8592765050830,1,8592765050830,1,28592765050834,"8536209090",116]
[105083,"Ex9ASD32 3P F","Air Circuit Switch Disconnectors, frame size A32, In=3200A, 3-pole, Fixed ","NCC",12845.52,0,12845.52,8592765050847,1,8592765050847,1,28592765050841,"8536209090",70]
[105084,"Ex9ASD36 3P D/O ","Air Circuit Switch Disconnectors, frame size A40, In=3600A, 3-pole, Withdrawable ","NCC",16806.12,0,16806.12,8592765050854,1,8592765050854,1,28592765050858,"8536209090",116]
[105085,"Ex9ASD36 3P F","Air Circuit Switch Disconnectors, frame size A40, In=3600A, 3-pole, Fixed ","NCC",17294.46,0,17294.46,8592765050861,1,8592765050861,1,28592765050865,"8536209090",70]
[105086,"Ex9ASD40 3P D/O ","Air Circuit Switch Disconnectors, frame size A40, In=4000A, 3-pole, Withdrawable ","NCC",20695.05,0,20695.05,8592765050878,1,8592765050878,1,28592765050872,"8536209090",116]
[105087,"Ex9ASD40 3P F","Air Circuit Switch Disconnectors, frame size A40, In=4000A, 3-pole, Fixed ","NCC",20326.37,0,20326.37,8592765050885,1,8592765050885,1,28592765050889,"8536209090",70]
[105089,"Ex9ASD04 4P D/O","Air Circuit Switch Disconnectors, frame size A16, In=400A, 4-pole, Withdrawable ","NCC",3286.86,0,3286.86,8592765050908,1,8592765050908,1,28592765050902,"8536209090",52]
[105090,"Ex9ASD04 4P F","Air Circuit Switch Disconnectors, frame size A16, In=400A, 4-pole, Fixed ","NCC",2805.24,0,2805.24,8592765050915,1,8592765050915,1,28592765050919,"8536209090",24]
[105091,"Ex9ASD06 4P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=600A, 4-pole, Withdrawable ","NCC",3545.62,0,3545.62,8592765050922,1,8592765050922,1,28592765050926,"8536209090",52]
[105092,"Ex9ASD06 4P F","Air Circuit Switch Disconnectors, frame size A16, In=600A, 4-pole, Fixed ","NCC",2952.89,0,2952.89,8592765050939,1,8592765050939,1,28592765050933,"8536209090",24]
[105093,"Ex9ASD08 4P D/O","Air Circuit Switch Disconnectors, frame size A16, In=800A, 4-pole, Withdrawable ","NCC",3780.39,0,3780.39,8592765050946,1,8592765050946,1,28592765050940,"8536209090",52]
[105094,"Ex9ASD08 4P F","Air Circuit Switch Disconnectors, frame size A16, In=800A, 4-pole, Fixed ","NCC",3187.63,0,3187.63,8592765050953,1,8592765050953,1,28592765050957,"8536209090",24]
[105095,"Ex9ASD10 4P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=1000A, 4-pole, Withdrawable ","NCC",4225.16,0,4225.16,8592765050960,1,8592765050960,1,28592765050964,"8536209090",52]
[105096,"Ex9ASD10 4P F","Air Circuit Switch Disconnectors, frame size A16, In=1000A, 4-pole, Fixed ","NCC",3632.42,0,3632.42,8592765050977,1,8592765050977,1,28592765050971,"8536209090",24]
[105097,"Ex9ASD12 4P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=1200A, 4-pole, Withdrawable ","NCC",4830.57,0,4830.57,8592765050984,1,8592765050984,1,28592765050988,"8536209090",52]
[105098,"Ex9ASD12 4P F","Air Circuit Switch Disconnectors, frame size A16, In=1200A, 4-pole, Fixed ","NCC",4237.83,0,4237.83,8592765050991,1,8592765050991,1,28592765050995,"8536209090",24]
[105099,"Ex9ASD16 4P D/O ","Air Circuit Switch Disconnectors, frame size A16, In=1600A, 4-pole, Withdrawable ","NCC",7375.72,0,7375.72,8592765051004,1,8592765051004,1,28592765051008,"8536209090",52]
[105100,"Ex9ASD16 4P F","Air Circuit Switch Disconnectors, frame size A16, In=1600A, 4-pole, Fixed ","NCC",6782.97,0,6782.97,8592765051011,1,8592765051011,1,28592765051015,"8536209090",24]
[107112,"Ex9ASD16b 4P D/O ","Air Circuit Switch Disconnectors, frame size A32, In=1600A, 4-pole, Withdrawable ","NCC",9877.92,0,9877.92,8592765071132,1,8592765071132,1,28592765071136,"8536209090",138]
[107113,"Ex9ASD16b 4P F","Air Circuit Switch Disconnectors, frame size A32, In=1600A, 4-pole, Fixed ","NCC",8135.29,0,8135.29,8592765071149,1,8592765071149,1,28592765071143,"8536209090",84]
[105102,"Ex9ASD20 4P D/O ","Air Circuit Switch Disconnectors, frame size A32, In=2000A, 4-pole, Withdrawable ","NCC",12120.23,0,12120.23,8592765051035,1,8592765051035,1,28592765051039,"8536209090",138]
[105103,"Ex9ASD20 4P F","Air Circuit Switch Disconnectors, frame size A32, In=2000A, 4-pole, Fixed ","NCC",9470.01,0,9470.01,8592765051042,1,8592765051042,1,28592765051046,"8536209090",84]
[105104,"Ex9ASD25 4P D/O","Air Circuit Switch Disconnectors, frame size A32, In=2500A, 4-pole, Withdrawable ","NCC",16811.22,0,16811.22,8592765051059,1,8592765051059,1,28592765051053,"8536209090",138]
[105105,"Ex9ASD25 4P F","Air Circuit Switch Disconnectors, frame size A32, In=2500A, 4-pole, Fixed ","NCC",13642.07,0,13642.07,8592765051066,1,8592765051066,1,28592765051060,"8536209090",84]
[105106,"Ex9ASD29 4P D/O ","Air Circuit Switch Disconnectors, frame size A32, In=2900A, 4-pole, Withdrawable ","NCC",15998.75,0,15998.75,8592765051073,1,8592765051073,1,28592765051077,"8536209090",138]
[105107,"Ex9ASD29 4P F","Air Circuit Switch Disconnectors, frame size A32, In=2900A, 4-pole, Fixed ","NCC",13803.84,0,13803.84,8592765051080,1,8592765051080,1,28592765051084,"8536209090",84]
[105108,"Ex9ASD32 4P D/O","Air Circuit Switch Disconnectors, frame size A32, In=3200A, 4-pole, Withdrawable ","NCC",21470.77,0,21470.77,8592765051097,1,8592765051097,1,28592765051091,"8536209090",138]
[105109,"Ex9ASD32 4P F","Air Circuit Switch Disconnectors, frame size A32, In=3200A, 4-pole, Fixed ","NCC",17036.88,0,17036.88,8592765051103,1,8592765051103,1,28592765051107,"8536209090",84]
[105110,"Ex9ASD36 4P D/O ","Air Circuit Switch Disconnectors, frame size A40, In=3600A, 4-pole, Withdrawable ","NCC",29747.8,0,29747.8,8592765051110,1,8592765051110,1,28592765051114,"8536209090",138]
[105111,"Ex9ASD36 4P F","Air Circuit Switch Disconnectors, frame size A40, In=3600A, 4-pole, Fixed ","NCC",23006.01,0,23006.01,8592765051127,1,8592765051127,1,28592765051121,"8536209090",84]
[105112,"Ex9ASD40 4P D/O ","Air Circuit Switch Disconnectors, frame size A40, In=4000A, 4-pole, Withdrawable ","NCC",25422.18,0,25422.18,8592765051134,1,8592765051134,1,28592765051138,"8536209090",138]
[105113,"Ex9ASD40 4P F","Air Circuit Switch Disconnectors, frame size A40, In=4000A, 4-pole, Fixed ","NCC",24917.31,0,24917.31,8592765051141,1,8592765051141,1,28592765051145,"8536209090",84]
[]
["Accessories for Air Circuit Breakers Ex9A and Air Switch Disconnectors Ex9ASD"]
[105115,"+XF 11 AC220-240V","Closing release for Ex9A, 220-240 V AC, Premounted ","NCC",259.20999999999998,{"$f":"NCC","v":0},{"$f":"E3143*(1-F3143)","v":259.20999999999998},8592765051165,null,8592765051165,null,28592765051169,"8536209090"]
[105116,"+XF 11 AC380-415V","Closing release for Ex9A, 380-400 V AC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051172,null,8592765051172,null,28592765051176,"8536209090"]
[105117,"+XF 11 DC110V","Closing release for Ex9A, 110 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051189,null,8592765051189,null,28592765051183,"8536209090"]
[105118,"+XF 11 DC220V","Closing release for Ex9A, 220 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051196,null,8592765051196,null,28592765051190,"8536209090"]
[105799,"+XF 11 DC24V","Closing release for Ex9A, 24 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765058003,null,8592765058003,null,28592765058007]
[105800,"+XF 11 DC48V","Closing release for Ex9A, 48 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765058010,null,8592765058010,null,28592765058014]
[105231,"XF 11 AC220-240V","Closing release for Ex9A, 220-240 V AC, Separately orderable ","NCC",475.22,0,475.22,8592765052322,null,8592765052322,null,28592765052326,"8538909999"]
[105232,"XF 11 AC380-415V","Closing release for Ex9A, 380-400 V AC, Separately orderable ","NCC",475.22,0,475.22,8592765052339,null,8592765052339,null,28592765052333,"8538909999"]
[105233,"XF 11 DC110V","Closing release for Ex9A, 110 V DC, Separately orderable ","NCC",475.22,0,475.22,8592765052346,null,8592765052346,null,28592765052340,"8538909999"]
[105234,"XF 11 DC220V","Closing release for Ex9A, 220 V DC, Separately orderable ","NCC",475.22,0,475.22,8592765052353,null,8592765052353,null,28592765052357,"8538909999"]
[105801,"XF 11 DC24V","Closing release for Ex9A, 24 V DC, Separately orderable ","NCC",475.22,0,475.22,8592765058027,null,8592765058027,null,28592765058021]
[105802,"XF 11 DC48V","Closing release for Ex9A, 48 V DC, Separately orderable ","NCC",475.22,0,475.22,8592765058034,null,8592765058034,null,28592765058038]
[105119,"+SHT 11 AC220-240V","Shunt trip release for Ex9A, 220-240 V AC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051202,null,8592765051202,null,28592765051206,"8536209090"]
[105120,"+SHT 11 AC380-415V","Shunt trip release for Ex9A, 380-415 V AC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051219,null,8592765051219,null,28592765051213,"8536209090"]
[105121,"+SHT 11 DC110V","Shunt trip release for Ex9A, 110 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051226,null,8592765051226,null,28592765051220,"8536209090"]
[105122,"+SHT 11 DC220V","Shunt trip release for Ex9A, 220 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051233,null,8592765051233,null,28592765051237,"8536209090"]
[105123,"+SHT 11 AC220-240V D","Second shunt trip release for Ex9A, 220-240 V AC, Premounted ","NCC",259.45999999999998,0,259.45999999999998,8592765051240,null,8592765051240,null,28592765051244,"8536209090"]
[105124,"+SHT 11 AC380-415V D","Second shunt trip release for Ex9A, 380-415 V AC, Premounted ","NCC",259.45999999999998,0,259.45999999999998,8592765051257,null,8592765051257,null,28592765051251,"8536209090"]
[105125,"+SHT 11 DC110V D","Second shunt trip release for Ex9A, 110 V DC, Premounted ","NCC",259.45999999999998,0,259.45999999999998,8592765051264,null,8592765051264,null,28592765051268,"8536209090"]
[105126,"+SHT 11 DC220V D","Second shunt trip release for Ex9A, 220 V DC, Premounted ","NCC",259.45999999999998,0,259.45999999999998,8592765051271,null,8592765051271,null,28592765051275,"8536209090"]
[105803,"+SHT 11 DC24V","Shunt trip release for Ex9A, 24 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765058041,null,8592765058041,null,28592765058045,"8536209090"]
[105804,"+SHT 11 DC48V","Shunt trip release for Ex9A, 48 V DC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765058058,null,8592765058058,null,28592765058052]
[105807,"+SHT 11 DC24V D","Second shunt trip release for Ex9A, 24 V DC, Premounted ","NCC",259.45999999999998,0,259.45999999999998,8592765058089,null,8592765058089,null,28592765058083]
[105808,"+SHT 11 DC48V D","Second shunt trip release for Ex9A, 48 V DC, Premounted ","NCC",259.45999999999998,0,259.45999999999998,8592765058096,null,8592765058096,null,28592765058090]
[105235,"SHT 11 AC220-240V","Shunt trip release for Ex9A, 220-240 V AC, Separately orderable ","NCC",479.54,0,479.54,8592765052360,null,8592765052360,null,28592765052364,"8538909999"]
[105236,"SHT 11 AC380-415V","Shunt trip release for Ex9A, 380-415 V AC, Separately orderable ","NCC",479.54,0,479.54,8592765052377,null,8592765052377,null,28592765052371,"8538909999"]
[105237,"SHT 11 DC110V","Shunt trip release for Ex9A, 110 V DC, Separately orderable ","NCC",479.54,0,479.54,8592765052384,null,8592765052384,null,28592765052388,"8538909999"]
[105238,"SHT 11 DC220V","Shunt trip release for Ex9A, 220 V DC, Separately orderable ","NCC",479.54,0,479.54,8592765052391,null,8592765052391,null,28592765052395,"8538909999"]
[105805,"SHT 11 DC24V","Shunt trip release for Ex9A, 24 V DC, Separately orderable ","NCC",479.54,0,479.54,8592765058065,null,8592765058065,null,28592765058069,"8536419089"]
[105806,"SHT 11 DC48V","Shunt trip release for Ex9A, 48 V DC, Separately orderable ","NCC",479.54,0,479.54,8592765058072,null,8592765058072,null,28592765058076]
[105127,"+UVT 11 AC220-240V UD","Undervoltage release for frame size A16/32/40, undelayed, 220-240 V AC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051288,null,8592765051288,null,28592765051282,"8536209090"]
[105128,"+UVT 11 AC380-415V UD","Undervoltage release for frame size A16/32/40, undelayed, 380-415 V AC, Premounted ","NCC",259.20999999999998,0,259.20999999999998,8592765051295,null,8592765051295,null,28592765051299,"8536209090"]
[105129,"+UVT 11 AC220-240V D1","Undervoltage release for frame size A16/32/40, 1s delay, 220-240 V AC, Premounted ","NCC",735.65,0,735.65,8592765051301,null,8592765051301,null,28592765051305,"8536209090"]
[105130,"+UVT 11 AC380-415V D1","Undervoltage release for frame size A16/32/40, 1s delay, 380-415 V AC, Premounted ","NCC",735.65,0,735.65,8592765051318,null,8592765051318,null,28592765051312,"8536209090"]
[105131,"+UVT 11 AC220-240V D3","Undervoltage release for frame size A16/32/40, 3s delay, 220-240 V AC, Premounted ","NCC",735.65,0,735.65,8592765051325,null,8592765051325,null,28592765051329,"8536209090"]
[105132,"+UVT 11 AC380-415V D3","Undervoltage release for frame size A16/32/40, 3s delay, 380-415 V AC, Premounted ","NCC",735.65,0,735.65,8592765051332,null,8592765051332,null,28592765051336,"8536209090"]
[105133,"+UVT 11 AC220-240V D5","Undervoltage release for frame size A16/32/40, 5s delay, 220-240 V AC, Premounted ","NCC",735.65,0,735.65,8592765051349,null,8592765051349,null,28592765051343,"8536209090"]
[105134,"+UVT 11 AC380-415V D5","Undervoltage release for frame size A16/32/40, 5s delay, 380-415 V AC, Premounted ","NCC",735.65,0,735.65,8592765051356,null,8592765051356,null,28592765051350,"8536209090"]
[105239,"UVT AC220-240V UD","Undervoltage release for frame size A16/32/40, undelayed, 220-240 V AC, Separately orderable ","NCC",466.58,0,466.58,8592765052407,null,8592765052407,null,28592765052401,"8538909999"]
[105240,"UVT AC380-415V UD","Undervoltage release for frame size A16/32/40, undelayed, 380-415 V AC, Separately orderable ","NCC",466.58,0,466.58,8592765052414,null,8592765052414,null,28592765052418,"8538909999"]
[105241,"UVT AC220-240V D1","Undervoltage release for frame size A16/32/40, 1s delay, 220-240 V AC, Separately orderable ","NCC",1324.17,0,1324.17,8592765052421,null,8592765052421,null,28592765052425,"8538909999"]
[105242,"UVT AC380-415V D1","Undervoltage release for frame size A16/32/40, 1s delay, 380-415 V AC, Separately orderable ","NCC",1324.17,0,1324.17,8592765052438,null,8592765052438,null,28592765052432,"8538909999"]
[105243,"UVT AC220-240V D3","Undervoltage release for frame size A16/32/40, 3s delay, 220-240 V AC, Separately orderable ","NCC",1324.17,0,1324.17,8592765052445,null,8592765052445,null,28592765052449,"8538909999"]
[105244,"UVT AC380-415V D3","Undervoltage release for frame size A16/32/40, 3s delay, 380-415 V AC, Separately orderable ","NCC",1324.17,0,1324.17,8592765052452,null,8592765052452,null,28592765052456,"8538909999"]
[105245,"UVT AC220-240V D5","Undervoltage release for frame size A16/32/40, 5s delay, 220-240 V AC, Separately orderable ","NCC",1324.17,0,1324.17,8592765052469,null,8592765052469,null,28592765052463,"8538909999"]
[105246,"UVT AC380-415V D5","Undervoltage release for frame size A16/32/40, 5s delay, 380-415 V AC, Separately orderable ","NCC",1324.17,0,1324.17,8592765052476,null,8592765052476,null,28592765052470,"8538909999"]
[105135,"+VCP","Vertically mounted main terminals","NCC",1.19,0,1.19,8592765051363,null,8592765051363,null,28592765051367,"8536209090"]
[105139,"+CAS 11 3P 630","Cassete for frame size A16, In=630A, 3-pole, Premounted ","NCC",1283.6600000000001,0,1283.6600000000001,8592765051400,null,8592765051400,null,28592765051404,"8536209090"]
[105140,"+CAS 11 3P 1600","Cassete for frame size A16, In=1600A, 3-pole, Premounted ","NCC",1283.6600000000001,0,1283.6600000000001,8592765051417,null,8592765051417,null,28592765051411,"8536209090"]
[105141,"+CAS 11 4P 630","Cassete for frame size A16, In=630A, 4-pole, Premounted ","NCC",1629.27,0,1629.27,8592765051424,null,8592765051424,null,28592765051428,"8536209090"]
[105142,"+CAS 11 4P 1600","Cassete for frame size A16, In=1600A, 4-pole, Premounted ","NCC",1629.27,0,1629.27,8592765051431,null,8592765051431,null,28592765051435,"8536209090"]
[105157,"CAS 11 3P 630","Cassete for frame size A16, In=630A, 3-pole, Separately orderable ","NCC",2068.11,0,2068.11,8592765051585,null,8592765051585,null,28592765051589,"8536209090"]
[105158,"CAS 11 3P 1600","Cassete for frame size A16, In=1600A, 3-pole, Separately orderable ","NCC",2026.82,0,2026.82,8592765051592,null,8592765051592,null,28592765051596,"8536209090"]
[105159,"CAS 11 4P 630","Cassete for frame size A16, In=630A, 4-pole, Separately orderable ","NCC",2631.9,0,2631.9,8592765051608,null,8592765051608,null,28592765051602,"8536209090"]
[105160,"CAS 11 4P 1600","Cassete for frame size A16, In=1600A, 4-pole, Separately orderable ","NCC",2560.2800000000002,0,2560.2800000000002,8592765051615,null,8592765051615,null,28592765051619,"8536209090"]
[105136,"+MD 11 AC230/DC220","Motor operator for frame size A16, 230 V AC/ 220V DC, Premounted ","NCC",970.99,0,970.99,8592765051370,null,8592765051370,null,28592765051374,"8536209090"]
[105137,"+MD 11 AC380-415V","Motor operator for frame size A16, 380-415 V AC, Premounted ","NCC",970.99,0,970.99,8592765051387,null,8592765051387,null,28592765051381,"8536209090"]
[105138,"+MD 11 DC110V","Motor operator for frame size A16, 110 V DC, Premounted ","NCC",970.99,0,970.99,8592765051394,null,8592765051394,null,28592765051398,"8536209090"]
[105817,"+MD 11 DC24V","Motor operator for frame size A16, 24 V DC, Premounted ","NCC",970.99,0,970.99,8592765058188,null,8592765058188,null,28592765058182]
[105818,"+MD 11 DC48V","Motor operator for frame size A16, 48 V DC, Premounted ","NCC",970.99,0,970.99,8592765058195,null,8592765058195,null,28592765058199]
[105161,"MD 11 AC230/DC220","Motor operator for frame size A16, 230 V AC/ 220V DC, Separately orderable ","NCC",1463.14,0,1463.14,8592765051622,null,8592765051622,null,28592765051626,"8536209090"]
[105162,"MD 11 AC380-415V","Motor operator for frame size A16, 380-415 V AC, Separately orderable ","NCC",1463.14,0,1463.14,8592765051639,null,8592765051639,null,28592765051633,"8536209090"]
[105225,"MD 11 DC110V","Motor operator for frame size A16, 110 V DC, Separately orderable ","NCC",1463.14,0,1463.14,8592765052261,null,8592765052261,null,28592765052265,"8538909999"]
[105826,"MD 11 DC24V","Motor operator for frame size A16, 24 V DC, Separately orderable ","NCC",1463.14,0,1463.14,8592765058270,null,8592765058270,null,28592765058274]
[105827,"MD 11 DC48V","Motor operator for frame size A16, 48 V DC, Separately orderable ","NCC",1463.14,{"$f":"NCC","v":0},{"$f":"E3207*(1-F3207)","v":1463.14},8592765058287,null,8592765058287,null,28592765058281]
[105143,"+VBP 11","Pushbuttons lock device for frame size A16, Premounted ","NCC",92.08,0,92.08,8592765051448,null,8592765051448,null,28592765051442,"8536209090"]
[105145,"+AX 11 44","Auxiliary contacts for frame size A16, Premounted ","NCC",141.63,0,141.63,8592765051462,null,8592765051462,null,28592765051466,"8536209090"]
[105146,"+AX 11 66","Auxiliary contacts for frame size A16, Premounted ","NCC",188.84,0,188.84,8592765051479,null,8592765051479,null,28592765051473,"8536209090"]
[105154,"AX 11 44","Auxiliary contacts for frame size A16, Separately orderable  ","NCC",221.3,0,221.3,8592765051554,null,8592765051554,null,28592765051558,"8536209090"]
[105155,"AX 11 66","Auxiliary contacts for frame size A16, Separately orderable  ","NCC",236.03,0,236.03,8592765051561,null,8592765051561,null,28592765051565,"8536209090"]
[105147,"+KLK 11 1L1K","OFF position keylock for frame size A16, 1 lock, 1 key","NCC",318.61,0,318.61,8592765051486,null,8592765051486,null,28592765051480,"8536209090"]
[105148,"+KLK 11 2L1K","OFF position keylock for frame size A16, 2 locks, 1 key","NCC",318.61,0,318.61,8592765051493,null,8592765051493,null,28592765051497,"8536209090"]
[105149,"+KLK 11 3L2K","OFF position keylock for frame size A16, 3 locks, 2 keys","NCC",318.61,0,318.61,8592765051509,null,8592765051509,null,28592765051503,"8536209090"]
[105267,"VPEC 11","Door interlock for withdrawable version, for frame size A16","NCC",245.76,0,245.76,8592765052681,null,8592765052681,null,28592765052685,"8538909999"]
[105251,"RCP 11 3P 400-630A","Rear connection plates, for frame size A16, In=400-630A, 3-pole, Separately orderable ","NCC",368.64,0,368.64,8592765052520,null,8592765052520,null,28592765052524,"8538909999"]
[105252,"RCP 11 3P 800-1600A","Rear connection plates, for frame size A16, In=800-1600A, 3-pole, Separately orderable ","NCC",378.89,0,378.89,8592765052537,null,8592765052537,null,28592765052531,"8538909999"]
[105253,"RCP 11 4P 400-630A","Rear connection plates, for frame size A16, In=400-630A, 4-pole, Separately orderable ","NCC",491.52,0,491.52,8592765052544,null,8592765052544,null,28592765052548,"8538909999"]
[105254,"RCP 11 4P 800-1600A","Rear connection plates, for frame size A16, In=800-1600A, 4-pole, Separately orderable ","NCC",501.76,0,501.76,8592765052551,null,8592765052551,null,28592765052555,"8538909999"]
[105150,"+TEX 11 3P 400-630A","Connection terminals with spreaders, for frame size A16, In=400-630A, 3-pole, Premounted ","NCC",368.64,0,368.64,8592765051516,null,8592765051516,null,28592765051510,"8536209090"]
[105151,"+TEX 11 3P 800-1600A","Connection terminals with spreaders, for frame size A16, In=800-1600A, 3-pole, Premounted ","NCC",378.89,0,378.89,8592765051523,null,8592765051523,null,28592765051527,"8536209090"]
[105152,"+TEX 11 4P 400-630A","Connection terminals with spreaders, for frame size A16, In=400-630A, 4-pole, Premounted ","NCC",491.52,0,491.52,8592765051530,null,8592765051530,null,28592765051534,"8536209090"]
[105153,"+TEX 11 4P 800-1600A","Connection terminals with spreaders, for frame size A16, In=800-1600A, 4-pole, Premounted ","NCC",501.76,0,501.76,8592765051547,null,8592765051547,null,28592765051541,"8536209090"]
[105255,"TEX 11 3P 400-630A","Connection terminals with spreaders, for frame size A16, In=400-630A, 3-pole, Separately orderable  ","NCC",516.09,0,516.09,8592765052568,null,8592765052568,null,28592765052562,"8538909999"]
[105256,"TEX 11 3P 800-1600A","Connection terminals with spreaders, for frame size A16, In=800-1600A, 3-pole, Separately orderable  ","NCC",530.44000000000005,0,530.44000000000005,8592765052575,null,8592765052575,null,28592765052579,"8538909999"]
[105257,"TEX 11 4P 400-630A","Connection terminals with spreaders, for frame size A16, In=400-630A, 4-pole, Separately orderable  ","NCC",688.12,0,688.12,8592765052582,null,8592765052582,null,28592765052586,"8538909999"]
[105258,"TEX 11 4P 800-1600A","Connection terminals with spreaders, for frame size A16, In=800-1600A, 4-pole, Separately orderable  ","NCC",702.47,0,702.47,8592765052599,null,8592765052599,null,28592765052593,"8538909999"]
[105156,"+EF 11","Position indicator for frame size A16, Premonted ","NCC",144.54,0,144.54,8592765051578,null,8592765051578,null,28592765051572,"8536209090"]
[105163,"+CDM 11","Operation counter for frame size A16, Premounted ","NCC",341.34,0,341.34,8592765051646,null,8592765051646,null,28592765051640,"8536209090"]
[105268,"IN 11 400A","Rating plug for frame size A16, In=400A, Separately orderable ","NCC",153.13999999999999,0,153.13999999999999,8592765052698,null,8592765052698,null,28592765052692,"8538909999"]
[105269,"IN 11 630A","Rating plug for frame size A16/25, In=630A, Separately orderable ","NCC",153.13999999999999,0,153.13999999999999,8592765052704,null,8592765052704,null,28592765052708,"8538909999"]
[105270,"IN 11 800A","Rating plug for frame size A16/25, In=800A, Separately orderable ","NCC",153.13999999999999,0,153.13999999999999,8592765052711,null,8592765052711,null,28592765052715,"8538909999"]
[105271,"IN 11 1000A","Rating plug for frame size A16/25, In=1000A, Separately orderable ","NCC",172.3,0,172.3,8592765052728,null,8592765052728,null,28592765052722,"8538909999"]
[105272,"IN 11 1250A","Rating plug for frame size A16/25, In=1250A, Separately orderable ","NCC",172.3,0,172.3,8592765052735,null,8592765052735,null,28592765052739,"8538909999"]
[105247,"DDP 11","Doorframe for withdrawable version,for frame size A16,  Separately orderable ","NCC",134.63,0,134.63,8592765052483,null,8592765052483,null,28592765052487,"8538909999"]
[105248,"CDP 11 ","Doorframe for fixed version, for frame size A16, Separately orderable ","NCC",134.63,0,134.63,8592765052490,null,8592765052490,null,28592765052494,"8538909999"]
[105249,"DPS 11 3P","Phase barriers for withdrawable version, for frame size A16, 3-pole, Separately orderable ","NCC",122.88,0,122.88,8592765052506,null,8592765052506,null,28592765052500,"8538909999"]
[105250,"DPS 11 4P","Phase barriers for withdrawable version, for frame size A16, 4-pole, Separately orderable ","NCC",122.88,0,122.88,8592765052513,null,8592765052513,null,28592765052517,"8538909999"]
[105259,"PHS 11 3P","Phase barriers for fixed version, for frame size A16, 3-pole, Separately orderable ","NCC",122.88,0,122.88,8592765052605,null,8592765052605,null,28592765052609,"4008219000"]
[105260,"PHS 11 4P","Phase barriers for fixed version, for frame size A16, 4-pole, Separately orderable ","NCC",122.88,0,122.88,8592765052612,null,8592765052612,null,28592765052616,"4008219000"]
[105857,"NEC 11 800A","Current sensor for neutral conductor, for frame size A16, In=800A ","NCC",539.94000000000005,0,539.94000000000005,8592765058584,null,8592765058584,null,28592765058588,"8536209090"]
[105266,"NEC 11 1600A","Current sensor for neutral conductor, for frame size A16, In=1600A ","NCC",568.36,0,568.36,8592765052674,null,8592765052674,null,28592765052678,"8538909999"]
[105261,"IPA 11F 2-2","Mechanical interlock for frame size A16, for fixed version, for 2 devices","NCC",1481.61,0,1481.61,8592765052629,null,8592765052629,null,28592765052623,"8538909999"]
[105262,"IPA 11D/O 2-2","Mechanical interlock for frame size A16, for withdrawable version, for 2 devices","NCC",1481.61,0,1481.61,8592765052636,null,8592765052636,null,28592765052630,"8538909999"]
[105170,"+CAS 12 3P 2500","Cassete for frame size A32, In=2500A, 3-pole, Premounted ","NCC",2630.89,0,2630.89,8592765051714,null,8592765051714,null,28592765051718,"8536209090"]
[105171,"+CAS 12 3P 3200","Cassete for frame size A32, In=3200A, 3-pole, Premounted ","NCC",3584.31,0,3584.31,8592765051721,null,8592765051721,null,28592765051725,"8536209090"]
[105172,"+CAS 12 4P 2500","Cassete for frame size A32, In=2500A, 4-pole, Premounted ","NCC",3508.28,0,3508.28,8592765051738,null,8592765051738,null,28592765051732,"8536209090"]
[105173,"+CAS 12 4P 3200","Cassete for frame size A32, In=3200A, 4-pole, Premounted ","NCC",4779.09,0,4779.09,8592765051745,null,8592765051745,null,28592765051749,"8536209090"]
[105181,"CAS 12 3P 2500","Cassete for frame size A32, In=2500A, 3-pole, Separately orderable ","NCC",4209.41,0,4209.41,8592765051820,null,8592765051820,null,28592765051824,"8536209090"]
[105182,"CAS 12 3P 3200","Cassete for frame size A32, In=3200A, 3-pole, Separately orderable ","NCC",5692.73,0,5692.73,8592765051837,null,8592765051837,null,28592765051831,"8536209090"]
[105193,"CAS 12 4P 2500","Cassete for frame size A32, In=2500A, 4-pole, Separately orderable ","NCC",5680.07,0,5680.07,8592765051943,null,8592765051943,null,28592765051947,"8538909999"]
[105194,"CAS 12 4P 3200","Cassete for frame size A32, In=3200A, 4-pole, Separately orderable ","NCC",7566.87,0,7566.87,8592765051950,null,8592765051950,null,28592765051954,"8538909999"]
[105174,"+MD 12 AC230/DC220V","Motor operator for frame size A32/40, 230 V AC/ 220V DC, Premounted ","NCC",1136.8499999999999,0,1136.8499999999999,8592765051752,null,8592765051752,null,28592765051756,"8536209090"]
[105175,"+MD 12 AC380-415V","Motor operator for frame size A32/40, 380-415 V AC, Premounted ","NCC",1136.8499999999999,0,1136.8499999999999,8592765051769,null,8592765051769,null,28592765051763,"8536209090"]
[105176,"+MD 12 DC110V","Motor operator for frame size A32/40, 110 V DC, Premounted ","NCC",1136.8499999999999,0,1136.8499999999999,8592765051776,null,8592765051776,null,28592765051770,"8536209090"]
[105824,"+MD 12 DC24V","Motor operator for frame size A32/40, 24 V DC, Premounted ","NCC",1136.8499999999999,0,1136.8499999999999,8592765058256,null,8592765058256,null,28592765058250]
[105825,"+MD 12 DC48V","Motor operator for frame size A32/40, 48 V DC, Premounted ","NCC",1136.8499999999999,0,1136.8499999999999,8592765058263,null,8592765058263,null,28592765058267]
[105195,"MD 12 AC230/DC220V","Motor operator for frame size A32/40, 230 V AC/ 220V DC, Separately orderable ","NCC",1689.92,0,1689.92,8592765051967,null,8592765051967,null,28592765051961,"8538909999"]
[105196,"MD 12 AC380-415V","Motor operator for frame size A32/40, 380-415 V AC, Separately orderable ","NCC",1689.92,0,1689.92,8592765051974,null,8592765051974,null,28592765051978,"8538909999"]
[105833,"MD 12 DC24V","Motor operator for frame size A32/40, 24 V DC, Separately orderable ","NCC",1689.92,0,1689.92,8592765058348,null,8592765058348,null,28592765058342]
[105834,"MD 12 DC48V","Motor operator for frame size A32/40, 48 V DC, Separately orderable ","NCC",1689.92,0,1689.92,8592765058355,null,8592765058355,null,28592765058359]
[105197,"MD 12 DC110V","Motor operator for frame size A32/40, 110 V DC, Separately orderable ","NCC",1689.92,0,1689.92,8592765051981,null,8592765051981,null,28592765051985,"8538909999"]
[105178,"+AX 12 22","Auxiliary contacts for frame size A25/32/40, Premounted ","NCC",113.54,0,113.54,8592765051790,null,8592765051790,null,28592765051794,"8536209090"]
[105179,"+AX 12 44","Auxiliary contacts for frame size A25/32/40, Premounted ","NCC",259.45999999999998,0,259.45999999999998,8592765051806,null,8592765051806,null,28592765051800,"8536209090"]
[105180,"+AX 12 66","Auxiliary contacts for frame size A25/32/40, Premounted ","NCC",599.78,0,599.78,8592765051813,null,8592765051813,null,28592765051817,"8536209090"]
[105206,"AX 12 22","Auxiliary contacts for frame size A25/32/40, Separately orderable  ","NCC",166.54,0,166.54,8592765052070,null,8592765052070,null,28592765052074,"8538909999"]
[105207,"AX 12 44","Auxiliary contacts for frame size A25/32/40, Separately orderable  ","NCC",432.44,0,432.44,8592765052087,null,8592765052087,null,28592765052081,"8538909999"]
[105208,"AX 12 66","Auxiliary contacts for frame size A25/32/40, Separately orderable  ","NCC",1119.58,0,1119.58,8592765052094,null,8592765052094,null,28592765052098,"8538909999"]
[105280,"RCP 12 3P 1600-2500A","Rear connection plates, for frame size A32/40, In=1600-2500A, 3-pole, Separately orderable ","NCC",497.2,0,497.2,8592765052810,null,8592765052810,null,28592765052814,"8538909999"]
[105281,"RCP 12 3P 2900-3200A","Rear connection plates, for frame size A32/40, In=2900-3200A, 3-pole, Horizontally mounted, Separately orderable ","NCC",497.2,{"$f":"NCC","v":0},{"$f":"E3271*(1-F3271)","v":497.2},8592765052827,null,8592765052827,null,28592765052821,"8538909999"]
[106772,"RCPV 12 3P 2900-3200A","Rear connection plates, for frame size A32/40, In=2900-3200A, 3-pole, Vertically mounted, Separately orderable ","NCC",497.2,0,497.2,8592765067739,null,8592765067739,null,28592765067733,"8536209090"]
[105282,"RCP 12 4P 1600-2500A","Rear connection plates, for frame size A32/40, In=1600-2500A, 4-pole, Separately orderable ","NCC",617.91,0,617.91,8592765052834,null,8592765052834,null,28592765052838,"8538909999"]
[105283,"RCP 12 4P 2900-3200A","Rear connection plates, for frame size A32/40, In=2900-3200A, 4-pole, Horizontally mounted, Separately orderable ","NCC",617.91,0,617.91,8592765052841,null,8592765052841,null,28592765052845,"8538909999"]
[106773,"RCPV 12 4P 2900-3200A","Rear connection plates, for frame size A32/40, In=2900-3200A, 4-pole, Vertically mounted, Separately orderable ","NCC",617.91,0,617.91,8592765067746,null,8592765067746,null,28592765067740,"8536209090"]
[105189,"+KLK 12 1L1K","OFF position keylock for frame size A25/32/40, 1 lock, 1 key","NCC",318.61,0,318.61,8592765051905,null,8592765051905,null,28592765051909,"8536209090"]
[105190,"+KLK 12 2L1K","OFF position keylock for frame size A25/32/40, 2 locks, 1 key","NCC",318.61,0,318.61,8592765051912,null,8592765051912,null,28592765051916,"8536209090"]
[105191,"+KLK 12 3L2K","OFF position keylock for frame size A25/32/40, 3 locks, 2 keys","NCC",318.61,0,318.61,8592765051929,null,8592765051929,null,28592765051923,"8536209090"]
[105177,"+VBP 12","Pushbuttons lock device for frame size A25/32/40, Premounted ","NCC",92.08,0,92.08,8592765051783,null,8592765051783,null,28592765051787,"8536209090"]
[105295,"VPEC 12","Door interlock for withdrawable, for frame size A32/40","NCC",245.76,0,245.76,8592765052964,null,8592765052964,null,28592765052968,"8538909999"]
[105192,"+EF 12","Position indicator for frame size A25/32/40, Premonted ","NCC",218.43,0,218.43,8592765051936,null,8592765051936,null,28592765051930,"8536209090"]
[105198,"+CDM 12","Operation counter for frame size A25/32/40, Premounted ","NCC",341.34,0,341.34,8592765051998,null,8592765051998,null,28592765051992,"8536209090"]
[105296,"IN 12 1600A","Rating plug for frame size A25/32/40, In=1600A, Separately orderable ","NCC",153.13999999999999,0,153.13999999999999,8592765052971,null,8592765052971,null,28592765052975,"8538909999"]
[105297,"IN 12 2000A","Rating plug for frame size A25/32/40, In=2000A, Separately orderable ","NCC",153.13999999999999,0,153.13999999999999,8592765052988,null,8592765052988,null,28592765052982,"8538909999"]
[105298,"IN 12 2500A","Rating plug for frame size A32/40, In=2500A, Separately orderable ","NCC",172.3,0,172.3,8592765052995,null,8592765052995,null,28592765052999,"8538909999"]
[105299,"IN 12 2900A","Rating plug for frame size A32/40, In=2900A, Separately orderable ","NCC",172.3,0,172.3,8592765053008,null,8592765053008,null,28592765053002,"8538909999"]
[105300,"IN 12 3200A","Rating plug for frame size A32/40, In=3200A, Separately orderable ","NCC",191.45,0,191.45,8592765053015,null,8592765053015,null,28592765053019,"8538909999"]
[105274,"DDP 12 ","Doorframe for withdrawable version,for frame size A32/40,  Separately orderable ","NCC",150.87,0,150.87,8592765052759,null,8592765052759,null,28592765052753,"8538909999"]
[105275,"CDP 12 ","Doorframe for fixed version, for frame size A32/40, Separately orderable ","NCC",150.87,0,150.87,8592765052766,null,8592765052766,null,28592765052760,"8538909999"]
[105276,"DPS 12 3P","Phase barriers for withdrawable version, for frame size A25/32, 3-pole, Separately orderable ","NCC",81.92,0,81.92,8592765052773,null,8592765052773,null,28592765052777,"8538909999"]
[105277,"DPS 12 4P","Phase barriers for withdrawable version, for frame size A25/32, 4-pole, Separately orderable ","NCC",122.88,0,122.88,8592765052780,null,8592765052780,null,28592765052784,"8538909999"]
[105278,"PHS 12 3P","Phase barriers for fixed version, for frame size A25/32, 3-pole, Separately orderable ","NCC",81.92,0,81.92,8592765052797,null,8592765052797,null,28592765052791,"4008219000"]
[105279,"PHS 12 4P","Phase barriers for fixed version, for frame size A25/32, 4-pole, Separately orderable ","NCC",122.88,0,122.88,8592765052803,null,8592765052803,null,28592765052807,"4008219000"]
[105204,"+CAS 13 3P 4000","Cassete for frame size A40, In=4000A, 3-pole, Premounted ","NCC",4211.8500000000004,0,4211.8500000000004,8592765052056,null,8592765052056,null,28592765052050,"8536209090"]
[105205,"+CAS 13 4P 4000","Cassete for frame size A40, In=4000A, 4-pole, Premounted ","NCC",5616.59,0,5616.59,8592765052063,null,8592765052063,null,28592765052067,"8536209090"]
[107008,"CAS 13 3P 4000","Cassete for frame size A40, In=4000A, 3-pole, Separately orderable ","NCC",6819.19,0,6819.19,8592765070098,null,8592765070098,null,28592765070092,"8538909999"]
[107009,"CAS 13 4P 4000","Cassete for frame size A40, In=4000A, 4-pole, Separately orderable ","NCC",8909.07,0,8909.07,8592765070104,null,8592765070104,null,28592765070108,"8538909999"]
[105307,"RCP 13 4P 3200-4000A","Rear connection plates, for frame size A40, In=3200-4000A, 4-pole, Horizontally mounted, Separately orderable ","NCC",614.4,0,614.4,8592765053084,null,8592765053084,null,28592765053088,"8538909999"]
[106774,"RCPV 13 4P 3200-4000A","Rear connection plates, for frame size A40, In=3200-4000A, 4-pole, Vertically mounted, Separately orderable ","NCC",614.4,0,614.4,8592765067753,null,8592765067753,null,28592765067757,"8536209090"]
[105308,"RCP 13 3P 3200-4000A","Rear connection plates, for frame size A40, In=3200-4000A, 3-pole, Horizontally mounted, Separately orderable ","NCC",460.8,0,460.8,8592765053091,null,8592765053091,null,28592765053095,"8538909999"]
[106775,"RCPV 13 3P 3200-4000A","Rear connection plates, for frame size A40, In=3200-4000A, 3-pole, Vertically mounted, Separately orderable ","NCC",460.8,0,460.8,8592765067760,null,8592765067760,null,28592765067764,"8536209090"]
[105302,"DPS 13 3P","Phase barriers for withdrawable version, for frame size A40, 3-pole, Separately orderable ","NCC",51.2,0,51.2,8592765053039,null,8592765053039,null,28592765053033,"8538909999"]
[105303,"DPS 13 4P","Phase barriers for withdrawable version, for frame size A40, 4-pole, Separately orderable ","NCC",61.44,0,61.44,8592765053046,null,8592765053046,null,28592765053040,"8538909999"]
[105304,"PHS 13 3P","Phase barriers for fixed version, for frame size A40, 3-pole, Separately orderable ","NCC",48.5,0,48.5,8592765053053,null,8592765053053,null,28592765053057,"4008219000"]
[105305,"PHS 13 4P","Phase barriers for fixed version, for frame size A40, 4-pole, Separately orderable ","NCC",61.44,0,61.44,8592765053060,null,8592765053060,null,28592765053064,"4008219000"]
[105306,"NEC 13 4000A","Current sensor for neutral conductor, for frame size A32/40, In=4000A","NCC",722.87,0,722.87,8592765053077,null,8592765053077,null,28592765053071,"8538909999"]
[105292,"IPA 12F 2-2","Mechanical interlock for frame size A32/40 fixed, for 2 devices","NCC",1481.61,0,1481.61,8592765052933,null,8592765052933,null,28592765052937,"8538909999"]
[105293,"IPA 12D/O 2-2","Mechanical interlock for frame size A32/40 withdrawable, for 2 devices","NCC",1481.61,0,1481.61,8592765052940,null,8592765052940,null,28592765052944,"8538909999"]
[105061,"+COM MODBUS","ModBus communicatoin function for tripping units ","NCC",889.76,0,889.76,8592765050625,null,8592765050625,null,28592765050629,"8536209090"]
[105062,"LEC 11","Earth-leakage current transformer","NCC",722.87,0,722.87,8592765050632,null,8592765050632,null,28592765050636,"8536209090"]
[107109,"+ZSI","ZSI function for tripping units ","NCC",349.96,0,349.96,8592765071101,null,8592765071101,null,28592765071105,"8536209090"]
[105731,"+DO2","Programmable digital outputs DO for SU type SUx0.x with +ZSI","NCC",163.66,0,163.66,8592765057327,null,8592765057327,null,28592765057321]
[105732,"+DO4","Programmable digital outputs DO for SU type SUx0.x without +ZSI","NCC",272.95999999999998,0,272.95999999999998,8592765057334,null,8592765057334,null,28592765057338]
[105734,"+VM3P4W","Tripping unit configuration for measuring by 3P ACB in 4wire system","NCC",6,0,6,8592765057358,null,8592765057358,null,28592765057352]
[]
["Panel mounted control devices Ex9P1"]
[105578,"Ex9P1 1NO","Single contact unit for Ex9P1, 1NO contact","NBF",2.59,{"$f":"NBF","v":0},{"$f":"E3317*(1-F3317)","v":2.59},8592765055798,90,18592765055795,1620,28592765055792,"8536508090",8.0000000000000002E-3]
[105579,"Ex9P1 1NC","Single contact unit for Ex9P1, 1NC contact","NBF",2.59,{"$f":"NBF","v":0},2.59,8592765055804,90,18592765055801,1620,28592765055808,"8536508090",8.0000000000000002E-3]
[105580,"Ex9P1 MC","Part for middle contact unit control, suitable for illuminated type Ex9P1 F/R/M heads","NBF",0.45,0,0.45,8592765055811,150,18592765055818,2700,28592765055815,"8536508090",2E-3]
[105581,"Ex9P1 LEDw 6V AC/DC","LED unit for Ex9P1, white, 6V AC/DC","NBF",5.24,0,5.24,8592765055828,60,18592765055825,1080,28592765055822,"8531807000",1.0999999999999999E-2]
[105582,"Ex9P1 LEDw 12V AC/DC","LED unit for Ex9P1, white, 12V AC/DC","NBF",5.24,0,5.24,8592765055835,60,18592765055832,1080,28592765055839,"8531807000",1.0999999999999999E-2]
[105583,"Ex9P1 LEDw 24V AC/DC","LED unit for Ex9P1, white, 24V AC/DC","NBF",5.24,0,5.24,8592765055842,60,18592765055849,1080,28592765055846,"8531807000",1.0999999999999999E-2]
[105584,"Ex9P1 LEDw 36V AC/DC","LED unit for Ex9P1, white, 36V AC/DC","NBF",5.24,0,5.24,8592765055859,60,18592765055856,1080,28592765055853,"8531807000",1.0999999999999999E-2]
[105585,"Ex9P1 LEDw 110V-230V AC","LED unit for Ex9P1, white, 110V-230V AC","NBF",7.79,0,7.79,8592765055866,60,18592765055863,1080,28592765055860,"8531807000",1.0999999999999999E-2]
[105587,"Ex9P1 LEDr 6V AC/DC","LED unit for Ex9P1, red, 6V AC/DC","NBF",5.24,0,5.24,8592765055880,60,18592765055887,1080,28592765055884,"8531807000",1.0999999999999999E-2]
[105588,"Ex9P1 LEDr 12V AC/DC","LED unit for Ex9P1, red, 12V AC/DC","NBF",5.24,0,5.24,8592765055897,60,18592765055894,1080,28592765055891,"8531807000",1.0999999999999999E-2]
[105589,"Ex9P1 LEDr 24V AC/DC","LED unit for Ex9P1, red, 24V AC/DC","NBF",5.24,0,5.24,8592765055903,60,18592765055900,1080,28592765055907,"8531807000",1.0999999999999999E-2]
[105590,"Ex9P1 LEDr 36V AC/DC","LED unit for Ex9P1, red, 36V AC/DC","NBF",5.24,0,5.24,8592765055910,60,18592765055917,1080,28592765055914,"8531807000",1.0999999999999999E-2]
[105591,"Ex9P1 LEDr 110V-230V AC","LED unit for Ex9P1, red, 110V-230V AC","NBF",7.79,0,7.79,8592765055927,60,18592765055924,1080,28592765055921,"8531807000",1.0999999999999999E-2]
[105593,"Ex9P1 LEDg 6V AC/DC","LED unit for Ex9P1, green, 6V AC/DC","NBF",5.24,0,5.24,8592765055941,60,18592765055948,1080,28592765055945,"8531807000",1.0999999999999999E-2]
[105594,"Ex9P1 LEDg 12V AC/DC","LED unit for Ex9P1, green, 12V AC/DC","NBF",5.24,0,5.24,8592765055958,60,18592765055955,1080,28592765055952,"8531807000",1.0999999999999999E-2]
[105595,"Ex9P1 LEDg 24V AC/DC","LED unit for Ex9P1, green, 24V AC/DC","NBF",5.24,0,5.24,8592765055965,60,18592765055962,1080,28592765055969,"8531807000",1.0999999999999999E-2]
[105596,"Ex9P1 LEDg 36V AC/DC","LED unit for Ex9P1, green, 36V AC/DC","NBF",5.24,0,5.24,8592765055972,60,18592765055979,1080,28592765055976,"8531807000",1.0999999999999999E-2]
[105597,"Ex9P1 LEDg 110V-230V AC","LED unit for Ex9P1, green, 110V-230V AC","NBF",7.79,0,7.79,8592765055989,60,18592765055986,1080,28592765055983,"8531807000",1.0999999999999999E-2]
[105599,"Ex9P1 LEDy 6V AC/DC","LED unit for Ex9P1, yellow, 6V AC/DC","NBF",5.24,0,5.24,8592765056009,60,18592765056006,1080,28592765056003,"8531807000",1.0999999999999999E-2]
[105600,"Ex9P1 LEDy 12V AC/DC","LED unit for Ex9P1, yellow, 12V AC/DC","NBF",5.24,0,5.24,8592765056016,60,18592765056013,1080,28592765056010,"8531807000",1.0999999999999999E-2]
[105601,"Ex9P1 LEDy 24V AC/DC","LED unit for Ex9P1, yellow, 24V AC/DC","NBF",5.24,0,5.24,8592765056023,60,18592765056020,1080,28592765056027,"8531807000",1.0999999999999999E-2]
[105602,"Ex9P1 LEDy 36V AC/DC","LED unit for Ex9P1, yellow, 36V AC/DC","NBF",5.24,0,5.24,8592765056030,60,18592765056037,1080,28592765056034,"8531807000",1.0999999999999999E-2]
[105603,"Ex9P1 LEDy 110V-230V AC","LED unit for Ex9P1, yellow, 110V-230V AC","NBF",7.79,0,7.79,8592765056047,60,18592765056044,1080,28592765056041,"8531807000",1.0999999999999999E-2]
[105605,"Ex9P1 LEDb 6V AC/DC","LED unit for Ex9P1, blue, 6V AC/DC","NBF",5.24,0,5.24,8592765056061,60,18592765056068,1080,28592765056065,"8531807000",1.0999999999999999E-2]
[105606,"Ex9P1 LEDb 12V AC/DC","LED unit for Ex9P1, blue, 12V AC/DC","NBF",5.24,0,5.24,8592765056078,60,18592765056075,1080,28592765056072,"8531807000",1.0999999999999999E-2]
[105607,"Ex9P1 LEDb 24V AC/DC","LED unit for Ex9P1, blue, 24V AC/DC","NBF",5.24,0,5.24,8592765056085,60,18592765056082,1080,28592765056089,"8531807000",1.0999999999999999E-2]
[105608,"Ex9P1 LEDb 36V AC/DC","LED unit for Ex9P1, blue, 36V AC/DC","NBF",5.24,0,5.24,8592765056092,60,18592765056099,1080,28592765056096,"8531807000",1.0999999999999999E-2]
[105609,"Ex9P1 LEDb 110V-230V AC","LED unit for Ex9P1, blue, 110V-230V AC","NBF",7.79,0,7.79,8592765056108,60,18592765056105,1080,28592765056102,"8531807000",1.0999999999999999E-2]
[105611,"Ex9P1 B3","Basement for head and 3 functional units of Ex9P1, flush mounting","NBF",1.24,0,1.24,8592765056122,60,18592765056129,1080,28592765056126,"8536508090",7.0000000000000001E-3]
[105612,"Ex9P1 F w","Flat button head, momentary, without printing, white","NBF",3.75,0,3.75,8592765056139,20,18592765056136,360,28592765056133,"8536508090",1.4E-2]
[105613,"Ex9P1 F k","Flat button head, momentary, without printing, black","NBF",3.75,0,3.75,8592765056146,20,18592765056143,360,28592765056140,"8536508090",1.4E-2]
[105614,"Ex9P1 F g","Flat button head, momentary, without printing, green","NBF",3.75,0,3.75,8592765056153,20,18592765056150,360,28592765056157,"8536508090",1.4E-2]
[105615,"Ex9P1 F r","Flat button head, momentary, without printing, red","NBF",3.75,0,3.75,8592765056160,20,18592765056167,360,28592765056164,"8536508090",1.4E-2]
[105616,"Ex9P1 F y","Flat button head, momentary, without printing, yellow","NBF",3.75,0,3.75,8592765056177,20,18592765056174,360,28592765056171,"8536508090",1.4E-2]
[105617,"Ex9P1 F b","Flat button head, momentary, without printing, blue","NBF",3.75,0,3.75,8592765056184,20,18592765056181,360,28592765056188,"8536508090",1.4E-2]
[105618,"Ex9P1 FI w","Flat button head, momentary, without printing, illumination possibility, white","NBF",5.65,0,5.65,8592765056191,20,18592765056198,360,28592765056195,"8536508090",1.4E-2]
[105619,"Ex9P1 FI g","Flat button head, momentary, without printing, illumination possibility, green","NBF",5.65,0,5.65,8592765056207,20,18592765056204,360,28592765056201,"8536508090",1.4E-2]
[105620,"Ex9P1 FI r","Flat button head, momentary, without printing, illumination possibility, red","NBF",5.65,0,5.65,8592765056214,20,18592765056211,360,28592765056218,"8536508090",1.4E-2]
[105621,"Ex9P1 FI y","Flat button head, momentary, without printing, illumination possibility, yellow","NBF",5.65,0,5.65,8592765056221,20,18592765056228,360,28592765056225,"8536508090",1.4E-2]
[105622,"Ex9P1 FI b","Flat button head, momentary, without printing, illumination possibility, blue","NBF",5.65,0,5.65,8592765056238,20,18592765056235,360,28592765056232,"8536508090",1.4E-2]
[105623,"Ex9P1 R w","Raised button head, momentary, without printing, white","NBF",4.66,0,4.66,8592765056245,10,18592765056242,320,28592765056249,"8536508000",1.6E-2]
[105624,"Ex9P1 R k","Raised button head, momentary, without printing, black","NBF",4.66,0,4.66,8592765056252,10,18592765056259,320,28592765056256,"8536508000",1.6E-2]
[105625,"Ex9P1 R g","Raised button head, momentary, without printing, green","NBF",4.66,0,4.66,8592765056269,10,18592765056266,320,28592765056263,"8536508090",1.6E-2]
[105626,"Ex9P1 R r","Raised button head, momentary, without printing, red","NBF",4.66,0,4.66,8592765056276,10,18592765056273,320,28592765056270,"8536508090",1.6E-2]
[105627,"Ex9P1 R y","Raised button head, momentary, without printing, yellow","NBF",4.66,0,4.66,8592765056283,10,18592765056280,320,28592765056287,"8536508090",1.6E-2]
[105628,"Ex9P1 R b","Raised button head, momentary, without printing, blue","NBF",4.66,0,4.66,8592765056290,10,18592765056297,320,28592765056294,"8536508090",1.6E-2]
[105629,"Ex9P1 RI w","Raised button head, momentary, without printing, illumination possibility, white","NBF",6.52,0,6.52,8592765056306,10,18592765056303,320,28592765056300,"8536508000",1.6E-2]
[105630,"Ex9P1 RI g","Raised button head, momentary, without printing, illumination possibility, green","NBF",6.52,0,6.52,8592765056313,10,18592765056310,320,28592765056317,"8536508090",1.6E-2]
[105631,"Ex9P1 RI r","Raised button head, momentary, without printing, illumination possibility, red","NBF",6.52,0,6.52,8592765056320,10,18592765056327,320,28592765056324,"8536508000",1.6E-2]
[105632,"Ex9P1 RI y","Raised button head, momentary, without printing, illumination possibility, yellow","NBF",6.52,0,6.52,8592765056337,10,18592765056334,320,28592765056331,"8536508000",1.6E-2]
[105633,"Ex9P1 RI b","Raised button head, momentary, without printing, illumination possibility, blue","NBF",6.52,0,6.52,8592765056344,10,18592765056341,320,28592765056348,"8536508090",1.6E-2]
[105634,"Ex9P1 M w","Mushroom button head, 40 mm, momentary, white","NBF",6.49,0,6.49,8592765056351,10,18592765056358,210,28592765056355,"8536508090",0.02]
[105635,"Ex9P1 M k","Mushroom button head, 40 mm, momentary, black","NBF",6.49,0,6.49,8592765056368,10,18592765056365,210,28592765056362,"8536508090",0.02]
[105636,"Ex9P1 M g","Mushroom button head, 40 mm, momentary, green","NBF",6.49,0,6.49,8592765056375,10,18592765056372,210,28592765056379,"8536508090",0.02]
[105637,"Ex9P1 M r","Mushroom button head, 40 mm, momentary, red","NBF",6.49,0,6.49,8592765056382,10,18592765056389,210,28592765056386,"8536508090",0.02]
[105638,"Ex9P1 M y","Mushroom button head, 40 mm, momentary, yellow","NBF",6.49,0,6.49,8592765056399,10,18592765056396,210,28592765056393,"8536508090",0.02]
[105639,"Ex9P1 M b","Mushroom button head, 40 mm, momentary, blue","NBF",6.49,0,6.49,8592765056405,10,18592765056402,210,28592765056409,"8536508090",0.02]
[105640,"Ex9P1 MI w","Mushroom button head, 40 mm, momentary, illumination possibility, white","NBF",9.09,0,9.09,8592765056412,10,18592765056419,210,28592765056416,"8536508090",0.02]
[105641,"Ex9P1 MI g","Mushroom button head, 40 mm, momentary, illumination possibility, green","NBF",9.09,0,9.09,8592765056429,10,18592765056426,210,28592765056423,"8536508090",0.02]
[105642,"Ex9P1 MI r","Mushroom button head, 40 mm, momentary, illumination possibility, red","NBF",9.09,0,9.09,8592765056436,10,18592765056433,210,28592765056430,"8536508090",0.02]
[105643,"Ex9P1 MI y","Mushroom button head, 40 mm, momentary, illumination possibility, yellow","NBF",9.09,0,9.09,8592765056443,10,18592765056440,210,28592765056447,"8536508090",0.02]
[105644,"Ex9P1 MI b","Mushroom button head, 40 mm, momentary, illumination possibility, blue","NBF",9.09,0,9.09,8592765056450,10,18592765056457,210,28592765056454,"8536508090",0.02]
[105645,"Ex9P1 M6 w","Mushroom button head, 60 mm, momentary, without printing, white","NBF",7.79,0,7.79,8592765056467,5,18592765056464,90,28592765056461,"8536508090",2.5999999999999999E-2]
[105646,"Ex9P1 M6 k","Mushroom button head, 60 mm, momentary, without printing, black","NBF",7.79,0,7.79,8592765056474,5,18592765056471,90,28592765056478,"8536508090",2.5999999999999999E-2]
[105647,"Ex9P1 M6 g","Mushroom button head, 60 mm, momentary, without printing, green","NBF",7.79,0,{"$f":"E3381*(1-F3381)","v":7.79},8592765056481,5,18592765056488,90,28592765056485,"8536508090",2.5999999999999999E-2]
[105648,"Ex9P1 M6 r","Mushroom button head, 60 mm, momentary, without printing, red","NBF",7.79,{"$f":"NBF","v":0},7.79,8592765056498,5,18592765056495,90,28592765056492,"8536508090",2.5999999999999999E-2]
[105649,"Ex9P1 M6 y","Mushroom button head, 60 mm, momentary, without printing, yellow","NBF",7.79,0,7.79,8592765056504,5,18592765056501,90,28592765056508,"8536508090",2.5999999999999999E-2]
[105650,"Ex9P1 M6 b","Mushroom button head, 60 mm, momentary, without printing, blue","NBF",7.79,0,7.79,8592765056511,5,18592765056518,90,28592765056515,"8536508090",2.5999999999999999E-2]
[105651,"Ex9P1 M6I w","Mushroom button head, 60 mm, momentary, without printing, illumination possibility, white","NBF",10.89,0,10.89,8592765056528,5,18592765056525,90,28592765056522,"8536508090",2.5999999999999999E-2]
[105652,"Ex9P1 M6I g","Mushroom button head, 60 mm, momentary, without printing, illumination possibility, green","NBF",10.89,0,10.89,8592765056535,5,18592765056532,90,28592765056539,"8536508090",2.5999999999999999E-2]
[105653,"Ex9P1 M6I r","Mushroom button head, 60 mm, momentary, without printing, illumination possibility, red","NBF",10.89,0,10.89,8592765056542,5,18592765056549,90,28592765056546,"8536508090",2.5999999999999999E-2]
[105654,"Ex9P1 M6I y","Mushroom button head, 60 mm, momentary, without printing, illumination possibility, yellow","NBF",10.89,0,10.89,8592765056559,5,18592765056556,90,28592765056553,"8536508090",2.5999999999999999E-2]
[105655,"Ex9P1 M6I b","Mushroom button head, 60 mm, momentary, without printing, illumination possibility, blue","NBF",10.89,0,10.89,8592765056566,5,18592765056563,90,28592765056560,"8536508090",2.5999999999999999E-2]
[105656,"Ex9P1 H r","Emergency stop mushroom button head, 40 mm, maintained, red","NBF",14.13,0,14.13,8592765056573,10,18592765056570,210,28592765056577,"8536508090",3.4000000000000002E-2]
[105657,"Ex9P1 H6 r","Emergency stop mushroom button head, 60 mm, maintained, red","NBF",14.97,0,14.97,8592765056580,5,18592765056587,90,28592765056584,"8536508090",3.7999999999999999E-2]
[105658,"Ex9P1 D gr","Dual colour button head, momentary, without printing, green+red","NBF",9.3800000000000008,0,9.3800000000000008,8592765056597,10,18592765056594,210,28592765056591,"8536508090",1.4E-2]
[105659,"Ex9P1 DI gr","Dual colour button head, momentary, without printing, illumination possibility, green+red","NBF",13.15,0,13.15,8592765056603,10,18592765056600,210,28592765056607,"8536508090",1.4E-2]
[105660,"Ex9P1 PI w","Signal lamp head, flat, without printing, white","NBF",2.85,0,2.85,8592765056610,20,18592765056617,360,28592765056614,"8531807000",1.2E-2]
[105661,"Ex9P1 PI g","Signal lamp head, flat, without printing, green","NBF",2.85,0,2.85,8592765056627,20,18592765056624,360,28592765056621,"8531807000",1.2E-2]
[105662,"Ex9P1 PI r","Signal lamp head, flat, without printing, red","NBF",2.85,0,2.85,8592765056634,20,18592765056631,360,28592765056638,"8531807000",1.2E-2]
[105663,"Ex9P1 PI y","Signal lamp head, flat, without printing, yellow","NBF",2.85,0,2.85,8592765056641,20,18592765056648,360,28592765056645,"8531807000",1.2E-2]
[105664,"Ex9P1 PI b","Signal lamp head, flat, without printing, blue","NBF",2.85,0,2.85,8592765056658,20,18592765056655,360,28592765056652,"8531807000",1.2E-2]
[105665,"Ex9P1 S w","2-position selector switch with handle head, maintained, white","NBF",7.12,0,7.12,8592765056665,10,18592765056662,320,28592765056669,"8536508090",1.7000000000000001E-2]
[105666,"Ex9P1 S k","2-position selector switch with handle head, maintained, black","NBF",7.12,0,7.12,8592765056672,10,18592765056679,320,28592765056676,"8536508090",1.7000000000000001E-2]
[105667,"Ex9P1 S g","2-position selector switch with handle head, maintained, green","NBF",7.12,0,7.12,8592765056689,10,18592765056686,320,28592765056683,"8536508090",1.7000000000000001E-2]
[105668,"Ex9P1 S r","2-position selector switch with handle head, maintained, red","NBF",7.12,0,7.12,8592765056696,10,18592765056693,320,28592765056690,"8536508090",1.7000000000000001E-2]
[105669,"Ex9P1 S y","2-position selector switch with handle head, maintained, yellow","NBF",7.12,0,7.12,8592765056702,10,18592765056709,320,28592765056706,"8536508090",1.7000000000000001E-2]
[105670,"Ex9P1 S b","2-position selector switch with handle head, maintained, blue","NBF",7.12,0,7.12,8592765056719,10,18592765056716,320,28592765056713,"8536508090",1.7000000000000001E-2]
[105671,"Ex9P1 SI w","2-position selector switch with handle head, maintained, illumination possibility, white","NBF",8.8000000000000007,0,8.8000000000000007,8592765056726,10,18592765056723,320,28592765056720,"8536508090",1.7000000000000001E-2]
[105672,"Ex9P1 SI g","2-position selector switch with handle head, maintained, illumination possibility, green","NBF",8.8000000000000007,0,8.8000000000000007,8592765056733,10,18592765056730,320,28592765056737,"8536508090",1.7000000000000001E-2]
[105673,"Ex9P1 SI r","2-position selector switch with handle head, maintained, illumination possibility, red","NBF",8.8000000000000007,0,8.8000000000000007,8592765056740,10,18592765056747,320,28592765056744,"8536508090",1.7000000000000001E-2]
[105674,"Ex9P1 SI y","2-position selector switch with handle head, maintained, illumination possibility, yellow","NBF",8.8000000000000007,0,8.8000000000000007,8592765056757,10,18592765056754,320,28592765056751,"8536508090",1.7000000000000001E-2]
[105675,"Ex9P1 SI b","2-position selector switch with handle head, maintained, illumination possibility, blue","NBF",8.8000000000000007,0,8.8000000000000007,8592765056764,10,18592765056761,320,28592765056768,"8536508090",1.7000000000000001E-2]
[105511,"Ex9P1 SS w","2-position selector switch with handle head, momentary, white","NBF",7.12,0,7.12,8592765055125,10,18592765055122,320,28592765055129,"8536508090",1.7000000000000001E-2]
[105512,"Ex9P1 SS k","2-position selector switch with handle head, momentary, black","NBF",7.12,0,7.12,8592765055132,10,18592765055139,320,28592765055136,"8536508090",1.7000000000000001E-2]
[105513,"Ex9P1 SS g","2-position selector switch with handle head, momentary, green","NBF",7.12,0,7.12,8592765055149,10,18592765055146,320,28592765055143,"8536508090",1.7000000000000001E-2]
[105514,"Ex9P1 SS r","2-position selector switch with handle head, momentary, red","NBF",7.12,0,7.12,8592765055156,10,18592765055153,320,28592765055150,"8536508090",1.7000000000000001E-2]
[105515,"Ex9P1 SS y","2-position selector switch with handle head, momentary, yellow","NBF",7.12,0,7.12,8592765055163,10,18592765055160,320,28592765055167,"8536508090",1.7000000000000001E-2]
[105516,"Ex9P1 SS b","2-position selector switch with handle head, momentary, blue","NBF",7.12,0,7.12,8592765055170,10,18592765055177,320,28592765055174,"8536508090",1.7000000000000001E-2]
[105517,"Ex9P1 SSI w","2-position selector switch with handle head, momentary, illumination possibility, white","NBF",8.8000000000000007,0,8.8000000000000007,8592765055187,10,18592765055184,320,28592765055181,"8536508090",1.7000000000000001E-2]
[105518,"Ex9P1 SSI g","2-position selector switch with handle head, momentary, illumination possibility, green","NBF",8.8000000000000007,0,8.8000000000000007,8592765055194,10,18592765055191,320,28592765055198,"8536508090",1.7000000000000001E-2]
[105519,"Ex9P1 SSI r","2-position selector switch with handle head, momentary, illumination possibility, red","NBF",8.8000000000000007,0,8.8000000000000007,8592765055200,10,18592765055207,320,28592765055204,"8536508090",1.7000000000000001E-2]
[105520,"Ex9P1 SSI y","2-position selector switch with handle head, momentary, illumination possibility, yellow","NBF",8.8000000000000007,0,8.8000000000000007,8592765055217,10,18592765055214,320,28592765055211,"8536508090",1.7000000000000001E-2]
[105521,"Ex9P1 SSI b","2-position selector switch with handle head, momentary, illumination possibility, blue","NBF",8.8000000000000007,0,8.8000000000000007,8592765055224,10,18592765055221,320,28592765055228,"8536508090",1.7000000000000001E-2]
[105677,"Ex9P1 S3 w","3-position selector switch with handle head, maintained, white","NBF",7.52,0,7.52,8592765056788,10,18592765056785,320,28592765056782,"8536508090",1.7000000000000001E-2]
[105678,"Ex9P1 S3 k","3-position selector switch with handle head, maintained, black","NBF",7.52,0,7.52,8592765056795,10,18592765056792,320,28592765056799,"8536508090",1.7000000000000001E-2]
[105679,"Ex9P1 S3 g","3-position selector switch with handle head, maintained, green","NBF",7.52,0,7.52,8592765056801,10,18592765056808,320,28592765056805,"8536508090",1.7000000000000001E-2]
[105680,"Ex9P1 S3 r","3-position selector switch with handle head, maintained, red","NBF",7.52,0,7.52,8592765056818,10,18592765056815,320,28592765056812,"8536508090",1.7000000000000001E-2]
[105681,"Ex9P1 S3 y","3-position selector switch with handle head, maintained, yellow","NBF",7.52,0,7.52,8592765056825,10,18592765056822,320,28592765056829,"8536508090",1.7000000000000001E-2]
[105682,"Ex9P1 S3 b","3-position selector switch with handle head, maintained, blue","NBF",7.52,0,7.52,8592765056832,10,18592765056839,320,28592765056836,"8536508090",1.7000000000000001E-2]
[105683,"Ex9P1 S3I w","3-position selector switch with handle head, maintained, illumination possibility, white","NBF",9.6199999999999992,0,9.6199999999999992,8592765056849,10,18592765056846,320,28592765056843,"8536508090",1.7000000000000001E-2]
[105684,"Ex9P1 S3I g","3-position selector switch with handle head, maintained, illumination possibility, green","NBF",9.6199999999999992,0,9.6199999999999992,8592765056856,10,18592765056853,320,28592765056850,"8536508090",1.7000000000000001E-2]
[105685,"Ex9P1 S3I r","3-position selector switch with handle head, maintained, illumination possibility, red","NBF",9.6199999999999992,0,9.6199999999999992,8592765056863,10,18592765056860,320,28592765056867,"8536508090",1.7000000000000001E-2]
[105686,"Ex9P1 S3I y","3-position selector switch with handle head, maintained, illumination possibility, yellow","NBF",9.6199999999999992,0,9.6199999999999992,8592765056870,10,18592765056877,320,28592765056874,"8536508090",1.7000000000000001E-2]
[105687,"Ex9P1 S3I b","3-position selector switch with handle head, maintained, illumination possibility, blue","NBF",9.6199999999999992,0,9.6199999999999992,8592765056887,10,18592765056884,320,28592765056881,"8536508090",1.7000000000000001E-2]
[105522,"Ex9P1 SS3 w","3-position selector switch with handle head, momentary, white","NBF",7.52,0,7.52,8592765055231,10,18592765055238,320,28592765055235,"8536508090",1.7000000000000001E-2]
[105523,"Ex9P1 SS3 k","3-position selector switch with handle head, momentary, black","NBF",7.52,0,7.52,8592765055248,10,18592765055245,320,28592765055242,"8536508090",1.7000000000000001E-2]
[105524,"Ex9P1 SS3 g","3-position selector switch with handle head, momentary, green","NBF",7.52,0,7.52,8592765055255,10,18592765055252,320,28592765055259,"8536508090",1.7000000000000001E-2]
[105525,"Ex9P1 SS3 r","3-position selector switch with handle head, momentary, red","NBF",7.52,0,7.52,8592765055262,10,18592765055269,320,28592765055266,"8536508090",1.7000000000000001E-2]
[105526,"Ex9P1 SS3 y","3-position selector switch with handle head, momentary, yellow","NBF",7.52,0,7.52,8592765055279,10,18592765055276,320,28592765055273,"8536508090",1.7000000000000001E-2]
[105527,"Ex9P1 SS3 b","3-position selector switch with handle head, momentary, blue","NBF",7.52,0,7.52,8592765055286,10,18592765055283,320,28592765055280,"8536508090",1.7000000000000001E-2]
[105528,"Ex9P1 SS3I w","3-position selector switch with handle head, momentary, illumination possibility, white","NBF",9.6199999999999992,0,9.6199999999999992,8592765055293,10,18592765055290,320,28592765055297,"8536508090",1.7000000000000001E-2]
[105529,"Ex9P1 SS3I g","3-position selector switch with handle head, momentary, illumination possibility, green","NBF",9.6199999999999992,0,9.6199999999999992,8592765055309,10,18592765055306,320,28592765055303,"8536508090",1.7000000000000001E-2]
[105530,"Ex9P1 SS3I r","3-position selector switch with handle head, momentary, illumination possibility, red","NBF",9.6199999999999992,0,9.6199999999999992,8592765055316,10,18592765055313,320,28592765055310,"8536508090",1.7000000000000001E-2]
[105531,"Ex9P1 SS3I y","3-position selector switch with handle head, momentary, illumination possibility, yellow","NBF",9.6199999999999992,0,9.6199999999999992,8592765055323,10,18592765055320,320,28592765055327,"8536508090",1.7000000000000001E-2]
[105532,"Ex9P1 SS3I b","3-position selector switch with handle head, momentary, illumination possibility, blue","NBF",9.6199999999999992,0,9.6199999999999992,8592765055330,10,18592765055337,320,28592765055334,"8536508090",1.7000000000000001E-2]
[105533,"Ex9P1 SSM3 w","3-position selector switch with handle head, momentary-maintained, white","NBF",7.52,0,7.52,8592765055347,10,18592765055344,320,28592765055341,"8536508090",1.7000000000000001E-2]
[105534,"Ex9P1 SSM3 k","3-position selector switch with handle head, momentary-maintained, black","NBF",7.52,0,7.52,8592765055354,10,18592765055351,320,28592765055358,"8536508090",1.7000000000000001E-2]
[105535,"Ex9P1 SSM3 g","3-position selector switch with handle head, momentary-maintained, green","NBF",7.52,0,{"$f":"E3445*(1-F3445)","v":7.52},8592765055361,10,18592765055368,320,28592765055365,"8536508090",1.7000000000000001E-2]
[105536,"Ex9P1 SSM3 r","3-position selector switch with handle head, momentary-maintained, red","NBF",7.52,{"$f":"NBF","v":0},7.52,8592765055378,10,18592765055375,320,28592765055372,"8536508090",1.7000000000000001E-2]
[105537,"Ex9P1 SSM3 y","3-position selector switch with handle head, momentary-maintained, yellow","NBF",7.52,0,7.52,8592765055385,10,18592765055382,320,28592765055389,"8536508090",1.7000000000000001E-2]
[105538,"Ex9P1 SSM3 b","3-position selector switch with handle head, momentary-maintained, blue","NBF",7.52,0,7.52,8592765055392,10,18592765055399,320,28592765055396,"8536508090",1.7000000000000001E-2]
[105539,"Ex9P1 SSM3I w","3-position selector switch with handle head, momentary-maintained, illumination possibility, white","NBF",9.6199999999999992,0,9.6199999999999992,8592765055408,10,18592765055405,320,28592765055402,"8536508090",1.7000000000000001E-2]
[105540,"Ex9P1 SSM3I g","3-position selector switch with handle head, momentary-maintained, illumination possibility, green","NBF",9.6199999999999992,0,9.6199999999999992,8592765055415,10,18592765055412,320,28592765055419,"8536508090",1.7000000000000001E-2]
[105541,"Ex9P1 SSM3I r","3-position selector switch with handle head, momentary-maintained, illumination possibility, red","NBF",9.6199999999999992,0,9.6199999999999992,8592765055422,10,18592765055429,320,28592765055426,"8536508090",1.7000000000000001E-2]
[105542,"Ex9P1 SSM3I y","3-position selector switch with handle head, momentary-maintained, illumination possibility, yellow","NBF",9.6199999999999992,0,9.6199999999999992,8592765055439,10,18592765055436,320,28592765055433,"8536508090",1.7000000000000001E-2]
[105543,"Ex9P1 SSM3I b","3-position selector switch with handle head, momentary-maintained, illumination possibility, blue","NBF",9.6199999999999992,0,9.6199999999999992,8592765055446,10,18592765055443,320,28592765055440,"8536508090",1.7000000000000001E-2]
[105544,"Ex9P1 SMS3 w","3-position selector switch with handle head, maintained-momentary, white","NBF",7.52,0,7.52,8592765055453,10,18592765055450,320,28592765055457,"8536508090",1.7000000000000001E-2]
[105545,"Ex9P1 SMS3 k","3-position selector switch with handle head, maintained-momentary, black","NBF",7.52,0,7.52,8592765055460,10,18592765055467,320,28592765055464,"8536508090",1.7000000000000001E-2]
[105546,"Ex9P1 SMS3 g","3-position selector switch with handle head, maintained-momentary, green","NBF",7.52,0,7.52,8592765055477,10,18592765055474,320,28592765055471,"8536508090",1.7000000000000001E-2]
[105547,"Ex9P1 SMS3 r","3-position selector switch with handle head, maintained-momentary, red","NBF",7.52,0,7.52,8592765055484,10,18592765055481,320,28592765055488,"8536508090",1.7000000000000001E-2]
[105548,"Ex9P1 SMS3 y","3-position selector switch with handle head, maintained-momentary, yellow","NBF",7.52,0,7.52,8592765055491,10,18592765055498,320,28592765055495,"8536508090",1.7000000000000001E-2]
[105549,"Ex9P1 SMS3 b","3-position selector switch with handle head, maintained-momentary, blue","NBF",7.52,0,7.52,8592765055507,10,18592765055504,320,28592765055501,"8536508090",1.7000000000000001E-2]
[105550,"Ex9P1 SMS3I w","3-position selector switch with handle head, maintained-momentary, illumination possibility, white","NBF",9.6199999999999992,0,9.6199999999999992,8592765055514,10,18592765055511,320,28592765055518,"8536508090",1.7000000000000001E-2]
[105551,"Ex9P1 SMS3I g","3-position selector switch with handle head, maintained-momentary, illumination possibility, green","NBF",9.6199999999999992,0,9.6199999999999992,8592765055521,10,18592765055528,320,28592765055525,"8536508090",1.7000000000000001E-2]
[105552,"Ex9P1 SMS3I r","3-position selector switch with handle head, maintained-momentary, illumination possibility, red","NBF",9.6199999999999992,0,9.6199999999999992,8592765055538,10,18592765055535,320,28592765055532,"8536508090",1.7000000000000001E-2]
[105553,"Ex9P1 SMS3I y","3-position selector switch with handle head, maintained-momentary, illumination possibility, yellow","NBF",9.6199999999999992,0,9.6199999999999992,8592765055545,10,18592765055542,320,28592765055549,"8536508090",1.7000000000000001E-2]
[105554,"Ex9P1 SMS3I b","3-position selector switch with handle head, maintained-momentary, illumination possibility, blue","NBF",9.6199999999999992,0,9.6199999999999992,8592765055552,10,18592765055559,320,28592765055556,"8536508090",1.7000000000000001E-2]
[105676,"Ex9P1 SK","2-position selector switch with key head, maintained","NBF",22.73,0,22.73,8592765056771,10,18592765056778,320,28592765056775,"8536508090",2.8000000000000001E-2]
[105555,"Ex9P1 SSK","2-position selector switch with key head, momentary","NBF",22.73,0,22.73,8592765055569,10,18592765055566,320,28592765055563,"8536508090",2.8000000000000001E-2]
[105688,"Ex9P1 S3K ","3-position selector switch with key head, maintained","NBF",23.89,0,23.89,8592765056894,10,18592765056891,320,28592765056898,"8536508090",2.8000000000000001E-2]
[105556,"Ex9P1 SS3K","3-position selector switch with key head, momentary","NBF",23.89,0,23.89,8592765055576,10,18592765055573,320,28592765055570,"8536508090",2.8000000000000001E-2]
[105557,"Ex9P1 SSM3K","3-position selector switch with key head, momentary-maintained","NBF",23.89,0,23.89,8592765055583,10,18592765055580,320,28592765055587,"8536508090",2.8000000000000001E-2]
[105558,"Ex9P1 SMS3K","3-position selector switch with key head, maintained-momentary","NBF",23.89,0,23.89,8592765055590,10,18592765055597,320,28592765055594,"8536508090",2.8000000000000001E-2]
[106776,"Ex9P1 S SH","Holder for labels 25x11 mm, empty, with opening for Ex9P1/Ex9IL/Ex9PB devices","NBF",0.42,0,0.42,8592765067777,1,18592765067774,null,28592765067771,"3926909790",5.0000000000000001E-3]
[106777,"Ex9P1 S S0","Empty label, aluminium foil, suitable for Ex9P1 S SH holder","NBF",0.36,0,0.36,8592765067784,10,18592765067781,null,28592765067788,"8538909999"]
[106778,"Ex9P1 S S1","OFF-ON label, aluminium foil with printing, suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067791,10,18592765067798,null,28592765067795,"8538909999"]
[106779,"Ex9P1 S S2","0-I label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067807,10,18592765067804,null,28592765067801,"8538909999"]
[106780,"Ex9P1 S S3","I-0-II label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067814,10,18592765067811,null,28592765067818,"8538909999"]
[106781,"Ex9P1 S S4","STOP-START label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067821,10,18592765067828,null,28592765067825,"8538909999"]
[106782,"Ex9P1 S S5","0-1 label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067838,10,18592765067835,null,28592765067832,"8538909999"]
[106783,"Ex9P1 S S6","1-0-2 label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067845,10,18592765067842,null,28592765067849,"8538909999"]
[106784,"Ex9P1 S S7","STOP label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067852,10,18592765067859,null,28592765067856,"8538909999"]
[106785,"Ex9P1 S S8","START label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067869,10,18592765067866,null,28592765067863,"8538909999"]
[106786,"Ex9P1 S S9","ON label, aluminium foil with printing,suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067876,10,18592765067873,null,28592765067870,"8538909999"]
[106787,"Ex9P1 S S10","OFF label, aluminium foil with printing, suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067883,10,18592765067880,null,28592765067887,"8538909999"]
[106788,"Ex9P1 S S11","RUN label, aluminium foil with printing, suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067890,10,18592765067897,null,28592765067894,"8538909999"]
[106789,"Ex9P1 S S12","AUTO label, aluminium foil with printing, suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067906,10,18592765067903,null,28592765067900,"8538909999"]
[106790,"Ex9P1 S S13","FAULT label, aluminium foil with printing, suitable for Ex9P1 S SH holder","NBF",0.98,0,0.98,8592765067913,10,18592765067910,null,28592765067917,"8538909999"]
[106791,"Ex9P1 H S6EN","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, EN","NBF",3.88,0,3.88,8592765067920,10,18592765067927,null,28592765067924,"3919908099"]
[106792,"Ex9P1 H S6CZ","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, CZ","NBF",3.88,0,3.88,8592765067937,10,18592765067934,null,28592765067931,"3919908099"]
[106793,"Ex9P1 H S6SK","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, SK","NBF",3.88,0,3.88,8592765067944,10,18592765067941,null,28592765067948,"3919908099"]
[106794,"Ex9P1 H S6PL","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, PL","NBF",3.88,0,3.88,8592765067951,10,18592765067958,null,28592765067955,"3919908099"]
[106795,"Ex9P1 H S6RO","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, RO","NBF",3.88,0,3.88,8592765067968,10,18592765067965,null,28592765067962,"3919908099"]
[106796,"Ex9P1 H S6DE","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, DE","NBF",3.88,0,3.88,8592765067975,10,18592765067972,null,28592765067979,"3919908099"]
[106797,"Ex9P1 H S6FR","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, FR","NBF",3.88,0,3.88,8592765067982,10,18592765067989,null,28592765067986,"3919908099"]
[106798,"Ex9P1 H S6ES","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, ES","NBF",3.88,0,3.88,8592765067999,10,18592765067996,null,28592765067993,"3919908099"]
[106799,"Ex9P1 H S6IT","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, IT","NBF",3.88,0,3.88,8592765068002,10,18592765068009,null,28592765068006,"3919908099"]
[106800,"Ex9P1 H S6RU","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, RU","NBF",3.88,0,3.88,8592765068019,10,18592765068016,null,28592765068013,"3919908099"]
[106801,"Ex9P1 H S6BG","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, BG","NBF",3.88,0,3.88,8592765068026,10,18592765068023,null,28592765068020,"3919908099"]
[106802,"Ex9P1 H S6RS","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, RS","NBF",3.88,0,3.88,8592765068033,10,18592765068030,null,28592765068037,"3919908099"]
[106803,"Ex9P1 H S6HU","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, HU","NBF",3.88,0,3.88,8592765068040,10,18592765068047,null,28592765068044,"3919908099"]
[106804,"Ex9P1 H S6LT","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, LT","NBF",3.88,0,3.88,8592765068057,10,18592765068054,null,28592765068051,"3919908099"]
[106805,"Ex9P1 H S6LV","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, LV","NBF",3.88,0,3.88,8592765068064,10,18592765068061,null,28592765068068,"3919908099"]
[106806,"Ex9P1 H S6EE","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, EE","NBF",3.88,0,3.88,8592765068071,10,18592765068078,null,28592765068075,"3919908099"]
[107868,"Ex9P1 H S6EMPTY","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, Empty","NBF",3.88,0,3.88,8592765078698,10,18592765078695,null,28592765078692,"8538909999"]
[107869,"Ex9P1 H S6EMS","Emergency Stop Sticker with opening for Ex9P1 H, circular 60 mm, self-adhesive, yellow, ES symbol only","NBF",3.88,0,3.88,8592765078704,10,18592765078701,null,28592765078708,"8538909999"]
[106807,"Ex9P1 H S9EN","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, EN","NBF",4.53,0,4.53,8592765068088,10,18592765068085,null,28592765068082,"3919908099"]
[106808,"Ex9P1 H S9CZ","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, CZ","NBF",4.53,0,4.53,8592765068095,10,18592765068092,null,28592765068099,"3919908099"]
[106809,"Ex9P1 H S9SK","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, SK","NBF",4.53,0,4.53,8592765068101,10,18592765068108,null,28592765068105,"3919908099"]
[106810,"Ex9P1 H S9PL","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, PL","NBF",4.53,0,4.53,8592765068118,10,18592765068115,null,28592765068112,"3919908099"]
[106811,"Ex9P1 H S9RO","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, RO","NBF",4.53,0,4.53,8592765068125,10,18592765068122,null,28592765068129,"3919908099"]
[106812,"Ex9P1 H S9DE","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, DE","NBF",4.53,0,{"$f":"E3509*(1-F3509)","v":4.53},8592765068132,10,18592765068139,null,28592765068136,"3919908099"]
[106813,"Ex9P1 H S9FR","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, FR","NBF",4.53,{"$f":"NBF","v":0},4.53,8592765068149,10,18592765068146,null,28592765068143,"3919908099"]
[106814,"Ex9P1 H S9ES","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, ES","NBF",4.53,0,4.53,8592765068156,10,18592765068153,null,28592765068150,"3919908099"]
[106815,"Ex9P1 H S9IT","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, IT","NBF",4.53,0,4.53,8592765068163,10,18592765068160,null,28592765068167,"3919908099"]
[106816,"Ex9P1 H S9RU","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, RU","NBF",4.53,0,4.53,8592765068170,10,18592765068177,null,28592765068174,"3919908099"]
[106817,"Ex9P1 H S9BG","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, BG","NBF",4.53,0,4.53,8592765068187,10,18592765068184,null,28592765068181,"3919908099"]
[106818,"Ex9P1 H S9RS","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, RS","NBF",4.53,0,4.53,8592765068194,10,18592765068191,null,28592765068198,"3919908099"]
[106819,"Ex9P1 H S9HU","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, HU","NBF",4.53,0,4.53,8592765068200,10,18592765068207,null,28592765068204,"3919908099"]
[106820,"Ex9P1 H S9LT","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, LT","NBF",4.53,0,4.53,8592765068217,10,18592765068214,null,28592765068211,"3919908099"]
[106821,"Ex9P1 H S9LV","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, LV","NBF",4.53,0,4.53,8592765068224,10,18592765068221,null,28592765068228,"3919908099"]
[106822,"Ex9P1 H S9EE","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, EE","NBF",4.53,0,4.53,8592765068231,10,18592765068238,null,28592765068235,"3919908099"]
[107870,"Ex9P1 H S9EMPTY","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, Empty","NBF",4.53,0,4.53,8592765078711,10,18592765078718,null,28592765078715,"8538909999"]
[107871,"Ex9P1 H S9EMS","Emergency Stop Sticker with opening for Ex9P1 H, circular 90 mm, self-adhesive, yellow, ES symbol only","NBF",4.53,0,4.53,8592765078728,10,18592765078725,null,28592765078722,"8538909999"]
[]
["Panel mounted signal lamps Ex9IL"]
[105403,"Ex9IL 1 w","Spare flat shaped head cover for Ex9IL, white","NBF",0.96,{"$f":"NBF","v":0},{"$f":"E3524*(1-F3524)","v":0.96},8592765054043,20,18592765054040,1200,28592765054047,"3926909790",0.02]
[105404,"Ex9IL 1 g","Spare flat shaped head cover for Ex9IL, green","NBF",0.96,0,0.96,8592765054050,20,18592765054057,1200,28592765054054,"3926909790",0.02]
[105405,"Ex9IL 1 r","Spare flat shaped head cover for Ex9IL, red","NBF",0.96,0,0.96,8592765054067,20,18592765054064,1200,28592765054061,"3926909790",0.02]
[105406,"Ex9IL 1 y","Spare flat shaped head cover for Ex9IL, yellow","NBF",0.96,0,0.96,8592765054074,20,18592765054071,1200,28592765054078,"3926909790",0.02]
[105407,"Ex9IL 1 b","Spare flat shaped head cover for Ex9IL, blue","NBF",0.96,0,0.96,8592765054081,20,18592765054088,1200,28592765054085,"3926909790",0.02]
[105408,"Ex9IL 2 w","Spare arc shaped head cover for Ex9IL, white","NBF",0.96,0,0.96,8592765054098,20,18592765054095,1200,28592765054092,"3926909790",0.02]
[105409,"Ex9IL 2 g","Spare arc shaped head cover for Ex9IL, green","NBF",0.96,0,0.96,8592765054104,20,18592765054101,1200,28592765054108,"3926909790",0.02]
[105410,"Ex9IL 2 r","Spare arc shaped head cover for Ex9IL, red","NBF",0.96,0,0.96,8592765054111,20,18592765054118,1200,28592765054115,"3926909790",0.02]
[105411,"Ex9IL 2 y","Spare arc shaped head cover for Ex9IL, yellow","NBF",0.96,0,0.96,8592765054128,20,18592765054125,1200,28592765054122,"3926909790",0.02]
[105412,"Ex9IL 2 b","Spare arc shaped head cover for Ex9IL, blue","NBF",0.96,0,0.96,8592765054135,20,18592765054132,1200,28592765054139,"3926909790",0.02]
[105413,"Ex9IL 1R w 6V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, white, 6V AC/DC","NBF",3.65,0,3.65,8592765054142,10,18592765054149,600,28592765054146,"8531807000",2.1999999999999999E-2]
[105414,"Ex9IL 1R g 6V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, green, 6V AC/DC","NBF",3.65,0,3.65,8592765054159,10,18592765054156,600,28592765054153,"8531807000",2.1999999999999999E-2]
[105415,"Ex9IL 1R r 6V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, red, 6V AC/DC","NBF",3.65,0,3.65,8592765054166,10,18592765054163,600,28592765054160,"8531807000",2.1999999999999999E-2]
[105416,"Ex9IL 1R y 6V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, yellow, 6V AC/DC","NBF",3.65,0,3.65,8592765054173,10,18592765054170,600,28592765054177,"8531807000",2.1999999999999999E-2]
[105417,"Ex9IL 1R b 6V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, blue, 6V AC/DC","NBF",3.65,0,3.65,8592765054180,10,18592765054187,600,28592765054184,"8531807000",2.1999999999999999E-2]
[105418,"Ex9IL 1R w 12V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, white, 12V AC/DC","NBF",3.65,0,3.65,8592765054197,10,18592765054194,600,28592765054191,"8531807000",2.1999999999999999E-2]
[105419,"Ex9IL 1R g 12V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, green, 12V AC/DC","NBF",3.65,0,3.65,8592765054203,10,18592765054200,600,28592765054207,"8531807000",2.1999999999999999E-2]
[105420,"Ex9IL 1R r 12V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, red, 12V AC/DC","NBF",3.65,0,3.65,8592765054210,10,18592765054217,600,28592765054214,"8531807000",2.1999999999999999E-2]
[105421,"Ex9IL 1R y 12V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, yellow, 12V AC/DC","NBF",3.65,0,3.65,8592765054227,10,18592765054224,600,28592765054221,"8531807000",2.1999999999999999E-2]
[105422,"Ex9IL 1R b 12V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, blue, 12V AC/DC","NBF",3.65,0,3.65,8592765054234,10,18592765054231,600,28592765054238,"8531807000",2.1999999999999999E-2]
[105423,"Ex9IL 1R w 24V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, white, 24V AC/DC","NBF",3.65,0,3.65,8592765054241,10,18592765054248,600,28592765054245,"8531807000",2.1999999999999999E-2]
[105424,"Ex9IL 1R g 24V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, green, 24V AC/DC","NBF",3.65,0,3.65,8592765054258,10,18592765054255,600,28592765054252,"8531807000",2.1999999999999999E-2]
[105425,"Ex9IL 1R r 24V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, red, 24V AC/DC","NBF",3.65,0,3.65,8592765054265,10,18592765054262,600,28592765054269,"8531807000",2.1999999999999999E-2]
[105426,"Ex9IL 1R y 24V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, yellow, 24V AC/DC","NBF",3.65,0,3.65,8592765054272,10,18592765054279,600,28592765054276,"8531807000",2.1999999999999999E-2]
[105427,"Ex9IL 1R b 24V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, blue, 24V AC/DC","NBF",3.65,0,3.65,8592765054289,10,18592765054286,600,28592765054283,"8531807000",2.1999999999999999E-2]
[105428,"Ex9IL 1R w 36V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, white, 36V AC/DC","NBF",3.65,0,3.65,8592765054296,10,18592765054293,600,28592765054290,"8531807000",2.1999999999999999E-2]
[105429,"Ex9IL 1R g 36V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, green, 36V AC/DC","NBF",3.65,0,3.65,8592765054302,10,18592765054309,600,28592765054306,"8531807000",2.1999999999999999E-2]
[105430,"Ex9IL 1R r 36V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, red, 36V AC/DC","NBF",3.65,0,3.65,8592765054319,10,18592765054316,600,28592765054313,"8531807000",2.1999999999999999E-2]
[105431,"Ex9IL 1R y 36V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, yellow, 36V AC/DC","NBF",3.65,0,3.65,8592765054326,10,18592765054323,600,28592765054320,"8531807000",2.1999999999999999E-2]
[105432,"Ex9IL 1R b 36V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, blue, 36V AC/DC","NBF",3.65,0,3.65,8592765054333,10,18592765054330,600,28592765054337,"8531807000",2.1999999999999999E-2]
[105433,"Ex9IL 1R w 48V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, white, 48V AC/DC","NBF",3.65,0,3.65,8592765054340,10,18592765054347,600,28592765054344,"8531807000",2.1999999999999999E-2]
[105434,"Ex9IL 1R g 48V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, green, 48V AC/DC","NBF",3.65,0,3.65,8592765054357,10,18592765054354,600,28592765054351,"8531807000",2.1999999999999999E-2]
[105435,"Ex9IL 1R r 48V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, red, 48V AC/DC","NBF",3.65,0,3.65,8592765054364,10,18592765054361,600,28592765054368,"8531807000",2.1999999999999999E-2]
[105436,"Ex9IL 1R y 48V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, yellow, 48V AC/DC","NBF",3.65,0,3.65,8592765054371,10,18592765054378,600,28592765054375,"8531807000",2.1999999999999999E-2]
[105437,"Ex9IL 1R b 48V AC/DC","Panel mounted signal lamp, flat shaped head, resistance, blue, 48V AC/DC","NBF",3.65,0,3.65,8592765054388,10,18592765054385,600,28592765054382,"8531807000",2.1999999999999999E-2]
[105438,"Ex9IL 1C w 110V AC","Panel mounted signal lamp, flat shaped head, capacitance, white, 110V AC","NBF",3.65,0,3.65,8592765054395,10,18592765054392,600,28592765054399,"8531807000",2.1999999999999999E-2]
[105439,"Ex9IL 1C g 110V AC","Panel mounted signal lamp, flat shaped head, capacitance, green, 110V AC","NBF",3.65,0,3.65,8592765054401,10,18592765054408,600,28592765054405,"8531807000",2.1999999999999999E-2]
[105440,"Ex9IL 1C r 110V AC","Panel mounted signal lamp, flat shaped head, capacitance, red, 110V AC","NBF",3.65,0,3.65,8592765054418,10,18592765054415,600,28592765054412,"8531807000",2.1999999999999999E-2]
[105441,"Ex9IL 1C y 110V AC","Panel mounted signal lamp, flat shaped head, capacitance, yellow, 110V AC","NBF",3.65,0,3.65,8592765054425,10,18592765054422,600,28592765054429,"8531807000",2.1999999999999999E-2]
[105442,"Ex9IL 1C b 110V AC","Panel mounted signal lamp, flat shaped head, capacitance, blue, 110V AC","NBF",3.65,0,3.65,8592765054432,10,18592765054439,600,28592765054436,"8531807000",2.1999999999999999E-2]
[105443,"Ex9IL 1C w 230V AC","Panel mounted signal lamp, flat shaped head, capacitance, white, 230V AC","NBF",3.65,0,3.65,8592765054449,10,18592765054446,600,28592765054443,"8531807000",2.1999999999999999E-2]
[105444,"Ex9IL 1C g 230V AC","Panel mounted signal lamp, flat shaped head, capacitance, green, 230V AC","NBF",3.65,0,3.65,8592765054456,10,18592765054453,600,28592765054450,"8531807000",2.1999999999999999E-2]
[105445,"Ex9IL 1C r 230V AC","Panel mounted signal lamp, flat shaped head, capacitance, red, 230V AC","NBF",3.65,0,3.65,8592765054463,10,18592765054460,600,28592765054467,"8531807000",2.1999999999999999E-2]
[105446,"Ex9IL 1C y 230V AC","Panel mounted signal lamp, flat shaped head, capacitance, yellow, 230V AC","NBF",3.65,0,3.65,8592765054470,10,18592765054477,600,28592765054474,"8531807000",2.1999999999999999E-2]
[105447,"Ex9IL 1C b 230V AC","Panel mounted signal lamp, flat shaped head, capacitance, blue, 230V AC","NBF",3.65,0,3.65,8592765054487,10,18592765054484,600,28592765054481,"8531807000",2.1999999999999999E-2]
[105448,"Ex9IL 1C w 400V AC","Panel mounted signal lamp, flat shaped head, capacitance, white, 400V AC","NBF",3.65,0,3.65,8592765054494,10,18592765054491,600,28592765054498,"8531807000",2.1999999999999999E-2]
[105449,"Ex9IL 1C g 400V AC","Panel mounted signal lamp, flat shaped head, capacitance, green, 400V AC","NBF",3.65,0,3.65,8592765054500,10,18592765054507,600,28592765054504,"8531807000",2.1999999999999999E-2]
[105450,"Ex9IL 1C r 400V AC","Panel mounted signal lamp, flat shaped head, capacitance, red, 400V AC","NBF",3.65,0,3.65,8592765054517,10,18592765054514,600,28592765054511,"8531807000",2.1999999999999999E-2]
[105451,"Ex9IL 1C y 400V AC","Panel mounted signal lamp, flat shaped head, capacitance, yellow, 400V AC","NBF",3.65,0,3.65,8592765054524,10,18592765054521,600,28592765054528,"8531807000",2.1999999999999999E-2]
[105452,"Ex9IL 1C b 400V AC","Panel mounted signal lamp, flat shaped head, capacitance, blue, 400V AC","NBF",3.65,0,3.65,8592765054531,10,18592765054538,600,28592765054535,"8531807000",2.1999999999999999E-2]
[105453,"Ex9IL 2R w 6V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, white, 6V AC/DC","NBF",3.65,0,3.65,8592765054548,10,18592765054545,600,28592765054542,"8531807000",2.1999999999999999E-2]
[105454,"Ex9IL 2R g 6V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, green, 6V AC/DC","NBF",3.65,0,3.65,8592765054555,10,18592765054552,600,28592765054559,"8531807000",2.1999999999999999E-2]
[105455,"Ex9IL 2R r 6V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, red, 6V AC/DC","NBF",3.65,0,3.65,8592765054562,10,18592765054569,600,28592765054566,"8531807000",2.1999999999999999E-2]
[105456,"Ex9IL 2R y 6V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, yellow, 6V AC/DC","NBF",3.65,0,3.65,8592765054579,10,18592765054576,600,28592765054573,"8531807000",2.1999999999999999E-2]
[105457,"Ex9IL 2R b 6V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, blue, 6V AC/DC","NBF",3.65,0,3.65,8592765054586,10,18592765054583,600,28592765054580,"8531807000",2.1999999999999999E-2]
[105458,"Ex9IL 2R w 12V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, white, 12V AC/DC","NBF",3.65,0,3.65,8592765054593,10,18592765054590,600,28592765054597,"8531807000",2.1999999999999999E-2]
[105459,"Ex9IL 2R g 12V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, green, 12V AC/DC","NBF",3.65,0,3.65,8592765054609,10,18592765054606,600,28592765054603,"8531807000",2.1999999999999999E-2]
[105460,"Ex9IL 2R r 12V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, red, 12V AC/DC","NBF",3.65,0,3.65,8592765054616,10,18592765054613,600,28592765054610,"8531807000",2.1999999999999999E-2]
[105461,"Ex9IL 2R y 12V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, yellow, 12V AC/DC","NBF",3.65,0,3.65,8592765054623,10,18592765054620,600,28592765054627,"8531807000",2.1999999999999999E-2]
[105462,"Ex9IL 2R b 12V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, blue, 12V AC/DC","NBF",3.65,0,3.65,8592765054630,10,18592765054637,600,28592765054634,"8531807000",2.1999999999999999E-2]
[105463,"Ex9IL 2R w 24V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, white, 24V AC/DC","NBF",3.65,0,3.65,8592765054647,10,18592765054644,600,28592765054641,"8531807000",2.1999999999999999E-2]
[105464,"Ex9IL 2R g 24V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, green, 24V AC/DC","NBF",3.65,0,3.65,8592765054654,10,18592765054651,600,28592765054658,"8531807000",2.1999999999999999E-2]
[105465,"Ex9IL 2R r 24V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, red, 24V AC/DC","NBF",3.65,0,3.65,8592765054661,10,18592765054668,600,28592765054665,"8531807000",2.1999999999999999E-2]
[105466,"Ex9IL 2R y 24V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, yellow, 24V AC/DC","NBF",3.65,0,3.65,8592765054678,10,18592765054675,600,28592765054672,"8531807000",2.1999999999999999E-2]
[105467,"Ex9IL 2R b 24V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, blue, 24V AC/DC","NBF",3.65,{"$f":"NBF","v":0},{"$f":"E3588*(1-F3588)","v":3.65},8592765054685,10,18592765054682,600,28592765054689,"8531807000",2.1999999999999999E-2]
[105468,"Ex9IL 2R w 36V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, white, 36V AC/DC","NBF",3.65,0,3.65,8592765054692,10,18592765054699,600,28592765054696,"8531807000",2.1999999999999999E-2]
[105469,"Ex9IL 2R g 36V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, green, 36V AC/DC","NBF",3.65,0,3.65,8592765054708,10,18592765054705,600,28592765054702,"8531807000",2.1999999999999999E-2]
[105470,"Ex9IL 2R r 36V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, red, 36V AC/DC","NBF",3.65,0,3.65,8592765054715,10,18592765054712,600,28592765054719,"8531807000",2.1999999999999999E-2]
[105471,"Ex9IL 2R y 36V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, yellow, 36V AC/DC","NBF",3.65,0,3.65,8592765054722,10,18592765054729,600,28592765054726,"8531807000",2.1999999999999999E-2]
[105472,"Ex9IL 2R b 36V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, blue, 36V AC/DC","NBF",3.65,0,3.65,8592765054739,10,18592765054736,600,28592765054733,"8531807000",2.1999999999999999E-2]
[105473,"Ex9IL 2R w 48V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, white, 48V AC/DC","NBF",3.65,0,3.65,8592765054746,10,18592765054743,600,28592765054740,"8531807000",2.1999999999999999E-2]
[105474,"Ex9IL 2R g 48V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, green, 48V AC/DC","NBF",3.65,0,3.65,8592765054753,10,18592765054750,600,28592765054757,"8531807000",2.1999999999999999E-2]
[105475,"Ex9IL 2R r 48V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, red, 48V AC/DC","NBF",3.65,0,3.65,8592765054760,10,18592765054767,600,28592765054764,"8531807000",2.1999999999999999E-2]
[105476,"Ex9IL 2R y 48V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, yellow, 48V AC/DC","NBF",3.65,0,3.65,8592765054777,10,18592765054774,600,28592765054771,"8531807000",2.1999999999999999E-2]
[105477,"Ex9IL 2R b 48V AC/DC","Panel mounted signal lamp, arc shaped head, resistance, blue, 48V AC/DC","NBF",3.65,0,3.65,8592765054784,10,18592765054781,600,28592765054788,"8531807000",2.1999999999999999E-2]
[105478,"Ex9IL 2C w 110V AC","Panel mounted signal lamp, arc shaped head, capacitance, white, 110V AC","NBF",3.65,0,3.65,8592765054791,10,18592765054798,600,28592765054795,"8531807000",2.1999999999999999E-2]
[105479,"Ex9IL 2C g 110V AC","Panel mounted signal lamp, arc shaped head, capacitance, green, 110V AC","NBF",3.65,0,3.65,8592765054807,10,18592765054804,600,28592765054801,"8531807000",2.1999999999999999E-2]
[105480,"Ex9IL 2C r 110V AC","Panel mounted signal lamp, arc shaped head, capacitance, red, 110V AC","NBF",3.65,0,3.65,8592765054814,10,18592765054811,600,28592765054818,"8531807000",2.1999999999999999E-2]
[105481,"Ex9IL 2C y 110V AC","Panel mounted signal lamp, arc shaped head, capacitance, yellow, 110V AC","NBF",3.65,0,3.65,8592765054821,10,18592765054828,600,28592765054825,"8531807000",2.1999999999999999E-2]
[105482,"Ex9IL 2C b 110V AC","Panel mounted signal lamp, arc shaped head, capacitance, blue, 110V AC","NBF",3.65,0,3.65,8592765054838,10,18592765054835,600,28592765054832,"8531807000",2.1999999999999999E-2]
[105483,"Ex9IL 2C w 230V AC","Panel mounted signal lamp, arc shaped head, capacitance, white, 230V AC","NBF",3.65,0,3.65,8592765054845,10,18592765054842,600,28592765054849,"8531807000",2.1999999999999999E-2]
[105484,"Ex9IL 2C g 230V AC","Panel mounted signal lamp, arc shaped head, capacitance, green, 230V AC","NBF",3.65,0,3.65,8592765054852,10,18592765054859,600,28592765054856,"8531807000",2.1999999999999999E-2]
[105485,"Ex9IL 2C r 230V AC","Panel mounted signal lamp, arc shaped head, capacitance, red, 230V AC","NBF",3.65,0,3.65,8592765054869,10,18592765054866,600,28592765054863,"8531807000",2.1999999999999999E-2]
[105486,"Ex9IL 2C y 230V AC","Panel mounted signal lamp, arc shaped head, capacitance, yellow, 230V AC","NBF",3.65,0,3.65,8592765054876,10,18592765054873,600,28592765054870,"8531807000",2.1999999999999999E-2]
[105487,"Ex9IL 2C b 230V AC","Panel mounted signal lamp, arc shaped head, capacitance, blue, 230V AC","NBF",3.65,0,3.65,8592765054883,10,18592765054880,600,28592765054887,"8531807000",2.1999999999999999E-2]
[105488,"Ex9IL 2C w 400V AC","Panel mounted signal lamp, arc shaped head, capacitance, white, 400V AC","NBF",3.65,0,3.65,8592765054890,10,18592765054897,600,28592765054894,"8531807000",2.1999999999999999E-2]
[105489,"Ex9IL 2C g 400V AC","Panel mounted signal lamp, arc shaped head, capacitance, green, 400V AC","NBF",3.65,0,3.65,8592765054906,10,18592765054903,600,28592765054900,"8531807000",2.1999999999999999E-2]
[105490,"Ex9IL 2C r 400V AC","Panel mounted signal lamp, arc shaped head, capacitance, red, 400V AC","NBF",3.65,0,3.65,8592765054913,10,18592765054910,600,28592765054917,"8531807000",2.1999999999999999E-2]
[105491,"Ex9IL 2C y 400V AC","Panel mounted signal lamp, arc shaped head, capacitance, yellow, 400V AC","NBF",3.65,0,3.65,8592765054920,10,18592765054927,600,28592765054924,"8531807000",2.1999999999999999E-2]
[105492,"Ex9IL 2C b 400V AC","Panel mounted signal lamp, arc shaped head, capacitance, blue, 400V AC","NBF",3.65,0,3.65,8592765054937,10,18592765054934,600,28592765054931,"8531807000",2.1999999999999999E-2]
[]
["Panel mounted buzzers Ex9PB"]
[105689,"Ex9PB I k 24V AC/DC","Panel mounted buzzer, interrupted, black, 24V AC/DC","NBF",17.88,{"$f":"NBF","v":0},{"$f":"E3616*(1-F3616)","v":17.88},8592765056900,10,18592765056907,480,28592765056904,"8531807000",2.1999999999999999E-2]
[105690,"Ex9PB I k 36V AC/DC","Panel mounted buzzer, interrupted, black, 36V AC/DC","NBF",17.88,0,17.88,8592765056917,10,18592765056914,480,28592765056911,"8531807000",2.1999999999999999E-2]
[105691,"Ex9PB I k 48V AC/DC","Panel mounted buzzer, interrupted, black, 48V AC/DC","NBF",17.88,0,17.88,8592765056924,10,18592765056921,480,28592765056928,"8531807000",2.1999999999999999E-2]
[105692,"Ex9PB I k 110V AC/DC","Panel mounted buzzer, interrupted, black, 110V AC/DC","NBF",17.88,0,17.88,8592765056931,10,18592765056938,480,28592765056935,"8531807000",2.1999999999999999E-2]
[105693,"Ex9PB I k 230V AC","Panel mounted buzzer, interrupted, black, 230V AC","NBF",17.88,0,17.88,8592765056948,10,18592765056945,480,28592765056942,"8531807000",2.1999999999999999E-2]
[105694,"Ex9PB I k 400V AC","Panel mounted buzzer, interrupted, black, 400V AC","NBF",17.88,0,17.88,8592765056955,10,18592765056952,480,28592765056959,"8531807000",2.1999999999999999E-2]
[105695,"Ex9PB I r 24V AC/DC","Panel mounted buzzer, interrupted, red, 24V AC/DC","NBF",17.88,0,17.88,8592765056962,10,18592765056969,480,28592765056966,"8531807000",2.1999999999999999E-2]
[105696,"Ex9PB I r 36V AC/DC","Panel mounted buzzer, interrupted, red, 36V AC/DC","NBF",17.88,0,17.88,8592765056979,10,18592765056976,480,28592765056973,"8531807000",2.1999999999999999E-2]
[105697,"Ex9PB I r 48V AC/DC","Panel mounted buzzer, interrupted, red, 48V AC/DC","NBF",17.88,0,17.88,8592765056986,10,18592765056983,480,28592765056980,"8531807000",2.1999999999999999E-2]
[105698,"Ex9PB I r 110V AC","Panel mounted buzzer, interrupted, red, 110V AC","NBF",17.88,0,17.88,8592765056993,10,18592765056990,480,28592765056997,"8531807000",2.1999999999999999E-2]
[105699,"Ex9PB I r 230V AC","Panel mounted buzzer, interrupted, red, 230V AC","NBF",17.88,0,17.88,8592765057006,10,18592765057003,480,28592765057000,"8531807000",2.1999999999999999E-2]
[105700,"Ex9PB I r 400V AC","Panel mounted buzzer, interrupted, red, 400V AC","NBF",17.88,0,17.88,8592765057013,10,18592765057010,480,28592765057017,"8531807000",2.1999999999999999E-2]
[105701,"Ex9PB B r 24V AC/DC","Panel mounted buzzer, interrupted, blinks, red, 24V AC/DC","NBF",21.47,0,21.47,8592765057020,10,18592765057027,480,28592765057024,"8531807000",2.1999999999999999E-2]
[105702,"Ex9PB B r 36V AC/DC","Panel mounted buzzer, interrupted, blinks, red, 36V AC/DC","NBF",21.47,0,21.47,8592765057037,10,18592765057034,480,28592765057031,"8531807000",2.1999999999999999E-2]
[105703,"Ex9PB B r 48V AC/DC","Panel mounted buzzer, interrupted, blinks, red, 48V AC/DC","NBF",21.47,0,21.47,8592765057044,10,18592765057041,480,28592765057048,"8531807000",2.1999999999999999E-2]
[105704,"Ex9PB B r 110V AC","Panel mounted buzzer, interrupted, blinks, red, 110V AC","NBF",21.47,0,21.47,8592765057051,10,18592765057058,480,28592765057055,"8531807000",2.1999999999999999E-2]
[105705,"Ex9PB B r 230V AC","Panel mounted buzzer, interrupted, blinks, red, 230V AC","NBF",21.47,0,21.47,8592765057068,10,18592765057065,480,28592765057062,"8531807000",2.1999999999999999E-2]
[105706,"Ex9PB B r 400V AC","Panel mounted buzzer, interrupted, blinks, red, 400V AC","NBF",21.47,0,21.47,8592765057075,10,18592765057072,480,28592765057079,"8531807000",2.1999999999999999E-2]
[105707,"Ex9PB C k 24V AC/DC","Panel mounted buzzer, continuous, black, 24V AC/DC","NBF",17.88,0,17.88,8592765057082,10,18592765057089,480,28592765057086,"8531807000",2.1999999999999999E-2]
[105708,"Ex9PB C k 36V AC/DC","Panel mounted buzzer, continuous, black, 36V AC/DC","NBF",17.88,0,17.88,8592765057099,10,18592765057096,480,28592765057093,"8531807000",2.1999999999999999E-2]
[105709,"Ex9PB C k 48V AC/DC","Panel mounted buzzer, continuous, black, 48V AC/DC","NBF",17.88,0,17.88,8592765057105,10,18592765057102,480,28592765057109,"8531807000",2.1999999999999999E-2]
[105710,"Ex9PB C k 110V AC","Panel mounted buzzer, continuous, black, 110V AC","NBF",17.88,0,17.88,8592765057112,10,18592765057119,480,28592765057116,"8531807000",2.1999999999999999E-2]
[105711,"Ex9PB C k 230V AC","Panel mounted buzzer, continuous, black, 230V AC","NBF",17.88,0,17.88,8592765057129,10,18592765057126,480,28592765057123,"8531807000",2.1999999999999999E-2]
[105712,"Ex9PB C k 400V AC","Panel mounted buzzer, continuous, black, 400V AC","NBF",17.88,0,17.88,8592765057136,10,18592765057133,480,28592765057130,"8531807000",2.1999999999999999E-2]
[105713,"Ex9PB C r 24V AC/DC","Panel mounted buzzer, continuous, red, 24V AC/DC","NBF",17.88,0,17.88,8592765057143,10,18592765057140,480,28592765057147,"8531807000",2.1999999999999999E-2]
[105714,"Ex9PB C r 36V AC/DC","Panel mounted buzzer, continuous, red, 36V AC/DC","NBF",17.88,0,17.88,8592765057150,10,18592765057157,480,28592765057154,"8531807000",2.1999999999999999E-2]
[105715,"Ex9PB C r 48V AC/DC","Panel mounted buzzer, continuous, red, 48V AC/DC","NBF",17.88,0,17.88,8592765057167,10,18592765057164,480,28592765057161,"8531807000",2.1999999999999999E-2]
[105716,"Ex9PB C r 110V AC","Panel mounted buzzer, continuous, red, 110V AC","NBF",17.88,0,17.88,8592765057174,10,18592765057171,480,28592765057178,"8531807000",2.1999999999999999E-2]
[105717,"Ex9PB C r 230V AC","Panel mounted buzzer, continuous, red, 230V AC","NBF",17.88,0,17.88,8592765057181,10,18592765057188,480,28592765057185,"8531807000",2.1999999999999999E-2]
[105718,"Ex9PB C r 400V AC","Panel mounted buzzer, continuous, red, 400V AC","NBF",17.88,0,17.88,8592765057198,10,18592765057195,480,28592765057192,"8531807000",2.1999999999999999E-2]
[105719,"Ex9PB L r 24V AC/DC","Panel mounted buzzer, continuous, lights, red, 24V AC/DC","NBF",21.47,0,21.47,8592765057204,10,18592765057201,480,28592765057208,"8531807000",2.1999999999999999E-2]
[105720,"Ex9PB L r 36V AC/DC","Panel mounted buzzer, continuous, lights, red, 36V AC/DC","NBF",21.47,0,21.47,8592765057211,10,18592765057218,480,28592765057215,"8531807000",2.1999999999999999E-2]
[105721,"Ex9PB L r 48V AC/DC","Panel mounted buzzer, continuous, lights, red, 48V AC/DC","NBF",21.47,0,21.47,8592765057228,10,18592765057225,480,28592765057222,"8531807000",2.1999999999999999E-2]
[105722,"Ex9PB L r 110V AC","Panel mounted buzzer, continuous, lights, red, 110V AC","NBF",21.47,0,21.47,8592765057235,10,18592765057232,480,28592765057239,"8531807000",2.1999999999999999E-2]
[105723,"Ex9PB L r 230V AC","Panel mounted buzzer, continuous, lights, red, 230V AC","NBF",21.47,0,21.47,8592765057242,10,18592765057249,480,28592765057246,"8531807000",2.1999999999999999E-2]
[105724,"Ex9PB L r 400V AC","Panel mounted buzzer, continuous, lights, red, 400V AC","NBF",21.47,0,21.47,8592765057259,10,18592765057256,480,28592765057253,"8531807000",2.1999999999999999E-2]
[]
["Push button boxes, Ex9P2 FH"]
[111409,"Ex9P2 FH 1 EU","Push button Box 1 hole grey","NBF",5.57,{"$f":"NBF","v":0},{"$f":"E3654*(1-F3654)","v":5.57},8592765114099,1,18592765114096,64,28592765114093,85389000000,0.123]
[111410,"Ex9P2 FH 2 EU","Push button Box 2 holes grey","NBF",5.63,{"$f":"NBF","v":0},{"$f":"E3655*(1-F3655)","v":5.63},8592765114105,1,18592765114102,56,28592765114109,85389000000,0.14199999999999999]
[111411,"Ex9P2 FH 3 EU","Push button Box 3 holes grey","NBF",7.13,{"$f":"NBF","v":0},7.13,8592765114112,1,18592765114119,40,28592765114116,85389000000,0.17199999999999999]
[111412,"Ex9P2 FH 1 y EU","Push button Box 1 hole yellow","NBF",5.57,{"$f":"NBF","v":0},5.57,8592765114129,1,18592765114126,64,28592765114123,85389000000,0.123]
[111413,"Ex9P2 FH 2 y EU","Push button Box 2 holes yellow","NBF",5.63,{"$f":"NBF","v":0},5.63,8592765114136,1,18592765114133,56,28592765114130,85389000000,0.14199999999999999]
[111414,"Ex9P2 FH 3 y EU","Push button Box 3 holes yellow","NBF",7.13,{"$f":"NBF","v":0},7.13,8592765114143,1,18592765114140,40,28592765114147,85389000000,0.17199999999999999]
[]
["Plug-in relays Ex9JM"]
[110291,"Ex9JM2L10 12VDC","Plug-in relay 10 A, 12 V DC, 2 contatcs","NBH",6.18,{"$f":"NBH","v":0},{"$f":"E3662*(1-F3662)","v":6.18},8592765102911,20,18592765102918,480,28592765102915,"8536419089",3.3000000000000002E-2]
[110292,"Ex9JM2L10 24VDC","Plug-in relay 10 A, 24 V DC, 2 contatcs","NBH",4.59,0,4.59,8592765102928,20,18592765102925,480,28592765102922,"8536419089",3.3000000000000002E-2]
[110293,"Ex9JM2L10 36VDC","Plug-in relay 10 A, 36 V DC, 2 contatcs","NBH",6.18,0,6.18,8592765102935,20,18592765102932,480,28592765102939,"8536419089",3.3000000000000002E-2]
[110294,"Ex9JM2L10 48VDC","Plug-in relay 10 A, 48 V DC, 2 contatcs","NBH",6.31,0,6.31,8592765102942,20,18592765102949,480,28592765102946,"8536419089",3.3000000000000002E-2]
[110295,"Ex9JM2L10 110VDC","Plug-in relay 10 A, 110 V DC, 2 contatcs","NBH",6.63,0,6.63,8592765102959,20,18592765102956,480,28592765102953,"8536419089",3.3000000000000002E-2]
[110296,"Ex9JM2L10 220VDC","Plug-in relay 10 A, 220 V DC, 2 contatcs","NBH",7.93,0,7.93,8592765102966,20,18592765102963,480,28592765102960,"8536419089",3.3000000000000002E-2]
[110297,"Ex9JM2L10 24VAC","Plug-in relay 10 A, 24 V AC, 2 contatcs","NBH",4.59,0,4.59,8592765102973,20,18592765102970,480,28592765102977,"8536419089",3.3000000000000002E-2]
[110298,"Ex9JM2L10 36VAC","Plug-in relay 10 A, 36 V AC, 2 contatcs","NBH",6.37,0,6.37,8592765102980,20,18592765102987,480,28592765102984,"8536419089",3.3000000000000002E-2]
[110299,"Ex9JM2L10 48VAC","Plug-in relay 10 A, 48 V AC, 2 contatcs","NBH",6.37,0,6.37,8592765102997,20,18592765102994,480,28592765102991,"8536419089",3.3000000000000002E-2]
[110300,"Ex9JM2L10 110VAC","Plug-in relay 10 A, 110 V AC, 2 contatcs","NBH",6.37,0,6.37,8592765103000,20,18592765103007,480,28592765103004,"8536419089",3.3000000000000002E-2]
[110301,"Ex9JM2L10 230VAC","Plug-in relay 10 A, 230 V AC, 2 contatcs","NBH",4.82,0,4.82,8592765103017,20,18592765103014,480,28592765103011,"8536419089",3.3000000000000002E-2]
[110302,"Ex9JM2DZ-10","Socket for plug-in relay 10 A, 2 contacts","NBH",3.4,0,3.4,8592765103024,10,18592765103021,270,28592765103028,"8538909999",4.9000000000000002E-2]
[110303,"Ex9JM2L05 12VDC","Plug-in relay 5 A, 12 V DC, 2 contatcs","NBH",5.53,0,5.53,8592765103031,20,18592765103038,480,28592765103035,"8536419089",3.3000000000000002E-2]
[110304,"Ex9JM2L05 24VDC","Plug-in relay 5 A, 24 V DC, 2 contatcs","NBH",5.53,0,5.53,8592765103048,20,18592765103045,480,28592765103042,"8536419089",3.3000000000000002E-2]
[110305,"Ex9JM2L05 36VDC","Plug-in relay 5 A, 36 V DC, 2 contatcs","NBH",5.53,0,5.53,8592765103055,20,18592765103052,480,28592765103059,"8536419089",3.3000000000000002E-2]
[110306,"Ex9JM2L05 48VDC","Plug-in relay 5 A, 48 V DC, 2 contatcs","NBH",5.53,0,5.53,8592765103062,20,18592765103069,480,28592765103066,"8536419089",3.3000000000000002E-2]
[110307,"Ex9JM2L05 110VDC","Plug-in relay 5 A, 110 V DC, 2 contatcs","NBH",5.98,0,5.98,8592765103079,20,18592765103076,480,28592765103073,"8536419089",3.3000000000000002E-2]
[110308,"Ex9JM2L05 220VDC","Plug-in relay 5 A, 220 V DC, 2 contatcs","NBH",7.28,0,7.28,8592765103086,20,18592765103083,480,28592765103080,"8536419089",3.3000000000000002E-2]
[110309,"Ex9JM2L05 24VAC","Plug-in relay 5 A, 24 V AC, 2 contatcs","NBH",5.53,0,5.53,8592765103093,20,18592765103090,480,28592765103097,"8536419089",3.3000000000000002E-2]
[110310,"Ex9JM2L05 36VAC","Plug-in relay 5 A, 36 V AC, 2 contatcs","NBH",5.72,0,5.72,8592765103109,20,18592765103106,480,28592765103103,"8536419089",3.3000000000000002E-2]
[110311,"Ex9JM2L05 48VAC","Plug-in relay 5 A, 48 V AC, 2 contatcs","NBH",5.72,0,5.72,8592765103116,20,18592765103113,480,28592765103110,"8536419089",3.3000000000000002E-2]
[110312,"Ex9JM2L05 110VAC","Plug-in relay 5 A, 110 V AC, 2 contatcs","NBH",5.79,0,5.79,8592765103123,20,18592765103120,480,28592765103127,"8536419089",3.3000000000000002E-2]
[110313,"Ex9JM2L05 230VAC","Plug-in relay 5 A, 230 V AC, 2 contatcs","NBH",6.31,0,6.31,8592765103130,20,18592765103137,480,28592765103134,"8536419089",3.3000000000000002E-2]
[110314,"Ex9JM2DZ-05","Socket for plug-in relay 5 A, 2 contacts","NBH",2.23,0,2.23,8592765103147,10,18592765103144,480,28592765103141,"8538909999",3.5000000000000003E-2]
[110315,"Ex9JM4L03 12VDC","Plug-in relay 3 A, 12 V DC, 4 contatcs","NBH",4.12,0,4.12,8592765103154,20,18592765103151,480,28592765103158,"8536419089",3.3000000000000002E-2]
[110316,"Ex9JM4L03 24VDC","Plug-in relay 3 A, 24 V DC, 4 contatcs","NBH",3.76,0,3.76,8592765103161,20,18592765103168,480,28592765103165,"8536419089",3.3000000000000002E-2]
[110317,"Ex9JM4L03 36VDC","Plug-in relay 3 A, 36 V DC, 4 contatcs","NBH",6.37,0,6.37,8592765103178,20,18592765103175,480,28592765103172,"8536419089",3.3000000000000002E-2]
[110318,"Ex9JM4L03 48VDC","Plug-in relay 3 A, 48 V DC, 4 contatcs","NBH",6.5,0,6.5,8592765103185,20,18592765103182,480,28592765103189,"8536419089",3.3000000000000002E-2]
[110319,"Ex9JM4L03 110VDC","Plug-in relay 3 A, 110 V DC, 4 contatcs","NBH",4.59,0,4.59,8592765103192,20,18592765103199,480,28592765103196,"8536419089",3.3000000000000002E-2]
[110320,"Ex9JM4L03 220VDC","Plug-in relay 3 A, 220 V DC, 4 contatcs","NBH",5.29,0,5.29,8592765103208,20,18592765103205,480,28592765103202,"8536419089",3.3000000000000002E-2]
[110321,"Ex9JM4L03 24VAC","Plug-in relay 3 A, 24 V AC, 4 contatcs","NBH",4,0,4,8592765103215,20,18592765103212,480,28592765103219,"8536419089",3.3000000000000002E-2]
[110322,"Ex9JM4L03 36VAC","Plug-in relay 3 A, 36 V AC, 4 contatcs","NBH",6.5,0,6.5,8592765103222,20,18592765103229,480,28592765103226,"8536419089",3.3000000000000002E-2]
[110323,"Ex9JM4L03 48VAC","Plug-in relay 3 A, 48 V AC, 4 contatcs","NBH",6.37,0,6.37,8592765103239,20,18592765103236,480,28592765103233,"8536419089",3.3000000000000002E-2]
[110324,"Ex9JM4L03 110VAC","Plug-in relay 3 A, 110 V AC, 4 contatcs","NBH",6.5,0,6.5,8592765103246,20,18592765103243,480,28592765103240,"8536419089",3.3000000000000002E-2]
[110325,"Ex9JM4L03 230VAC","Plug-in relay 3 A, 230 V AC, 4 contatcs","NBH",4.2300000000000004,0,4.2300000000000004,8592765103253,20,18592765103250,480,28592765103257,"8536419089",3.3000000000000002E-2]
[110326,"Ex9JM4DZ-03","Socket for plug-in relay 3 A, 4 contacts","NBH",2.94,0,2.94,8592765103260,10,18592765103267,300,28592765103264,"8538909999",0.05]
[]
["Monitoring relay Ex9JP"]
[110230,"Ex9JP-1 AC400V ","Monitoring relay, phase failure and phase sequence protection.","NBH",28.97,{"$f":"NBH","v":0},{"$f":"E3700*(1-F3700)","v":28.97},8592765102300,1,18592765102307,90,28592765102304,85364900,0.18099999999999999]
[110231,"Ex9JP-1P AC400V ","Monitoring relay, phase failure and phase sequence with motor temperature protection.","NBH",28.97,{"$f":"NBH","v":0},28.97,8592765102317,1,18592765102314,90,28592765102311,85364900,0.18099999999999999]
[110232,"Ex9JP-2 AC400V ","Monitoring relay, adjustable overvoltage protection with phase failure detection.","NBH",29.6,{"$f":"NBH","v":0},29.6,8592765102324,1,18592765102321,90,28592765102328,85364900,0.18099999999999999]
[110233,"Ex9JP-3 AC400V ","Monitoring relay 3P-3W: Adjustable undervoltage protection with phase failure detection.","NBH",29.6,{"$f":"NBH","v":0},29.6,8592765102331,1,18592765102338,90,28592765102335,85364900,0.18099999999999999]
[110234,"Ex9JP-4 AC400V ","Monitoring relay 3P-3W: Adjustable under/over voltage protection with phase failure detection.","NBH",36.32,{"$f":"NBH","v":0},36.32,8592765102348,1,18592765102345,90,28592765102342,85364900,0.18099999999999999]
[110235,"Ex9JP-5 AC400V ","Monitoring relay 3P-3W: Adjustable under/over voltage protection with phase sequence and phase failure detection.","NBH",36.32,{"$f":"NBH","v":0},36.32,8592765102355,1,18592765102352,90,28592765102359,85364900,0.18099999999999999]
[110236,"Ex9JP-6 AC400V ","Monitoring relay 3P-3W: Adjustable under/over voltage protection, fixed unbalance protection with phase sequence and phase failure detection.","NBH",36.32,{"$f":"NBH","v":0},36.32,8592765102362,1,18592765102369,90,28592765102366,85364900,0.18099999999999999]
[110237,"Ex9JP-6P AC400V ","Monitoring relay 3P-3W: Adjustable under/over voltage protection, fixed unbalance protection with phase sequence, phase failure detection and motor temperature protection.","NBH",42.48,{"$f":"NBH","v":0},42.48,8592765102379,1,18592765102376,90,28592765102373,85364900,0.18099999999999999]
[110238,"Ex9JP-7 AC400V ","Monitoring relay 3P-3W: Fixed under/over voltage protection, adjustable unbalance protection with phase failure and phase sequence detection.","NBH",36.32,{"$f":"NBH","v":0},36.32,8592765102386,1,18592765102383,90,28592765102380,85364900,0.18099999999999999]
[110239,"Ex9JP-7P AC400V ","Monitoring relay 3P-3W: Fixed under/over voltage protection, adjustable unbalance protection with phase failure, phase sequence detection and motor temperature protection.","NBH",42.48,{"$f":"NBH","v":0},42.48,8592765102393,1,18592765102390,90,28592765102397,85364900,0.18099999999999999]
[110240,"Ex9JP-8 AC400V ","Monitoring relay 3P-3W: Adjustable under/over voltage protection, adjustable unbalance protection with phase failure and phase sequence detection.","NBH",51.88,{"$f":"NBH","v":0},51.88,8592765102409,1,18592765102406,90,28592765102403,85364900,0.18099999999999999]
[110241,"Ex9JP-8P AC400V ","Monitoring relay 3P-3W: Adjustable under/over voltage protection, adjustable unbalance protection with phase failure, phase sequence detection and motor temperature protection.","NBH",60.68,{"$f":"NBH","v":0},60.68,8592765102416,1,18592765102413,90,28592765102410,85364900,0.18099999999999999]
[110242,"Ex9JP-9 AC230V ","Monitoring relay 3P/2P/1P-4W: Adjustable overvoltage protection with phase failure detection.","NBH",51.28,{"$f":"NBH","v":0},51.28,8592765102423,1,18592765102420,90,28592765102427,85364900,0.18099999999999999]
[110243,"Ex9JP-10 AC230V ","Monitoring relay 3P/2P/1P-4W: Adjustable undervoltage protection with phase failure detection.","NBH",51.28,{"$f":"NBH","v":0},51.28,8592765102430,1,18592765102437,90,28592765102434,85364900,0.18099999999999999]
[110244,"Ex9JP-11 AC230V ","Monitoring relay 3P/2P/1P-4W: Adjustable under/overvoltage protection with phase failure detection.","NBH",41.39,{"$f":"NBH","v":0},41.39,8592765102447,1,18592765102444,90,28592765102441,85364900,0.18099999999999999]
[110245,"Ex9JP-12 AC230V ","Monitoring relay 3P-4W: Adjustable over/under voltage protection with phase failure and phase sequence detection","NBH",41.39,{"$f":"NBH","v":0},41.39,8592765102454,1,18592765102451,90,28592765102458,85364900,0.18099999999999999]
[110246,"Ex9JP-13 AC230V ","Monitoring relay 3P-4W: Adjustable over/under voltage protection with phase failure and phase sequence detection and fixed fixed unbalance protection.","NBH",46.71,{"$f":"NBH","v":0},46.71,8592765102461,1,18592765102468,90,28592765102465,85364900,0.18099999999999999]
[110247,"Ex9JP-13P AC230V ","Monitoring relay 3P-4W: Adjustable under/over voltage protection, fixed unbalance protection with phase failure and phase sequence detection and motor temeprature protection","NBH",60.68,{"$f":"NBH","v":0},60.68,8592765102478,1,18592765102475,90,28592765102472,85364900,0.18099999999999999]
[110248,"Ex9JP-14 AC230V ","Monitoring relay 3P-4W: Fixed under/over voltage protection,fixed unbalance protection with phase failure and phase sequence detection.","NBH",45.6,{"$f":"NBH","v":0},45.6,8592765102485,1,18592765102482,90,28592765102489,85364900,0.18099999999999999]
[110249,"Ex9JP-14P AC230V ","Monitoring relay 3P-4W: Fixed under/over voltage protection, adjustable unbalance protection with phase failure, phase sequence detection and motor temperature protection.","NBH",60.68,{"$f":"NBH","v":0},60.68,8592765102492,1,18592765102499,90,28592765102496,85364900,0.18099999999999999]
[110250,"Ex9JP-15 AC230V ","Monitoring relay 3P-4W: Adjustable under/over voltage protection, adjustable unbalance protection with phase failure and phase sequence detection.","NBH",59,{"$f":"NBH","v":0},59,8592765102508,1,18592765102505,90,28592765102502,85364900,0.18099999999999999]
[110251,"Ex9JP-15P AC230V ","Monitoring relay 3P-4W: Adjustable under/over voltage protection, adjsutable unbalance protection with phase failure, phase sequence detection and motor temperature protection.","NBH",60.68,{"$f":"NBH","v":0},60.68,8592765102515,1,18592765102512,90,28592765102519,85364900,0.18099999999999999]
[110252,"Ex9JP-16 AC230V ","Monitoring relay 3P-4W: Phase sequence and phase failure detection. ","NBH",42.29,{"$f":"NBH","v":0},42.29,8592765102522,1,18592765102529,90,28592765102526,85364900,0.18099999999999999]
[110253,"Ex9JP-16P AC230V ","Monitoring relay 3P-4W: Phase sequence and phase failure detection with motor temperature protection.","NBH",49.23,{"$f":"NBH","v":0},49.23,8592765102539,1,18592765102536,90,28592765102533,85364900,0.18099999999999999]
[110254,"Ex9JP-17P AC400V ","Monitoring relay 3P-3W: Phase failure and motor temperature protection.","NBH",42.74,{"$f":"NBH","v":0},42.74,8592765102546,1,18592765102543,90,28592765102540,85364900,0.18099999999999999]
[110255,"Ex9JP-18 AC400V","Monitoring relay 3P-3W: Adjustable over/under voltage protection, fixed unbalance protection with phase sequence, phase failure and load end detection","NBH",43.2,{"$f":"NBH","v":0},43.2,8592765102553,1,18592765102550,90,28592765102557,85364900,0.18099999999999999]
[]
["Miniature Contactors Ex9CS"]
[100956,"Ex9CS06  01 3P 415V","Miniature Contactor, 3-pole, 6A AC-3, cont. 415 V AC, 1 NC built-in auxiliary contact","NBA",16.28,{"$f":"NBA","v":0},{"$f":"E3728*(1-F3728)","v":16.28},8592765009579,1,8592765009579,72,28592765009573,"8536490099",0.36]
[100957,"Ex9CS06  01 3P 400V","Miniature Contactor, 3-pole, 6A AC-3, cont. 400 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009586,1,8592765009586,72,28592765009580,"8536490099",0.36]
[100958,"Ex9CS06  01 3P 380V","Miniature Contactor, 3-pole, 6A AC-3, cont. 380 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009593,1,8592765009593,72,28592765009597,"8536490099",0.36]
[100959,"Ex9CS06  01 3P 240V","Miniature Contactor, 3-pole, 6A AC-3, cont. 240 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009609,1,8592765009609,72,28592765009603,"8536490099",0.36]
[100960,"Ex9CS06  01 3P 230V","Miniature Contactor, 3-pole, 6A AC-3, cont. 230 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009616,1,8592765009616,72,28592765009610,"8536490099",0.36]
[100961,"Ex9CS06  01 3P 220V","Miniature Contactor, 3-pole, 6A AC-3, cont. 220 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009623,1,8592765009623,72,28592765009627,"8536490099",0.36]
[100962,"Ex9CS06  01 3P 127V","Miniature Contactor, 3-pole, 6A AC-3, cont. 127 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009630,1,8592765009630,72,28592765009634,"8536490099",0.36]
[100963,"Ex9CS06  01 3P 110V ","Miniature Contactor, 3-pole, 6A AC-3, cont. 110 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009647,1,8592765009647,72,28592765009641,"8536490099",0.36]
[100964,"Ex9CS06  01 3P 48V","Miniature Contactor, 3-pole, 6A AC-3, cont. 48 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009654,1,8592765009654,72,28592765009658,"8536419089",0.36]
[100965,"Ex9CS06  01 3P 42V","Miniature Contactor, 3-pole, 6A AC-3, cont. 42 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009661,1,8592765009661,72,28592765009665,"8536419089",0.36]
[100966,"Ex9CS06  01 3P 36V ","Miniature Contactor, 3-pole, 6A AC-3, cont. 36 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009678,1,8592765009678,72,28592765009672,"8536419089",0.36]
[100967,"Ex9CS06  01 3P 24V ","Miniature Contactor, 3-pole, 6A AC-3, cont. 24 V AC, 1 NC built-in auxiliary contact","NBA",16.28,0,16.28,8592765009685,1,8592765009685,72,28592765009689,"8536419089",0.36]
[100968,"Ex9CS06  10 3P 415V","Miniature Contactor, 3-pole, 6A AC-3, cont. 415 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009692,1,8592765009692,72,28592765009696,"8536490099",0.36]
[100969,"Ex9CS06  10 3P 400V","Miniature Contactor, 3-pole, 6A AC-3, cont. 400 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009708,1,8592765009708,72,28592765009702,"8536490099",0.36]
[100970,"Ex9CS06  10 3P 380V","Miniature Contactor, 3-pole, 6A AC-3, cont. 380 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009715,1,8592765009715,72,28592765009719,"8536490099",0.36]
[100971,"Ex9CS06  10 3P 240V","Miniature Contactor, 3-pole, 6A AC-3, cont. 240 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009722,1,8592765009722,72,28592765009726,"8536490099",0.36]
[100972,"Ex9CS06  10 3P 230V","Miniature Contactor, 3-pole, 6A AC-3, cont. 230 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009739,1,8592765009739,72,28592765009733,"8536490099",0.36]
[100973,"Ex9CS06  10 3P 220V","Miniature Contactor, 3-pole, 6A AC-3, cont. 220 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009746,1,8592765009746,72,28592765009740,"8536490099",0.36]
[100974,"Ex9CS06  10 3P 127V","Miniature Contactor, 3-pole, 6A AC-3, cont. 127 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009753,1,8592765009753,72,28592765009757,"8536490099",0.36]
[100975,"Ex9CS06  10 3P 110V ","Miniature Contactor, 3-pole, 6A AC-3, cont. 110 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009760,1,8592765009760,72,28592765009764,"8536490099",0.36]
[100976,"Ex9CS06  10 3P 48V","Miniature Contactor, 3-pole, 6A AC-3, cont. 48 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009777,1,8592765009777,72,28592765009771,"8536419089",0.36]
[100977,"Ex9CS06  10 3P 42V","Miniature Contactor, 3-pole, 6A AC-3, cont. 42 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009784,1,8592765009784,72,28592765009788,"8536419089",0.36]
[100978,"Ex9CS06  10 3P 36V ","Miniature Contactor, 3-pole, 6A AC-3, cont. 36 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009791,1,8592765009791,72,28592765009795,"8536419089",0.36]
[100979,"Ex9CS06  10 3P 24V ","Miniature Contactor, 3-pole, 6A AC-3, cont. 24 V AC, 1 NO built-in auxiliary contact","NBA",16.28,0,16.28,8592765009807,1,8592765009807,72,28592765009801,"8536419089",0.36]
[100980,"Ex9CS06   4P 415V","Miniature Contactor, 4-pole, 6A AC-3, cont. 415 V AC","NBA",27.9,0,27.9,8592765009814,1,8592765009814,72,28592765009818,"8536490099",0.36]
[100981,"Ex9CS06   4P 400V","Miniature Contactor, 4-pole, 6A AC-3, cont. 400 V AC","NBA",27.9,0,27.9,8592765009821,1,8592765009821,72,28592765009825,"8536490099",0.36]
[100982,"Ex9CS06   4P 380V","Miniature Contactor, 4-pole, 6A AC-3, cont. 380 V AC","NBA",27.9,0,27.9,8592765009838,1,8592765009838,72,28592765009832,"8536490099",0.36]
[100983,"Ex9CS06   4P 240V","Miniature Contactor, 4-pole, 6A AC-3, cont. 240 V AC","NBA",27.9,0,27.9,8592765009845,1,8592765009845,72,28592765009849,"8536490099",0.36]
[100984,"Ex9CS06   4P 230V","Miniature Contactor, 4-pole, 6A AC-3, cont. 230 V AC","NBA",27.9,0,27.9,8592765009852,1,8592765009852,72,28592765009856,"8536490099",0.36]
[100985,"Ex9CS06   4P 220V","Miniature Contactor, 4-pole, 6A AC-3, cont. 220 V AC","NBA",27.9,0,27.9,8592765009869,1,8592765009869,72,28592765009863,"8536490099",0.36]
[100986,"Ex9CS06   4P 127V","Miniature Contactor, 4-pole, 6A AC-3, cont. 127 V AC","NBA",27.9,0,27.9,8592765009876,1,8592765009876,72,28592765009870,"8536490099",0.36]
[100987,"Ex9CS06   4P 110V ","Miniature Contactor, 4-pole, 6A AC-3, cont. 110 V AC","NBA",27.9,0,27.9,8592765009883,1,8592765009883,72,28592765009887,"8536490099",0.36]
[100988,"Ex9CS06   4P 48V","Miniature Contactor, 4-pole, 6A AC-3, cont. 48 V AC","NBA",27.9,{"$f":"NBA","v":0},27.9,8592765009890,1,8592765009890,72,28592765009894,"8536419089",0.36]
[100989,"Ex9CS06   4P 42V","Miniature Contactor, 4-pole, 6A AC-3, cont. 42 V AC","NBA",27.9,0,27.9,8592765009906,1,8592765009906,72,28592765009900,"8536419089",0.36]
[100990,"Ex9CS06   4P 36V ","Miniature Contactor, 4-pole, 6A AC-3, cont. 36 V AC","NBA",27.9,0,27.9,8592765009913,1,8592765009913,72,28592765009917,"8536419089",0.36]
[100991,"Ex9CS06   4P 24V ","Miniature Contactor, 4-pole, 6A AC-3, cont. 24 V AC","NBA",27.9,0,27.9,8592765009920,1,8592765009920,72,28592765009924,"8536419089",0.36]
[100992,"Ex9CS06   4P/22 415V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 415 V AC","NBA",33.81,0,33.81,8592765009937,1,8592765009937,72,28592765009931,"8536490099",0.36]
[100993,"Ex9CS06   4P/22 400V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 400 V AC","NBA",33.81,0,33.81,8592765009944,1,8592765009944,72,28592765009948,"8536490099",0.36]
[100994,"Ex9CS06   4P/22 380V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 380 V AC","NBA",33.81,0,33.81,8592765009951,1,8592765009951,72,28592765009955,"8536490099",0.36]
[100995,"Ex9CS06   4P/22 240V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 240 V AC","NBA",33.81,0,33.81,8592765009968,1,8592765009968,72,28592765009962,"8536490099",0.36]
[100996,"Ex9CS06   4P/22 230V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 230 V AC","NBA",33.81,0,33.81,8592765009975,1,8592765009975,72,28592765009979,"8536490099",0.36]
[100997,"Ex9CS06   4P/22 220V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 220 V AC","NBA",33.81,0,33.81,8592765009982,1,8592765009982,72,28592765009986,"8536490099",0.36]
[100998,"Ex9CS06   4P/22 127V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 127 V AC","NBA",33.81,0,33.81,8592765009999,1,8592765009999,72,28592765009993,"8536490099",0.36]
[100999,"Ex9CS06   4P/22 110V ","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 110 V AC","NBA",33.81,0,33.81,8592765010001,1,8592765010001,72,28592765010005,"8536490099",0.36]
[101000,"Ex9CS06   4P/22 48V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 48 V AC","NBA",33.81,0,33.81,8592765010018,1,8592765010018,72,28592765010012,"8536419089",0.36]
[101001,"Ex9CS06   4P/22 42V","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 42 V AC","NBA",33.81,0,33.81,8592765010025,1,8592765010025,72,28592765010029,"8536419089",0.36]
[101002,"Ex9CS06   4P/22 36V ","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 36 V AC","NBA",33.81,0,33.81,8592765010032,1,8592765010032,72,28592765010036,"8536419089",0.36]
[101003,"Ex9CS06   4P/22 24V ","Miniature Contactor, 4-pole, shifting 2+2, 6A AC-3, cont. 24 V AC","NBA",33.81,0,33.81,8592765010049,1,8592765010049,72,28592765010043,"8536419089",0.36]
[101004,"Ex9CS09  01 3P 415V","Miniature Contactor, 3-pole, 9A AC-3, cont. 415 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010056,1,8592765010056,72,28592765010050,"8536490099",0.36]
[101005,"Ex9CS09  01 3P 400V","Miniature Contactor, 3-pole, 9A AC-3, cont. 400 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010063,1,8592765010063,72,28592765010067,"8536490099",0.36]
[101006,"Ex9CS09  01 3P 380V","Miniature Contactor, 3-pole, 9A AC-3, cont. 380 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010070,1,8592765010070,72,28592765010074,"8536490099",0.36]
[101007,"Ex9CS09  01 3P 240V","Miniature Contactor, 3-pole, 9A AC-3, cont. 240 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010087,1,8592765010087,72,28592765010081,"8536490099",0.36]
[101008,"Ex9CS09  01 3P 230V","Miniature Contactor, 3-pole, 9A AC-3, cont. 230 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010094,1,8592765010094,72,28592765010098,"8536490099",0.36]
[101009,"Ex9CS09  01 3P 220V","Miniature Contactor, 3-pole, 9A AC-3, cont. 220 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010100,1,8592765010100,72,28592765010104,"8536490099",0.36]
[101010,"Ex9CS09  01 3P 127V","Miniature Contactor, 3-pole, 9A AC-3, cont. 127 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010117,1,8592765010117,72,28592765010111,"8536490099",0.36]
[101011,"Ex9CS09  01 3P 110V ","Miniature Contactor, 3-pole, 9A AC-3, cont. 110 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010124,1,8592765010124,72,28592765010128,"8536490099",0.36]
[101012,"Ex9CS09  01 3P 48V","Miniature Contactor, 3-pole, 9A AC-3, cont. 48 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010131,1,8592765010131,72,28592765010135,"8536419089",0.36]
[101013,"Ex9CS09  01 3P 42V","Miniature Contactor, 3-pole, 9A AC-3, cont. 42 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010148,1,8592765010148,72,28592765010142,"8536419089",0.36]
[101014,"Ex9CS09  01 3P 36V ","Miniature Contactor, 3-pole, 9A AC-3, cont. 36 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010155,1,8592765010155,72,28592765010159,"8536419089",0.36]
[101015,"Ex9CS09  01 3P 24V ","Miniature Contactor, 3-pole, 9A AC-3, cont. 24 V AC, 1 NC built-in auxiliary contact","NBA",17.52,0,17.52,8592765010162,1,8592765010162,72,28592765010166,"8536419089",0.36]
[101016,"Ex9CS09  10 3P 415V","Miniature Contactor, 3-pole, 9A AC-3, cont. 415 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010179,1,8592765010179,72,28592765010173,"8536490099",0.36]
[101017,"Ex9CS09  10 3P 400V","Miniature Contactor, 3-pole, 9A AC-3, cont. 400 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010186,1,8592765010186,72,28592765010180,"8536490099",0.36]
[101018,"Ex9CS09  10 3P 380V","Miniature Contactor, 3-pole, 9A AC-3, cont. 380 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010193,1,8592765010193,72,28592765010197,"8536490099",0.36]
[101019,"Ex9CS09  10 3P 240V","Miniature Contactor, 3-pole, 9A AC-3, cont. 240 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010209,1,8592765010209,72,28592765010203,"8536490099",0.36]
[101020,"Ex9CS09  10 3P 230V","Miniature Contactor, 3-pole, 9A AC-3, cont. 230 V AC, 1 NO built-in auxiliary contact","NBA",17.52,{"$f":"NBA","v":0},{"$f":"E3792*(1-F3792)","v":17.52},8592765010216,1,8592765010216,72,28592765010210,"8536490099",0.36]
[101021,"Ex9CS09  10 3P 220V","Miniature Contactor, 3-pole, 9A AC-3, cont. 220 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010223,1,8592765010223,72,28592765010227,"8536490099",0.36]
[101022,"Ex9CS09  10 3P 127V","Miniature Contactor, 3-pole, 9A AC-3, cont. 127 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010230,1,8592765010230,72,28592765010234,"8536490099",0.36]
[101023,"Ex9CS09  10 3P 110V ","Miniature Contactor, 3-pole, 9A AC-3, cont. 110 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010247,1,8592765010247,72,28592765010241,"8536490099",0.36]
[101024,"Ex9CS09  10 3P 48V","Miniature Contactor, 3-pole, 9A AC-3, cont. 48 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010254,1,8592765010254,72,28592765010258,"8536419089",0.36]
[101025,"Ex9CS09  10 3P 42V","Miniature Contactor, 3-pole, 9A AC-3, cont. 42 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010261,1,8592765010261,72,28592765010265,"8536419089",0.36]
[101026,"Ex9CS09  10 3P 36V ","Miniature Contactor, 3-pole, 9A AC-3, cont. 36 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010278,1,8592765010278,72,28592765010272,"8536419089",0.36]
[101027,"Ex9CS09  10 3P 24V ","Miniature Contactor, 3-pole, 9A AC-3, cont. 24 V AC, 1 NO built-in auxiliary contact","NBA",17.52,0,17.52,8592765010285,1,8592765010285,72,28592765010289,"8536419089",0.36]
[101028,"Ex9CS09   4P 415V","Miniature Contactor, 4-pole, 9A AC-3, cont. 415 V AC","NBA",30.11,0,30.11,8592765010292,1,8592765010292,72,28592765010296,"8536490099",0.36]
[101029,"Ex9CS09   4P 400V","Miniature Contactor, 4-pole, 9A AC-3, cont. 400 V AC","NBA",30.11,0,30.11,8592765010308,1,8592765010308,72,28592765010302,"8536490099",0.36]
[101030,"Ex9CS09   4P 380V","Miniature Contactor, 4-pole, 9A AC-3, cont. 380 V AC","NBA",30.11,0,30.11,8592765010315,1,8592765010315,72,28592765010319,"8536490099",0.36]
[101031,"Ex9CS09   4P 240V","Miniature Contactor, 4-pole, 9A AC-3, cont. 240 V AC","NBA",30.11,0,30.11,8592765010322,1,8592765010322,72,28592765010326,"8536490099",0.36]
[101032,"Ex9CS09   4P 230V","Miniature Contactor, 4-pole, 9A AC-3, cont. 230 V AC","NBA",30.11,0,30.11,8592765010339,1,8592765010339,72,28592765010333,"8536490099",0.36]
[101033,"Ex9CS09   4P 220V","Miniature Contactor, 4-pole, 9A AC-3, cont. 220 V AC","NBA",30.11,0,30.11,8592765010346,1,8592765010346,72,28592765010340,"8536490099",0.36]
[101034,"Ex9CS09   4P 127V","Miniature Contactor, 4-pole, 9A AC-3, cont. 127 V AC","NBA",30.11,0,30.11,8592765010353,1,8592765010353,72,28592765010357,"8536490099",0.36]
[101035,"Ex9CS09   4P 110V ","Miniature Contactor, 4-pole, 9A AC-3, cont. 110 V AC","NBA",30.11,0,30.11,8592765010360,1,8592765010360,72,28592765010364,"8536490099",0.36]
[101036,"Ex9CS09   4P 48V","Miniature Contactor, 4-pole, 9A AC-3, cont. 48 V AC","NBA",30.11,0,30.11,8592765010377,1,8592765010377,72,28592765010371,"8536419089",0.36]
[101037,"Ex9CS09   4P 42V","Miniature Contactor, 4-pole, 9A AC-3, cont. 42 V AC","NBA",30.11,0,30.11,8592765010384,1,8592765010384,72,28592765010388,"8536419089",0.36]
[101038,"Ex9CS09   4P 36V ","Miniature Contactor, 4-pole, 9A AC-3, cont. 36 V AC","NBA",30.11,0,30.11,8592765010391,1,8592765010391,72,28592765010395,"8536419089",0.36]
[101039,"Ex9CS09   4P 24V ","Miniature Contactor, 4-pole, 9A AC-3, cont. 24 V AC","NBA",30.11,0,30.11,8592765010407,1,8592765010407,72,28592765010401,"8536419089",0.36]
[101040,"Ex9CS09   4P/22 415V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 415 V AC","NBA",36.25,0,36.25,8592765010414,1,8592765010414,72,28592765010418,"8536490099",0.36]
[101041,"Ex9CS09   4P/22 400V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 400 V AC","NBA",36.25,0,36.25,8592765010421,1,8592765010421,72,28592765010425,"8536490099",0.36]
[101042,"Ex9CS09   4P/22 380V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 380 V AC","NBA",36.25,0,36.25,8592765010438,1,8592765010438,72,28592765010432,"8536490099",0.36]
[101043,"Ex9CS09   4P/22 240V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 240 V AC","NBA",36.25,0,36.25,8592765010445,1,8592765010445,72,28592765010449,"8536490099",0.36]
[101044,"Ex9CS09   4P/22 230V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 230 V AC","NBA",36.25,0,36.25,8592765010452,1,8592765010452,72,28592765010456,"8536490099",0.36]
[101045,"Ex9CS09   4P/22 220V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 220 V AC","NBA",36.25,0,36.25,8592765010469,1,8592765010469,72,28592765010463,"8536490099",0.36]
[101046,"Ex9CS09   4P/22 127V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 127 V AC","NBA",36.25,0,36.25,8592765010476,1,8592765010476,72,28592765010470,"8536490099",0.36]
[101047,"Ex9CS09   4P/22 110V ","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 110 V AC","NBA",36.25,0,36.25,8592765010483,1,8592765010483,72,28592765010487,"8536490099",0.36]
[101048,"Ex9CS09   4P/22 48V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 48 V AC","NBA",36.25,0,36.25,8592765010490,1,8592765010490,72,28592765010494,"8536419089",0.36]
[101049,"Ex9CS09   4P/22 42V","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 42 V AC","NBA",36.25,0,36.25,8592765010506,1,8592765010506,72,28592765010500,"8536419089",0.36]
[101050,"Ex9CS09   4P/22 36V ","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 36 V AC","NBA",36.25,0,36.25,8592765010513,1,8592765010513,72,28592765010517,"8536419089",0.36]
[101051,"Ex9CS09   4P/22 24V ","Miniature Contactor, 4-pole, shifting 2+2, 9A AC-3, cont. 24 V AC","NBA",36.25,0,36.25,8592765010520,1,8592765010520,72,28592765010524,"8536419089",0.36]
[101052,"Ex9CS12  01 3P 415V","Miniature Contactor, 3-pole, 12A AC-3, cont. 415 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,{"$f":"NBA","v":0},18.510000000000002,8592765010537,1,8592765010537,72,28592765010531,"8536490099",0.36]
[101053,"Ex9CS12  01 3P 400V","Miniature Contactor, 3-pole, 12A AC-3, cont. 400 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010544,1,8592765010544,72,28592765010548,"8536490099",0.36]
[101054,"Ex9CS12  01 3P 380V","Miniature Contactor, 3-pole, 12A AC-3, cont. 380 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010551,1,8592765010551,72,28592765010555,"8536490099",0.36]
[101055,"Ex9CS12  01 3P 240V","Miniature Contactor, 3-pole, 12A AC-3, cont. 240 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010568,1,8592765010568,72,28592765010562,"8536490099",0.36]
[101056,"Ex9CS12  01 3P 230V","Miniature Contactor, 3-pole, 12A AC-3, cont. 230 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010575,1,8592765010575,72,28592765010579,"8536490099",0.36]
[101057,"Ex9CS12  01 3P 220V","Miniature Contactor, 3-pole, 12A AC-3, cont. 220 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010582,1,8592765010582,72,28592765010586,"8536490099",0.36]
[101058,"Ex9CS12  01 3P 127V","Miniature Contactor, 3-pole, 12A AC-3, cont. 127 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010599,1,8592765010599,72,28592765010593,"8536490099",0.36]
[101059,"Ex9CS12  01 3P 110V ","Miniature Contactor, 3-pole, 12A AC-3, cont. 110 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010605,1,8592765010605,72,28592765010609,"8536490099",0.36]
[101060,"Ex9CS12  01 3P 48V","Miniature Contactor, 3-pole, 12A AC-3, cont. 48 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010612,1,8592765010612,72,28592765010616,"8536419089",0.36]
[101061,"Ex9CS12  01 3P 42V","Miniature Contactor, 3-pole, 12A AC-3, cont. 42 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010629,1,8592765010629,72,28592765010623,"8536419089",0.36]
[101062,"Ex9CS12  01 3P 36V ","Miniature Contactor, 3-pole, 12A AC-3, cont. 36 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010636,1,8592765010636,72,28592765010630,"8536419089",0.36]
[101063,"Ex9CS12  01 3P 24V ","Miniature Contactor, 3-pole, 12A AC-3, cont. 24 V AC, 1 NC built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010643,1,8592765010643,72,28592765010647,"8536419089",0.36]
[101064,"Ex9CS12  10 3P 415V","Miniature Contactor, 3-pole, 12A AC-3, cont. 415 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010650,1,8592765010650,72,28592765010654,"8536490099",0.36]
[101065,"Ex9CS12  10 3P 400V","Miniature Contactor, 3-pole, 12A AC-3, cont. 400 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010667,1,8592765010667,72,28592765010661,"8536490099",0.36]
[101066,"Ex9CS12  10 3P 380V","Miniature Contactor, 3-pole, 12A AC-3, cont. 380 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010674,1,8592765010674,72,28592765010678,"8536490099",0.36]
[101067,"Ex9CS12  10 3P 240V","Miniature Contactor, 3-pole, 12A AC-3, cont. 240 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010681,1,8592765010681,72,28592765010685,"8536490099",0.36]
[101068,"Ex9CS12  10 3P 230V","Miniature Contactor, 3-pole, 12A AC-3, cont. 230 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010698,1,8592765010698,72,28592765010692,"8536490099",0.36]
[101069,"Ex9CS12  10 3P 220V","Miniature Contactor, 3-pole, 12A AC-3, cont. 220 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010704,1,8592765010704,72,28592765010708,"8536490099",0.36]
[101070,"Ex9CS12  10 3P 127V","Miniature Contactor, 3-pole, 12A AC-3, cont. 127 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010711,1,8592765010711,72,28592765010715,"8536490099",0.36]
[101071,"Ex9CS12  10 3P 110V ","Miniature Contactor, 3-pole, 12A AC-3, cont. 110 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010728,1,8592765010728,72,28592765010722,"8536490099",0.36]
[101072,"Ex9CS12  10 3P 48V","Miniature Contactor, 3-pole, 12A AC-3, cont. 48 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010735,1,8592765010735,72,28592765010739,"8536419089",0.36]
[101073,"Ex9CS12  10 3P 42V","Miniature Contactor, 3-pole, 12A AC-3, cont. 42 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010742,1,8592765010742,72,28592765010746,"8536419089",0.36]
[101074,"Ex9CS12  10 3P 36V ","Miniature Contactor, 3-pole, 12A AC-3, cont. 36 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010759,1,8592765010759,72,28592765010753,"8536419089",0.36]
[101075,"Ex9CS12  10 3P 24V ","Miniature Contactor, 3-pole, 12A AC-3, cont. 24 V AC, 1 NO built-in auxiliary contact","NBA",18.510000000000002,0,18.510000000000002,8592765010766,1,8592765010766,72,28592765010760,"8536419089",0.36]
[101076,"Ex9CS12   4P 415V","Miniature Contactor, 4-pole, 12A AC-3, cont. 415 V AC","NBA",25.54,0,25.54,8592765010773,1,8592765010773,72,28592765010777,"8536490099",0.36]
[101077,"Ex9CS12   4P 400V","Miniature Contactor, 4-pole, 12A AC-3, cont. 400 V AC","NBA",25.54,0,25.54,8592765010780,1,8592765010780,72,28592765010784,"8536490099",0.36]
[101078,"Ex9CS12   4P 380V","Miniature Contactor, 4-pole, 12A AC-3, cont. 380 V AC","NBA",25.54,0,25.54,8592765010797,1,8592765010797,72,28592765010791,"8536490099",0.36]
[101079,"Ex9CS12   4P 240V","Miniature Contactor, 4-pole, 12A AC-3, cont. 240 V AC","NBA",25.54,0,25.54,8592765010803,1,8592765010803,72,28592765010807,"8536490099",0.36]
[101080,"Ex9CS12   4P 230V","Miniature Contactor, 4-pole, 12A AC-3, cont. 230 V AC","NBA",25.54,0,25.54,8592765010810,1,8592765010810,72,28592765010814,"8536490099",0.36]
[101081,"Ex9CS12   4P 220V","Miniature Contactor, 4-pole, 12A AC-3, cont. 220 V AC","NBA",25.54,0,25.54,8592765010827,1,8592765010827,72,28592765010821,"8536490099",0.36]
[101082,"Ex9CS12   4P 127V","Miniature Contactor, 4-pole, 12A AC-3, cont. 127 V AC","NBA",25.54,0,25.54,8592765010834,1,8592765010834,72,28592765010838,"8536490099",0.36]
[101083,"Ex9CS12   4P 110V ","Miniature Contactor, 4-pole, 12A AC-3, cont. 110 V AC","NBA",25.54,0,25.54,8592765010841,1,8592765010841,72,28592765010845,"8536490099",0.36]
[101084,"Ex9CS12   4P 48V","Miniature Contactor, 4-pole, 12A AC-3, cont. 48 V AC","NBA",25.54,{"$f":"NBA","v":0},{"$f":"E3856*(1-F3856)","v":25.54},8592765010858,1,8592765010858,72,28592765010852,"8536419089",0.36]
[101085,"Ex9CS12   4P 42V","Miniature Contactor, 4-pole, 12A AC-3, cont. 42 V AC","NBA",25.54,0,25.54,8592765010865,1,8592765010865,72,28592765010869,"8536419089",0.36]
[101086,"Ex9CS12   4P 36V ","Miniature Contactor, 4-pole, 12A AC-3, cont. 36 V AC","NBA",25.54,0,25.54,8592765010872,1,8592765010872,72,28592765010876,"8536419089",0.36]
[101087,"Ex9CS12   4P 24V ","Miniature Contactor, 4-pole, 12A AC-3, cont. 24 V AC","NBA",25.54,0,25.54,8592765010889,1,8592765010889,72,28592765010883,"8536419089",0.36]
[101088,"Ex9CS12   4P/22 415V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 415 V AC","NBA",30.71,0,30.71,8592765010896,1,8592765010896,72,28592765010890,"8536490099",0.36]
[101089,"Ex9CS12   4P/22 400V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 400 V AC","NBA",30.71,0,30.71,8592765010902,1,8592765010902,72,28592765010906,"8536490099",0.36]
[101090,"Ex9CS12   4P/22 380V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 380 V AC","NBA",30.71,0,30.71,8592765010919,1,8592765010919,72,28592765010913,"8536490099",0.36]
[101091,"Ex9CS12   4P/22 240V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 240 V AC","NBA",30.71,0,30.71,8592765010926,1,8592765010926,72,28592765010920,"8536490099",0.36]
[101092,"Ex9CS12   4P/22 230V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 230 V AC","NBA",30.71,0,30.71,8592765010933,1,8592765010933,72,28592765010937,"8536490099",0.36]
[101093,"Ex9CS12   4P/22 220V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 220 V AC","NBA",30.71,0,30.71,8592765010940,1,8592765010940,72,28592765010944,"8536490099",0.36]
[101094,"Ex9CS12   4P/22 127V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 127 V AC","NBA",30.71,0,30.71,8592765010957,1,8592765010957,72,28592765010951,"8536490099",0.36]
[101095,"Ex9CS12   4P/22 110V ","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 110 V AC","NBA",30.71,0,30.71,8592765010964,1,8592765010964,72,28592765010968,"8536490099",0.36]
[101096,"Ex9CS12   4P/22 48V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 48 V AC","NBA",30.71,0,30.71,8592765010971,1,8592765010971,72,28592765010975,"8536419089",0.36]
[101097,"Ex9CS12   4P/22 42V","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 42 V AC","NBA",30.71,0,30.71,8592765010988,1,8592765010988,72,28592765010982,"8536419089",0.36]
[101098,"Ex9CS12   4P/22 36V ","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 36 V AC","NBA",30.71,0,30.71,8592765010995,1,8592765010995,72,28592765010999,"8536419089",0.36]
[101099,"Ex9CS12   4P/22 24V ","Miniature Contactor, 4-pole, shifting 2+2, 12A AC-3, cont. 24 V AC","NBA",30.71,0,30.71,8592765011008,1,8592765011008,72,28592765011002,"8536419089",0.36]
[]
["Reversible Miniature contactors Ex9CSR"]
[104504,"Ex9CSR06 10 3P 48V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 48 V AC, 1 NO built-in auxiliary contact","NBA",60.5,{"$f":"NBA","v":0},{"$f":"E3874*(1-F3874)","v":60.5},8592765045058,1,8592765045058,null,28592765045052,"8536419089",0.37]
[104505,"Ex9CSR06 10 3P 42V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 42 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,{"$f":"E3875*(1-F3875)","v":60.5},8592765045065,1,8592765045065,null,28592765045069,"8536419089",0.37]
[104506,"Ex9CSR06 10 3P 415V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 415 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045072,1,8592765045072,null,28592765045076,"8536490099",0.37]
[104507,"Ex9CSR06 10 3P 400V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 400 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045089,1,8592765045089,null,28592765045083,"8536490099",0.37]
[104508,"Ex9CSR06 10 3P 380V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 380 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045096,1,8592765045096,null,28592765045090,"8536490099",0.37]
[104509,"Ex9CSR06 10 3P 36V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 36 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045102,1,8592765045102,null,28592765045106,"8536419089",0.37]
[104510,"Ex9CSR06 10 3P 24V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 24 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045119,1,8592765045119,null,28592765045113,"8536419089",0.37]
[104511,"Ex9CSR06 10 3P 240V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 240 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045126,1,8592765045126,null,28592765045120,"8536490099",0.37]
[104512,"Ex9CSR06 10 3P 230V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 230 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045133,1,8592765045133,null,28592765045137,"8536490099",0.37]
[104513,"Ex9CSR06 10 3P 220V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 220 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045140,1,8592765045140,null,28592765045144,"8536490099",0.37]
[104514,"Ex9CSR06 10 3P 127V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 127 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045157,1,8592765045157,null,28592765045151,"8536490099",0.37]
[104515,"Ex9CSR06 10 3P 110V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 110 V AC, 1 NO built-in auxiliary contact","NBA",60.5,0,60.5,8592765045164,1,8592765045164,null,28592765045168,"8536490099",0.37]
[104516,"Ex9CSR06 01 3P 48V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 48 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045171,1,8592765045171,null,28592765045175,"8536419089",0.37]
[104517,"Ex9CSR06 01 3P 42V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 42 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045188,1,8592765045188,null,28592765045182,"8536419089",0.37]
[104518,"Ex9CSR06 01 3P 415V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 415 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045195,1,8592765045195,null,28592765045199,"8536490099",0.37]
[104519,"Ex9CSR06 01 3P 400V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 400 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045201,1,8592765045201,null,28592765045205,"8536490099",0.37]
[104520,"Ex9CSR06 01 3P 380V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 380 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045218,1,8592765045218,null,28592765045212,"8536490099",0.37]
[104521,"Ex9CSR06 01 3P 36V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 36 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045225,1,8592765045225,null,28592765045229,"8536419089",0.37]
[104522,"Ex9CSR06 01 3P 24V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 24 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045232,1,8592765045232,null,28592765045236,"8536419089",0.37]
[104523,"Ex9CSR06 01 3P 240V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 240 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045249,1,8592765045249,null,28592765045243,"8536490099",0.37]
[104524,"Ex9CSR06 01 3P 230V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 230 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045256,1,8592765045256,null,28592765045250,"8536490099",0.37]
[104525,"Ex9CSR06 01 3P 220V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 220 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045263,1,8592765045263,null,28592765045267,"8536490099",0.37]
[104526,"Ex9CSR06 01 3P 127V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 127 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045270,1,8592765045270,null,28592765045274,"8536490099",0.37]
[104527,"Ex9CSR06 01 3P 110V","Reversible miniature contactor, 3-pole, 6A AC-3, cont. 110 V AC, 1 NC built-in auxiliary contact","NBA",60.5,0,60.5,8592765045287,1,8592765045287,null,28592765045281,"8536490099",0.37]
[104528,"Ex9CSR06  4P/22 48V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 48 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045294,1,8592765045294,null,28592765045298,"8536419089",0.37]
[104529,"Ex9CSR06  4P/22 42V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 42 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045300,1,8592765045300,null,28592765045304,"8536419089",0.37]
[104530,"Ex9CSR06  4P/22 415V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 415 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045317,1,8592765045317,null,28592765045311,"8536490099",0.37]
[104531,"Ex9CSR06  4P/22 400V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 400 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045324,1,8592765045324,null,28592765045328,"8536490099",0.37]
[104532,"Ex9CSR06  4P/22 380V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 380 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045331,1,8592765045331,null,28592765045335,"8536490099",0.37]
[104533,"Ex9CSR06  4P/22 36V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 36 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045348,1,8592765045348,null,28592765045342,"8536419089",0.37]
[104534,"Ex9CSR06  4P/22 24V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 24 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045355,1,8592765045355,null,28592765045359,"8536419089",0.37]
[104535,"Ex9CSR06  4P/22 240V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 240 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045362,1,8592765045362,null,28592765045366,"8536490099",0.37]
[104536,"Ex9CSR06  4P/22 230V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 230 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,{"$f":"NBA","v":0},66.569999999999993,8592765045379,1,8592765045379,null,28592765045373,"8536490099",0.37]
[104537,"Ex9CSR06  4P/22 220V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 220 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045386,1,8592765045386,null,28592765045380,"8536490099",0.37]
[104538,"Ex9CSR06  4P/22 127V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 127 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045393,1,8592765045393,null,28592765045397,"8536490099",0.37]
[104539,"Ex9CSR06  4P/22 110V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 110 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",66.569999999999993,0,66.569999999999993,8592765045409,1,8592765045409,null,28592765045403,"8536490099",0.37]
[104540,"Ex9CSR06  4P 48V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 48 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045416,1,8592765045416,null,28592765045410,"8536419089",0.37]
[104541,"Ex9CSR06  4P 42V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 42 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045423,1,8592765045423,null,28592765045427,"8536419089",0.37]
[104542,"Ex9CSR06  4P 415V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 415 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045430,1,8592765045430,null,28592765045434,"8536490099",0.37]
[104543,"Ex9CSR06  4P 400V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 400 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045447,1,8592765045447,null,28592765045441,"8536490099",0.37]
[104544,"Ex9CSR06  4P 380V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 380 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045454,1,8592765045454,null,28592765045458,"8536490099",0.37]
[104545,"Ex9CSR06  4P 36V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 36 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045461,1,8592765045461,null,28592765045465,"8536419089",0.37]
[104546,"Ex9CSR06  4P 24V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 24 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045478,1,8592765045478,null,28592765045472,"8536419089",0.37]
[104547,"Ex9CSR06  4P 240V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 240 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045485,1,8592765045485,null,28592765045489,"8536490099",0.37]
[104548,"Ex9CSR06  4P 230V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 230 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045492,1,8592765045492,null,28592765045496,"8536490099",0.37]
[104549,"Ex9CSR06  4P 220V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 220 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045508,1,8592765045508,null,28592765045502,"8536490099",0.37]
[104550,"Ex9CSR06  4P 127V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 127 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045515,1,8592765045515,null,28592765045519,"8536490099",0.37]
[104551,"Ex9CSR06  4P 110V","Reversible miniature contactor, 4-pole, 6A AC-3, cont. 110 V AC","NBA",66.569999999999993,0,66.569999999999993,8592765045522,1,8592765045522,null,28592765045526,"8536490099",0.37]
[104552,"Ex9CSR09 10 3P 48V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 48 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045539,1,8592765045539,null,28592765045533,"8536419089",0.37]
[104553,"Ex9CSR09 10 3P 42V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 42 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045546,1,8592765045546,null,28592765045540,"8536419089",0.37]
[104554,"Ex9CSR09 10 3P 415V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 415 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045553,1,8592765045553,null,28592765045557,"8536490099",0.37]
[104555,"Ex9CSR09 10 3P 400V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 400 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045560,1,8592765045560,null,28592765045564,"8536490099",0.37]
[104556,"Ex9CSR09 10 3P 380V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 380 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045577,1,8592765045577,null,28592765045571,"8536490099",0.37]
[104557,"Ex9CSR09 10 3P 36V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 36 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045584,1,8592765045584,null,28592765045588,"8536419089",0.37]
[104558,"Ex9CSR09 10 3P 24V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 24 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045591,1,8592765045591,null,28592765045595,"8536419089",0.37]
[104559,"Ex9CSR09 10 3P 240V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 240 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045607,1,8592765045607,null,28592765045601,"8536490099",0.37]
[104560,"Ex9CSR09 10 3P 230V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 230 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045614,1,8592765045614,null,28592765045618,"8536490099",0.37]
[104561,"Ex9CSR09 10 3P 220V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 220 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045621,1,8592765045621,null,28592765045625,"8536490099",0.37]
[104562,"Ex9CSR09 10 3P 127V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 127 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045638,1,8592765045638,null,28592765045632,"8536490099",0.37]
[104563,"Ex9CSR09 10 3P 110V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 110 V AC, 1 NO built-in auxiliary contact","NBA",62.69,0,62.69,8592765045645,1,8592765045645,null,28592765045649,"8536490099",0.37]
[104564,"Ex9CSR09 01 3P 48V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 48 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045652,1,8592765045652,null,28592765045656,"8536419089",0.37]
[104565,"Ex9CSR09 01 3P 42V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 42 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045669,1,8592765045669,null,28592765045663,"8536419089",0.37]
[104566,"Ex9CSR09 01 3P 415V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 415 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045676,1,8592765045676,null,28592765045670,"8536490099",0.37]
[104567,"Ex9CSR09 01 3P 400V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 400 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045683,1,8592765045683,null,28592765045687,"8536490099",0.37]
[104568,"Ex9CSR09 01 3P 380V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 380 V AC, 1 NC built-in auxiliary contact","NBA",62.69,{"$f":"NBA","v":0},62.69,8592765045690,1,8592765045690,null,28592765045694,"8536490099",0.37]
[104569,"Ex9CSR09 01 3P 36V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 36 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,{"$f":"E3939*(1-F3939)","v":62.69},8592765045706,1,8592765045706,null,28592765045700,"8536419089",0.37]
[104570,"Ex9CSR09 01 3P 24V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 24 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045713,1,8592765045713,null,28592765045717,"8536419089",0.37]
[104571,"Ex9CSR09 01 3P 240V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 240 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045720,1,8592765045720,null,28592765045724,"8536490099",0.37]
[104572,"Ex9CSR09 01 3P 230V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 230 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045737,1,8592765045737,null,28592765045731,"8536490099",0.37]
[104573,"Ex9CSR09 01 3P 220V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 220 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045744,1,8592765045744,null,28592765045748,"8536490099",0.37]
[104574,"Ex9CSR09 01 3P 127V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 127 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045751,1,8592765045751,null,28592765045755,"8536490099",0.37]
[104575,"Ex9CSR09 01 3P 110V","Reversible miniature contactor, 3-pole, 9A AC-3, cont. 110 V AC, 1 NC built-in auxiliary contact","NBA",62.69,0,62.69,8592765045768,1,8592765045768,null,28592765045762,"8536490099",0.37]
[104576,"Ex9CSR09  4P/22 48V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 48 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045775,1,8592765045775,null,28592765045779,"8536419089",0.37]
[104577,"Ex9CSR09  4P/22 42V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 42 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045782,1,8592765045782,null,28592765045786,"8536419089",0.37]
[104578,"Ex9CSR09  4P/22 415V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 415 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045799,1,8592765045799,null,28592765045793,"8536490099",0.37]
[104579,"Ex9CSR09  4P/22 400V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 400 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045805,1,8592765045805,null,28592765045809,"8536490099",0.37]
[104580,"Ex9CSR09  4P/22 380V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 380 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045812,1,8592765045812,null,28592765045816,"8536490099",0.37]
[104581,"Ex9CSR09  4P/22 36V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 36 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045829,1,8592765045829,null,28592765045823,"8536419089",0.37]
[104582,"Ex9CSR09  4P/22 24V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 24 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045836,1,8592765045836,null,28592765045830,"8536419089",0.37]
[104583,"Ex9CSR09  4P/22 240V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 240 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045843,1,8592765045843,null,28592765045847,"8536490099",0.37]
[104584,"Ex9CSR09  4P/22 230V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 230 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045850,1,8592765045850,null,28592765045854,"8536490099",0.37]
[104585,"Ex9CSR09  4P/22 220V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 220 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045867,1,8592765045867,null,28592765045861,"8536490099",0.37]
[104586,"Ex9CSR09  4P/22 127V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 127 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045874,1,8592765045874,null,28592765045878,"8536490099",0.37]
[104587,"Ex9CSR09  4P/22 110V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 110 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",68.959999999999994,0,68.959999999999994,8592765045881,1,8592765045881,null,28592765045885,"8536490099",0.37]
[104588,"Ex9CSR09  4P 48V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 48 V AC","NBA",64.42,0,64.42,8592765045898,1,8592765045898,null,28592765045892,"8536419089",0.37]
[104589,"Ex9CSR09  4P 42V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 42 V AC","NBA",64.42,0,64.42,8592765045904,1,8592765045904,null,28592765045908,"8536419089",0.37]
[104590,"Ex9CSR09  4P 415V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 415 V AC","NBA",64.42,0,64.42,8592765045911,1,8592765045911,null,28592765045915,"8536490099",0.37]
[104591,"Ex9CSR09  4P 400V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 400 V AC","NBA",64.42,0,64.42,8592765045928,1,8592765045928,null,28592765045922,"8536490099",0.37]
[104592,"Ex9CSR09  4P 380V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 380 V AC","NBA",64.42,0,64.42,8592765045935,1,8592765045935,null,28592765045939,"8536490099",0.37]
[104593,"Ex9CSR09  4P 36V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 36 V AC","NBA",64.42,0,64.42,8592765045942,1,8592765045942,null,28592765045946,"8536419089",0.37]
[104594,"Ex9CSR09  4P 24V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 24 V AC","NBA",64.42,0,64.42,8592765045959,1,8592765045959,null,28592765045953,"8536419089",0.37]
[104595,"Ex9CSR09  4P 240V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 240 V AC","NBA",64.42,0,64.42,8592765045966,1,8592765045966,null,28592765045960,"8536490099",0.37]
[104596,"Ex9CSR09  4P 230V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 230 V AC","NBA",64.42,0,64.42,8592765045973,1,8592765045973,null,28592765045977,"8536490099",0.37]
[104597,"Ex9CSR09  4P 220V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 220 V AC","NBA",64.42,0,64.42,8592765045980,1,8592765045980,null,28592765045984,"8536490099",0.37]
[104598,"Ex9CSR09  4P 127V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 127 V AC","NBA",64.42,0,64.42,8592765045997,1,8592765045997,null,28592765045991,"8536490099",0.37]
[104599,"Ex9CSR09  4P 110V","Reversible miniature contactor, 4-pole, 9A AC-3, cont. 110 V AC","NBA",64.42,0,64.42,8592765046000,1,8592765046000,null,28592765046004,"8536490099",0.37]
[104600,"Ex9CSR12 10 3P 48V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 48 V AC, 1 NO built-in auxiliary contact","NBA",69.42,{"$f":"NBA","v":0},69.42,8592765046017,1,8592765046017,null,28592765046011,"8536419089",0.37]
[104601,"Ex9CSR12 10 3P 42V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 42 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046024,1,8592765046024,null,28592765046028,"8536419089",0.37]
[104602,"Ex9CSR12 10 3P 415V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 415 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046031,1,8592765046031,null,28592765046035,"8536490099",0.37]
[104603,"Ex9CSR12 10 3P 400V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 400 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046048,1,8592765046048,null,28592765046042,"8536490099",0.37]
[104604,"Ex9CSR12 10 3P 380V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 380 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046055,1,8592765046055,null,28592765046059,"8536490099",0.37]
[104605,"Ex9CSR12 10 3P 36V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 36 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046062,1,8592765046062,null,28592765046066,"8536419089",0.37]
[104606,"Ex9CSR12 10 3P 24V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 24 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046079,1,8592765046079,null,28592765046073,"8536419089",0.37]
[104607,"Ex9CSR12 10 3P 240V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 240 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046086,1,8592765046086,null,28592765046080,"8536490099",0.37]
[104608,"Ex9CSR12 10 3P 230V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 230 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046093,1,8592765046093,null,28592765046097,"8536490099",0.37]
[104609,"Ex9CSR12 10 3P 220V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 220 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046109,1,8592765046109,null,28592765046103,"8536490099",0.37]
[104610,"Ex9CSR12 10 3P 127V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 127 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046116,1,8592765046116,null,28592765046110,"8536490099",0.37]
[104611,"Ex9CSR12 10 3P 110V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 110 V AC, 1 NO built-in auxiliary contact","NBA",69.42,0,69.42,8592765046123,1,8592765046123,null,28592765046127,"8536490099",0.37]
[104612,"Ex9CSR12 01 3P 48V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 48 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046130,1,8592765046130,null,28592765046134,"8536419089",0.37]
[104613,"Ex9CSR12 01 3P 42V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 42 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046147,1,8592765046147,null,28592765046141,"8536419089",0.37]
[104614,"Ex9CSR12 01 3P 415V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 415 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046154,1,8592765046154,null,28592765046158,"8536490099",0.37]
[104615,"Ex9CSR12 01 3P 400V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 400 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046161,1,8592765046161,null,28592765046165,"8536490099",0.37]
[104616,"Ex9CSR12 01 3P 380V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 380 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046178,1,8592765046178,null,28592765046172,"8536490099",0.37]
[104617,"Ex9CSR12 01 3P 36V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 36 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046185,1,8592765046185,null,28592765046189,"8536419089",0.37]
[104618,"Ex9CSR12 01 3P 24V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 24 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046192,1,8592765046192,null,28592765046196,"8536419089",0.37]
[104619,"Ex9CSR12 01 3P 240V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 240 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046208,1,8592765046208,null,28592765046202,"8536490099",0.37]
[104620,"Ex9CSR12 01 3P 230V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 230 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046215,1,8592765046215,null,28592765046219,"8536490099",0.37]
[104621,"Ex9CSR12 01 3P 220V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 220 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046222,1,8592765046222,null,28592765046226,"8536490099",0.37]
[104622,"Ex9CSR12 01 3P 127V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 127 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046239,1,8592765046239,null,28592765046233,"8536490099",0.37]
[104623,"Ex9CSR12 01 3P 110V","Reversible miniature contactor, 3-pole, 12A AC-3, cont. 110 V AC, 1 NC built-in auxiliary contact","NBA",69.42,0,69.42,8592765046246,1,8592765046246,null,28592765046240,"8536490099",0.37]
[104624,"Ex9CSR12  4P/22 48V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 48 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046253,1,8592765046253,null,28592765046257,"8536419089",0.37]
[104625,"Ex9CSR12  4P/22 42V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 42 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046260,1,8592765046260,null,28592765046264,"8536419089",0.37]
[104626,"Ex9CSR12  4P/22 415V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 415 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046277,1,8592765046277,null,28592765046271,"8536490099",0.37]
[104627,"Ex9CSR12  4P/22 400V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 400 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046284,1,8592765046284,null,28592765046288,"8536490099",0.37]
[104628,"Ex9CSR12  4P/22 380V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 380 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046291,1,8592765046291,null,28592765046295,"8536490099",0.37]
[104629,"Ex9CSR12  4P/22 36V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 36 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046307,1,8592765046307,null,28592765046301,"8536419089",0.37]
[104630,"Ex9CSR12  4P/22 24V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 24 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046314,1,8592765046314,null,28592765046318,"8536419089",0.37]
[104631,"Ex9CSR12  4P/22 240V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 240 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046321,1,8592765046321,null,28592765046325,"8536490099",0.37]
[104632,"Ex9CSR12  4P/22 230V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 230 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,{"$f":"NBA","v":0},76.58,8592765046338,1,8592765046338,null,28592765046332,"8536490099",0.37]
[104633,"Ex9CSR12  4P/22 220V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 220 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,{"$f":"E4003*(1-F4003)","v":76.58},8592765046345,1,8592765046345,null,28592765046349,"8536490099",0.37]
[104634,"Ex9CSR12  4P/22 127V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 127 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046352,1,8592765046352,null,28592765046356,"8536490099",0.37]
[104635,"Ex9CSR12  4P/22 110V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 110 V AC, 2 NC + 2 NO built-in auxiliary contact","NBA",76.58,0,76.58,8592765046369,1,8592765046369,null,28592765046363,"8536490099",0.37]
[104636,"Ex9CSR12  4P 48V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 48 V AC","NBA",76.58,0,76.58,8592765046376,1,8592765046376,null,28592765046370,"8536419089",0.37]
[104637,"Ex9CSR12  4P 42V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 42 V AC","NBA",76.58,0,76.58,8592765046383,1,8592765046383,null,28592765046387,"8536419089",0.37]
[104638,"Ex9CSR12  4P 415V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 415 V AC","NBA",76.58,0,76.58,8592765046390,1,8592765046390,null,28592765046394,"8536490099",0.37]
[104639,"Ex9CSR12  4P 400V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 400 V AC","NBA",76.58,0,76.58,8592765046406,1,8592765046406,null,28592765046400,"8536490099",0.37]
[104640,"Ex9CSR12  4P 380V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 380 V AC","NBA",76.58,0,76.58,8592765046413,1,8592765046413,null,28592765046417,"8536490099",0.37]
[104641,"Ex9CSR12  4P 36V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 36 V AC","NBA",76.58,0,76.58,8592765046420,1,8592765046420,null,28592765046424,"8536419089",0.37]
[104642,"Ex9CSR12  4P 24V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 24 V AC","NBA",76.58,0,76.58,8592765046437,1,8592765046437,null,28592765046431,"8536419089",0.37]
[104643,"Ex9CSR12  4P 240V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 240 V AC","NBA",76.58,0,76.58,8592765046444,1,8592765046444,null,28592765046448,"8536490099",0.37]
[104644,"Ex9CSR12  4P 230V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 230 V AC","NBA",76.58,0,76.58,8592765046451,1,8592765046451,null,28592765046455,"8536490099",0.37]
[104645,"Ex9CSR12  4P 220V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 220 V AC","NBA",76.58,0,76.58,8592765046468,1,8592765046468,null,28592765046462,"8536490099",0.37]
[104646,"Ex9CSR12  4P 127V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 127 V AC","NBA",76.58,0,76.58,8592765046475,1,8592765046475,null,28592765046479,"8536490099",0.37]
[104647,"Ex9CSR12  4P 110V","Reversible miniature contactor, 4-pole, 12A AC-3, cont. 110 V AC","NBA",76.58,0,76.58,8592765046482,1,8592765046482,null,28592765046486,"8536490099",0.37]
[]
["Accessories for Miniature Contactors Ex9CS"]
[101435,"AX4104","Front-mounted auxiliary contact unit for Ex9CS, 4 NC","NBA",7.93,{"$f":"NBA","v":0},{"$f":"E4020*(1-F4020)","v":7.93},8592765014368,6,18592765014365,216,28592765014362,"8536508090",0.28999999999999998]
[101280,"AX4113","Front-mounted auxiliary contact unit for Ex9CS, 1 NO, 3 NC","NBA",7.93,{"$f":"NBA","v":0},7.93,8592765012814,6,18592765012811,216,28592765012818,"8536508090",0.28999999999999998]
[101281,"AX4122","Front-mounted auxiliary contact unit for Ex9CS, 2 NO, 2 NC","NBA",7.93,{"$f":"NBA","v":0},7.93,8592765012821,6,18592765012828,216,28592765012825,"8536508090",0.28999999999999998]
[101282,"AX4131","Front-mounted auxiliary contact unit for Ex9CS, 3 NO, 1 NC","NBA",7.93,{"$f":"NBA","v":0},7.93,8592765012838,6,18592765012835,216,28592765012832,"8536508090",0.28999999999999998]
[101283,"AX4140","Front-mounted auxiliary contact unit for Ex9CS, 4 NO","NBA",7.93,{"$f":"NBA","v":0},7.93,8592765012845,6,18592765012842,216,28592765012849,"8536508090",0.28999999999999998]
[104501,"CCU41 48","Surge suppressor blocks, protection range 24-48V, with varistor","NBA",10.220000000000001,{"$f":"NBA","v":0},10.220000000000001,8592765045027,1,8592765045027,null,28592765045021,"8538909999",0.02]
[104502,"CCU41 415","Surge suppressor blocks, protection range 380-415V, with varistor","NBA",10.220000000000001,0,10.220000000000001,8592765045034,1,8592765045034,null,28592765045038,"8538909999",0.02]
[104503,"CCU41 240","Surge suppressor blocks, protection range 110-240V, with varistor","NBA",10.220000000000001,0,10.220000000000001,8592765045041,1,8592765045041,null,28592765045045,"8538909999",0.02]
[107959,"MIT41","Mechanical interlocks for contactors Ex9CS","NBA",5.44,{"$f":"NBA","v":0},5.44,8592765079602,1,18592765079609,400,28592765079606,"8538909999"]
[]
["Motor protective circuit breakers Ex9S32A"]
[108096,"Ex9S32A 0.16A","Motor Protective Circuit-Breaker 0.16A","NBG",36.950000000000003,{"$f":"NBG","v":0},{"$f":"E4031*(1-F4031)","v":36.950000000000003},8592765080967,1,18592765080964,30,28592765080961,"8536201090",0.25800000000000001]
[108097,"Ex9S32A 0.25A","Motor Protective Circuit-Breaker 0.25A","NBG",36.950000000000003,0,36.950000000000003,8592765080974,1,18592765080971,30,28592765080978,"8536201090",0.25800000000000001]
[108098,"Ex9S32A 0.4A","Motor Protective Circuit-Breaker 0.4A","NBG",38.93,0,38.93,8592765080981,1,18592765080988,30,28592765080985,"8536201090",0.25800000000000001]
[108099,"Ex9S32A 0.63A","Motor Protective Circuit-Breaker 0.63A","NBG",38.93,0,38.93,8592765080998,1,18592765080995,30,28592765080992,"8536201090",0.25800000000000001]
[108100,"Ex9S32A 1A","Motor Protective Circuit-Breaker 1A","NBG",39.340000000000003,0,39.340000000000003,8592765081001,1,18592765081008,30,28592765081005,"8536201090",0.25800000000000001]
[108101,"Ex9S32A 1.6A","Motor Protective Circuit-Breaker 1.6A","NBG",39.340000000000003,0,39.340000000000003,8592765081018,1,18592765081015,30,28592765081012,"8536201090",0.32500000000000001]
[108102,"Ex9S32A 2.5A","Motor Protective Circuit-Breaker 2.5A","NBG",39.86,0,39.86,8592765081025,1,18592765081022,30,28592765081029,"8536201090",0.32500000000000001]
[108103,"Ex9S32A 4A","Motor Protective Circuit-Breaker 4A","NBG",39.86,0,39.86,8592765081032,1,18592765081039,30,28592765081036,"8536201090",0.32500000000000001]
[108104,"Ex9S32A 6.3A","Motor Protective Circuit-Breaker 6.3A","NBG",39.86,0,39.86,8592765081049,1,18592765081046,30,28592765081043,"8536201090",0.32500000000000001]
[108105,"Ex9S32A 10A","Motor Protective Circuit-Breaker 10A","NBG",41.76,0,41.76,8592765081056,1,18592765081053,30,28592765081050,"8536201090",0.32500000000000001]
[108106,"Ex9S32A 14A","Motor Protective Circuit-Breaker 14A","NBG",41.76,0,41.76,8592765081063,1,18592765081060,30,28592765081067,"8536201090",0.32500000000000001]
[108107,"Ex9S32A 18A","Motor Protective Circuit-Breaker 18A","NBG",41.96,0,41.96,8592765081070,1,18592765081077,30,28592765081074,"8536201090",0.32500000000000001]
[108108,"Ex9S32A 23A","Motor Protective Circuit-Breaker 23A","NBG",44.06,0,44.06,8592765081087,1,18592765081084,30,28592765081081,"8536201090",0.32500000000000001]
[108109,"Ex9S32A 25A","Motor Protective Circuit-Breaker 25A","NBG",47.2,0,47.2,8592765081094,1,18592765081091,30,28592765081098,"8536201090",0.32500000000000001]
[108110,"Ex9S32A 32A","Motor Protective Circuit-Breaker 32A","NBG",50.36,0,50.36,8592765081100,1,18592765081107,30,28592765081104,"8536201090",0.32500000000000001]
["Acc."]
[108143,"AX51 11","Front-mounted auxiliary contact unit for Ex9S32, 1NO+1NC","NBG",6.2,0,6.2,8592765081438,10,18592765081435,720,28592765081432,"8536508090",1.6E-2]
[108144,"AX51 20","Front-mounted auxiliary contact unit for Ex9S32, 2NO","NBG",6.2,0,6.2,8592765081445,10,18592765081442,720,28592765081449,"8536508090",1.6E-2]
[108145,"AX52 11","Side-mounted auxiliary contact unit for Ex9S32, 1NO+1NC","NBG",10.07,0,10.07,8592765081452,2,18592765081459,192,28592765081456,"8536508090",4.2000000000000003E-2]
[108146,"AX52 20","Side-mounted auxiliary contact unit for Ex9S32, 2NO","NBG",10.07,0,10.07,8592765081469,2,18592765081466,192,28592765081463,"8536508090",4.2000000000000003E-2]
[108147,"AX52 02","Side-mounted auxiliary contact unit for Ex9S32, 2NC","NBG",10.6,0,10.6,8592765081476,2,18592765081473,192,28592765081470,"8536508090",4.2000000000000003E-2]
[108148,"UVT51I","Undervoltage release 110~115V 50Hz, 127V 60Hz","NBG",10.01,0,10.01,8592765081483,1,18592765081480,96,28592765081487,"8536490099",0.125]
[108149,"UVT51J","Undervoltage release 220~240V 50Hz","NBG",9.94,0,9.94,8592765081490,1,18592765081497,96,28592765081494,"8536490099",0.125]
[108150,"UVT51K","Undervoltage release 380~400V 50Hz, 440V 60Hz","NBG",11.96,0,11.96,8592765081506,1,18592765081503,96,28592765081500,"8536490099",0.125]
[108151,"SHT51F","Shunt release 110~115V 50Hz, 127V 60Hz","NBG",9.42,0,9.42,8592765081513,1,18592765081510,96,28592765081517,"8536490099",0.10199999999999999]
[108152,"SHT51G","Shunt release 220~240V 50Hz","NBG",11.43,0,11.43,8592765081520,1,18592765081527,96,28592765081524,"8536490099",0.10199999999999999]
[108153,"SHT51H","Shunt release 380~400V 50Hz, 440V 60Hz","NBG",10.33,0,10.33,8592765081537,1,18592765081534,96,28592765081531,"8536490099",0.10199999999999999]
[108154,"AL51","Fault indicating contact","NBG",11.8,0,11.8,8592765081544,null,18592765081541,null,28592765081548,"8536201090"]
[108155,"CC51","CC51 Terminal adapter for Ex9CS06,09,12","NBG",15.56,0,15.56,8592765081551,null,18592765081558,null,28592765081555,"8538909999"]
[109077,"CC52","CC52 Terminal adapter for Ex9C09,12,18","NBG",18.27,{"$f":"NBG","v":0},{"$f":"E4060*(1-F4060)","v":18.27},8592765090775,3,18592765090772,120,28592765090779,"8538909999",5.1499999999999997E-2]
[109078,"CC53 ","CC53 Terminal adapter for Ex9C25,32,38","NBG",18.27,{"$f":"NBG","v":0},{"$f":"E4061*(1-F4061)","v":18.27},8592765090782,3,18592765090789,60,28592765090786,"8538909999",5.7599999999999998E-2]
[109079,"DRA51","DRA51 Adapter holder","NBG",5.49,{"$f":"NBG","v":0},{"$f":"E4062*(1-F4062)","v":5.49},8592765090799,16,18592765090796,96,28592765090793,"8538909999",8.9099999999999999E-2]
[]
["Motor protective circuit breakers Ex9SN25B",null,null,null,null,null,null,"","","","","",null,""]
[108940,"Ex9SN25B0.16A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 0.10-0.16A","NBG",28.2,{"$f":"NBG","v":0},{"$f":"E4065*(1-F4065)","v":28.2},8592765089403,1,8592765089403,64,28592765089407,"8536201090",0.24]
[108941,"Ex9SN25B0.25A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 0.16-0.25A","NBG",28.2,{"$f":"NBG","v":0},28.2,8592765089410,1,8592765089410,64,28592765089414,"8536201090",0.24]
[108942,"Ex9SN25B0.4A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 0.25-0.40A","NBG",28.2,0,28.2,8592765089427,1,8592765089427,64,28592765089421,"8536201090",0.24]
[108943,"Ex9SN25B0.63A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 0.40-0.63A","NBG",23.75,0,23.75,8592765089434,1,8592765089434,64,28592765089438,"8536201090",0.24]
[108944,"Ex9SN25B1A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 0.63-1A","NBG",24.66,0,24.66,8592765089441,1,8592765089441,64,28592765089445,"8536201090",0.24]
[108945,"Ex9SN25B1.6A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 1-1.6A","NBG",24.66,0,24.66,8592765089458,1,8592765089458,64,28592765089452,"8536201090",0.28999999999999998]
[108946,"Ex9SN25B2.5A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 1.6-2.5A","NBG",25.02,0,25.02,8592765089465,1,8592765089465,64,28592765089469,"8536201090",0.28999999999999998]
[108947,"Ex9SN25B4A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 2.5-4A","NBG",25.02,0,25.02,8592765089472,1,8592765089472,64,28592765089476,"8536201090",0.28999999999999998]
[108948,"Ex9SN25B6.3A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 4-6.3A","NBG",25.02,0,25.02,8592765089489,1,8592765089489,64,28592765089483,"8536201090",0.28999999999999998]
[108949,"Ex9SN25B10A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 6-10A","NBG",27.12,0,27.12,8592765089496,1,8592765089496,64,28592765089490,"8536201090",0.28999999999999998]
[108950,"Ex9SN25B14A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 9-14A","NBG",27.12,0,27.12,8592765089502,1,8592765089502,64,28592765089506,"8536201090",0.28999999999999998]
[108951,"Ex9SN25B18A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 13-18A","NBG",29.07,0,29.07,8592765089519,1,8592765089519,64,28592765089513,"8536201090",0.28999999999999998]
[108952,"Ex9SN25B23A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 17-23A","NBG",29.07,0,29.07,8592765089526,1,8592765089526,64,28592765089520,"8536201090",0.28999999999999998]
[108953,"Ex9SN25B25A","Manual Motor Starter, Ex9SN, 25A, Pushbutton, 20-25A","NBG",29.07,0,29.07,8592765089533,1,8592765089533,64,28592765089537,"8536201090",0.28999999999999998]
["Acc."]
[108954,"ASNA20","Auxiliary Contact, Ex9SN, Side Mount, 2NO ","NBG",9.25,0,{"$f":"E4080*(1-F4080)","v":9.25},8592765089540,4,18592765089547,256,28592765089544,"8536508090",0.04]
[108955,"ASNA11","Auxiliary Contact, Ex9SN, Side Mount, 1NO+1NC ","NBG",7.41,0,7.41,8592765089557,4,18592765089554,256,28592765089551,"8536508090",0.04]
[108956,"ASNB20","Auxiliary Contact, Ex9SN, Front Mount , 2NO","NBG",7.88,0,7.88,8592765089564,20,18592765089561,1280,28592765089568,"8536508090",0.02]
[108957,"ASNB11","Auxiliary Contact, Ex9SN, Front Mount, 1NO+1NC ","NBG",7.88,0,7.88,8592765089571,20,18592765089578,1280,28592765089575,"8536508090",0.02]
[108958,"ASNUVA","Under-Voltage Release, Ex9SN, Side Mount, 110-115V 50Hz/127V 50Hz","NBG",8.35,0,8.35,8592765089588,2,18592765089585,128,28592765089582,"8536508090",0.09]
[108959,"ASNUVB","Under-Voltage Release, Ex9SN, Side Mount, 220-240V 50Hz","NBG",8.44,0,8.44,8592765089595,2,18592765089592,128,28592765089599,"8536508090",0.09]
[108960,"ASNUVC","Under-Voltage Release, Ex9SN, Side Mount, 380-400V 50Hz/440V 50Hz","NBG",8.6,0,8.6,8592765089601,2,18592765089608,128,28592765089605,"8536508090",0.09]
[108961,"ASNTA","Shunt Trip Release, Ex9SN, Side Mount, 110-115V 50Hz/127V 50Hz","NBG",8.7899999999999991,0,8.7899999999999991,8592765089618,2,18592765089615,128,28592765089612,"8536508090",0.09]
[108962,"ASNTB","Shunt Trip Release, Ex9SN, Side Mount, 220-240V 50Hz","NBG",8.9600000000000009,0,8.9600000000000009,8592765089625,2,18592765089622,128,28592765089629,"8536508090",0.09]
[108963,"ASNTC","Shunt Trip Release, Ex9SN, Side Mount, 380-400V 50Hz/440V 50Hz","NBG",9.2200000000000006,0,9.2200000000000006,8592765089632,2,18592765089639,128,28592765089636,"8536508090",0.09]
[108964,"ASNF1001","Auxiliary Contact, Ex9SN, with Fault Signal Contact, 1NO(Fault)+1NC(Aux)","NBG",4.68,0,4.68,8592765089649,3,18592765089646,192,28592765089643,"8536508090",0.04]
[108965,"ASNF0101","Auxiliary Contact, Ex9SN, with Fault Signal Contact, 1NC(Fault)+1NC(Aux)","NBG",4.7,0,4.7,8592765089656,3,18592765089653,192,28592765089650,"8536508090",0.04]
[108966,"ASNF1010","Auxiliary Contact, Ex9SN, with Fault Signal Contact, 1NO(Fault)+1NO(Aux)","NBG",4.6900000000000004,0,4.6900000000000004,8592765089663,3,18592765089660,192,28592765089667,"8536508090",0.04]
[108967,"ASNF0110","Auxiliary Contact, Ex9SN, with Fault Signal Contact, 1NC(Fault)+1NO(Aux)","NBG",4.72,0,4.72,8592765089670,3,18592765089677,192,28592765089674,"8536508090",0.04]
[108968,"ASNEA","Enclosure, Ex9SN, with Actuating Diaphragm","NBG",7.88,0,7.88,8592765089687,1,8592765089687,20,28592765089681,"8536508090",0.26]
[108969,"ASNEB","Enclosure, Ex9SN, Emergency Stop Pushbutton","NBG",9.68,0,9.68,8592765089694,1,8592765089694,12,28592765089698,"8536508090",0.32]
[]
["Contactors Ex9C"]
[101100,"Ex9C09  11 3P 415V ","Contactor, 3-pole, 9A AC-3, cont. 415 V AC, built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,{"$f":"NBA","v":0},{"$f":"E4098*(1-F4098)","v":15.46},8592765011015,1,8592765011015,40,28592765011019,"8536490099",0.37]
[101101,"Ex9C09  11 3P 400V ","Contactor, 3-pole, 9A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011022,1,8592765011022,40,28592765011026,"8536490099",0.37]
[101102,"Ex9C09  11 3P 380V ","Contactor, 3-pole, 9A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011039,1,8592765011039,40,28592765011033,"8536490099",0.37]
[101103,"Ex9C09  11 3P 240V ","Contactor, 3-pole, 9A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011046,1,8592765011046,40,28592765011040,"8536490099",0.37]
[101104,"Ex9C09  11 3P 230V ","Contactor, 3-pole, 9A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",17.78,0,17.78,8592765011053,1,8592765011053,40,28592765011057,"8536490099",0.37]
[101105,"Ex9C09  11 3P 220V ","Contactor, 3-pole, 9A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011060,1,8592765011060,40,28592765011064,"8536490099",0.37]
[101106,"Ex9C09  11 3P 127V ","Contactor, 3-pole, 9A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011077,1,8592765011077,40,28592765011071,"8536490099",0.37]
[101107,"Ex9C09  11 3P 110V ","Contactor, 3-pole, 9A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011084,1,8592765011084,40,28592765011088,"8536490099",0.37]
[101108,"Ex9C09  11 3P 48V ","Contactor, 3-pole, 9A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011091,1,8592765011091,40,28592765011095,"8536419089",0.37]
[101109,"Ex9C09  11 3P 42V ","Contactor, 3-pole, 9A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011107,1,8592765011107,40,28592765011101,"8536419089",0.37]
[101110,"Ex9C09  11 3P 36V ","Contactor, 3-pole, 9A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",15.46,0,15.46,8592765011114,1,8592765011114,40,28592765011118,"8536419089",0.37]
[101111,"Ex9C09  11 3P 24V ","Contactor, 3-pole, 9A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",17.78,0,17.78,8592765011121,1,8592765011121,40,28592765011125,"8536419089",0.37]
[101112,"Ex9C09  22 3P 415V ","Contactor, 3-pole, 9A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011138,1,8592765011138,40,28592765011132,"8536490099",0.37]
[101113,"Ex9C09  22 3P 400V ","Contactor, 3-pole, 9A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011145,1,8592765011145,40,28592765011149,"8536490099",0.37]
[101114,"Ex9C09  22 3P 380V ","Contactor, 3-pole, 9A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011152,1,8592765011152,40,28592765011156,"8536490099",0.37]
[101115,"Ex9C09  22 3P 240V ","Contactor, 3-pole, 9A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011169,1,8592765011169,40,28592765011163,"8536490099",0.37]
[101116,"Ex9C09  22 3P 230V ","Contactor, 3-pole, 9A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011176,1,8592765011176,40,28592765011170,"8536490099",0.37]
[101117,"Ex9C09  22 3P 220V ","Contactor, 3-pole, 9A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011183,1,8592765011183,40,28592765011187,"8536490099",0.37]
[101118,"Ex9C09  22 3P 127V ","Contactor, 3-pole, 9A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011190,1,8592765011190,40,28592765011194,"8536490099",0.37]
[101119,"Ex9C09  22 3P 110V ","Contactor, 3-pole, 9A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011206,1,8592765011206,40,28592765011200,"8536490099",0.37]
[101120,"Ex9C09  22 3P 48V ","Contactor, 3-pole, 9A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011213,1,8592765011213,40,28592765011217,"8536419089",0.37]
[101121,"Ex9C09  22 3P 42V ","Contactor, 3-pole, 9A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011220,1,8592765011220,40,28592765011224,"8536419089",0.37]
[101122,"Ex9C09  22 3P 36V ","Contactor, 3-pole, 9A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011237,1,8592765011237,40,28592765011231,"8536419089",0.37]
[101123,"Ex9C09  22 3P 24V ","Contactor, 3-pole, 9A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",20.59,0,20.59,8592765011244,1,8592765011244,40,28592765011248,"8536419089",0.37]
[101124,"Ex9C12  11 3P 415V ","Contactor, 3-pole, 12A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011251,1,8592765011251,40,28592765011255,"8536490099",0.37]
[101125,"Ex9C12  11 3P 400V ","Contactor, 3-pole, 12A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011268,1,8592765011268,40,28592765011262,"8536490099",0.37]
[101126,"Ex9C12  11 3P 380V ","Contactor, 3-pole, 12A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011275,1,8592765011275,40,28592765011279,"8536490099",0.37]
[101127,"Ex9C12  11 3P 240V ","Contactor, 3-pole, 12A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011282,1,8592765011282,40,28592765011286,"8536490099",0.37]
[101128,"Ex9C12  11 3P 230V ","Contactor, 3-pole, 12A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",19.88,0,19.88,8592765011299,1,8592765011299,40,28592765011293,"8536490099",0.37]
[101129,"Ex9C12  11 3P 220V ","Contactor, 3-pole, 12A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011305,1,8592765011305,40,28592765011309,"8536490099",0.37]
[101130,"Ex9C12  11 3P 127V ","Contactor, 3-pole, 12A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011312,1,8592765011312,40,28592765011316,"8536490099",0.37]
[101131,"Ex9C12  11 3P 110V ","Contactor, 3-pole, 12A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011329,1,8592765011329,40,28592765011323,"8536490099",0.37]
[101132,"Ex9C12  11 3P 48V ","Contactor, 3-pole, 12A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011336,1,8592765011336,40,28592765011330,"8536419089",0.37]
[101133,"Ex9C12  11 3P 42V ","Contactor, 3-pole, 12A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011343,1,8592765011343,40,28592765011347,"8536419089",0.37]
[101134,"Ex9C12  11 3P 36V ","Contactor, 3-pole, 12A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",18.07,0,18.07,8592765011350,1,8592765011350,40,28592765011354,"8536419089",0.37]
[101135,"Ex9C12  11 3P 24V ","Contactor, 3-pole, 12A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",19.88,0,19.88,8592765011367,1,8592765011367,40,28592765011361,"8536419089",0.37]
[101136,"Ex9C12  22 3P 415V ","Contactor, 3-pole, 12A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011374,1,8592765011374,40,28592765011378,"8536490099",0.37]
[101137,"Ex9C12  22 3P 400V ","Contactor, 3-pole, 12A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011381,1,8592765011381,40,28592765011385,"8536490099",0.37]
[101138,"Ex9C12  22 3P 380V ","Contactor, 3-pole, 12A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011398,1,8592765011398,40,28592765011392,"8536490099",0.37]
[101139,"Ex9C12  22 3P 240V ","Contactor, 3-pole, 12A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011404,1,8592765011404,40,28592765011408,"8536490099",0.37]
[101140,"Ex9C12  22 3P 230V ","Contactor, 3-pole, 12A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011411,1,8592765011411,40,28592765011415,"8536490099",0.37]
[101141,"Ex9C12  22 3P 220V ","Contactor, 3-pole, 12A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011428,1,8592765011428,40,28592765011422,"8536490099",0.37]
[101142,"Ex9C12  22 3P 127V ","Contactor, 3-pole, 12A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011435,1,8592765011435,40,28592765011439,"8536490099",0.37]
[101143,"Ex9C12  22 3P 110V ","Contactor, 3-pole, 12A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011442,1,8592765011442,40,28592765011446,"8536490099",0.37]
[101144,"Ex9C12  22 3P 48V ","Contactor, 3-pole, 12A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011459,1,8592765011459,40,28592765011453,"8536419089",0.37]
[101145,"Ex9C12  22 3P 42V ","Contactor, 3-pole, 12A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011466,1,8592765011466,40,28592765011460,"8536419089",0.37]
[101146,"Ex9C12  22 3P 36V ","Contactor, 3-pole, 12A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011473,1,8592765011473,40,28592765011477,"8536419089",0.37]
[101147,"Ex9C12  22 3P 24V ","Contactor, 3-pole, 12A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",24.63,0,24.63,8592765011480,1,8592765011480,40,28592765011484,"8536419089",0.37]
[101148,"Ex9C18  11 3P 415V ","Contactor, 3-pole, 18A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011497,1,8592765011497,40,28592765011491,"8536490099",0.37]
[101149,"Ex9C18  11 3P 400V ","Contactor, 3-pole, 18A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011503,1,8592765011503,40,28592765011507,"8536490099",0.37]
[101150,"Ex9C18  11 3P 380V ","Contactor, 3-pole, 18A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011510,1,8592765011510,40,28592765011514,"8536490099",0.37]
[101151,"Ex9C18  11 3P 240V ","Contactor, 3-pole, 18A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011527,1,8592765011527,40,28592765011521,"8536490099",0.37]
[101152,"Ex9C18  11 3P 230V ","Contactor, 3-pole, 18A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011534,1,8592765011534,40,28592765011538,"8536490099",0.37]
[101153,"Ex9C18  11 3P 220V ","Contactor, 3-pole, 18A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011541,1,8592765011541,40,28592765011545,"8536490099",0.37]
[101154,"Ex9C18  11 3P 127V ","Contactor, 3-pole, 18A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011558,1,8592765011558,40,28592765011552,"8536490099",0.37]
[101155,"Ex9C18  11 3P 110V ","Contactor, 3-pole, 18A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011565,1,8592765011565,40,28592765011569,"8536490099",0.37]
[101156,"Ex9C18  11 3P 48V ","Contactor, 3-pole, 18A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011572,1,8592765011572,40,28592765011576,"8536419089",0.37]
[101157,"Ex9C18  11 3P 42V ","Contactor, 3-pole, 18A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011589,1,8592765011589,40,28592765011583,"8536419089",0.37]
[101158,"Ex9C18  11 3P 36V ","Contactor, 3-pole, 18A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011596,1,8592765011596,40,28592765011590,"8536419089",0.37]
[101159,"Ex9C18  11 3P 24V ","Contactor, 3-pole, 18A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",24.21,0,24.21,8592765011602,1,8592765011602,40,28592765011606,"8536419089",0.37]
[101160,"Ex9C18  22 3P 415V ","Contactor, 3-pole, 18A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011619,1,8592765011619,40,28592765011613,"8536490099",0.37]
[101161,"Ex9C18  22 3P 400V ","Contactor, 3-pole, 18A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011626,1,8592765011626,40,28592765011620,"8536490099",0.37]
[101162,"Ex9C18  22 3P 380V ","Contactor, 3-pole, 18A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011633,1,8592765011633,40,28592765011637,"8536490099",0.37]
[101163,"Ex9C18  22 3P 240V ","Contactor, 3-pole, 18A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011640,1,8592765011640,40,28592765011644,"8536490099",0.37]
[101164,"Ex9C18  22 3P 230V ","Contactor, 3-pole, 18A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,{"$f":"NBA","v":0},{"$f":"E4162*(1-F4162)","v":31.58},8592765011657,1,8592765011657,40,28592765011651,"8536490099",0.37]
[101165,"Ex9C18  22 3P 220V ","Contactor, 3-pole, 18A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011664,1,8592765011664,40,28592765011668,"8536490099",0.37]
[101166,"Ex9C18  22 3P 127V ","Contactor, 3-pole, 18A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011671,1,8592765011671,40,28592765011675,"8536490099",0.37]
[101167,"Ex9C18  22 3P 110V ","Contactor, 3-pole, 18A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011688,1,8592765011688,40,28592765011682,"8536490099",0.37]
[101168,"Ex9C18  22 3P 48V ","Contactor, 3-pole, 18A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011695,1,8592765011695,40,28592765011699,"8536419089",0.37]
[101169,"Ex9C18  22 3P 42V ","Contactor, 3-pole, 18A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011701,1,8592765011701,40,28592765011705,"8536419089",0.37]
[101170,"Ex9C18  22 3P 36V ","Contactor, 3-pole, 18A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011718,1,8592765011718,40,28592765011712,"8536419089",0.37]
[101171,"Ex9C18  22 3P 24V ","Contactor, 3-pole, 18A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",31.58,0,31.58,8592765011725,1,8592765011725,40,28592765011729,"8536419089",0.37]
[101172,"Ex9C25  11 3P 415V ","Contactor, 3-pole, 25A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011732,1,8592765011732,20,28592765011736,"8536490099",0.45]
[101173,"Ex9C25  11 3P 400V ","Contactor, 3-pole, 25A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011749,1,8592765011749,20,28592765011743,"8536490099",0.45]
[101174,"Ex9C25  11 3P 380V ","Contactor, 3-pole, 25A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011756,1,8592765011756,20,28592765011750,"8536490099",0.45]
[101175,"Ex9C25  11 3P 240V ","Contactor, 3-pole, 25A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011763,1,8592765011763,20,28592765011767,"8536490099",0.45]
[101176,"Ex9C25  11 3P 230V ","Contactor, 3-pole, 25A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011770,1,8592765011770,20,28592765011774,"8536490099",0.45]
[101177,"Ex9C25  11 3P 220V ","Contactor, 3-pole, 25A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011787,1,8592765011787,20,28592765011781,"8536490099",0.45]
[101178,"Ex9C25  11 3P 127V ","Contactor, 3-pole, 25A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011794,1,8592765011794,20,28592765011798,"8536490099",0.45]
[101179,"Ex9C25  11 3P 110V ","Contactor, 3-pole, 25A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011800,1,8592765011800,20,28592765011804,"8536490099",0.45]
[101180,"Ex9C25  11 3P 48V ","Contactor, 3-pole, 25A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011817,1,8592765011817,20,28592765011811,"8536419089",0.45]
[101181,"Ex9C25  11 3P 42V ","Contactor, 3-pole, 25A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011824,1,8592765011824,20,28592765011828,"8536419089",0.45]
[101182,"Ex9C25  11 3P 36V ","Contactor, 3-pole, 25A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011831,1,8592765011831,20,28592765011835,"8536419089",0.45]
[101183,"Ex9C25  11 3P 24V ","Contactor, 3-pole, 25A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",32.78,0,32.78,8592765011848,1,8592765011848,20,28592765011842,"8536419089",0.45]
[101184,"Ex9C25  22 3P 415V ","Contactor, 3-pole, 25A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011855,1,8592765011855,20,28592765011859,"8536490099",0.45]
[101185,"Ex9C25  22 3P 400V ","Contactor, 3-pole, 25A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011862,1,8592765011862,20,28592765011866,"8536490099",0.45]
[101186,"Ex9C25  22 3P 380V ","Contactor, 3-pole, 25A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011879,1,8592765011879,20,28592765011873,"8536490099",0.45]
[101187,"Ex9C25  22 3P 240V ","Contactor, 3-pole, 25A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011886,1,8592765011886,20,28592765011880,"8536490099",0.45]
[101188,"Ex9C25  22 3P 230V ","Contactor, 3-pole, 25A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011893,1,8592765011893,20,28592765011897,"8536490099",0.45]
[101189,"Ex9C25  22 3P 220V ","Contactor, 3-pole, 25A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011909,1,8592765011909,20,28592765011903,"8536490099",0.45]
[101190,"Ex9C25  22 3P 127V ","Contactor, 3-pole, 25A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011916,1,8592765011916,20,28592765011910,"8536490099",0.45]
[101191,"Ex9C25  22 3P 110V ","Contactor, 3-pole, 25A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011923,1,8592765011923,20,28592765011927,"8536490099",0.45]
[101192,"Ex9C25  22 3P 48V ","Contactor, 3-pole, 25A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011930,1,8592765011930,20,28592765011934,"8536419089",0.45]
[101193,"Ex9C25  22 3P 42V ","Contactor, 3-pole, 25A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011947,1,8592765011947,20,28592765011941,"8536419089",0.45]
[101194,"Ex9C25  22 3P 36V ","Contactor, 3-pole, 25A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011954,1,8592765011954,20,28592765011958,"8536419089",0.45]
[101195,"Ex9C25  22 3P 24V ","Contactor, 3-pole, 25A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",41.21,0,41.21,8592765011961,1,8592765011961,20,28592765011965,"8536419089",0.45]
[101196,"Ex9C32  11 3P 415V ","Contactor, 3-pole, 32A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765011978,1,8592765011978,20,28592765011972,"8536490099",0.45]
[101197,"Ex9C32  11 3P 400V ","Contactor, 3-pole, 32A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765011985,1,8592765011985,20,28592765011989,"8536490099",0.45]
[101198,"Ex9C32  11 3P 380V ","Contactor, 3-pole, 32A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765011992,1,8592765011992,20,28592765011996,"8536490099",0.45]
[101199,"Ex9C32  11 3P 240V ","Contactor, 3-pole, 32A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012005,1,8592765012005,20,28592765012009,"8536490099",0.45]
[101200,"Ex9C32  11 3P 230V ","Contactor, 3-pole, 32A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012012,1,8592765012012,20,28592765012016,"8536490099",0.45]
[101201,"Ex9C32  11 3P 220V ","Contactor, 3-pole, 32A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012029,1,8592765012029,20,28592765012023,"8536490099",0.45]
[101202,"Ex9C32  11 3P 127V ","Contactor, 3-pole, 32A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012036,1,8592765012036,20,28592765012030,"8536490099",0.45]
[101203,"Ex9C32  11 3P 110V ","Contactor, 3-pole, 32A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012043,1,8592765012043,20,28592765012047,"8536490099",0.45]
[101204,"Ex9C32  11 3P 48V ","Contactor, 3-pole, 32A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012050,1,8592765012050,20,28592765012054,"8536419089",0.45]
[101205,"Ex9C32  11 3P 42V ","Contactor, 3-pole, 32A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012067,1,8592765012067,20,28592765012061,"8536419089",0.45]
[101206,"Ex9C32  11 3P 36V ","Contactor, 3-pole, 32A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012074,1,8592765012074,20,28592765012078,"8536419089",0.45]
[101207,"Ex9C32  11 3P 24V ","Contactor, 3-pole, 32A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",49.19,0,49.19,8592765012081,1,8592765012081,20,28592765012085,"8536419089",0.45]
[101208,"Ex9C32  22 3P 415V ","Contactor, 3-pole, 32A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012098,1,8592765012098,20,28592765012092,"8536490099",0.45]
[101209,"Ex9C32  22 3P 400V ","Contactor, 3-pole, 32A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012104,1,8592765012104,20,28592765012108,"8536490099",0.45]
[101210,"Ex9C32  22 3P 380V ","Contactor, 3-pole, 32A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012111,1,8592765012111,20,28592765012115,"8536490099",0.45]
[101211,"Ex9C32  22 3P 240V ","Contactor, 3-pole, 32A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012128,1,8592765012128,20,28592765012122,"8536490099",0.45]
[101212,"Ex9C32  22 3P 230V ","Contactor, 3-pole, 32A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012135,1,8592765012135,20,28592765012139,"8536490099",0.45]
[101213,"Ex9C32  22 3P 220V ","Contactor, 3-pole, 32A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012142,1,8592765012142,20,28592765012146,"8536490099",0.45]
[101214,"Ex9C32  22 3P 127V ","Contactor, 3-pole, 32A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012159,1,8592765012159,20,28592765012153,"8536490099",0.45]
[101215,"Ex9C32  22 3P 110V ","Contactor, 3-pole, 32A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012166,1,8592765012166,20,28592765012160,"8536490099",0.45]
[101216,"Ex9C32  22 3P 48V ","Contactor, 3-pole, 32A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012173,1,8592765012173,20,28592765012177,"8536419089",0.45]
[101217,"Ex9C32  22 3P 42V ","Contactor, 3-pole, 32A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012180,1,8592765012180,20,28592765012184,"8536419089",0.45]
[101218,"Ex9C32  22 3P 36V ","Contactor, 3-pole, 32A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012197,1,8592765012197,20,28592765012191,"8536419089",0.45]
[101219,"Ex9C32  22 3P 24V ","Contactor, 3-pole, 32A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",57.27,0,57.27,8592765012203,1,8592765012203,20,28592765012207,"8536419089",0.45]
[101220,"Ex9C38  11 3P 415V ","Contactor, 3-pole, 38A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012210,1,8592765012210,20,28592765012214,"8536490099",0.45]
[101221,"Ex9C38  11 3P 400V ","Contactor, 3-pole, 38A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012227,1,8592765012227,20,28592765012221,"8536490099",0.45]
[101222,"Ex9C38  11 3P 380V ","Contactor, 3-pole, 38A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012234,1,8592765012234,20,28592765012238,"8536490099",0.45]
[101223,"Ex9C38  11 3P 240V ","Contactor, 3-pole, 38A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012241,1,8592765012241,20,28592765012245,"8536490099",0.45]
[101224,"Ex9C38  11 3P 230V ","Contactor, 3-pole, 38A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.5,0,57.5,8592765012258,1,8592765012258,20,28592765012252,"8536490099",0.45]
[101225,"Ex9C38  11 3P 220V ","Contactor, 3-pole, 38A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012265,1,8592765012265,20,28592765012269,"8536490099",0.45]
[101226,"Ex9C38  11 3P 127V ","Contactor, 3-pole, 38A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012272,1,8592765012272,20,28592765012276,"8536490099",0.45]
[101227,"Ex9C38  11 3P 110V ","Contactor, 3-pole, 38A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012289,1,8592765012289,20,28592765012283,"8536490099",0.45]
[101228,"Ex9C38  11 3P 48V ","Contactor, 3-pole, 38A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,{"$f":"NBA","v":0},{"$f":"E4226*(1-F4226)","v":64.06},8592765012296,1,8592765012296,20,28592765012290,"8536419089",0.45]
[101229,"Ex9C38  11 3P 42V ","Contactor, 3-pole, 38A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012302,1,8592765012302,20,28592765012306,"8536419089",0.45]
[101230,"Ex9C38  11 3P 36V ","Contactor, 3-pole, 38A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",64.06,0,64.06,8592765012319,1,8592765012319,20,28592765012313,"8536419089",0.45]
[101231,"Ex9C38  11 3P 24V ","Contactor, 3-pole, 38A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.5,0,57.5,8592765012326,1,8592765012326,20,28592765012320,"8536419089",0.45]
[101232,"Ex9C38  22 3P 415V ","Contactor, 3-pole, 38A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012333,1,8592765012333,20,28592765012337,"8536490099",0.45]
[101233,"Ex9C38  22 3P 400V ","Contactor, 3-pole, 38A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012340,1,8592765012340,20,28592765012344,"8536490099",0.45]
[101234,"Ex9C38  22 3P 380V ","Contactor, 3-pole, 38A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012357,1,8592765012357,20,28592765012351,"8536490099",0.45]
[101235,"Ex9C38  22 3P 240V ","Contactor, 3-pole, 38A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012364,1,8592765012364,20,28592765012368,"8536490099",0.45]
[101236,"Ex9C38  22 3P 230V ","Contactor, 3-pole, 38A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012371,1,8592765012371,20,28592765012375,"8536490099",0.45]
[101237,"Ex9C38  22 3P 220V ","Contactor, 3-pole, 38A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012388,1,8592765012388,20,28592765012382,"8536490099",0.45]
[101238,"Ex9C38  22 3P 127V ","Contactor, 3-pole, 38A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012395,1,8592765012395,20,28592765012399,"8536490099",0.45]
[101239,"Ex9C38  22 3P 110V ","Contactor, 3-pole, 38A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012401,1,8592765012401,20,28592765012405,"8536490099",0.45]
[101240,"Ex9C38  22 3P 48V ","Contactor, 3-pole, 38A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012418,1,8592765012418,20,28592765012412,"8536419089",0.45]
[101241,"Ex9C38  22 3P 42V ","Contactor, 3-pole, 38A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012425,1,8592765012425,20,28592765012429,"8536419089",0.45]
[101242,"Ex9C38  22 3P 36V ","Contactor, 3-pole, 38A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012432,1,8592765012432,20,28592765012436,"8536419089",0.45]
[101243,"Ex9C38  22 3P 24V ","Contactor, 3-pole, 38A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",72.930000000000007,0,72.930000000000007,8592765012449,1,8592765012449,20,28592765012443,"8536419089",0.45]
[101244,"Ex9C40  11 3P 415V ","Contactor, 3-pole, 40A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012456,1,8592765012456,12,28592765012450,"8536490099",1.3]
[101245,"Ex9C40  11 3P 400V ","Contactor, 3-pole, 40A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012463,1,8592765012463,12,28592765012467,"8536490099",1.3]
[101246,"Ex9C40  11 3P 380V ","Contactor, 3-pole, 40A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012470,1,8592765012470,12,28592765012474,"8536490099",1.3]
[101247,"Ex9C40  11 3P 240V ","Contactor, 3-pole, 40A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012487,1,8592765012487,12,28592765012481,"8536490099",1.3]
[101248,"Ex9C40  11 3P 230V ","Contactor, 3-pole, 40A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",63.22,0,63.22,8592765012494,1,8592765012494,12,28592765012498,"8536490099",1.3]
[101249,"Ex9C40  11 3P 220V ","Contactor, 3-pole, 40A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012500,1,8592765012500,12,28592765012504,"8536490099",1.3]
[101250,"Ex9C40  11 3P 127V ","Contactor, 3-pole, 40A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012517,1,8592765012517,12,28592765012511,"8536490099",1.3]
[101251,"Ex9C40  11 3P 110V ","Contactor, 3-pole, 40A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012524,1,8592765012524,12,28592765012528,"8536490099",1.3]
[101252,"Ex9C40  11 3P 48V ","Contactor, 3-pole, 40A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012531,1,8592765012531,12,28592765012535,"8536419089",1.3]
[101253,"Ex9C40  11 3P 42V ","Contactor, 3-pole, 40A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012548,1,8592765012548,12,28592765012542,"8536419089",1.3]
[101254,"Ex9C40  11 3P 36V ","Contactor, 3-pole, 40A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",71.040000000000006,0,71.040000000000006,8592765012555,1,8592765012555,12,28592765012559,"8536419089",1.3]
[101255,"Ex9C40  11 3P 24V ","Contactor, 3-pole, 40A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",63.22,0,63.22,8592765012562,1,8592765012562,12,28592765012566,"8536419089",1.3]
[101256,"Ex9C50  11 3P 415V ","Contactor, 3-pole, 50A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012579,1,8592765012579,12,28592765012573,"8536490099",1.3]
[101257,"Ex9C50  11 3P 400V ","Contactor, 3-pole, 50A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012586,1,8592765012586,12,28592765012580,"8536490099",1.3]
[101258,"Ex9C50  11 3P 380V ","Contactor, 3-pole, 50A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012593,1,8592765012593,12,28592765012597,"8536490099",1.3]
[101259,"Ex9C50  11 3P 240V ","Contactor, 3-pole, 50A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012609,1,8592765012609,12,28592765012603,"8536490099",1.3]
[101260,"Ex9C50  11 3P 230V ","Contactor, 3-pole, 50A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012616,1,8592765012616,12,28592765012610,"8536490099",1.3]
[101261,"Ex9C50  11 3P 220V ","Contactor, 3-pole, 50A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012623,1,8592765012623,12,28592765012627,"8536490099",1.3]
[101262,"Ex9C50  11 3P 127V ","Contactor, 3-pole, 50A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012630,1,8592765012630,12,28592765012634,"8536490099",1.3]
[101263,"Ex9C50  11 3P 110V ","Contactor, 3-pole, 50A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012647,1,8592765012647,12,28592765012641,"8536490099",1.3]
[101264,"Ex9C50  11 3P 48V ","Contactor, 3-pole, 50A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012654,1,8592765012654,12,28592765012658,"8536419089",1.3]
[101265,"Ex9C50  11 3P 42V ","Contactor, 3-pole, 50A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012661,1,8592765012661,12,28592765012665,"8536419089",1.3]
[101266,"Ex9C50  11 3P 36V ","Contactor, 3-pole, 50A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012678,1,8592765012678,12,28592765012672,"8536419089",1.3]
[101267,"Ex9C50  11 3P 24V ","Contactor, 3-pole, 50A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",83.65,0,83.65,8592765012685,1,8592765012685,12,28592765012689,"8536419089",1.3]
[101268,"Ex9C65  11 3P 415V ","Contactor, 3-pole, 65A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012692,1,8592765012692,12,28592765012696,"8536490099",1.3]
[101269,"Ex9C65  11 3P 400V ","Contactor, 3-pole, 65A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012708,1,8592765012708,12,28592765012702,"8536490099",1.3]
[101270,"Ex9C65  11 3P 380V ","Contactor, 3-pole, 65A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012715,1,8592765012715,12,28592765012719,"8536490099",1.3]
[101271,"Ex9C65  11 3P 240V ","Contactor, 3-pole, 65A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012722,1,8592765012722,12,28592765012726,"8536490099",1.3]
[101272,"Ex9C65  11 3P 230V ","Contactor, 3-pole, 65A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012739,1,8592765012739,12,28592765012733,"8536490099",1.3]
[101273,"Ex9C65  11 3P 220V ","Contactor, 3-pole, 65A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012746,1,8592765012746,12,28592765012740,"8536490099",1.3]
[101274,"Ex9C65  11 3P 127V ","Contactor, 3-pole, 65A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012753,1,8592765012753,12,28592765012757,"8536490099",1.3]
[101275,"Ex9C65  11 3P 110V ","Contactor, 3-pole, 65A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012760,1,8592765012760,12,28592765012764,"8536490099",1.3]
[101276,"Ex9C65  11 3P 48V ","Contactor, 3-pole, 65A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012777,1,8592765012777,12,28592765012771,"8536419089",1.3]
[101277,"Ex9C65  11 3P 42V ","Contactor, 3-pole, 65A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012784,1,8592765012784,12,28592765012788,"8536419089",1.3]
[101278,"Ex9C65  11 3P 36V ","Contactor, 3-pole, 65A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012791,1,8592765012791,12,28592765012795,"8536419089",1.3]
[101279,"Ex9C65  11 3P 24V ","Contactor, 3-pole, 65A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",116.98,0,116.98,8592765012807,1,8592765012807,12,28592765012801,"8536419089",1.3]
[101335,"Ex9C80 11 3P 415V ","Contactor, 3-pole, 80A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013361,1,8592765013361,12,28592765013365,"8536490099",1.6]
[101336,"Ex9C80 11 3P 400V ","Contactor, 3-pole, 80A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013378,1,8592765013378,12,28592765013372,"8536490099",1.6]
[101337,"Ex9C80 11 3P 380V ","Contactor, 3-pole, 80A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013385,1,8592765013385,12,28592765013389,"8536490099",1.6]
[101338,"Ex9C80 11 3P 240V ","Contactor, 3-pole, 80A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013392,1,8592765013392,12,28592765013396,"8536490099",1.6]
[101339,"Ex9C80 11 3P 230V ","Contactor, 3-pole, 80A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013408,1,8592765013408,12,28592765013402,"8536490099",1.6]
[101340,"Ex9C80 11 3P 220V ","Contactor, 3-pole, 80A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013415,1,8592765013415,12,28592765013419,"8536490099",1.6]
[101341,"Ex9C80 11 3P 127V ","Contactor, 3-pole, 80A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013422,1,8592765013422,12,28592765013426,"8536490099",1.6]
[101342,"Ex9C80 11 3P 110V ","Contactor, 3-pole, 80A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013439,1,8592765013439,12,28592765013433,"8536490099",1.6]
[101343,"Ex9C80 11 3P 48V ","Contactor, 3-pole, 80A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013446,1,8592765013446,12,28592765013440,"8536419089",1.6]
[101344,"Ex9C80 11 3P 42V ","Contactor, 3-pole, 80A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013453,1,8592765013453,12,28592765013457,"8536419089",1.6]
[101345,"Ex9C80 11 3P 36V ","Contactor, 3-pole, 80A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013460,1,8592765013460,12,28592765013464,"8536419089",1.6]
[101346,"Ex9C80 11 3P 24V ","Contactor, 3-pole, 80A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",139.99,0,139.99,8592765013477,1,8592765013477,12,28592765013471,"8536419089",1.6]
[101347,"Ex9C100 11 3P 415V ","Contactor, 3-pole, 100A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,{"$f":"NBA","v":0},{"$f":"E4290*(1-F4290)","v":200.71},8592765013484,1,8592765013484,12,28592765013488,"8536490099",1.6]
[101348,"Ex9C100 11 3P 400V ","Contactor, 3-pole, 100A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013491,1,8592765013491,12,28592765013495,"8536490099",1.6]
[101349,"Ex9C100 11 3P 380V ","Contactor, 3-pole, 100A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013507,1,8592765013507,12,28592765013501,"8536490099",1.6]
[101350,"Ex9C100 11 3P 240V ","Contactor, 3-pole, 100A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013514,1,8592765013514,12,28592765013518,"8536490099",1.6]
[101351,"Ex9C100 11 3P 230V ","Contactor, 3-pole, 100A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",180.64,0,180.64,8592765013521,1,8592765013521,12,28592765013525,"8536490099",1.6]
[101352,"Ex9C100 11 3P 220V ","Contactor, 3-pole, 100A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013538,1,8592765013538,12,28592765013532,"8536490099",1.6]
[101353,"Ex9C100 11 3P 127V","Contactor, 3-pole, 100A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013545,1,8592765013545,12,28592765013549,"8536490099",1.6]
[101354,"Ex9C100 11 3P 110V ","Contactor, 3-pole, 100A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013552,1,8592765013552,12,28592765013556,"8536490099",1.6]
[101355,"Ex9C100 11 3P 48V ","Contactor, 3-pole, 100A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013569,1,8592765013569,12,28592765013563,"8536419089",1.6]
[101356,"Ex9C100 11 3P 42V ","Contactor, 3-pole, 100A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013576,1,8592765013576,12,28592765013570,"8536419089",1.6]
[101357,"Ex9C100 11 3P 36V ","Contactor, 3-pole, 100A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",200.71,0,200.71,8592765013583,1,8592765013583,12,28592765013587,"8536419089",1.6]
[101358,"Ex9C100 11 3P 24V ","Contactor, 3-pole, 100A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",180.64,0,180.64,8592765013590,1,8592765013590,12,28592765013594,"8536419089",1.6]
[]
["Contactors Ex9C up to 500A"]
[106211,"Ex9C115 22 3P 48V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,{"$f":"NBA","v":0},{"$f":"E4304*(1-F4304)","v":299.07},8592765062123,1,8592765062123,2,28592765062127,"8536419089",3]
[106212,"Ex9C115 22 3P 42V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,{"$f":"NBA","v":0},299.07,8592765062130,1,8592765062130,2,28592765062134,"8536419089",3]
[106213,"Ex9C115 22 3P 415V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062147,1,8592765062147,2,28592765062141,"8536490099",3]
[106214,"Ex9C115 22 3P 400V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062154,1,8592765062154,2,28592765062158,"8536490099",3]
[106215,"Ex9C115 22 3P 380V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062161,1,8592765062161,2,28592765062165,"8536490099",3]
[106216,"Ex9C115 22 3P 36V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062178,1,8592765062178,2,28592765062172,"8536419089",3]
[106217,"Ex9C115 22 3P 24V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 24V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062185,1,8592765062185,2,28592765062189,"8536419089",3]
[106218,"Ex9C115 22 3P 240V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062192,1,8592765062192,2,28592765062196,"8536490099",3]
[106219,"Ex9C115 22 3P 230V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",269.66000000000003,0,269.66000000000003,8592765062208,1,8592765062208,2,28592765062202,"8536490099",3]
[106220,"Ex9C115 22 3P 220V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062215,1,8592765062215,2,28592765062219,"8536490099",3]
[106221,"Ex9C115 22 3P 127V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062222,1,8592765062222,2,28592765062226,"8536490099",3]
[106222,"Ex9C115 22 3P 110V AC/DC","Contactor, 3-pole, 115A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",299.07,0,299.07,8592765062239,1,8592765062239,2,28592765062233,"8536490099",3]
[106223,"Ex9C150 22 3P 48V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062246,1,8592765062246,2,28592765062240,"8536419089",3]
[106224,"Ex9C150 22 3P 42V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062253,1,8592765062253,2,28592765062257,"8536419089",3]
[106225,"Ex9C150 22 3P 415V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062260,1,8592765062260,2,28592765062264,"8536490099",3]
[106226,"Ex9C150 22 3P 400V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062277,1,8592765062277,2,28592765062271,"8536490099",3]
[106227,"Ex9C150 22 3P 380V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062284,1,8592765062284,2,28592765062288,"8536490099",3]
[106228,"Ex9C150 22 3P 36V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062291,1,8592765062291,2,28592765062295,"8536419089",3]
[106229,"Ex9C150 22 3P 24V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 24V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062307,1,8592765062307,2,28592765062301,"8536419089",3]
[106230,"Ex9C150 22 3P 240V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062314,1,8592765062314,2,28592765062318,"8536490099",3]
[106231,"Ex9C150 22 3P 230V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062321,1,8592765062321,2,28592765062325,"8536490099",3]
[106232,"Ex9C150 22 3P 220V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062338,1,8592765062338,2,28592765062332,"8536490099",3]
[106233,"Ex9C150 22 3P 127V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062345,1,8592765062345,2,28592765062349,"8536490099",3]
[106234,"Ex9C150 22 3P 110V AC/DC","Contactor, 3-pole, 150A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",366.44,0,366.44,8592765062352,1,8592765062352,2,28592765062356,"8536490099",3]
[106235,"Ex9C185 22 3P 48V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062369,1,8592765062369,2,28592765062363,"8536419089",3]
[106236,"Ex9C185 22 3P 42V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062376,1,8592765062376,2,28592765062370,"8536419089",3]
[106237,"Ex9C185 22 3P 415V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062383,1,8592765062383,2,28592765062387,"8536490099",3]
[106238,"Ex9C185 22 3P 400V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062390,1,8592765062390,2,28592765062394,"8536490099",3]
[106239,"Ex9C185 22 3P 380V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062406,1,8592765062406,2,28592765062400,"8536490099",3]
[106240,"Ex9C185 22 3P 36V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062413,1,8592765062413,2,28592765062417,"8536419089",3]
[106241,"Ex9C185 22 3P 24V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 24V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062420,1,8592765062420,2,28592765062424,"8536419089",3]
[106242,"Ex9C185 22 3P 240V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062437,1,8592765062437,2,28592765062431,"8536490099",3]
[106243,"Ex9C185 22 3P 230V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062444,1,8592765062444,2,28592765062448,"8536490099",3]
[106244,"Ex9C185 22 3P 220V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062451,1,8592765062451,2,28592765062455,"8536490099",3]
[106245,"Ex9C185 22 3P 127V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062468,1,8592765062468,2,28592765062462,"8536490099",3]
[106246,"Ex9C185 22 3P 110V AC/DC","Contactor, 3-pole, 185A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",428.06,0,428.06,8592765062475,1,8592765062475,2,28592765062479,"8536490099",3]
[106247,"Ex9C225 22 3P 48V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062482,1,8592765062482,2,28592765062486,"8536419089",6]
[106248,"Ex9C225 22 3P 42V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062499,1,8592765062499,2,28592765062493,"8536419089",6]
[106249,"Ex9C225 22 3P 415V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062505,1,8592765062505,2,28592765062509,"8536490099",6]
[106250,"Ex9C225 22 3P 400V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062512,1,8592765062512,2,28592765062516,"8536490099",6]
[106251,"Ex9C225 22 3P 380V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062529,1,8592765062529,2,28592765062523,"8536490099",6]
[106252,"Ex9C225 22 3P 36V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062536,1,8592765062536,2,28592765062530,"8536419089",6]
[106253,"Ex9C225 22 3P 24V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 24V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062543,1,8592765062543,2,28592765062547,"8536419089",6]
[106254,"Ex9C225 22 3P 240V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062550,1,8592765062550,2,28592765062554,"8536490099",6]
[106255,"Ex9C225 22 3P 230V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062567,1,8592765062567,2,28592765062561,"8536490099",6]
[106256,"Ex9C225 22 3P 220V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062574,1,8592765062574,2,28592765062578,"8536490099",6]
[106257,"Ex9C225 22 3P 127V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062581,1,8592765062581,2,28592765062585,"8536490099",6]
[106258,"Ex9C225 22 3P 110V AC/DC","Contactor, 3-pole, 225A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",491.35,0,491.35,8592765062598,1,8592765062598,2,28592765062592,"8536490099",6]
[106259,"Ex9C265 22 3P 48V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062604,1,8592765062604,2,28592765062608,"8536419089",6]
[106260,"Ex9C265 22 3P 42V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062611,1,8592765062611,2,28592765062615,"8536419089",6]
[106261,"Ex9C265 22 3P 415V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062628,1,8592765062628,2,28592765062622,"8536490099",6]
[106262,"Ex9C265 22 3P 400V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062635,1,8592765062635,2,28592765062639,"8536490099",6]
[106263,"Ex9C265 22 3P 380V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062642,1,8592765062642,2,28592765062646,"8536490099",6]
[106264,"Ex9C265 22 3P 36V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062659,1,8592765062659,2,28592765062653,"8536419089",6]
[106265,"Ex9C265 22 3P 24V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 24V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062666,1,8592765062666,2,28592765062660,"8536419089",6]
[106266,"Ex9C265 22 3P 240V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062673,1,8592765062673,2,28592765062677,"8536490099",6]
[106267,"Ex9C265 22 3P 230V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",599.80999999999995,0,599.80999999999995,8592765062680,1,8592765062680,2,28592765062684,"8536490099",6]
[106268,"Ex9C265 22 3P 220V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062697,1,8592765062697,2,28592765062691,"8536490099",6]
[106269,"Ex9C265 22 3P 127V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062703,1,8592765062703,2,28592765062707,"8536490099",6]
[106270,"Ex9C265 22 3P 110V AC/DC","Contactor, 3-pole, 265A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",722.65,0,722.65,8592765062710,1,8592765062710,2,28592765062714,"8536490099",6]
[106271,"Ex9C300 22 3P 48V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062727,1,8592765062727,2,28592765062721,"8536419089",6]
[106272,"Ex9C300 22 3P 42V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062734,1,8592765062734,2,28592765062738,"8536419089",6]
[106273,"Ex9C300 22 3P 415V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062741,1,8592765062741,2,28592765062745,"8536490099",6]
[106274,"Ex9C300 22 3P 400V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062758,1,8592765062758,2,28592765062752,"8536490099",6]
[106275,"Ex9C300 22 3P 380V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,{"$f":"E4368*(1-F4368)","v":864.69},8592765062765,1,8592765062765,2,28592765062769,"8536490099",6]
[106276,"Ex9C300 22 3P 36V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,{"$f":"NBA","v":0},864.69,8592765062772,1,8592765062772,2,28592765062776,"8536419089",6]
[106277,"Ex9C300 22 3P 24V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 24V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062789,1,8592765062789,2,28592765062783,"8536419089",6]
[106278,"Ex9C300 22 3P 240V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062796,1,8592765062796,2,28592765062790,"8536490099",6]
[106279,"Ex9C300 22 3P 230V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062802,1,8592765062802,2,28592765062806,"8536490099",6]
[106280,"Ex9C300 22 3P 220V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062819,1,8592765062819,2,28592765062813,"8536490099",6]
[106281,"Ex9C300 22 3P 127V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062826,1,8592765062826,2,28592765062820,"8536490099",6]
[106282,"Ex9C300 22 3P 110V AC/DC","Contactor, 3-pole, 300A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",864.69,0,864.69,8592765062833,1,8592765062833,2,28592765062837,"8536490099",6]
[106283,"Ex9C400 22 3P 48V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062840,1,8592765062840,1,28592765062844,"8536419089",9.5]
[106284,"Ex9C400 22 3P 42V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062857,1,8592765062857,1,28592765062851,"8536419089",9.5]
[106285,"Ex9C400 22 3P 415V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062864,1,8592765062864,1,28592765062868,"8536490099",9.5]
[106286,"Ex9C400 22 3P 400V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062871,1,8592765062871,1,28592765062875,"8536490099",9.5]
[106287,"Ex9C400 22 3P 380V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062888,1,8592765062888,1,28592765062882,"8536490099",9.5]
[106288,"Ex9C400 22 3P 36V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062895,1,8592765062895,1,28592765062899,"8536419089",9.5]
[106290,"Ex9C400 22 3P 240V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062918,1,8592765062918,1,28592765062912,"8536490099",9.5]
[106291,"Ex9C400 22 3P 230V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062925,1,8592765062925,1,28592765062929,"8536490099",9.5]
[106292,"Ex9C400 22 3P 220V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062932,1,8592765062932,1,28592765062936,"8536490099",9.5]
[106293,"Ex9C400 22 3P 127V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062949,1,8592765062949,1,28592765062943,"8536490099",9.5]
[106294,"Ex9C400 22 3P 110V AC/DC","Contactor, 3-pole, 400A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1264.75,0,1264.75,8592765062956,1,8592765062956,1,28592765062950,"8536490099",9.5]
[106295,"Ex9C500 22 3P 48V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 48V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765062963,1,8592765062963,1,28592765062967,"8536419089",9.5]
[106296,"Ex9C500 22 3P 42V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 42V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765062970,1,8592765062970,1,28592765062974,"8536419089",9.5]
[106297,"Ex9C500 22 3P 415V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 415V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765062987,1,8592765062987,1,28592765062981,"8536490099",9.5]
[106298,"Ex9C500 22 3P 400V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 400V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765062994,1,8592765062994,1,28592765062998,"8536490099",9.5]
[106299,"Ex9C500 22 3P 380V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 380V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765063007,1,8592765063007,1,28592765063001,"8536490099",9.5]
[106300,"Ex9C500 22 3P 36V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 36V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765063014,1,8592765063014,1,28592765063018,"8536419089",9.5]
[106302,"Ex9C500 22 3P 240V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 240V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765063038,1,8592765063038,1,28592765063032,"8536490099",9.5]
[106303,"Ex9C500 22 3P 230V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 230V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765063045,1,8592765063045,1,28592765063049,"8536490099",9.5]
[106304,"Ex9C500 22 3P 220V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 220V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765063052,1,8592765063052,1,28592765063056,"8536490099",9.5]
[106305,"Ex9C500 22 3P 127V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 127V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765063069,1,8592765063069,1,28592765063063,"8536490099",9.5]
[106306,"Ex9C500 22 3P 110V AC/DC","Contactor, 3-pole, 500A AC-3, control voltage 110V AC/DC, built-in 2NO+2NC aux. contacts","NBA",1742.31,0,1742.31,8592765063076,1,8592765063076,1,28592765063070,"8536490099",9.5]
[]
["Capacitor Contactors Ex9CC"]
[104194,"Ex9CC25 12 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,{"$f":"NBC","v":0},{"$f":"E4400*(1-F4400)","v":55.72},8592765041951,1,8592765041951,null,28592765041955,"8536490099",0.62]
[104195,"Ex9CC25 12 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,{"$f":"NBC","v":0},{"$f":"E4401*(1-F4401)","v":55.72},8592765041968,1,8592765041968,null,28592765041962,"8536490099",0.62]
[104196,"Ex9CC25 12 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,{"$f":"E4402*(1-F4402)","v":55.72},8592765041975,1,8592765041975,null,28592765041979,"8536490099",0.62]
[104197,"Ex9CC25 12 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765041982,1,8592765041982,null,28592765041986,"8536490099",0.62]
[104198,"Ex9CC25 12 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765041999,1,8592765041999,null,28592765041993,"8536490099",0.62]
[104199,"Ex9CC25 12 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042002,1,8592765042002,null,28592765042006,"8536419089",0.62]
[104200,"Ex9CC25 12 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042019,1,8592765042019,null,28592765042013,"8536419089",0.62]
[104201,"Ex9CC25 12 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042026,1,8592765042026,null,28592765042020,"8536490099",0.62]
[104202,"Ex9CC25 12 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042033,1,8592765042033,null,28592765042037,"8536490099",0.62]
[104203,"Ex9CC25 12 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042040,1,8592765042040,null,28592765042044,"8536490099",0.62]
[104204,"Ex9CC25 12 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042057,1,8592765042057,null,28592765042051,"8536419089",0.62]
[104205,"Ex9CC25 12 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042064,1,8592765042064,null,28592765042068,"8536419089",0.62]
[104206,"Ex9CC25 21 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042071,1,8592765042071,null,28592765042075,"8536490099",0.62]
[104207,"Ex9CC25 21 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042088,1,8592765042088,null,28592765042082,"8536490099",0.62]
[104208,"Ex9CC25 21 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042095,1,8592765042095,null,28592765042099,"8536490099",0.62]
[104209,"Ex9CC25 21 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042101,1,8592765042101,null,28592765042105,"8536490099",0.62]
[104210,"Ex9CC25 21 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042118,1,8592765042118,null,28592765042112,"8536490099",0.62]
[104211,"Ex9CC25 21 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042125,1,8592765042125,null,28592765042129,"8536419089",0.62]
[104212,"Ex9CC25 21 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042132,1,8592765042132,null,28592765042136,"8536419089",0.62]
[104213,"Ex9CC25 21 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042149,1,8592765042149,null,28592765042143,"8536490099",0.62]
[104214,"Ex9CC25 21 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042156,1,8592765042156,null,28592765042150,"8536490099",0.62]
[104215,"Ex9CC25 21 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042163,1,8592765042163,null,28592765042167,"8536490099",0.62]
[104216,"Ex9CC25 21 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042170,1,8592765042170,null,28592765042174,"8536419089",0.62]
[104217,"Ex9CC25 21 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",55.72,0,55.72,8592765042187,1,8592765042187,null,28592765042181,"8536419089",0.62]
[104218,"Ex9CC25 23 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042194,1,8592765042194,null,28592765042198,"8536490099",0.62]
[104219,"Ex9CC25 23 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042200,1,8592765042200,null,28592765042204,"8536490099",0.62]
[104220,"Ex9CC25 23 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042217,1,8592765042217,null,28592765042211,"8536490099",0.62]
[104221,"Ex9CC25 23 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042224,1,8592765042224,null,28592765042228,"8536490099",0.62]
[104222,"Ex9CC25 23 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042231,1,8592765042231,null,28592765042235,"8536490099",0.62]
[104223,"Ex9CC25 23 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042248,1,8592765042248,null,28592765042242,"8536419089",0.62]
[104224,"Ex9CC25 23 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042255,1,8592765042255,null,28592765042259,"8536419089",0.62]
[104225,"Ex9CC25 23 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042262,1,8592765042262,null,28592765042266,"8536490099",0.62]
[104226,"Ex9CC25 23 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042279,1,8592765042279,null,28592765042273,"8536490099",0.62]
[104227,"Ex9CC25 23 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042286,1,8592765042286,null,28592765042280,"8536490099",0.62]
[104228,"Ex9CC25 23 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042293,1,8592765042293,null,28592765042297,"8536419089",0.62]
[104229,"Ex9CC25 23 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042309,1,8592765042309,null,28592765042303,"8536419089",0.62]
[104230,"Ex9CC25 32 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042316,1,8592765042316,null,28592765042310,"8536490099",0.62]
[104231,"Ex9CC25 32 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042323,1,8592765042323,null,28592765042327,"8536490099",0.62]
[104232,"Ex9CC25 32 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042330,1,8592765042330,null,28592765042334,"8536490099",0.62]
[104233,"Ex9CC25 32 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042347,1,8592765042347,null,28592765042341,"8536490099",0.62]
[104234,"Ex9CC25 32 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042354,1,8592765042354,null,28592765042358,"8536490099",0.62]
[104235,"Ex9CC25 32 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042361,1,8592765042361,null,28592765042365,"8536419089",0.62]
[104236,"Ex9CC25 32 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042378,1,8592765042378,null,28592765042372,"8536419089",0.62]
[104237,"Ex9CC25 32 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042385,1,8592765042385,null,28592765042389,"8536490099",0.62]
[104238,"Ex9CC25 32 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042392,1,8592765042392,null,28592765042396,"8536490099",0.62]
[104239,"Ex9CC25 32 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042408,1,8592765042408,null,28592765042402,"8536490099",0.62]
[104240,"Ex9CC25 32 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042415,1,8592765042415,null,28592765042419,"8536419089",0.62]
[104241,"Ex9CC25 32 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 25 A, for compensation up to 16 kvar at 400 V AC","NBC",66.37,0,66.37,8592765042422,1,8592765042422,null,28592765042426,"8536419089",0.62]
[104242,"Ex9CC38 12 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042439,1,8592765042439,null,28592765042433,"8536490099",0.62]
[104243,"Ex9CC38 12 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042446,1,8592765042446,null,28592765042440,"8536490099",0.62]
[104244,"Ex9CC38 12 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042453,1,8592765042453,null,28592765042457,"8536490099",0.62]
[104245,"Ex9CC38 12 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042460,1,8592765042460,null,28592765042464,"8536490099",0.62]
[104246,"Ex9CC38 12 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042477,1,8592765042477,null,28592765042471,"8536490099",0.62]
[104247,"Ex9CC38 12 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042484,1,8592765042484,null,28592765042488,"8536419089",0.62]
[104248,"Ex9CC38 12 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042491,1,8592765042491,null,28592765042495,"8536419089",0.62]
[104249,"Ex9CC38 12 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042507,1,8592765042507,null,28592765042501,"8536490099",0.62]
[104250,"Ex9CC38 12 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042514,1,8592765042514,null,28592765042518,"8536490099",0.62]
[104251,"Ex9CC38 12 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042521,1,8592765042521,null,28592765042525,"8536490099",0.62]
[104252,"Ex9CC38 12 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042538,1,8592765042538,null,28592765042532,"8536419089",0.62]
[104253,"Ex9CC38 12 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042545,1,8592765042545,null,28592765042549,"8536419089",0.62]
[104254,"Ex9CC38 21 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042552,1,8592765042552,null,28592765042556,"8536490099",0.62]
[104255,"Ex9CC38 21 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042569,1,8592765042569,null,28592765042563,"8536490099",0.62]
[104256,"Ex9CC38 21 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042576,1,8592765042576,null,28592765042570,"8536490099",0.62]
[104257,"Ex9CC38 21 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042583,1,8592765042583,null,28592765042587,"8536490099",0.62]
[104258,"Ex9CC38 21 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042590,1,8592765042590,null,28592765042594,"8536490099",0.62]
[104259,"Ex9CC38 21 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,{"$f":"NBC","v":0},72.14,8592765042606,1,8592765042606,null,28592765042600,"8536419089",0.62]
[104260,"Ex9CC38 21 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,{"$f":"E4466*(1-F4466)","v":72.14},8592765042613,1,8592765042613,null,28592765042617,"8536419089",0.62]
[104261,"Ex9CC38 21 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042620,1,8592765042620,null,28592765042624,"8536490099",0.62]
[104262,"Ex9CC38 21 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042637,1,8592765042637,null,28592765042631,"8536490099",0.62]
[104263,"Ex9CC38 21 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042644,1,8592765042644,null,28592765042648,"8536490099",0.62]
[104264,"Ex9CC38 21 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042651,1,8592765042651,null,28592765042655,"8536419089",0.62]
[104265,"Ex9CC38 21 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042668,1,8592765042668,null,28592765042662,"8536419089",0.62]
[104266,"Ex9CC38 23 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042675,1,8592765042675,null,28592765042679,"8536490099",0.62]
[104267,"Ex9CC38 23 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042682,1,8592765042682,null,28592765042686,"8536490099",0.62]
[104268,"Ex9CC38 23 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042699,1,8592765042699,null,28592765042693,"8536490099",0.62]
[104269,"Ex9CC38 23 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042705,1,8592765042705,null,28592765042709,"8536490099",0.62]
[104270,"Ex9CC38 23 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",72.14,0,72.14,8592765042712,1,8592765042712,null,28592765042716,"8536490099",0.62]
[104271,"Ex9CC38 23 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042729,1,8592765042729,null,28592765042723,"8536419089",0.62]
[104272,"Ex9CC38 23 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042736,1,8592765042736,null,28592765042730,"8536419089",0.62]
[104273,"Ex9CC38 23 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042743,1,8592765042743,null,28592765042747,"8536490099",0.62]
[104274,"Ex9CC38 23 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042750,1,8592765042750,null,28592765042754,"8536490099",0.62]
[104275,"Ex9CC38 23 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042767,1,8592765042767,null,28592765042761,"8536490099",0.62]
[104276,"Ex9CC38 23 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042774,1,8592765042774,null,28592765042778,"8536419089",0.62]
[104277,"Ex9CC38 23 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042781,1,8592765042781,null,28592765042785,"8536419089",0.62]
[104278,"Ex9CC38 32 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042798,1,8592765042798,null,28592765042792,"8536490099",0.62]
[104279,"Ex9CC38 32 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042804,1,8592765042804,null,28592765042808,"8536490099",0.62]
[104280,"Ex9CC38 32 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042811,1,8592765042811,null,28592765042815,"8536490099",0.62]
[104281,"Ex9CC38 32 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042828,1,8592765042828,null,28592765042822,"8536490099",0.62]
[104282,"Ex9CC38 32 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042835,1,8592765042835,null,28592765042839,"8536490099",0.62]
[104283,"Ex9CC38 32 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042842,1,8592765042842,null,28592765042846,"8536419089",0.62]
[104284,"Ex9CC38 32 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042859,1,8592765042859,null,28592765042853,"8536419089",0.62]
[104285,"Ex9CC38 32 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042866,1,8592765042866,null,28592765042860,"8536490099",0.62]
[104286,"Ex9CC38 32 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042873,1,8592765042873,null,28592765042877,"8536490099",0.62]
[104287,"Ex9CC38 32 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042880,1,8592765042880,null,28592765042884,"8536490099",0.62]
[104288,"Ex9CC38 32 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042897,1,8592765042897,null,28592765042891,"8536419089",0.62]
[104289,"Ex9CC38 32 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 38 A, for compensation up to 25 kvar at 400 V AC","NBC",85.93,0,85.93,8592765042903,1,8592765042903,null,28592765042907,"8536419089",0.62]
[104290,"Ex9CC50 12 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042910,1,8592765042910,null,28592765042914,"8536490099",1.65]
[104291,"Ex9CC50 12 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042927,1,8592765042927,null,28592765042921,"8536490099",1.65]
[104292,"Ex9CC50 12 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042934,1,8592765042934,null,28592765042938,"8536490099",1.65]
[104293,"Ex9CC50 12 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042941,1,8592765042941,null,28592765042945,"8536490099",1.65]
[104294,"Ex9CC50 12 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042958,1,8592765042958,null,28592765042952,"8536490099",1.65]
[104295,"Ex9CC50 12 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042965,1,8592765042965,null,28592765042969,"8536419089",1.65]
[104296,"Ex9CC50 12 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042972,1,8592765042972,null,28592765042976,"8536419089",1.65]
[104297,"Ex9CC50 12 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042989,1,8592765042989,null,28592765042983,"8536490099",1.65]
[104298,"Ex9CC50 12 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765042996,1,8592765042996,null,28592765042990,"8536490099",1.65]
[104299,"Ex9CC50 12 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765043009,1,8592765043009,null,28592765043003,"8536490099",1.65]
[104300,"Ex9CC50 12 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765043016,1,8592765043016,null,28592765043010,"8536419089",1.65]
[104301,"Ex9CC50 12 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",98.09,0,98.09,8592765043023,1,8592765043023,null,28592765043027,"8536419089",1.65]
[104302,"Ex9CC50 21 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043030,1,8592765043030,null,28592765043034,"8536490099",1.65]
[104303,"Ex9CC50 21 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043047,1,8592765043047,null,28592765043041,"8536490099",1.65]
[104304,"Ex9CC50 21 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043054,1,8592765043054,null,28592765043058,"8536490099",1.65]
[104305,"Ex9CC50 21 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043061,1,8592765043061,null,28592765043065,"8536490099",1.65]
[104306,"Ex9CC50 21 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043078,1,8592765043078,null,28592765043072,"8536490099",1.65]
[104307,"Ex9CC50 21 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043085,1,8592765043085,null,28592765043089,"8536419089",1.65]
[104308,"Ex9CC50 21 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043092,1,8592765043092,null,28592765043096,"8536419089",1.65]
[104309,"Ex9CC50 21 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043108,1,8592765043108,null,28592765043102,"8536490099",1.65]
[104310,"Ex9CC50 21 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043115,1,8592765043115,null,28592765043119,"8536490099",1.65]
[104311,"Ex9CC50 21 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043122,1,8592765043122,null,28592765043126,"8536490099",1.65]
[104312,"Ex9CC50 21 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043139,1,8592765043139,null,28592765043133,"8536419089",1.65]
[104313,"Ex9CC50 21 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 50 A, for compensation up to 30 kvar at 400 V AC","NBC",101.6,0,101.6,8592765043146,1,8592765043146,null,28592765043140,"8536419089",1.65]
[104314,"Ex9CC65 12 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043153,1,8592765043153,null,28592765043157,"8536490099",1.65]
[104315,"Ex9CC65 12 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043160,1,8592765043160,null,28592765043164,"8536490099",1.65]
[104316,"Ex9CC65 12 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043177,1,8592765043177,null,28592765043171,"8536490099",1.65]
[104317,"Ex9CC65 12 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043184,1,8592765043184,null,28592765043188,"8536490099",1.65]
[104318,"Ex9CC65 12 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043191,1,8592765043191,null,28592765043195,"8536490099",1.65]
[104319,"Ex9CC65 12 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043207,1,8592765043207,null,28592765043201,"8536419089",1.65]
[104320,"Ex9CC65 12 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043214,1,8592765043214,null,28592765043218,"8536419089",1.65]
[104321,"Ex9CC65 12 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043221,1,8592765043221,null,28592765043225,"8536490099",1.65]
[104322,"Ex9CC65 12 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043238,1,8592765043238,null,28592765043232,"8536490099",1.65]
[104323,"Ex9CC65 12 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,{"$f":"NBC","v":0},121.06,8592765043245,1,8592765043245,null,28592765043249,"8536490099",1.65]
[104324,"Ex9CC65 12 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,{"$f":"E4530*(1-F4530)","v":121.06},8592765043252,1,8592765043252,null,28592765043256,"8536419089",1.65]
[104325,"Ex9CC65 12 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043269,1,8592765043269,null,28592765043263,"8536419089",1.65]
[104326,"Ex9CC65 21 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043276,1,8592765043276,null,28592765043270,"8536490099",1.65]
[104327,"Ex9CC65 21 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043283,1,8592765043283,null,28592765043287,"8536490099",1.65]
[104328,"Ex9CC65 21 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043290,1,8592765043290,null,28592765043294,"8536490099",1.65]
[104329,"Ex9CC65 21 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043306,1,8592765043306,null,28592765043300,"8536490099",1.65]
[104330,"Ex9CC65 21 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043313,1,8592765043313,null,28592765043317,"8536490099",1.65]
[104331,"Ex9CC65 21 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043320,1,8592765043320,null,28592765043324,"8536419089",1.65]
[104332,"Ex9CC65 21 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043337,1,8592765043337,null,28592765043331,"8536419089",1.65]
[104333,"Ex9CC65 21 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043344,1,8592765043344,null,28592765043348,"8536490099",1.65]
[104334,"Ex9CC65 21 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043351,1,8592765043351,null,28592765043355,"8536490099",1.65]
[104335,"Ex9CC65 21 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043368,1,8592765043368,null,28592765043362,"8536490099",1.65]
[104336,"Ex9CC65 21 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043375,1,8592765043375,null,28592765043379,"8536419089",1.65]
[104337,"Ex9CC65 21 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 65 A, for compensation up to 40 kvar at 400 V AC","NBC",121.06,0,121.06,8592765043382,1,8592765043382,null,28592765043386,"8536419089",1.65]
[104338,"Ex9CC80 12 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043399,1,8592765043399,null,28592765043393,"8536490099",1.9]
[104339,"Ex9CC80 12 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043405,1,8592765043405,null,28592765043409,"8536490099",1.9]
[104340,"Ex9CC80 12 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043412,1,8592765043412,null,28592765043416,"8536490099",1.9]
[104341,"Ex9CC80 12 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043429,1,8592765043429,null,28592765043423,"8536490099",1.9]
[104342,"Ex9CC80 12 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043436,1,8592765043436,null,28592765043430,"8536490099",1.9]
[104343,"Ex9CC80 12 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043443,1,8592765043443,null,28592765043447,"8536419089",1.9]
[104344,"Ex9CC80 12 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043450,1,8592765043450,null,28592765043454,"8536419089",1.9]
[104345,"Ex9CC80 12 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043467,1,8592765043467,null,28592765043461,"8536490099",1.9]
[104346,"Ex9CC80 12 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043474,1,8592765043474,null,28592765043478,"8536490099",1.9]
[104347,"Ex9CC80 12 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043481,1,8592765043481,null,28592765043485,"8536490099",1.9]
[104348,"Ex9CC80 12 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043498,1,8592765043498,null,28592765043492,"8536419089",1.9]
[104349,"Ex9CC80 12 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043504,1,8592765043504,null,28592765043508,"8536419089",1.9]
[104350,"Ex9CC80 21 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043511,1,8592765043511,null,28592765043515,"8536490099",1.9]
[104351,"Ex9CC80 21 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043528,1,8592765043528,null,28592765043522,"8536490099",1.9]
[104352,"Ex9CC80 21 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043535,1,8592765043535,null,28592765043539,"8536490099",1.9]
[104353,"Ex9CC80 21 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043542,1,8592765043542,null,28592765043546,"8536490099",1.9]
[104354,"Ex9CC80 21 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043559,1,8592765043559,null,28592765043553,"8536490099",1.9]
[104355,"Ex9CC80 21 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043566,1,8592765043566,null,28592765043560,"8536419089",1.9]
[104356,"Ex9CC80 21 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043573,1,8592765043573,null,28592765043577,"8536419089",1.9]
[104357,"Ex9CC80 21 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043580,1,8592765043580,null,28592765043584,"8536490099",1.9]
[104358,"Ex9CC80 21 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043597,1,8592765043597,null,28592765043591,"8536490099",1.9]
[104359,"Ex9CC80 21 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043603,1,8592765043603,null,28592765043607,"8536490099",1.9]
[104360,"Ex9CC80 21 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043610,1,8592765043610,null,28592765043614,"8536419089",1.9]
[104361,"Ex9CC80 21 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 80 A, for compensation up to 50 kvar at 400 V AC","NBC",159.94,0,159.94,8592765043627,1,8592765043627,null,28592765043621,"8536419089",1.9]
[104362,"Ex9CC100 12 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043634,1,8592765043634,null,28592765043638,"8536490099",1.9]
[104363,"Ex9CC100 12 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043641,1,8592765043641,null,28592765043645,"8536490099",1.9]
[104364,"Ex9CC100 12 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043658,1,8592765043658,null,28592765043652,"8536490099",1.9]
[104365,"Ex9CC100 12 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043665,1,8592765043665,null,28592765043669,"8536490099",1.9]
[104366,"Ex9CC100 12 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043672,1,8592765043672,null,28592765043676,"8536490099",1.9]
[104367,"Ex9CC100 12 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043689,1,8592765043689,null,28592765043683,"8536419089",1.9]
[104368,"Ex9CC100 12 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043696,1,8592765043696,null,28592765043690,"8536419089",1.9]
[104369,"Ex9CC100 12 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043702,1,8592765043702,null,28592765043706,"8536490099",1.9]
[104370,"Ex9CC100 12 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043719,1,8592765043719,null,28592765043713,"8536490099",1.9]
[104371,"Ex9CC100 12 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043726,1,8592765043726,null,28592765043720,"8536490099",1.9]
[104372,"Ex9CC100 12 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043733,1,8592765043733,null,28592765043737,"8536419089",1.9]
[104373,"Ex9CC100 12 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043740,1,8592765043740,null,28592765043744,"8536419089",1.9]
[104374,"Ex9CC100 21 3P 110V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043757,1,8592765043757,null,28592765043751,"8536490099",1.9]
[104375,"Ex9CC100 21 3P 127V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043764,1,8592765043764,null,28592765043768,"8536490099",1.9]
[104376,"Ex9CC100 21 3P 220V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043771,1,8592765043771,null,28592765043775,"8536490099",1.9]
[104377,"Ex9CC100 21 3P 230V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043788,1,8592765043788,null,28592765043782,"8536490099",1.9]
[104378,"Ex9CC100 21 3P 240V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043795,1,8592765043795,null,28592765043799,"8536490099",1.9]
[104379,"Ex9CC100 21 3P 24V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043801,1,8592765043801,null,28592765043805,"8536419089",1.9]
[104380,"Ex9CC100 21 3P 36V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043818,1,8592765043818,null,28592765043812,"8536419089",1.9]
[104381,"Ex9CC100 21 3P 380V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043825,1,8592765043825,null,28592765043829,"8536490099",1.9]
[104382,"Ex9CC100 21 3P 400V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043832,1,8592765043832,null,28592765043836,"8536490099",1.9]
[104383,"Ex9CC100 21 3P 415V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043849,1,8592765043849,null,28592765043843,"8536490099",1.9]
[104384,"Ex9CC100 21 3P 42V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043856,1,8592765043856,null,28592765043850,"8536419089",1.9]
[104385,"Ex9CC100 21 3P 48V","Contactor for switching of capacity loads,rated current AC-6b up to 100 A, for compensation up to 60 kvar at 400 V AC","NBC",207.94,0,207.94,8592765043863,1,8592765043863,null,28592765043867,"8536419089",1.9]
[]
["Reversible contactors Ex9CR"]
[104648,"Ex9CR09 22 3P 48V","Reversible contactor, 3-pole, 9A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,{"$f":"NBA","v":0},{"$f":"E4594*(1-F4594)","v":62.88},8592765046499,1,8592765046499,null,28592765046493,"8536419089",0.72]
[104649,"Ex9CR09 22 3P 42V","Reversible contactor, 3-pole, 9A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,{"$f":"E4595*(1-F4595)","v":62.88},8592765046505,1,8592765046505,null,28592765046509,"8536419089",0.72]
[104650,"Ex9CR09 22 3P 415V","Reversible contactor, 3-pole, 9A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046512,1,8592765046512,null,28592765046516,"8536490099",0.72]
[104651,"Ex9CR09 22 3P 400V","Reversible contactor, 3-pole, 9A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046529,1,8592765046529,null,28592765046523,"8536490099",0.72]
[104652,"Ex9CR09 22 3P 380V","Reversible contactor, 3-pole, 9A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046536,1,8592765046536,null,28592765046530,"8536490099",0.72]
[104653,"Ex9CR09 22 3P 36V","Reversible contactor, 3-pole, 9A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046543,1,8592765046543,null,28592765046547,"8536419089",0.72]
[104654,"Ex9CR09 22 3P 24V","Reversible contactor, 3-pole, 9A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046550,1,8592765046550,null,28592765046554,"8536419089",0.72]
[104655,"Ex9CR09 22 3P 240V","Reversible contactor, 3-pole, 9A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046567,1,8592765046567,null,28592765046561,"8536490099",0.72]
[104656,"Ex9CR09 22 3P 230V","Reversible contactor, 3-pole, 9A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046574,1,8592765046574,null,28592765046578,"8536490099",0.72]
[104657,"Ex9CR09 22 3P 220V","Reversible contactor, 3-pole, 9A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046581,1,8592765046581,null,28592765046585,"8536490099",0.72]
[104658,"Ex9CR09 22 3P 127V","Reversible contactor, 3-pole, 9A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046598,1,8592765046598,null,28592765046592,"8536490099",0.72]
[104659,"Ex9CR09 22 3P 110V","Reversible contactor, 3-pole, 9A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",62.88,0,62.88,8592765046604,1,8592765046604,null,28592765046608,"8536490099",0.72]
[104660,"Ex9CR09 11 3P 48V","Reversible contactor, 3-pole, 9A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046611,1,8592765046611,null,28592765046615,"8536419089",0.72]
[104661,"Ex9CR09 11 3P 42V","Reversible contactor, 3-pole, 9A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046628,1,8592765046628,null,28592765046622,"8536419089",0.72]
[104662,"Ex9CR09 11 3P 415V","Reversible contactor, 3-pole, 9A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046635,1,8592765046635,null,28592765046639,"8536490099",0.72]
[104663,"Ex9CR09 11 3P 400V","Reversible contactor, 3-pole, 9A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046642,1,8592765046642,null,28592765046646,"8536490099",0.72]
[104664,"Ex9CR09 11 3P 380V","Reversible contactor, 3-pole, 9A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046659,1,8592765046659,null,28592765046653,"8536490099",0.72]
[104665,"Ex9CR09 11 3P 36V","Reversible contactor, 3-pole, 9A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046666,1,8592765046666,null,28592765046660,"8536419089",0.72]
[104666,"Ex9CR09 11 3P 24V","Reversible contactor, 3-pole, 9A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046673,1,8592765046673,null,28592765046677,"8536419089",0.72]
[104667,"Ex9CR09 11 3P 240V","Reversible contactor, 3-pole, 9A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046680,1,8592765046680,null,28592765046684,"8536490099",0.72]
[104668,"Ex9CR09 11 3P 230V","Reversible contactor, 3-pole, 9A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046697,1,8592765046697,null,28592765046691,"8536490099",0.72]
[104669,"Ex9CR09 11 3P 220V","Reversible contactor, 3-pole, 9A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046703,1,8592765046703,null,28592765046707,"8536490099",0.72]
[104670,"Ex9CR09 11 3P 127V","Reversible contactor, 3-pole, 9A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046710,1,8592765046710,null,28592765046714,"8536490099",0.72]
[104671,"Ex9CR09 11 3P 110V","Reversible contactor, 3-pole, 9A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",57.17,0,57.17,8592765046727,1,8592765046727,null,28592765046721,"8536490099",0.72]
[104672,"Ex9CR12 22 3P 48V","Reversible contactor, 3-pole, 12A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046734,1,8592765046734,null,28592765046738,"8536419089",0.72]
[104673,"Ex9CR12 22 3P 42V","Reversible contactor, 3-pole, 12A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046741,1,8592765046741,null,28592765046745,"8536419089",0.72]
[104674,"Ex9CR12 22 3P 415V","Reversible contactor, 3-pole, 12A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046758,1,8592765046758,null,28592765046752,"8536490099",0.72]
[104675,"Ex9CR12 22 3P 400V","Reversible contactor, 3-pole, 12A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046765,1,8592765046765,null,28592765046769,"8536490099",0.72]
[104676,"Ex9CR12 22 3P 380V","Reversible contactor, 3-pole, 12A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046772,1,8592765046772,null,28592765046776,"8536490099",0.72]
[104677,"Ex9CR12 22 3P 36V","Reversible contactor, 3-pole, 12A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046789,1,8592765046789,null,28592765046783,"8536419089",0.72]
[104678,"Ex9CR12 22 3P 24V","Reversible contactor, 3-pole, 12A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046796,1,8592765046796,null,28592765046790,"8536419089",0.72]
[104679,"Ex9CR12 22 3P 240V","Reversible contactor, 3-pole, 12A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046802,1,8592765046802,null,28592765046806,"8536490099",0.72]
[104680,"Ex9CR12 22 3P 230V","Reversible contactor, 3-pole, 12A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046819,1,8592765046819,null,28592765046813,"8536490099",0.72]
[104681,"Ex9CR12 22 3P 220V","Reversible contactor, 3-pole, 12A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046826,1,8592765046826,null,28592765046820,"8536490099",0.72]
[104682,"Ex9CR12 22 3P 127V","Reversible contactor, 3-pole, 12A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046833,1,8592765046833,null,28592765046837,"8536490099",0.72]
[104683,"Ex9CR12 22 3P 110V","Reversible contactor, 3-pole, 12A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",76.430000000000007,0,76.430000000000007,8592765046840,1,8592765046840,null,28592765046844,"8536490099",0.72]
[104684,"Ex9CR12 11 3P 48V","Reversible contactor, 3-pole, 12A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046857,1,8592765046857,null,28592765046851,"8536419089",0.72]
[104685,"Ex9CR12 11 3P 42V","Reversible contactor, 3-pole, 12A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046864,1,8592765046864,null,28592765046868,"8536419089",0.72]
[104686,"Ex9CR12 11 3P 415V","Reversible contactor, 3-pole, 12A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046871,1,8592765046871,null,28592765046875,"8536490099",0.72]
[104687,"Ex9CR12 11 3P 400V","Reversible contactor, 3-pole, 12A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046888,1,8592765046888,null,28592765046882,"8536490099",0.72]
[104688,"Ex9CR12 11 3P 380V","Reversible contactor, 3-pole, 12A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046895,1,8592765046895,null,28592765046899,"8536490099",0.72]
[104689,"Ex9CR12 11 3P 36V","Reversible contactor, 3-pole, 12A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046901,1,8592765046901,null,28592765046905,"8536419089",0.72]
[104690,"Ex9CR12 11 3P 24V","Reversible contactor, 3-pole, 12A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046918,1,8592765046918,null,28592765046912,"8536419089",0.72]
[104691,"Ex9CR12 11 3P 240V","Reversible contactor, 3-pole, 12A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046925,1,8592765046925,null,28592765046929,"8536490099",0.72]
[104692,"Ex9CR12 11 3P 230V","Reversible contactor, 3-pole, 12A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046932,1,8592765046932,null,28592765046936,"8536490099",0.72]
[104693,"Ex9CR12 11 3P 220V","Reversible contactor, 3-pole, 12A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046949,1,8592765046949,null,28592765046943,"8536490099",0.72]
[104694,"Ex9CR12 11 3P 127V","Reversible contactor, 3-pole, 12A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046956,1,8592765046956,null,28592765046950,"8536490099",0.72]
[104695,"Ex9CR12 11 3P 110V","Reversible contactor, 3-pole, 12A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",69.48,0,69.48,8592765046963,1,8592765046963,null,28592765046967,"8536490099",0.72]
[104696,"Ex9CR18 22 3P 48V","Reversible contactor, 3-pole, 18A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765046970,1,8592765046970,null,28592765046974,"8536419089",0.72]
[104697,"Ex9CR18 22 3P 42V","Reversible contactor, 3-pole, 18A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765046987,1,8592765046987,null,28592765046981,"8536419089",0.72]
[104698,"Ex9CR18 22 3P 415V","Reversible contactor, 3-pole, 18A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765046994,1,8592765046994,null,28592765046998,"8536490099",0.72]
[104699,"Ex9CR18 22 3P 400V","Reversible contactor, 3-pole, 18A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047007,1,8592765047007,null,28592765047001,"8536490099",0.72]
[104700,"Ex9CR18 22 3P 380V","Reversible contactor, 3-pole, 18A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047014,1,8592765047014,null,28592765047018,"8536490099",0.72]
[104701,"Ex9CR18 22 3P 36V","Reversible contactor, 3-pole, 18A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047021,1,8592765047021,null,28592765047025,"8536419089",0.72]
[104702,"Ex9CR18 22 3P 24V","Reversible contactor, 3-pole, 18A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047038,1,8592765047038,null,28592765047032,"8536419089",0.72]
[104703,"Ex9CR18 22 3P 240V","Reversible contactor, 3-pole, 18A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047045,1,8592765047045,null,28592765047049,"8536490099",0.72]
[104704,"Ex9CR18 22 3P 230V","Reversible contactor, 3-pole, 18A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047052,1,8592765047052,null,28592765047056,"8536490099",0.72]
[104705,"Ex9CR18 22 3P 220V","Reversible contactor, 3-pole, 18A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047069,1,8592765047069,null,28592765047063,"8536490099",0.72]
[104706,"Ex9CR18 22 3P 127V","Reversible contactor, 3-pole, 18A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047076,1,8592765047076,null,28592765047070,"8536490099",0.72]
[104707,"Ex9CR18 22 3P 110V","Reversible contactor, 3-pole, 18A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",101.9,0,101.9,8592765047083,1,8592765047083,null,28592765047087,"8536490099",0.72]
[104708,"Ex9CR18 11 3P 48V","Reversible contactor, 3-pole, 18A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047090,1,8592765047090,null,28592765047094,"8536419089",0.72]
[104709,"Ex9CR18 11 3P 42V","Reversible contactor, 3-pole, 18A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047106,1,8592765047106,null,28592765047100,"8536419089",0.72]
[104710,"Ex9CR18 11 3P 415V","Reversible contactor, 3-pole, 18A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047113,1,8592765047113,null,28592765047117,"8536490099",0.72]
[104711,"Ex9CR18 11 3P 400V","Reversible contactor, 3-pole, 18A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047120,1,8592765047120,null,28592765047124,"8536490099",0.72]
[104712,"Ex9CR18 11 3P 380V","Reversible contactor, 3-pole, 18A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,{"$f":"NBA","v":0},92.64,8592765047137,1,8592765047137,null,28592765047131,"8536490099",0.72]
[104713,"Ex9CR18 11 3P 36V","Reversible contactor, 3-pole, 18A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,{"$f":"E4659*(1-F4659)","v":92.64},8592765047144,1,8592765047144,null,28592765047148,"8536419089",0.72]
[104714,"Ex9CR18 11 3P 24V","Reversible contactor, 3-pole, 18A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047151,1,8592765047151,null,28592765047155,"8536419089",0.72]
[104715,"Ex9CR18 11 3P 240V","Reversible contactor, 3-pole, 18A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047168,1,8592765047168,null,28592765047162,"8536490099",0.72]
[104716,"Ex9CR18 11 3P 230V","Reversible contactor, 3-pole, 18A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047175,1,8592765047175,null,28592765047179,"8536490099",0.72]
[104717,"Ex9CR18 11 3P 220V","Reversible contactor, 3-pole, 18A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047182,1,8592765047182,null,28592765047186,"8536490099",0.72]
[104718,"Ex9CR18 11 3P 127V","Reversible contactor, 3-pole, 18A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047199,1,8592765047199,null,28592765047193,"8536490099",0.72]
[104719,"Ex9CR18 11 3P 110V","Reversible contactor, 3-pole, 18A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",92.64,0,92.64,8592765047205,1,8592765047205,null,28592765047209,"8536490099",0.72]
[104720,"Ex9CR25 22 3P 48V","Reversible contactor, 3-pole, 25A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047212,1,8592765047212,null,28592765047216,"8536419089",0.82]
[104721,"Ex9CR25 22 3P 42V","Reversible contactor, 3-pole, 25A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047229,1,8592765047229,null,28592765047223,"8536419089",0.82]
[104722,"Ex9CR25 22 3P 415V","Reversible contactor, 3-pole, 25A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047236,1,8592765047236,null,28592765047230,"8536490099",0.82]
[104723,"Ex9CR25 22 3P 400V","Reversible contactor, 3-pole, 25A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047243,1,8592765047243,null,28592765047247,"8536490099",0.82]
[104724,"Ex9CR25 22 3P 380V","Reversible contactor, 3-pole, 25A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047250,1,8592765047250,null,28592765047254,"8536490099",0.82]
[104725,"Ex9CR25 22 3P 36V","Reversible contactor, 3-pole, 25A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047267,1,8592765047267,null,28592765047261,"8536419089",0.82]
[104726,"Ex9CR25 22 3P 24V","Reversible contactor, 3-pole, 25A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047274,1,8592765047274,null,28592765047278,"8536419089",0.82]
[104727,"Ex9CR25 22 3P 240V","Reversible contactor, 3-pole, 25A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047281,1,8592765047281,null,28592765047285,"8536490099",0.82]
[104728,"Ex9CR25 22 3P 230V","Reversible contactor, 3-pole, 25A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047298,1,8592765047298,null,28592765047292,"8536490099",0.82]
[104729,"Ex9CR25 22 3P 220V","Reversible contactor, 3-pole, 25A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047304,1,8592765047304,null,28592765047308,"8536490099",0.82]
[104730,"Ex9CR25 22 3P 127V","Reversible contactor, 3-pole, 25A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047311,1,8592765047311,null,28592765047315,"8536490099",0.82]
[104731,"Ex9CR25 22 3P 110V","Reversible contactor, 3-pole, 25A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",132.41999999999999,0,132.41999999999999,8592765047328,1,8592765047328,null,28592765047322,"8536490099",0.82]
[104732,"Ex9CR25 11 3P 48V","Reversible contactor, 3-pole, 25A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047335,1,8592765047335,null,28592765047339,"8536419089",0.82]
[104733,"Ex9CR25 11 3P 42V","Reversible contactor, 3-pole, 25A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047342,1,8592765047342,null,28592765047346,"8536419089",0.82]
[104734,"Ex9CR25 11 3P 415V","Reversible contactor, 3-pole, 25A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047359,1,8592765047359,null,28592765047353,"8536490099",0.82]
[104735,"Ex9CR25 11 3P 400V","Reversible contactor, 3-pole, 25A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047366,1,8592765047366,null,28592765047360,"8536490099",0.82]
[104736,"Ex9CR25 11 3P 380V","Reversible contactor, 3-pole, 25A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047373,1,8592765047373,null,28592765047377,"8536490099",0.82]
[104737,"Ex9CR25 11 3P 36V","Reversible contactor, 3-pole, 25A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047380,1,8592765047380,null,28592765047384,"8536419089",0.82]
[104738,"Ex9CR25 11 3P 24V","Reversible contactor, 3-pole, 25A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047397,1,8592765047397,null,28592765047391,"8536419089",0.82]
[104739,"Ex9CR25 11 3P 240V","Reversible contactor, 3-pole, 25A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047403,1,8592765047403,null,28592765047407,"8536490099",0.82]
[104740,"Ex9CR25 11 3P 230V","Reversible contactor, 3-pole, 25A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047410,1,8592765047410,null,28592765047414,"8536490099",0.82]
[104741,"Ex9CR25 11 3P 220V","Reversible contactor, 3-pole, 25A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047427,1,8592765047427,null,28592765047421,"8536490099",0.82]
[104742,"Ex9CR25 11 3P 127V","Reversible contactor, 3-pole, 25A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047434,1,8592765047434,null,28592765047438,"8536490099",0.82]
[104743,"Ex9CR25 11 3P 110V","Reversible contactor, 3-pole, 25A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",120.39,0,120.39,8592765047441,1,8592765047441,null,28592765047445,"8536490099",0.82]
[104744,"Ex9CR32 22 3P 48V","Reversible contactor, 3-pole, 32A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047458,1,8592765047458,null,28592765047452,"8536419089",0.82]
[104745,"Ex9CR32 22 3P 42V","Reversible contactor, 3-pole, 32A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047465,1,8592765047465,null,28592765047469,"8536419089",0.82]
[104746,"Ex9CR32 22 3P 415V","Reversible contactor, 3-pole, 32A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047472,1,8592765047472,null,28592765047476,"8536490099",0.82]
[104747,"Ex9CR32 22 3P 400V","Reversible contactor, 3-pole, 32A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047489,1,8592765047489,null,28592765047483,"8536490099",0.82]
[104748,"Ex9CR32 22 3P 380V","Reversible contactor, 3-pole, 32A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047496,1,8592765047496,null,28592765047490,"8536490099",0.82]
[104749,"Ex9CR32 22 3P 36V","Reversible contactor, 3-pole, 32A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047502,1,8592765047502,null,28592765047506,"8536419089",0.82]
[104750,"Ex9CR32 22 3P 24V","Reversible contactor, 3-pole, 32A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047519,1,8592765047519,null,28592765047513,"8536419089",0.82]
[104751,"Ex9CR32 22 3P 240V","Reversible contactor, 3-pole, 32A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047526,1,8592765047526,null,28592765047520,"8536490099",0.82]
[104752,"Ex9CR32 22 3P 230V","Reversible contactor, 3-pole, 32A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047533,1,8592765047533,null,28592765047537,"8536490099",0.82]
[104753,"Ex9CR32 22 3P 220V","Reversible contactor, 3-pole, 32A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047540,1,8592765047540,null,28592765047544,"8536490099",0.82]
[104754,"Ex9CR32 22 3P 127V","Reversible contactor, 3-pole, 32A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047557,1,8592765047557,null,28592765047551,"8536490099",0.82]
[104755,"Ex9CR32 22 3P 110V","Reversible contactor, 3-pole, 32A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",184.31,0,184.31,8592765047564,1,8592765047564,null,28592765047568,"8536490099",0.82]
[104756,"Ex9CR32 11 3P 48V","Reversible contactor, 3-pole, 32A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047571,1,8592765047571,null,28592765047575,"8536419089",0.82]
[104757,"Ex9CR32 11 3P 42V","Reversible contactor, 3-pole, 32A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047588,1,8592765047588,null,28592765047582,"8536419089",0.82]
[104758,"Ex9CR32 11 3P 415V","Reversible contactor, 3-pole, 32A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047595,1,8592765047595,null,28592765047599,"8536490099",0.82]
[104759,"Ex9CR32 11 3P 400V","Reversible contactor, 3-pole, 32A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047601,1,8592765047601,null,28592765047605,"8536490099",0.82]
[104760,"Ex9CR32 11 3P 380V","Reversible contactor, 3-pole, 32A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047618,1,8592765047618,null,28592765047612,"8536490099",0.82]
[104761,"Ex9CR32 11 3P 36V","Reversible contactor, 3-pole, 32A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047625,1,8592765047625,null,28592765047629,"8536419089",0.82]
[104762,"Ex9CR32 11 3P 24V","Reversible contactor, 3-pole, 32A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047632,1,8592765047632,null,28592765047636,"8536419089",0.82]
[104763,"Ex9CR32 11 3P 240V","Reversible contactor, 3-pole, 32A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047649,1,8592765047649,null,28592765047643,"8536490099",0.82]
[104764,"Ex9CR32 11 3P 230V","Reversible contactor, 3-pole, 32A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047656,1,8592765047656,null,28592765047650,"8536490099",0.82]
[104765,"Ex9CR32 11 3P 220V","Reversible contactor, 3-pole, 32A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047663,1,8592765047663,null,28592765047667,"8536490099",0.82]
[104766,"Ex9CR32 11 3P 127V","Reversible contactor, 3-pole, 32A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047670,1,8592765047670,null,28592765047674,"8536490099",0.82]
[104767,"Ex9CR32 11 3P 110V","Reversible contactor, 3-pole, 32A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",167.55,0,167.55,8592765047687,1,8592765047687,null,28592765047681,"8536490099",0.82]
[104768,"Ex9CR38 22 3P 48V","Reversible contactor, 3-pole, 38A AC-3, cont. 48 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047694,1,8592765047694,null,28592765047698,"8536419089",0.82]
[104769,"Ex9CR38 22 3P 42V","Reversible contactor, 3-pole, 38A AC-3, cont. 42 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047700,1,8592765047700,null,28592765047704,"8536419089",0.82]
[104770,"Ex9CR38 22 3P 415V","Reversible contactor, 3-pole, 38A AC-3, cont. 415 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047717,1,8592765047717,null,28592765047711,"8536490099",0.82]
[104771,"Ex9CR38 22 3P 400V","Reversible contactor, 3-pole, 38A AC-3, cont. 400 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047724,1,8592765047724,null,28592765047728,"8536490099",0.82]
[104772,"Ex9CR38 22 3P 380V","Reversible contactor, 3-pole, 38A AC-3, cont. 380 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047731,1,8592765047731,null,28592765047735,"8536490099",0.82]
[104773,"Ex9CR38 22 3P 36V","Reversible contactor, 3-pole, 38A AC-3, cont. 36 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047748,1,8592765047748,null,28592765047742,"8536419089",0.82]
[104774,"Ex9CR38 22 3P 24V","Reversible contactor, 3-pole, 38A AC-3, cont. 24 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047755,1,8592765047755,null,28592765047759,"8536419089",0.82]
[104775,"Ex9CR38 22 3P 240V","Reversible contactor, 3-pole, 38A AC-3, cont. 240 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047762,1,8592765047762,null,28592765047766,"8536490099",0.82]
[104776,"Ex9CR38 22 3P 230V","Reversible contactor, 3-pole, 38A AC-3, cont. 230 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,{"$f":"NBA","v":0},195.49,8592765047779,1,8592765047779,null,28592765047773,"8536490099",0.82]
[104777,"Ex9CR38 22 3P 220V","Reversible contactor, 3-pole, 38A AC-3, cont. 220 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,{"$f":"E4723*(1-F4723)","v":195.49},8592765047786,1,8592765047786,null,28592765047780,"8536490099",0.82]
[104778,"Ex9CR38 22 3P 127V","Reversible contactor, 3-pole, 38A AC-3, cont. 127 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047793,1,8592765047793,null,28592765047797,"8536490099",0.82]
[104779,"Ex9CR38 22 3P 110V","Reversible contactor, 3-pole, 38A AC-3, cont. 110 V AC,built-in 2 NC + 2 NO auxiliary contacts","NBA",195.49,0,195.49,8592765047809,1,8592765047809,null,28592765047803,"8536490099",0.82]
[104780,"Ex9CR38 11 3P 48V","Reversible contactor, 3-pole, 38A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047816,1,8592765047816,null,28592765047810,"8536419089",0.82]
[104781,"Ex9CR38 11 3P 42V","Reversible contactor, 3-pole, 38A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047823,1,8592765047823,null,28592765047827,"8536419089",0.82]
[104782,"Ex9CR38 11 3P 415V","Reversible contactor, 3-pole, 38A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047830,1,8592765047830,null,28592765047834,"8536490099",0.82]
[104783,"Ex9CR38 11 3P 400V","Reversible contactor, 3-pole, 38A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047847,1,8592765047847,null,28592765047841,"8536490099",0.82]
[104784,"Ex9CR38 11 3P 380V","Reversible contactor, 3-pole, 38A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047854,1,8592765047854,null,28592765047858,"8536490099",0.82]
[104785,"Ex9CR38 11 3P 36V","Reversible contactor, 3-pole, 38A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047861,1,8592765047861,null,28592765047865,"8536419089",0.82]
[104786,"Ex9CR38 11 3P 24V","Reversible contactor, 3-pole, 38A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047878,1,8592765047878,null,28592765047872,"8536419089",0.82]
[104787,"Ex9CR38 11 3P 240V","Reversible contactor, 3-pole, 38A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047885,1,8592765047885,null,28592765047889,"8536490099",0.82]
[104788,"Ex9CR38 11 3P 230V","Reversible contactor, 3-pole, 38A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047892,1,8592765047892,null,28592765047896,"8536490099",0.82]
[104789,"Ex9CR38 11 3P 220V","Reversible contactor, 3-pole, 38A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047908,1,8592765047908,null,28592765047902,"8536490099",0.82]
[104790,"Ex9CR38 11 3P 127V","Reversible contactor, 3-pole, 38A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047915,1,8592765047915,null,28592765047919,"8536490099",0.82]
[104791,"Ex9CR38 11 3P 110V","Reversible contactor, 3-pole, 38A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",177.84,0,177.84,8592765047922,1,8592765047922,null,28592765047926,"8536490099",0.82]
[104792,"Ex9CR40 11 3P 48V","Reversible contactor, 3-pole, 40A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765047939,1,8592765047939,null,28592765047933,"8536419089",2.5]
[104793,"Ex9CR40 11 3P 42V","Reversible contactor, 3-pole, 40A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765047946,1,8592765047946,null,28592765047940,"8536419089",2.5]
[104794,"Ex9CR40 11 3P 415V","Reversible contactor, 3-pole, 40A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765047953,1,8592765047953,null,28592765047957,"8536490099",2.5]
[104795,"Ex9CR40 11 3P 400V","Reversible contactor, 3-pole, 40A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765047960,1,8592765047960,null,28592765047964,"8536490099",2.5]
[104796,"Ex9CR40 11 3P 380V","Reversible contactor, 3-pole, 40A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765047977,1,8592765047977,null,28592765047971,"8536490099",2.5]
[104797,"Ex9CR40 11 3P 36V","Reversible contactor, 3-pole, 40A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765047984,1,8592765047984,null,28592765047988,"8536419089",2.5]
[104798,"Ex9CR40 11 3P 24V","Reversible contactor, 3-pole, 40A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765047991,1,8592765047991,null,28592765047995,"8536419089",2.5]
[104799,"Ex9CR40 11 3P 240V","Reversible contactor, 3-pole, 40A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765048004,1,8592765048004,null,28592765048008,"8536490099",2.5]
[104800,"Ex9CR40 11 3P 230V","Reversible contactor, 3-pole, 40A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765048011,1,8592765048011,null,28592765048015,"8536490099",2.5]
[104801,"Ex9CR40 11 3P 220V","Reversible contactor, 3-pole, 40A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765048028,1,8592765048028,null,28592765048022,"8536490099",2.5]
[104802,"Ex9CR40 11 3P 127V","Reversible contactor, 3-pole, 40A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765048035,1,8592765048035,null,28592765048039,"8536490099",2.5]
[104803,"Ex9CR40 11 3P 110V","Reversible contactor, 3-pole, 40A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",191.49,0,191.49,8592765048042,1,8592765048042,null,28592765048046,"8536490099",2.5]
[104804,"Ex9CR50 11 3P 48V","Reversible contactor, 3-pole, 50A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048059,1,8592765048059,null,28592765048053,"8536419089",2.5]
[104805,"Ex9CR50 11 3P 42V","Reversible contactor, 3-pole, 50A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048066,1,8592765048066,null,28592765048060,"8536419089",2.5]
[104806,"Ex9CR50 11 3P 415V","Reversible contactor, 3-pole, 50A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048073,1,8592765048073,null,28592765048077,"8536490099",2.5]
[104807,"Ex9CR50 11 3P 400V","Reversible contactor, 3-pole, 50A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048080,1,8592765048080,null,28592765048084,"8536490099",2.5]
[104808,"Ex9CR50 11 3P 380V","Reversible contactor, 3-pole, 50A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048097,1,8592765048097,null,28592765048091,"8536490099",2.5]
[104809,"Ex9CR50 11 3P 36V","Reversible contactor, 3-pole, 50A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048103,1,8592765048103,null,28592765048107,"8536419089",2.5]
[104810,"Ex9CR50 11 3P 24V","Reversible contactor, 3-pole, 50A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048110,1,8592765048110,null,28592765048114,"8536419089",2.5]
[104811,"Ex9CR50 11 3P 240V","Reversible contactor, 3-pole, 50A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048127,1,8592765048127,null,28592765048121,"8536490099",2.5]
[104812,"Ex9CR50 11 3P 230V","Reversible contactor, 3-pole, 50A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048134,1,8592765048134,null,28592765048138,"8536490099",2.5]
[104813,"Ex9CR50 11 3P 220V","Reversible contactor, 3-pole, 50A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048141,1,8592765048141,null,28592765048145,"8536490099",2.5]
[104814,"Ex9CR50 11 3P 127V","Reversible contactor, 3-pole, 50A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048158,1,8592765048158,null,28592765048152,"8536490099",2.5]
[104815,"Ex9CR50 11 3P 110V","Reversible contactor, 3-pole, 50A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",243.22,0,243.22,8592765048165,1,8592765048165,null,28592765048169,"8536490099",2.5]
[104816,"Ex9CR65 11 3P 48V","Reversible contactor, 3-pole, 65A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048172,1,8592765048172,null,28592765048176,"8536419089",2.5]
[104817,"Ex9CR65 11 3P 42V","Reversible contactor, 3-pole, 65A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048189,1,8592765048189,null,28592765048183,"8536419089",2.5]
[104818,"Ex9CR65 11 3P 415V","Reversible contactor, 3-pole, 65A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048196,1,8592765048196,null,28592765048190,"8536490099",2.5]
[104819,"Ex9CR65 11 3P 400V","Reversible contactor, 3-pole, 65A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048202,1,8592765048202,null,28592765048206,"8536490099",2.5]
[104820,"Ex9CR65 11 3P 380V","Reversible contactor, 3-pole, 65A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048219,1,8592765048219,null,28592765048213,"8536490099",2.5]
[104821,"Ex9CR65 11 3P 36V","Reversible contactor, 3-pole, 65A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048226,1,8592765048226,null,28592765048220,"8536419089",2.5]
[104822,"Ex9CR65 11 3P 24V","Reversible contactor, 3-pole, 65A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048233,1,8592765048233,null,28592765048237,"8536419089",2.5]
[104823,"Ex9CR65 11 3P 240V","Reversible contactor, 3-pole, 65A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048240,1,8592765048240,null,28592765048244,"8536490099",2.5]
[104824,"Ex9CR65 11 3P 230V","Reversible contactor, 3-pole, 65A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048257,1,8592765048257,null,28592765048251,"8536490099",2.5]
[104825,"Ex9CR65 11 3P 220V","Reversible contactor, 3-pole, 65A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048264,1,8592765048264,null,28592765048268,"8536490099",2.5]
[104826,"Ex9CR65 11 3P 127V","Reversible contactor, 3-pole, 65A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048271,1,8592765048271,null,28592765048275,"8536490099",2.5]
[104827,"Ex9CR65 11 3P 110V","Reversible contactor, 3-pole, 65A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",337.18,0,337.18,8592765048288,1,8592765048288,null,28592765048282,"8536490099",2.5]
[104828,"Ex9CR80 11 3P 48V","Reversible contactor, 3-pole, 80A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048295,1,8592765048295,null,28592765048299,"8536419089",3]
[104829,"Ex9CR80 11 3P 42V","Reversible contactor, 3-pole, 80A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048301,1,8592765048301,null,28592765048305,"8536419089",3]
[104830,"Ex9CR80 11 3P 415V","Reversible contactor, 3-pole, 80A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048318,1,8592765048318,null,28592765048312,"8536490099",3]
[104831,"Ex9CR80 11 3P 400V","Reversible contactor, 3-pole, 80A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048325,1,8592765048325,null,28592765048329,"8536490099",3]
[104832,"Ex9CR80 11 3P 380V","Reversible contactor, 3-pole, 80A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048332,1,8592765048332,null,28592765048336,"8536490099",3]
[104833,"Ex9CR80 11 3P 36V","Reversible contactor, 3-pole, 80A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048349,1,8592765048349,null,28592765048343,"8536419089",3]
[104834,"Ex9CR80 11 3P 24V","Reversible contactor, 3-pole, 80A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048356,1,8592765048356,null,28592765048350,"8536419089",3]
[104835,"Ex9CR80 11 3P 240V","Reversible contactor, 3-pole, 80A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048363,1,8592765048363,null,28592765048367,"8536490099",3]
[104836,"Ex9CR80 11 3P 230V","Reversible contactor, 3-pole, 80A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048370,1,8592765048370,null,28592765048374,"8536490099",3]
[104837,"Ex9CR80 11 3P 220V","Reversible contactor, 3-pole, 80A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048387,1,8592765048387,null,28592765048381,"8536490099",3]
[104838,"Ex9CR80 11 3P 127V","Reversible contactor, 3-pole, 80A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048394,1,8592765048394,null,28592765048398,"8536490099",3]
[104839,"Ex9CR80 11 3P 110V","Reversible contactor, 3-pole, 80A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",450.15,0,450.15,8592765048400,1,8592765048400,null,28592765048404,"8536490099",3]
[104840,"Ex9CR100 11 3P 48V","Reversible contactor, 3-pole, 100A AC-3, cont. 48 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,{"$f":"NBA","v":0},683.08,8592765048417,1,8592765048417,null,28592765048411,"8536419089",3]
[104841,"Ex9CR100 11 3P 42V","Reversible contactor, 3-pole, 100A AC-3, cont. 42 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,{"$f":"E4787*(1-F4787)","v":683.08},8592765048424,1,8592765048424,null,28592765048428,"8536419089",3]
[104842,"Ex9CR100 11 3P 415V","Reversible contactor, 3-pole, 100A AC-3, cont. 415 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048431,1,8592765048431,null,28592765048435,"8536490099",3]
[104843,"Ex9CR100 11 3P 400V","Reversible contactor, 3-pole, 100A AC-3, cont. 400 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048448,1,8592765048448,null,28592765048442,"8536490099",3]
[104844,"Ex9CR100 11 3P 380V","Reversible contactor, 3-pole, 100A AC-3, cont. 380 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048455,1,8592765048455,null,28592765048459,"8536490099",3]
[104845,"Ex9CR100 11 3P 36V","Reversible contactor, 3-pole, 100A AC-3, cont. 36 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048462,1,8592765048462,null,28592765048466,"8536419089",3]
[104846,"Ex9CR100 11 3P 24V","Reversible contactor, 3-pole, 100A AC-3, cont. 24 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048479,1,8592765048479,null,28592765048473,"8536419089",3]
[104847,"Ex9CR100 11 3P 240V","Reversible contactor, 3-pole, 100A AC-3, cont. 240 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048486,1,8592765048486,null,28592765048480,"8536490099",3]
[104848,"Ex9CR100 11 3P 230V","Reversible contactor, 3-pole, 100A AC-3, cont. 230 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048493,1,8592765048493,null,28592765048497,"8536490099",3]
[104849,"Ex9CR100 11 3P 220V","Reversible contactor, 3-pole, 100A AC-3, cont. 220 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048509,1,8592765048509,null,28592765048503,"8536490099",3]
[104850,"Ex9CR100 11 3P 127V","Reversible contactor, 3-pole, 100A AC-3, cont. 127 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048516,1,8592765048516,null,28592765048510,"8536490099",3]
[104851,"Ex9CR100 11 3P 110V","Reversible contactor, 3-pole, 100A AC-3, cont. 110 V AC,built-in 1 NC + 1 NO auxiliary contacts","NBA",683.08,0,683.08,8592765048523,1,8592765048523,null,28592765048527,"8536490099",3]
[]
["Accessories for Contactors Ex9C"]
[101284,"AX4202","Front-mounted auxiliary contact unit for Ex9C, 2 NC","NBA",4.2,{"$f":"NBA","v":0},{"$f":"E4800*(1-F4800)","v":4.2},8592765012852,12,18592765012859,624,28592765012856,"8536508090",0.41]
[101285,"AX4211","Front-mounted auxiliary contact unit for Ex9C, 1 NO, 1 NC","NBA",4.2,0,4.2,8592765012869,12,18592765012866,624,28592765012863,"8536508090",0.41]
[101286,"AX4220","Front-mounted auxiliary contact unit for Ex9C, 2 NO","NBA",4.2,0,4.2,8592765012876,12,18592765012873,624,28592765012870,"8536508090",0.41]
[101287,"AX4204","Front-mounted auxiliary contact unit for Ex9C, 4 NC","NBA",7.1,0,7.1,8592765012883,6,18592765012880,312,28592765012887,"8536508090",0.41]
[101288,"AX4213","Front-mounted auxiliary contact unit for Ex9C, 1 NO, 3 NC","NBA",7.1,0,7.1,8592765012890,6,18592765012897,312,28592765012894,"8536508090",0.41]
[101289,"AX4222","Front-mounted auxiliary contact unit for Ex9C, 2 NO, 2 NC","NBA",7.1,0,7.1,8592765012906,6,18592765012903,312,28592765012900,"8536508090",0.41]
[101290,"AX4231","Front-mounted auxiliary contact unit for Ex9C, 3 NO, 1 NC","NBA",7.1,0,7.1,8592765012913,6,18592765012910,312,28592765012917,"8536508090",0.41]
[101291,"AX4240","Front-mounted auxiliary contact unit for Ex9C, 4 NO","NBA",7.1,0,7.1,8592765012920,6,18592765012927,312,28592765012924,"8536508090",0.41]
[101292,"AX4311","Side-mounted auxiliary contact unit for Ex9C, 1 NO, 1 NC","NBA",13.47,0,13.47,8592765012937,10,18592765012934,120,28592765012931,"8536508090",0.38]
[104489,"TDD42C","Pneumatic time delay blocks, OFF delay, range 10 - 180 s, 1NO + 1NC internal auxiliary contact","NBA",44.92,{"$f":"NBA","v":0},{"$f":"E4809*(1-F4809)","v":44.92},8592765044907,1,8592765044907,null,28592765044901,"8536508090",0.06]
[104490,"TDD42B ","Pneumatic time delay blocks, OFF delay, range 0,1 - 30 s, 1NO + 1NC internal auxiliary contact","NBA",44.92,0,{"$f":"E4810*(1-F4810)","v":44.92},8592765044914,1,8592765044914,null,28592765044918,"8536508090",0.06]
[104491,"TDD42A","Pneumatic time delay blocks, OFF delay, range 0,1 - 3 s, 1NO + 1NC internal auxiliary contact","NBA",44.92,0,44.92,8592765044921,1,8592765044921,null,28592765044925,"8536508090",0.06]
[104492,"TDD41C ","Pneumatic time delay blocks, ON delay, range 10 - 180 s, 1NO + 1NC internal auxiliary contact","NBA",44.92,0,44.92,8592765044938,1,8592765044938,null,28592765044932,"8536508090",0.06]
[104493,"TDD41B ","Pneumatic time delay blocks, ON delay, range 0,1 - 30 s, 1NO + 1NC internal auxiliary contact","NBA",44.92,0,44.92,8592765044945,1,8592765044945,null,28592765044949,"8536508090",0.06]
[104494,"TDD41A ","Pneumatic time delay blocks, ON delay, range 0,1 - 3 s, 1NO + 1NC internal auxiliary contact","NBA",44.92,0,44.92,8592765044952,1,8592765044952,null,28592765044956,"8536508090",0.06]
[104495,"CCU43 48","Surge suppressor blocks, protection range 24-48V, with RC circuit technology","NBA",8.48,0,8.48,8592765044969,1,8592765044969,null,28592765044963,"8538909999",0.02]
[104496,"CCU43 415","Surge suppressor blocks, protection range 380-415V, with RC circuit technology","NBA",8.48,0,8.48,8592765044976,1,8592765044976,null,28592765044970,"8538909999",0.02]
[104497,"CCU43 240","Surge suppressor blocks, protection range 110-240V, with RC circuit technology","NBA",8.48,0,8.48,8592765044983,1,8592765044983,null,28592765044987,"8538909999",0.02]
[104498,"CCU42 48","Surge suppressor blocks, protection range 24-48V, with RC circuit technology","NBA",8.48,0,8.48,8592765044990,1,8592765044990,null,28592765044994,"8538909999",0.02]
[104499,"CCU42 415","Surge suppressor blocks, protection range 380-415V, with RC circuit technology","NBA",8.48,0,8.48,8592765045003,1,8592765045003,null,28592765045007,"8538909999",0.02]
[104500,"CCU42 240","Surge suppressor blocks, protection range 110-240V, with RC circuit technology","NBA",8.48,0,8.48,8592765045010,1,8592765045010,null,28592765045014,"8538909999",0.02]
[106322,"AX4411","Side-mounted auxiliary contact unit for Ex9C115-500, 1NO+1NC","NBA",10.63,{"$f":"NBA","v":0},{"$f":"E4821*(1-F4821)","v":10.63},8592765063236,1,18592765063233,12,28592765063230,"8538909999"]
[107957,"AX4402","Side-mounted auxiliary contact unit for Ex9C115-500, 2NC","NBA",10.63,0,{"$f":"E4822*(1-F4822)","v":10.63},8592765079589,1,18592765079586,12,28592765079583,"8538909999"]
[107958,"AX4420","Side-mounted auxiliary contact unit for Ex9C115-500, 2NO","NBA",10.63,0,{"$f":"E4823*(1-F4823)","v":10.63},8592765079596,1,18592765079593,12,28592765079590,"8538909999"]
[107960,"MIT42-11","Mechanical interlocks for contactors Ex9C09-38 11","NBA",8.83,{"$f":"NBA","v":0},{"$f":"E4824*(1-F4824)","v":8.83},8592765079619,1,18592765079616,72,28592765079613,"8538909999"]
[108095,"MIT42-22","Mechanical interlocks for contactors Ex9C09-38 22","NBA",8.83,0,8.83,8592765080950,1,18592765080957,72,28592765080954,"8536490099"]
[107961,"MIT43","Mechanical interlocks for contactors Ex9C40-100","NBA",8.83,0,8.83,8592765079626,1,18592765079623,96,28592765079620,"8538909999"]
[107962,"MIT44","Mechanical interlocks for contactors Ex9C115-185","NBA",27.33,0,27.33,8592765079633,1,18592765079630,15,28592765079637,"8538909999"]
[107963,"MIT45","Mechanical interlocks for contactors Ex9C225-300","NBA",30.45,0,30.45,8592765079640,1,18592765079647,12,28592765079644,"8538909999"]
[107964,"MIT46","Mechanical interlocks for contactors Ex9C400-500","NBA",31.87,0,31.87,8592765079657,1,18592765079654,12,28592765079651,"8538909999"]
[]
["Overload Thermal Relays Ex9R"]
[101359,"Ex9R12 0.16A","Overload Thermal Relay, 3-pole, In=0,16A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,{"$f":"NBB","v":0},{"$f":"E4832*(1-F4832)","v":20.16},8592765013606,1,8592765013606,80,28592765013600,"8536490099",0.21]
[101360,"Ex9R12 0.25A","Overload Thermal Relay, 3-pole, In=0,25A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013613,1,8592765013613,80,28592765013617,"8536490099",0.21]
[101361,"Ex9R12 0.4A","Overload Thermal Relay, 3-pole, In=0,4A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013620,1,8592765013620,80,28592765013624,"8536490099",0.21]
[101362,"Ex9R12 0.63A","Overload Thermal Relay, 3-pole, In=0,63A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013637,1,8592765013637,80,28592765013631,"8536490099",0.21]
[101363,"Ex9R12 1A","Overload Thermal Relay, 3-pole, In=1A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013644,1,8592765013644,80,28592765013648,"8536490099",0.21]
[101364,"Ex9R12 1.6A","Overload Thermal Relay, 3-pole, In=1,6A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013651,1,8592765013651,80,28592765013655,"8536490099",0.21]
[101365,"Ex9R12 2.5A","Overload Thermal Relay, 3-pole, In=2,5A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013668,1,8592765013668,80,28592765013662,"8536490099",0.21]
[101366,"Ex9R12 4A","Overload Thermal Relay, 3-pole, In=4A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013675,1,8592765013675,80,28592765013679,"8536490099",0.21]
[101367,"Ex9R12 6A","Overload Thermal Relay, 3-pole, In=6A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013682,1,8592765013682,80,28592765013686,"8536490099",0.21]
[101368,"Ex9R12 8A","Overload Thermal Relay, 3-pole, In=8A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013699,1,8592765013699,80,28592765013693,"8536490099",0.21]
[101369,"Ex9R12 10A","Overload Thermal Relay, 3-pole, In=10A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013705,1,8592765013705,80,28592765013709,"8536490099",0.21]
[101370,"Ex9R12 12A","Overload Thermal Relay, 3-pole, In=12A, can be combined with Miniature Contactors Ex9CS ","NBB",20.16,0,20.16,8592765013712,1,8592765013712,80,28592765013716,"8536490099",0.21]
[110327,"Ex9R38B 1A","Overload Thermal Relay, 3-pole, In=1A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,{"$f":"NBB","v":0},{"$f":"E4844*(1-F4844)","v":28.74},8592765103277,1,8592765103277,60,28592765103271,"8536490099",0.13500000000000001]
[110328,"Ex9R38B 1.6A","Overload Thermal Relay, 3-pole, In=1,6A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,{"$f":"NBB","v":0},{"$f":"E4845*(1-F4845)","v":28.74},8592765103284,1,8592765103284,60,28592765103288,"8536490099",0.13500000000000001]
[110329,"Ex9R38B 2.5A","Overload Thermal Relay, 3-pole, In=2,5A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103291,1,8592765103291,60,28592765103295,"8536490099",0.13500000000000001]
[110330,"Ex9R38B 4A","Overload Thermal Relay, 3-pole, In=4A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103307,1,8592765103307,60,28592765103301,"8536490099",0.13500000000000001]
[110331,"Ex9R38B 6A","Overload Thermal Relay, 3-pole, In=6A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103314,1,8592765103314,60,28592765103318,"8536490099",0.13500000000000001]
[110332,"Ex9R38B 8A","Overload Thermal Relay, 3-pole, In=8A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103321,1,8592765103321,60,28592765103325,"8536490099",0.13500000000000001]
[110333,"Ex9R38B 10A","Overload Thermal Relay, 3-pole, In=10A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103338,1,8592765103338,60,28592765103332,"8536490099",0.13500000000000001]
[110334,"Ex9R38B 13A","Overload Thermal Relay, 3-pole, In=12A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103345,1,8592765103345,60,28592765103349,"8536490099",0.13500000000000001]
[110335,"Ex9R38B 18A","Overload Thermal Relay, 3-pole, In=18A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103352,1,8592765103352,60,28592765103356,"8536490099",0.13500000000000001]
[110336,"Ex9R38B 24A","Overload Thermal Relay, 3-pole, In=24A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103369,1,8592765103369,60,28592765103363,"8536490099",0.13500000000000001]
[110337,"Ex9R38B 32A","Overload Thermal Relay, 3-pole, In=32A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103376,1,8592765103376,60,28592765103370,"8536490099",0.13500000000000001]
[110338,"Ex9R38B 38A","Overload Thermal Relay, 3-pole, In=38A, can be combined with Contactors Ex9C9 up to Ex9C38 ","NBB",28.74,0,28.74,8592765103383,1,8592765103383,60,28592765103387,"8536490099",0.13500000000000001]
[101380,"Ex9R100 32A","Overload Thermal Relay, 3-pole, In=32A, can be combined with Contactors Ex9C40 up to Ex9C100 ","NBB",40.26,0,40.26,8592765013811,1,8592765013811,24,28592765013815,"8536490099",0.56000000000000005]
[101381,"Ex9R100 40A","Overload Thermal Relay, 3-pole, In=40A, can be combined with Contactors Ex9C40 up to Ex9C100 ","NBB",40.26,0,40.26,8592765013828,1,8592765013828,24,28592765013822,"8536490099",0.56000000000000005]
[101382,"Ex9R100 50A","Overload Thermal Relay, 3-pole, In=50A, can be combined with Contactors Ex9C40 up to Ex9C100 ","NBB",48.94,0,48.94,8592765013835,1,8592765013835,24,28592765013839,"8536490099",0.56000000000000005]
[101383,"Ex9R100 65A","Overload Thermal Relay, 3-pole, In=65A, can be combined with Contactors Ex9C40 up to Ex9C100 ","NBB",74.31,0,74.31,8592765013842,1,8592765013842,24,28592765013846,"8536490099",0.56000000000000005]
[101384,"Ex9R100 70A","Overload Thermal Relay, 3-pole, In=70A, can be combined with Contactors Ex9C40 up to Ex9C100 ","NBB",74.31,0,74.31,8592765013859,1,8592765013859,24,28592765013853,"8536490099",0.56000000000000005]
[101385,"Ex9R100 80A","Overload Thermal Relay, 3-pole, In=80A, can be combined with Contactors Ex9C40 up to Ex9C100 ","NBB",74.31,0,74.31,8592765013866,1,8592765013866,24,28592765013860,"8536490099",0.56000000000000005]
[101386,"Ex9R100 100A","Overload Thermal Relay, 3-pole, In=100A, can be combined with Contactors Ex9C40 up to Ex9C100 ","NBB",74.31,0,74.31,8592765013873,1,8592765013873,24,28592765013877,"8536490099",0.56000000000000005]
[]
["Overload Thermal Relays Ex9R up to 500A"]
[106326,"Ex9R185 115A","Overload Thermal Relay, 3-pole, In=115A, can be combined with contactors Ex9C115-185 ","NBB",153.37,{"$f":"NBB","v":0},{"$f":"E4865*(1-F4865)","v":153.37},8592765063274,1,8592765063274,8,28592765063278,"8536490099",1.5]
[106327,"Ex9R185 150A","Overload Thermal Relay, 3-pole, In=150A, can be combined with contactors Ex9C115-185 ","NBB",157.62,{"$f":"NBB","v":0},157.62,8592765063281,1,8592765063281,8,28592765063285,"8536490099",1.5]
[106328,"Ex9R185 185A","Overload Thermal Relay, 3-pole, In=185A, can be combined with contactors Ex9C115-185 ","NBB",160.94999999999999,0,160.94999999999999,8592765063298,1,8592765063298,8,28592765063292,"8536490099",1.5]
[106329,"Ex9R500 225A","Overload Thermal Relay, 3-pole, In=225A, can be combined with contactors Ex9C225-500 ","NBB",173.07,0,173.07,8592765063304,1,8592765063304,8,28592765063308,"8536490099",1.9]
[106330,"Ex9R500 300A","Overload Thermal Relay, 3-pole, In=300A, can be combined with contactors Ex9C225-500 ","NBB",184.99,0,184.99,8592765063311,1,8592765063311,8,28592765063315,"8536490099",1.9]
[106331,"Ex9R500 400A","Overload Thermal Relay, 3-pole, In=400A, can be combined with contactors Ex9C225-500 ","NBB",267.93,0,267.93,8592765063328,1,8592765063328,8,28592765063322,"8536490099",1.9]
[106332,"Ex9R500 500A","Overload Thermal Relay, 3-pole, In=500A, can be combined with contactors Ex9C225-500 ","NBB",271.31,0,271.31,8592765063335,1,8592765063335,8,28592765063339,"8536490099",1.9]
[]
["Accessories for Overload Thermal Relays Ex9R"]
[101436,"AD51","Adapter for stand-alone use Ex9R12","NBB",5.57,{"$f":"NBB","v":0},{"$f":"E4874*(1-F4874)","v":5.57},8592765014375,null,18592765014372,null,28592765014379,"8538909999",0.14000000000000001]
[110339,"AD56","Adapter for stand-alone use Ex9R38B","NBB",6.22,{"$f":"NBB","v":0},6.22,8592765103390,2,18592765103397,60,28592765103394,"8538909999",0.2]
[101438,"AD53","Adapter for stand-alone use Ex9R100","NBB",7.28,{"$f":"NBB","v":0},7.28,8592765014399,null,18592765014396,null,28592765014393,"8538909999",0.52]
[107968,"AD54","Adapter for standalone use of Ex9R185","NBB",47.9,{"$f":"NBB","v":0},{"$f":"E4877*(1-F4877)","v":47.9},8592765079695,1,18592765079692,12,28592765079699,"8538909999"]
[107969,"AD55","Adapter for standalone use of Ex9R500","NBB",53.8,0,{"$f":"E4878*(1-F4878)","v":53.8},8592765079701,1,18592765079708,12,28592765079705,"8538909999"]
[]
["DIN rail service socket, Ex9DS",null,null,null,null,null,null,"","","","","",null,""]
[106194,"Ex9DS-F","Din rail service sockets with eart pin","NDB",5.95,{"$f":"NDB","v":0},{"$f":"E4881*(1-F4881)","v":5.95},8592765061959,5,18592765061956,75,28592765061953,"8536699099",0.11]
[106195,"Ex9DS-G","Din rail service socket Schucko","NDB",5.95,{"$f":"NDB","v":0},{"$f":"E4882*(1-F4882)","v":5.95},8592765061966,5,18592765061963,75,28592765061960,"8536699099",0.11]
[]
["Busbars BBU"]
[101446,"BBU 1L 10 M54","Busbar, 1-phase, 10mm2, 63A, 54 modules (1m)","NDB",7.68,{"$f":"NDB","v":0},{"$f":"E4885*(1-F4885)","v":7.68},8592765014474,null,18592765014471,100,28592765014478,"8536909599",0.22]
[101447,"BBU 1L 16 M54","Busbar, 1-phase, 16mm2, 80A, 54 modules (1m)","NDB",16.54,0,{"$f":"E4886*(1-F4886)","v":16.54},8592765014481,null,18592765014488,100,28592765014485,"8536909599",0.26]
[101448,"BBU 3L 10 M54","Busbar, 3-phase, 10mm2, 63A, 54 modules (1m)","NDB",17.940000000000001,0,17.940000000000001,8592765014498,null,18592765014495,50,28592765014492,"8536909599",0.51]
[101449,"BBU 3L 16 M54","Busbar, 3-phase, 16mm2, 80A, 54 modules (1m)","NDB",24.59,0,24.59,8592765014504,null,18592765014501,50,28592765014508,"8536909599",0.64]
[101450,"BBU 3L 10 M12 EC","Busbar, 3-phase, 10mm2, 63A, 12 modules, including end caps","NDB",4.7,0,4.7,8592765014511,null,18592765014518,200,28592765014515,"8536909599",0.1]
[101451,"BBU 3L 16 M12 EC","Busbar, 3-phase, 16mm2, 80A, 12 modules, including end caps","NDB",5.63,0,5.63,8592765014528,null,18592765014525,200,28592765014522,"8536909599",0.12]
[110830,"BBU 3L 10 M6 EU","Busbar U type 3P 10mm² 6 circuits for Ex9B 18mm","NDB",2.7,{"$f":"NDB","v":0},{"$f":"E4891*(1-F4891)","v":2.7},8592765108302,5,18592765108309,400,28592765108306,8536909599,4.7E-2]
[110831,"BBU 3L 10 M9 EU","Busbar U type 3P 10mm² 9 circuits for Ex9B 18mm","NDB",3.75,{"$f":"NDB","v":0},{"$f":"E4892*(1-F4892)","v":3.75},8592765108319,5,18592765108316,250,28592765108313,8536909599,7.8E-2]
[110832,"BBU 3L 16 M6 EU","Busbar U type 3P 16mm² 6 circuits for Ex9B 18mm","NDB",3.47,{"$f":"NDB","v":0},3.47,8592765108326,5,18592765108323,400,28592765108320,8536909599,6.4000000000000001E-2]
[110833,"BBU 3L 16 M9 EU","Busbar U type 3P 16mm² 9 circuits for Ex9B 18mm","NDB",5.57,{"$f":"NDB","v":0},5.57,8592765108333,5,18592765108330,250,28592765108337,8536909599,0.1]
[111405,"BBP 1L 10 M12 EU","Busbar Pin Type 1P 10mm² 12 circuits for Ex9B40J 13.5mm","NDB",2.09,{"$f":"NDB","v":0},2.09,8592765114051,10,18592765114058,300,28592765114055,8536909599,3.7999999999999999E-2]
[111406,"BBP 3L 10 M12 EU","Busbar Pin Type 3P 10mm² 12 circuits for Ex9B40J 13.5mm","NDB",5.21,{"$f":"NDB","v":0},5.21,8592765114068,5,18592765114065,150,28592765114062,8536909599,9.0999999999999998E-2]
[111407,"BBP 2LN 10 M12 EU","Busbar Pin Type 2P for Ex9NLE EL 18mm","NDB",4.8499999999999996,{"$f":"NDB","v":0},4.8499999999999996,8592765114075,5,18592765114072,150,28592765114079,8536909599,9.1999999999999998E-2]
[111408,"BBP 4LN 10 M12 EU","Busbar Pin Type 4P for Ex9NLE EL 18mm","NDB",9.16,{"$f":"NDB","v":0},9.16,8592765114082,5,18592765114089,100,28592765114086,8536909599,0.152]
[101452,"ECU 1L","End cap for BBU 1L, price per 1 piece","NDB",0.22,0,0.22,8592765014535,null,18592765014532,40000,28592765014539,"3926909790"]
[101453,"ECU 3L","End cap for BBU 3L, price per 1 piece","NDB",0.22,0,0.22,8592765014542,null,18592765014549,15000,28592765014546,"3926909790"]
[]
["Busbars BBUE"]
[103798,"BBUE 1L 10 M56","Busbar, 1-phase, 10mm2, 63A, 56 MU (1m)","NDB",21.3,{"$f":"NDB","v":0},{"$f":"E4903*(1-F4903)","v":21.3},8592765037992,null,18592765037999,null,28592765037996,"8536909599",0.24]
[103799,"BBUE 1L 10 M2","Busbar, 1-phase, 10mm2, 63A, 2 MU","NDB",2.36,0,2.36,8592765038005,null,18592765038002,null,28592765038009,"8536909599",8.9999999999999993E-3]
[103800,"BBUE 1L 10 M6","Busbar, 1-phase, 10mm2, 63A, 6 MU","NDB",4.51,0,4.51,8592765038012,null,18592765038019,null,28592765038016,"8536909599",2.1999999999999999E-2]
[103801,"BBUE 1L 10 M9","Busbar, 1-phase, 10mm2, 63A, 9 MU","NDB",4.82,0,4.82,8592765038029,null,18592765038026,null,28592765038023,"8536909599",0.04]
[103802,"BBUE 1L 10 M12","Busbar, 1-phase, 10mm2, 63A, 12 MU","NDB",5.0599999999999996,0,5.0599999999999996,8592765038036,null,18592765038033,null,28592765038030,"8536909599",5.1999999999999998E-2]
[103803,"BBUE 1L 10 M18","Busbar, 1-phase, 10mm2, 63A, 18 MU","NDB",5.68,0,5.68,8592765038043,null,18592765038040,null,28592765038047,"8536909599",7.8E-2]
[103804,"BBUE 1L 16 M56","Busbar, 1-phase, 16mm2, 80A, 56 MU (1m)","NDB",26.08,0,26.08,8592765038050,null,18592765038057,null,28592765038054,"8536909599",0.32]
[103805,"BBUE 1L 16 M12","Busbar, 1-phase, 16mm2, 80A, 12 MU","NDB",6.97,0,6.97,8592765038067,null,18592765038064,null,28592765038061,"8536909599",7.0999999999999994E-2]
[103806,"BBUE 1L 16 M18","Busbar, 1-phase, 16mm2, 80A, 18 MU","NDB",7.84,0,7.84,8592765038074,null,18592765038071,null,28592765038078,"8536909599",0.104]
[103807,"BBUE 1L 35 M1,5x37P","Busbar, 1-phase, 35mm2, 125A, 37 MU","NDB",56.36,0,56.36,8592765038081,null,18592765038088,null,28592765038085,"8536909599",0.75]
[103808,"BBUE 3L 10 M57","Busbar, 3-phase, 10mm2, 63A, 57 MU (1m)","NDB",41.56,0,41.56,8592765038098,null,18592765038095,null,28592765038092,"8536909599",0.505]
[103809,"BBUE 3L 10 M9","Busbar, 3-phase, 10mm2, 63A, 9 MU","NDB",11.64,0,11.64,8592765038104,null,18592765038101,null,28592765038108,"8536909599",8.3000000000000004E-2]
[103810,"BBUE 3L 10 M12","Busbar, 3-phase, 10mm2, 63A, 12 MU","NDB",10.44,0,10.44,8592765038111,null,18592765038118,null,28592765038115,"8536909599",0.108]
[103811,"BBUE 3L 10 M18","Busbar, 3-phase, 10mm2, 63A, 18 MU","NDB",12.63,0,12.63,8592765038128,null,18592765038125,null,28592765038122,"8536909599",0.16200000000000001]
[103812,"BBUE 3L 16 M57","Busbar, 3-phase, 16mm2, 80A, 57 MU (1m)","NDB",47.62,0,47.62,8592765038135,null,18592765038132,null,28592765038139,"8536909599",0.70699999999999996]
[103813,"BBUE 3L 16 M9","Busbar, 3-phase, 16mm2, 80A, 9 MU","NDB",8.24,0,8.24,8592765038142,null,18592765038149,null,28592765038146,"8536909599",0.11799999999999999]
[103814,"BBUE 3L 16 M12","Busbar, 3-phase, 16mm2, 80A, 12 MU","NDB",12.6,0,12.6,8592765038159,null,18592765038156,null,28592765038153,"8536909599",0.151]
[103815,"BBUE 3L 16 M18","Busbar, 3-phase, 16mm2, 80A, 18 MU","NDB",18.36,0,18.36,8592765038166,null,18592765038163,null,28592765038160,"8536909599",0.22700000000000001]
[103816,"BBUE 4L 10 M56","Busbar, 4-phase, 10mm2, 63A, 56 MU (1m)","NDB",66.06,0,66.06,8592765038173,null,18592765038170,null,28592765038177,"8536909599",0.80300000000000005]
[103817,"BBUE 4L 16 M56","Busbar, 4-phase, 16mm2, 80A, 56 MU (1m)","NDB",83.25,0,83.25,8592765038180,null,18592765038187,null,28592765038184,"8536909599",1.2050000000000001]
[103818,"BBUE 4LN 10 M54","Busbar, 4-phase, 10mm2, 63A, 54 MU (1m)","NDB",67.989999999999995,0,67.989999999999995,8592765038197,null,18592765038194,null,28592765038191,"8536909599",0.80500000000000005]
[103819,"BBUE 4LN 16 M54","Busbar, 4-phase, 16mm2, 80A, 54 MU (1m)","NDB",118.07,0,118.07,8592765038203,null,18592765038200,null,28592765038207,"8536909599",1.21]
[103820,"BBUE 3L 35 M1,5x39P","Busbar, 3-phase, 35mm2, 125A, 39 MU (1m)","NDB",148.94,0,148.94,8592765038210,null,18592765038217,null,28592765038214,"8536909599",1.655]
[103821,"BBUE 4L 30 M1,5x40P","Busbar, 4-phase, 30mm2, 115A, 40 MU (1m)","NDB",169.42,0,169.42,8592765038227,null,18592765038224,null,28592765038221,"8536909599",2.085]
[103822,"BBUE 4L 10 M12 NLLL+8xNLPN","Busbar, 4-phase, 10mm2, 63A, 12 MU, 4p Ex9CL, 8 x 1PN Ex9PN","NDB",26.28,0,26.28,8592765038234,null,18592765038231,null,28592765038238,"8536909599",0.23499999999999999]
[103823,"BBUE 4L 10 M12 LLLN+8xNLPN","Busbar, 4-phase, 10mm2, 63A, 12 MU, 3PN Ex9B, 8 x 1PN Ex9PN","NDB",26.94,0,26.94,8592765038241,null,18592765038248,null,28592765038245,"8536909599",0.23699999999999999]
[103824,"BBUE 4L 10 M12 NLLL+4xLN","Busbar, 4-phase, 10mm2, 63A, 12 MU, 4p Ex9CL, 4 x 1PN Ex9B","NDB",23.64,0,23.64,8592765038258,null,18592765038255,null,28592765038252,"8536909599",0.185]
[103825,"BBUE 4L 10 M18 NLLL+7xLN","Busbar, 4-phase, 10mm2, 63A, 18 MU, 4p Ex9CL, 7 x 1PN Ex9B","NDB",24.34,0,24.34,8592765038265,null,18592765038262,null,28592765038269,"8536909599",0.108]
[103864,"BBUE 2L 10 M56","Busbar, 2-phase, 10mm2, 63A, 56 MU (1m)","NDB",29.28,0,29.28,8592765038654,null,18592765038651,null,28592765038658,"8536909599",0.32]
[103865,"BBUE 2L 16 M56","Busbar, 2-phase, 16mm2, 80A, 56 MU (1m)","NDB",35.99,0,35.99,8592765038661,null,18592765038668,null,28592765038665,"8536909599",0.52500000000000002]
[103866,"BBUE 2L 10 M56 NLPN","Busbar, 2-phase, 10mm2, 63A, 56 MU (1m)  Ex9PN","NDB",29.28,0,29.28,8592765038678,null,18592765038675,null,28592765038672,"8536909599",0.32]
[103867,"BBUE 2L 10 M12 NL+10xNLPN","Busbar, 2-phase, 10mm2, 63A, 12 MU, 2P Ex9CL, 10 x 1PN Ex9PN","NDB",23.85,0,23.85,8592765038685,null,18592765038682,null,28592765038689,"8536909599",0.13500000000000001]
[103868,"BBUE 2L 10 M12 NL+5xLN","Busbar, 2-phase, 10mm2, 63A, 12 MU, 2P Ex9CL, 5 x 1PN Ex9B","NDB",12.63,0,12.63,8592765038692,null,18592765038699,null,28592765038696,"8536909599",0.121]
[107114,"BBUE 2L 10 M12 LN+10xNLPN","Busbar, 2-phase, 10mm2, 63A, 12 MU, 1PN Ex9CBL, 10 x 1PN Ex9PN","NDB",23.85,0,23.85,8592765071156,null,18592765071153,null,28592765071150,"8536909599",0.13500000000000001]
[103826,"ECUE 1L","Endcover for 1-phase busbar 10/16 mm2","NDB",1.1499999999999999,0,1.1499999999999999,8592765038272,50,18592765038279,null,28592765038276,"3926909790"]
[103827,"ECUE 2L","Endcover for 2-phase busbar","NDB",0.56000000000000005,0,0.56000000000000005,8592765038289,50,18592765038286,null,28592765038283,"3926909790"]
[103828,"ECUE 3L","Endcover for 3-phase busbar","NDB",0.56000000000000005,0,0.56000000000000005,8592765038296,50,18592765038293,null,28592765038290,"3926909790"]
[103829,"ECUE 4L","Endcover for 4-phase busbar","NDB",1.1200000000000001,0,1.1200000000000001,8592765038302,50,18592765038309,null,28592765038306,"3926909790"]
[103830,"ECUE 3L 35","Endcover for 3-phase busbar 35 mm2","NDB",5.95,0,5.95,8592765038319,50,18592765038316,null,28592765038313,"8538909999"]
[103831,"ECUE 1L 35","Endcover for 1-phase busbar 35 / 50mm2","NDB",5.95,0,5.95,8592765038326,50,18592765038323,null,28592765038320,"8538909999"]
[]
["Busbars BBUM"]
[109949,"BBUM 245","Busbar for 2 motorstarters with pitch 45mm","NBG",9.91,{"$f":"NBG","v":0},{"$f":"E4945*(1-F4945)","v":9.91},8592765099495,10,18592765099492,200,28592765099499,"8536909599",3.5000000000000003E-2]
[109950,"BBUM 345","Busbar for 3 motorstarters with pitch 45mm","NBG",12.14,{"$f":"NBG","v":0},{"$f":"E4946*(1-F4946)","v":12.14},8592765099501,10,18592765099508,200,28592765099505,"8536909599",5.2999999999999999E-2]
[109951,"BBUM 445","Busbar for 4 motorstarters with pitch 45mm","NBG",13.89,0,13.89,8592765099518,10,18592765099515,100,28592765099512,"8536909599",7.0000000000000007E-2]
[109952,"BBUM 545","Busbar for 5 motorstarters with pitch 45mm","NBG",15.91,0,15.91,8592765099525,10,18592765099522,100,28592765099529,"8536909599",8.7999999999999995E-2]
[109953,"BBUM 254","Busbar for 2 motorstarters with pitch 54mm","NBG",10.25,0,10.25,8592765099532,10,18592765099539,250,28592765099536,"8536909599",4.4999999999999998E-2]
[109954,"BBUM 354","Busbar for 3 motorstarters with pitch 54mm","NBG",12.47,0,12.47,8592765099549,10,18592765099546,200,28592765099543,"8536909599",6.3E-2]
[109955,"BBUM 454","Busbar for 4 motorstarters with pitch 54mm","NBG",14.2,0,14.2,8592765099556,10,18592765099553,100,28592765099550,"8536909599",0.08]
[109956,"BBUM 554","Busbar for 5 motorstarters with pitch 54mm","NBG",16.23,0,16.23,8592765099563,10,18592765099560,100,28592765099567,"8536909599",9.8000000000000004E-2]
[109957,"BBUM 263","Busbar for 2 motorstarters with pitch 63mm","NBG",10.55,0,10.55,8592765099570,10,18592765099577,100,28592765099574,"8536909599",5.5E-2]
[109958,"BBUM 363","Busbar for 3 motorstarters with pitch 63mm","NBG",12.77,0,12.77,8592765099587,10,18592765099584,100,28592765099581,"8536909599",7.2999999999999995E-2]
[109959,"BBUM 463","Busbar for 4 motorstarters with pitch 63mm","NBG",15.3,0,15.3,8592765099594,10,18592765099591,100,28592765099598,"8536909599",0.09]
[109960,"BBUM 563","Busbar for 5 motorstarters with pitch 63mm","NBG",17.239999999999998,0,17.239999999999998,8592765099600,10,18592765099607,100,28592765099604,"8536909599",0.108]
[109961,"FTUM","Feeder Terminal","NBG",13.48,0,13.48,8592765099617,10,18592765099614,200,28592765099611,"85369010",3.5000000000000003E-2]
[]
["Terminals IT"]
[103832,"ITL F 63A G","Isolated Terminal Lenghtwise Fork 63A Grey","NDB",3.21,{"$f":"NDB","v":0},{"$f":"E4960*(1-F4960)","v":3.21},8592765038333,1,18592765038330,25,28592765038337,"8536901000",0.01]
[103833,"ITL F 63A B","Isolated Terminal Lenghtwise Fork 63A Blue","NDB",3.47,0,3.47,8592765038340,1,18592765038347,25,28592765038344,"8536901000",0.01]
[103834,"ITA F 63A G","Isolated Terminal Across Fork 63A Grey","NDB",3.21,0,3.21,8592765038357,1,18592765038354,25,28592765038351,"8536901000",0.01]
[103835,"ITA F 63A B","Isolated Terminal Across Fork 63A Blue","NDB",3.47,0,3.47,8592765038364,1,18592765038361,25,28592765038368,"8536901000",0.01]
[103836,"ITLL F 63A G","Isolated Terminal Lenghtwise Long Fork 63A Grey","NDB",6.19,0,6.19,8592765038371,1,18592765038378,25,28592765038375,"8536901000",0.01]
[103837,"ITLL F 63A B","Isolated Terminal Lenghtwise Long Fork 63A Blue","NDB",6.61,0,6.61,8592765038388,1,18592765038385,25,28592765038382,"8536901000",0.01]
[103838,"ITAL F 63A G","Isolated Terminal Across Long Fork 63A Grey","NDB",6.19,0,6.19,8592765038395,1,18592765038392,25,28592765038399,"8536901000",0.01]
[103839,"ITAL F 63A B","Isolated Terminal Across Long Fork 63A Blue","NDB",6.61,0,6.61,8592765038401,1,18592765038408,25,28592765038405,"8536901000",0.01]
[103840,"ITL P 63A G","Isolated Terminal Lenghtwise Pin 63A Grey","NDB",3.21,0,3.21,8592765038418,1,18592765038415,25,28592765038412,"8536901000",0.01]
[103841,"ITL P 63A B","Isolated Terminal Lenghtwise Pin 63A Blue","NDB",3.47,0,3.47,8592765038425,1,18592765038422,25,28592765038429,"8536901000",0.01]
[103842,"ITA P 63A G","Isolated Terminal Across Pin 63A Grey","NDB",3.21,0,3.21,8592765038432,1,18592765038439,25,28592765038436,"8536901000",0.01]
[103843,"ITA P 63A B","Isolated Terminal Across Pin 63A Blue","NDB",3.47,0,3.47,8592765038449,1,18592765038446,25,28592765038443,"8536901000",0.01]
[103844,"ITLW P 63A G","Isolated Terminal Lenghtwise Long Pin 63A Grey","NDB",3.21,0,3.21,8592765038456,1,18592765038453,25,28592765038450,"8536901000",0.01]
[103845,"ITLW P 63A B","Isolated Terminal Lenghtwise Wide Pin 63A Blue","NDB",3.47,0,3.47,8592765038463,1,18592765038460,25,28592765038467,"8536901000",0.01]
[103846,"ITAW P 63A G","Isolated Terminal Across Wide Pin 63A Grey","NDB",3.21,0,3.21,8592765038470,1,18592765038477,25,28592765038474,"8536901000",0.01]
[103847,"ITAW P 63A B","Isolated Terminal Across Wide Pin 63A Blue","NDB",3.21,0,3.21,8592765038487,1,18592765038484,25,28592765038481,"8536901000",0.01]
[103848,"ITL P 100A G","Isolated Terminal Lenghtwise Pin 100A Grey","NDB",6.93,0,6.93,8592765038494,1,18592765038491,25,28592765038498,"8536901000",0.02]
[103849,"ITL P 100A B","Isolated Terminal Lenghtwise Pin 100A Blue","NDB",7.26,0,7.26,8592765038500,1,18592765038507,25,28592765038504,"8536901000",0.02]
[]
["Distribution blocks PDB"]
[103778,"PDB 1P CU 1x4+2 80A","Power Distribution Block 1Pole CU 1 input x 4+2 outputs 80A","NDE",13.36,{"$f":"NDE","v":0},{"$f":"E4980*(1-F4980)","v":13.36},8592765037794,1,8592765037794,25,28592765037798,"8536901000",5.2999999999999999E-2]
[103779,"PDB 1P CU/AL 1x4+2 80/63A","Power Distribution Block 1Pole CU/AL 1 input x 4+2 outputs 80/63A","NDE",17.579999999999998,0,{"$f":"E4981*(1-F4981)","v":17.579999999999998},8592765037800,1,8592765037800,25,28592765037804,"8536901000",5.2999999999999999E-2]
[103780,"PDB 1P CU 1+1x6 125A","Power Distribution Block 1Pole CU 1+1 input x 6 outputs 125A","NDE",28.02,0,28.02,8592765037817,1,8592765037817,25,28592765037811,"8536901000",0.14199999999999999]
[103781,"PDB 1P CU/AL 1+1x6 125/100A","Power Distribution Block 1Pole CU/AL 1+1 input x 6 outputs 125/100A","NDE",32.229999999999997,0,32.229999999999997,8592765037824,1,8592765037824,25,28592765037828,"8536901000",0.14199999999999999]
[103782,"PDB 1P CU 1x6 160A","Power Distribution Block 1Pole CU 1 input x 6 outputs 160A","NDE",43.34,0,43.34,8592765037831,1,8592765037831,20,28592765037835,"8536901000",0.255]
[103783,"PDB 1P CU/AL 1x6 160/125A","Power Distribution Block 1Pole CU/AL 1 input x 6 outputs 160/125A","NDE",45.99,0,45.99,8592765037848,1,8592765037848,20,28592765037842,"8536901000",0.255]
[103784,"PDB 1P CU 1x2+5+4 250A","Power Distribution Block 1Pole CU 1 input x 2+5+4 outputs 250A","NDE",60.39,0,60.39,8592765037855,1,8592765037855,20,28592765037859,"8536901000",0.45500000000000002]
[103785,"PDB 1P CU/AL 1x2+5+4 250/200A","Power Distribution Block 1Pole CU/AL 1 input x 2+5+4 outputs 250/200A","NDE",64.59,0,64.59,8592765037862,1,8592765037862,20,28592765037866,"8536901000",0.45500000000000002]
[103786,"PDB 1P CU 1x2+5+4 400A","Power Distribution Block 1Pole CU 1 input x 2+5+4 outputs 400A","NDE",62.56,0,62.56,8592765037879,1,8592765037879,20,28592765037873,"8536901000",0.45500000000000002]
[103787,"PDB 1P CU/AL 1x2+5+4 400/300A","Power Distribution Block 1Pole CU/AL 1 input x 2+5+4 outputs 400/300A","NDE",71.89,0,71.89,8592765037886,1,8592765037886,20,28592765037880,"8536901000",0.45500000000000002]
[103788,"PDB 3P CU 1x6 175A","Power Distribution Block 3Pole CU 1 input x 6 outputs 175A","NDE",84.82,0,84.82,8592765037893,1,8592765037893,10,28592765037897,"8536901000",0.29799999999999999]
[103789,"PDB 3P CU/AL 1x6 175/125A","Power Distribution Block 3Pole CU/AL 1 input x 6 outputs 175/125A","NDE",99.12,0,99.12,8592765037909,1,8592765037909,10,28592765037903,"8536901000",0.29799999999999999]
[105509,"PDB 1P CU 1x6 400A","Power Distribution Block 1Pole CU 1 input x 6 outputs 400A","NDE",61.31,0,61.31,8592765055101,1,8592765055101,10,28592765055105,"8536901000",0.48099999999999998]
[105510,"PDB 1P CU 1x2 400A","Power Distribution Block 1Pole CU 1 input x 2 outputs 400A","NDE",63.54,0,63.54,8592765055118,1,8592765055118,10,28592765055112,"8536901000",0.55600000000000005]
[103795,"PDB 1P CU/AL 1x6 400/350A","Power Distribution Block 1Pole CU/AL 1 input x 6 outputs 400/350A","NDE",61.77,0,61.77,8592765037961,1,8592765037961,10,28592765037965,"8536901000",0.51200000000000001]
[103796,"PDB 1P CU/AL 1x2 400/350A","Power Distribution Block 1Pole CU/AL 1 input x 2 outputs 400/350A","NDE",64.36,0,64.36,8592765037978,1,8592765037978,10,28592765037972,"8536901000",0.57199999999999995]
[]
["Terminals TB"]
[103850,"TBB 7x16","Terminal Block, covered, plastic DIN rail clip, blue, 7x16mm2 ","NDE",3.08,{"$f":"NDE","v":0},{"$f":"E4998*(1-F4998)","v":3.08},8592765038517,1,18592765038514,10,28592765038511,"8536901000",0.03]
[103851,"TBG 7x16","Terminal Block, covered, plastic DIN rail clip, green/yellow, 7x16mm2 ","NDE",3.08,0,3.08,8592765038524,1,18592765038521,10,28592765038528,"8536901000",0.03]
[103852,"TBB 15x16","Terminal Block, covered, plastic DIN rail clip, blue, 15x16mm2 ","NDE",6,0,6,8592765038531,1,18592765038538,10,28592765038535,"8536901000",5.6000000000000001E-2]
[103853,"TBG 15x16","Terminal Block, covered, plastic DIN rail clip, green/yellow, 15x16mm2 ","NDE",6,0,6,8592765038548,1,18592765038545,10,28592765038542,"8536901000",5.6000000000000001E-2]
[103854,"TBB 7x10","Terminal Block, uncovered, plastic DIN rail clip, blue, 7x10mm2 ","NDE",2.42,0,2.42,8592765038555,1,18592765038552,10,28592765038559,"8536901000",0.03]
[103855,"TBG 7x10","Terminal Block, uncovered, plastic DIN rail clip, green/yellow, 7x10mm2 ","NDE",2.42,0,2.42,8592765038562,1,18592765038569,10,28592765038566,"8536901000",0.03]
[103856,"TBB 12x10","Terminal Block, uncovered, plastic DIN rail clip, blue, 12x10mm2 ","NDE",3.79,0,3.79,8592765038579,1,18592765038576,10,28592765038573,"8536901000",0.04]
[103857,"TBG 12x10","Terminal Block, uncovered, plastic DIN rail clip, green/yellow, 12x10mm2 ","NDE",3.79,0,3.79,8592765038586,1,18592765038583,10,28592765038580,"8536901000",0.04]
[103858,"TB 7x10","Terminal Block, uncovered, metal DIN rail clip, 7x10mm2 ","NDE",2.39,0,2.39,8592765038593,1,18592765038590,10,28592765038597,"8536901000",0.03]
[103859,"TB 12x10","Terminal Block, uncovered, metal DIN rail clip, 12x10mm2 ","NDE",3.47,0,3.47,8592765038609,1,18592765038606,10,28592765038603,"8536901000",0.04]
[]
["Plastic Consumer Units PHS, PNS, PNF, PXS, PXF"]
[101492,"PHS 4T","Plastic consumer unit, surface-mounted, IP65, 1 row, 4 modules","NDA",16.48,{"$f":"NDA","v":0},{"$f":"E5010*(1-F5010)","v":16.48},8592765014931,1,8592765014931,224,null,"8538909999",0.46]
[101493,"PHS 8T","Plastic consumer unit, surface-mounted, IP65, 1 row, 8 modules","NDA",20.059999999999999,0,20.059999999999999,8592765014948,1,8592765014948,150,null,"8538909999",0.68]
[101494,"PHS 12T","Plastic consumer unit, surface-mounted, IP65, 1 row, 12 modules","NDA",26.42,0,26.42,8592765014955,1,8592765014955,68,null,"8538909999",1.24]
[101495,"PHS 24T","Plastic consumer unit, surface-mounted, IP65, 2 rows, 2x12 modules","NDA",40.29,0,40.29,8592765014962,1,8592765014962,45,null,"8538909999",1.7]
[101496,"PHS 36T","Plastic consumer unit, surface-mounted, IP65, 3 rows, 3x12 modules","NDA",46.57,0,46.57,8592765014979,1,8592765014979,30,null,"8538909999",2.3199999999999998]
[110814,"PHS 48T","Plastic consumer unit, surface-mounted, IP65, 4 rows, 4x12 modules","NDA",73.47,{"$f":"NDC","v":0},73.47,8592765108142,1,8592765108142,26,null,"8538909999",3.2450000000000001]
[101497,"PNS 8T","Plastic consumer unit, transparent door, surface-mounted, IP40, 1 row, 8 modules","NDA",13.1,0,13.1,8592765014986,1,8592765014986,152,null,"8538909999",0.6]
[101498,"PNS 12T","Plastic consumer unit, transparent door, surface-mounted, IP40, 1 row, 12 modules","NDA",15.54,0,15.54,8592765014993,1,8592765014993,117,null,"8538909999",0.95]
[101499,"PNS 18T","Plastic consumer unit, transparent door, surface-mounted, IP40, 1 row, 18 modules","NDA",18.04,0,18.04,8592765015006,1,8592765015006,120,null,"8538909999",1.21]
[101500,"PNS 24T","Plastic consumer unit, transparent door, surface-mounted, IP40, 2 rows, 2x12 modules","NDA",19.91,0,19.91,8592765015013,1,8592765015013,72,null,"8538909999",1.44]
[101501,"PNS 2x18T","Plastic consumer unit, transparent door, surface-mounted, IP40, 2 rows, 2x18 modules","NDA",28.86,0,28.86,8592765015020,1,8592765015020,54,null,"8538909999",2.41]
[101502,"PNS 36T","Plastic consumer unit, transparent door, surface-mounted, IP40, 3 rows, 3x12 modules","NDA",28.86,0,28.86,8592765015037,1,8592765015037,54,null,"8538909999",1.97]
[101503,"PNS 48T","Plastic consumer unit, transparent door, surface-mounted, IP40, 4 rows, 4x12 modules","NDA",33.28,0,33.28,8592765015044,1,8592765015044,39,null,"8538909999",2.46]
[106196,"PNS 3x18T","Plastic consumer unit, transparent door, surface-mounted, IP40, 3 rows, 3x18 modules","NDA",38.729999999999997,{"$f":"NDA","v":0},{"$f":"E5023*(1-F5023)","v":38.729999999999997},8592765061973,1,8592765061973,36,null,"8538909999",2.6]
[101504,"PNS 8W","Plastic consumer unit, white door, surface-mounted, IP40, 1 row, 8 modules","NDA",13.1,0,13.1,8592765015051,1,8592765015051,152,null,"8538909999",0.6]
[101505,"PNS 12W","Plastic consumer unit, white door, surface-mounted, IP40, 1 row, 12 modules","NDA",15.54,0,15.54,8592765015068,1,8592765015068,117,null,"8538909999",0.95]
[101506,"PNS 18W","Plastic consumer unit, white door, surface-mounted, IP40, 1 row, 18 modules","NDA",18.04,0,18.04,8592765015075,1,8592765015075,120,null,"8538909999",1.21]
[101507,"PNS 24W","Plastic consumer unit, white door, surface-mounted, IP40, 2 rows, 2x12 modules","NDA",19.91,0,19.91,8592765015082,1,8592765015082,72,null,"8538909999",1.44]
[101508,"PNS 2x18W","Plastic consumer unit, white door, surface-mounted, IP40, 2 rows, 2x18 modules","NDA",28.86,0,28.86,8592765015099,1,8592765015099,36,null,"8538909999",2.41]
[101509,"PNS 36W","Plastic consumer unit, white door, surface-mounted, IP40, 3 rows, 3x12 modules","NDA",28.86,0,28.86,8592765015105,1,8592765015105,54,null,"8538909999",1.97]
[101510,"PNS 48W","Plastic consumer unit, white door, surface-mounted, IP40, 4 rows, 4x12 modules","NDA",33.28,0,33.28,8592765015112,1,8592765015112,39,null,"8538909999",2.46]
[106197,"PNS 3x18W","Plastic consumer unit, white door, surface-mounted, IP40, 3 rows, 3x18 modules","NDA",38.729999999999997,{"$f":"NDA","v":0},38.729999999999997,8592765061980,1,8592765061980,54,null,"8538909999",2.6]
[101511,"PNF 8T","Plastic consumer unit, transparent door, flush-mounted, IP40, 1 row, 8 modules","NDA",13.1,0,13.1,8592765015129,1,8592765015129,152,null,"8538909999",0.68]
[101512,"PNF 12T","Plastic consumer unit, transparent door, flush-mounted, IP40, 1 row, 12 modules","NDA",15.54,0,15.54,8592765015136,1,8592765015136,117,null,"8538909999",0.92]
[101513,"PNF 18T","Plastic consumer unit, transparent door, flush-mounted, IP40, 1 row, 18 modules","NDA",18.04,0,18.04,8592765015143,1,8592765015143,120,null,"8538909999",1.21]
[101514,"PNF 24T","Plastic consumer unit, transparent door, flush-mounted, IP40, 2 rows, 2x12 modules","NDA",19.91,0,19.91,8592765015150,1,8592765015150,72,null,"8538909999",1.34]
[101515,"PNF 2x18T","Plastic consumer unit, transparent door, flush-mounted, IP40, 2 rows, 2x18 modules","NDA",28.86,0,28.86,8592765015167,1,8592765015167,54,null,"8538909999",2.41]
[101516,"PNF 36T","Plastic consumer unit, transparent door, flush-mounted, IP40, 3 rows, 3x12 modules","NDA",28.86,0,28.86,8592765015174,1,8592765015174,54,null,"8538909999",1.79]
[106198,"PNF 3x18T","Plastic consumer unit, transparent door, flush-mounted, IP40, 3 rows, 3x18 modules","NDA",38.729999999999997,{"$f":"NDA","v":0},38.729999999999997,8592765061997,1,8592765061997,36,null,"8538909999",2.6]
[101517,"PNF 8W","Plastic consumer unit, white door, flush-mounted, IP40, 1 row, 8 modules","NDA",13.1,0,13.1,8592765015181,1,8592765015181,152,null,"8538909999",0.68]
[101518,"PNF 12W","Plastic consumer unit, white door, flush-mounted, IP40, 1 row, 12 modules","NDA",15.54,0,15.54,8592765015198,1,8592765015198,117,null,"8538909999",0.92]
[101519,"PNF 18W","Plastic consumer unit, white door, flush-mounted, IP40, 1 row, 18 modules","NDA",18.04,0,18.04,8592765015204,1,8592765015204,120,null,"8538909999",1.21]
[101520,"PNF 24W","Plastic consumer unit, white door, flush-mounted, IP40, 2 rows, 2x12 modules","NDA",19.91,0,19.91,8592765015211,1,8592765015211,72,null,"8538909999",1.34]
[101521,"PNF 2x18W","Plastic consumer unit, white door, flush-mounted, IP40, 2 rows, 2x18 modules","NDA",28.86,0,28.86,8592765015228,1,8592765015228,54,null,"8538909999",2.41]
[101522,"PNF 36W","Plastic consumer unit, white door, flush-mounted, IP40, 3 rows, 3x12 modules","NDA",28.86,0,28.86,8592765015235,1,8592765015235,54,null,"8538909999",1.79]
[106199,"PNF 3x18W","Plastic consumer unit, white door, flush-mounted, IP40, 3 rows, 3x18 modules","NDA",38.729999999999997,{"$f":"NDA","v":0},38.729999999999997,8592765062000,1,8592765062000,36,null,"8538909999",2.6]
[101525,"PXS 3","Plastic consumer unit, without door, surface-mounted, IP30, 1 row, 3 modules","NDA",9.6999999999999993,{"$f":"NDA","v":0},9.6999999999999993,8592765015266,1,8592765015266,804,null,"8538909999",0.17]
[101526,"PXS 12","Plastic consumer unit, without door, surface-mounted, IP30, 1 row, 12 modules","NDA",16.7,0,16.7,8592765015273,1,8592765015273,200,null,"8538909999",0.56999999999999995]
[101527,"PXS 24","Plastic consumer unit, without door, surface-mounted, IP30, 2 rows, 2x12 modules","NDA",22.11,0,22.11,8592765015280,1,8592765015280,132,null,"8538909999",0.82]
[101528,"PXS 36","Plastic consumer unit, without door, surface-mounted, IP30, 3 rows, 3x12 modules","NDA",28.66,0,28.66,8592765015297,1,8592765015297,100,null,"8538909999",1.01]
[101529,"PXF 12T","Plastic consumer unit, flat transparent door, flush-mounted, IP40, 1 row, 12 modules","NDA",20.39,0,20.39,8592765015303,1,8592765015303,105,null,"8538909999",1.31]
[101530,"PXF 24T","Plastic consumer unit, flat transparent door, flush-mounted, IP40, 2 rows, 2x12 modules","NDA",32.020000000000003,0,32.020000000000003,8592765015310,1,8592765015310,75,null,"8538909999",1.96]
[101532,"PXF 12W","Plastic consumer unit, flat white door, flush-mounted, IP40, 1 row, 12 modules","NDA",20.39,0,20.39,8592765015334,1,8592765015334,105,null,"8538909999",1.31]
[101523,"PXF 24W","Plastic consumer unit, flat white door, flush-mounted, IP40, 2 rows, 2x12 modules","NDA",32.020000000000003,0,32.020000000000003,8592765015242,1,8592765015242,75,null,"8538909999",1.96]
[101533,"DR PHS 4T","Spare door for PHS 4T","NDA",6.24,0,6.24,8592765015341,1,8592765015341,null,null,"8538909999",0.06]
[101534,"DR PHS 8T","Spare door for PHS 8T","NDA",7.64,0,7.64,8592765015358,1,8592765015358,null,null,"8538909999",0.1]
[101535,"DR PHS 12T","Spare door for PHS 12T","NDA",11.42,0,11.42,8592765015365,1,8592765015365,null,null,"8538909999",0.14000000000000001]
[101536,"DR PHS 24T","Spare door for PHS 24T","NDA",14.27,0,14.27,8592765015372,1,8592765015372,null,null,"8538909999",0.25]
[101537,"DR PHS 36T","Spare door for PHS 36T","NDA",18.88,{"$f":"NDA","v":0},18.88,8592765015389,1,8592765015389,null,null,"8538909999",0.47]
[101538,"DR PNS 8T","Spare door for PNS/PNF 8T, transparent","NDA",5.61,0,5.61,8592765015396,1,8592765015396,null,null,"8538909999",0.12]
[101539,"DR PNS 12T","Spare door for PNS/PNF 12T, transparent","NDA",6.76,0,6.76,8592765015402,1,8592765015402,null,null,"8538909999",0.15]
[101540,"DR PNS 18T","Spare door for PNS/PNF 18T, transparent","NDA",7.7,0,7.7,8592765015419,1,8592765015419,null,null,"8538909999",0.2]
[101541,"DR PNS 24T","Spare door for PNS/PNF 24T, transparent","NDA",10.23,0,10.23,8592765015426,1,8592765015426,null,null,"8538909999",0.34]
[101542,"DR PNS 2x18T","Spare door for PNS/PNF 2x18T, transparent","NDA",12.37,0,12.37,8592765015433,1,8592765015433,null,null,"8538909999",0.42]
[101543,"DR PNS 36T","Spare door for PNS/PNF 36T, transparent","NDA",12.31,0,12.31,8592765015440,1,8592765015440,null,null,"8538909999",0.41]
[101544,"DR PNS 48T","Spare door for PNS/PNF 48T, transparent","NDA",15.91,0,15.91,8592765015457,1,8592765015457,null,null,"8538909999",0.5]
[106200,"DR PNS 3x18T","Spare door for PNS/PNF 3x18T, transparent","NDA",19.22,{"$f":"NDA","v":0},19.22,8592765062017,1,8592765062017,null,null,"8538909999",0.6]
[101545,"DR PNS 8W","Spare door for PNS/PNF 8T, white","NDA",5.61,0,5.61,8592765015464,1,8592765015464,null,null,"8538909999",0.12]
[101546,"DR PNS 12W","Spare door for PNS/PNF 12T, white","NDA",6.76,0,6.76,8592765015471,1,8592765015471,null,null,"8538909999",0.15]
[101547,"DR PNS 18W","Spare door for PNS/PNF 18T, white","NDA",7.7,0,7.7,8592765015488,1,8592765015488,null,null,"8538909999",0.2]
[101548,"DR PNS 24W","Spare door for PNS/PNF 24T, white","NDA",10.23,0,10.23,8592765015495,1,8592765015495,null,null,"8538909999",0.34]
[101549,"DR PNS 2x18W","Spare door for PNS/PNF 2x18T, white","NDA",12.37,0,12.37,8592765015501,1,8592765015501,null,null,"8538909999",0.42]
[101550,"DR PNS 36W","Spare door for PNS/PNF 36T, white","NDA",12.31,0,12.31,8592765015518,1,8592765015518,null,null,"8538909999",0.41]
[101551,"DR PNS 48W","Spare door for PNS/PNF 48T, white","NDA",15.91,0,15.91,8592765015525,1,8592765015525,null,null,"8538909999",0.5]
[106201,"DR PNS 3x18W","Spare door for PNS/PNF 3x18W, white","NDA",19.22,{"$f":"NDA","v":0},19.22,8592765062024,1,8592765062024,null,null,"8538909999",0.6]
[101571,"LK PH M","Lock with key for PHS, metal","NDA",15.09,0,15.09,8592765015723,1,8592765015723,null,null,"8301409000",0.02]
[101573,"LK PN M","Lock with key for PNS/PNF, metal","NDA",15.09,0,15.09,8592765015747,1,8592765015747,null,null,"8301409000",0.02]
[101574,"B CC45","Cover for device cut-out 45mm, white","NDA",0.95,0,0.95,8592765015754,500,18592765015744,null,null,"3926909790",0.03]
[101564,"DR PXF 12T","Spare door for PXF 12T, transparent","NDA",6.61,{"$f":"NDA","v":0},{"$f":"E5078*(1-F5078)","v":6.61},8592765015655,1,8592765015655,null,null,"8538909999",0.25]
[101565,"DR PXF 24T","Spare door for PXF 24T, transparent","NDA",9.77,0,9.77,8592765015662,1,8592765015662,null,null,"8538909999",0.4]
[101567,"DR PXF 12W","Spare door for PXF 12W, white","NDA",6.61,0,6.61,8592765015686,1,8592765015686,null,null,"8538909999",0.25]
[101568,"DR PXF 24W","Spare door for PXF 24W, white","NDA",9.77,0,9.77,8592765015693,1,8592765015693,null,null,"8538909999",0.4]
[106158,"MF PNF 24","Mounting frame PNF 2x12","NDA",3.02,{"$f":"NDA","v":0},{"$f":"E5082*(1-F5082)","v":3.02},8592765061591,1,8592765061591,null,null,"8538909999",0.28000000000000003]
[106159,"MF PNF 36","Mounting frame PNF 3x12","NDA",3.64,0,{"$f":"E5083*(1-F5083)","v":3.64},8592765061607,1,8592765061607,null,null,"8538909999",0.44]
[106160,"MF PNF 2x18","Mounting frame PNF 2x18","NDA",4.49,0,4.49,8592765061614,1,8592765061614,null,null,"8538909999",0.34]
[107029,"MF PNF 3x18","Mounting frame PNF 3x18","NDA",5.71,{"$f":"NDA","v":0},5.71,8592765070302,1,8592765070302,null,null,"7326909890"]
[106161,"MF PXF 24","Mounting frame PXF 2x12","NDA",3.02,0,3.02,8592765061621,1,8592765061621,null,null,"8538909999",0.3]
[106182,"SMM IP65S","Spare mounting material IP65","NDA",0.69,0,0.69,8592765061836,1,8592765061836,null,null,"8538909999",0.04]
[106183,"SMM IP40F","Spare mounting material IP40 flush mounted","NDA",0.69,0,0.69,8592765061843,1,8592765061843,null,null,"8538909999",0.04]
[106184,"SMM IP40S","Spare mounting material IP40 surface mounted","NDA",0.69,0,0.69,8592765061850,1,8592765061850,null,null,"8538909999",0.04]
[]
["Plastic Consumer Units for hollow-walls mounting PNF-HW"]
[106165,"PNF-HW 8T","Plastic consumer unit, transparent door, for hollow-walls mounting, flush-mounted, IP40, 1 row, 8 modules","NDF",19.34,{"$f":"NDF","v":0},{"$f":"E5092*(1-F5092)","v":19.34},8592765061669,1,8592765061669,152,null,"8538909999",0.68]
[106166,"PNF-HW 12T","Plastic consumer unit, transparent door, for hollow-walls mounting, flush-mounted, IP40, 1 row, 12 modules","NDF",22.38,{"$f":"NDF","v":0},{"$f":"E5093*(1-F5093)","v":22.38},8592765061676,1,8592765061676,117,null,"8538909999",0.92]
[106167,"PNF-HW 18T","Plastic consumer unit, transparent door, for hollow-walls mounting, flush-mounted, IP40, 1 row, 18 modules","NDF",27.96,0,27.96,8592765061683,1,8592765061683,120,null,"8538909999",1.21]
[106168,"PNF-HW 24T","Plastic consumer unit, transparent door, for hollow-walls mounting, flush-mounted, IP40, 2 rows, 2x12 modules","NDF",35.54,0,35.54,8592765061690,1,8592765061690,72,null,"8538909999",1.34]
[106169,"PNF-HW 2x18T","Plastic consumer unit, transparent door, for hollow-walls mounting, flush-mounted, IP40, 2 rows, 2x18 modules","NDF",42.28,0,42.28,8592765061706,1,8592765061706,54,null,"8538909999",2.41]
[106170,"PNF-HW 36T","Plastic consumer unit, transparent door, for hollow-walls mounting, flush-mounted, IP40, 3 rows, 3x12 modules","NDF",46.67,0,46.67,8592765061713,1,8592765061713,54,null,"8538909999",1.79]
[106202,"PNF-HW 3x18T","Plastic consumer unit, transparent door, for hollow-walls mounting, flush-mounted, IP40, 3 rows, 3x18 modules","NDF",74.03,0,74.03,8592765062031,1,8592765062031,36,null,"8538909999",2.6]
[106171,"PNF-HW 8W","Plastic consumer unit, white door, for hollow-walls mounting, flush-mounted, IP40, 1 row, 8 modules","NDF",19.34,0,19.34,8592765061720,1,8592765061720,152,null,"8538909999",0.68]
[106172,"PNF-HW 12W","Plastic consumer unit, white door, for hollow-walls mounting, flush-mounted, IP40, 1 row, 12 modules","NDF",22.38,0,22.38,8592765061737,1,8592765061737,117,null,"8538909999",0.92]
[106173,"PNF-HW 18W","Plastic consumer unit, white door, for hollow-walls mounting, flush-mounted, IP40, 1 row, 18 modules","NDF",27.96,0,27.96,8592765061744,1,8592765061744,120,null,"8538909999",1.21]
[106174,"PNF-HW 24W","Plastic consumer unit, white door, for hollow-walls mounting, flush-mounted, IP40, 2 rows, 2x12 modules","NDF",35.54,0,35.54,8592765061751,1,8592765061751,72,null,"8538909999",1.34]
[106175,"PNF-HW 2x18W","Plastic consumer unit, white door, for hollow-walls mounting, flush-mounted, IP40, 2 rows, 2x18 modules","NDF",42.28,0,42.28,8592765061768,1,8592765061768,54,null,"8538909999",2.41]
[106176,"PNF-HW 36W","Plastic consumer unit, white door, for hollow-walls mounting, flush-mounted, IP40, 3 rows, 3x12 modules","NDF",46.67,0,46.67,8592765061775,1,8592765061775,54,null,"8538909999",1.79]
[106203,"PNF-HW 3x18W","Plastic consumer unit, white door, for hollow-walls mounting, flush-mounted, IP40, 3 rows, 3x18 modules","NDF",74.03,0,74.03,8592765062048,1,8592765062048,36,null,"8538909999",2.6]
[106163,"SHW PNF","Spare mounting material PNF-HW","NDF",3.15,{"$f":"NDF","v":0},3.15,8592765061645,1,8592765061645,null,null,"8538909999",0.04]
[]
["Plastic Consumer Units PNS-SD"]
[107274,"PNS-SD 12T","Surface-mounted consumer units, IP40, 12 modules ","NDA",25.38,{"$f":"NDA","v":0},{"$f":"E5109*(1-F5109)","v":25.38},8592765072740,1,8592765072740,120,null,"8538909999",1.2]
[107275,"PNS-SD 24T","Surface-mounted consumer units, IP40, 24 modules ","NDA",35.24,0,35.24,8592765072757,1,8592765072757,66,null,"8538909999",1.6]
[107276,"PNS-SD 36T","Surface-mounted consumer units, IP40, 36 modules ","NDA",46.26,0,46.26,8592765072764,1,8592765072764,40,null,"8538909999",2]
[107277,"DR PNS-SD 12T","Spare transparent door for PNS-SD 12T","NDA",7.94,0,7.94,8592765072771,1,8592765072771,null,null,"8538909999"]
[107278,"DR PNS-SD 24T","Spare transparent door for PNS-SD 24T","NDA",12.03,0,12.03,8592765072788,1,8592765072788,null,null,"8538909999"]
[107279,"DR PNS-SD 36T","Spare transparent door for PNS-SD 36T","NDA",14.48,0,14.48,8592765073785,1,8592765073785,null,null,"8538909999"]
[]
["Plastic Consumer Units with metal door PMF"]
[107101,"PMF 12","Plastic consumer unit with white metal door, flush-mounted, IP40, 1 row, 12 modules","NDC",32.69,{"$f":"NDC","v":0},{"$f":"E5117*(1-F5117)","v":32.69},8592765071026,1,8592765071026,60,null,"8538909999",2]
[107102,"PMF 24","Plastic consumer unit with white metal door, flush-mounted, IP40, 2 row, 24 modules","NDC",39.08,0,39.08,8592765071033,1,8592765071033,47,null,"8538909999",2.5]
[107103,"PMF 36","Plastic consumer unit with white metal door, flush-mounted, IP40, 3 row, 36 modules","NDC",52.33,0,52.33,8592765071040,1,8592765071040,33,null,"8538909999",3]
[107104,"PMF 48","Plastic consumer unit with white metal door, flush-mounted, IP40, 4 row, 48 modules","NDC",62.86,0,62.86,8592765071057,1,8592765071057,24,null,"8538909999",3.5]
[107262,"PMF 60","Plastic consumer unit with white metal door, flush-mounted, IP40, 5 row, 60 modules","NDC",106.79,{"$f":"NDC","v":0},{"$f":"E5121*(1-F5121)","v":106.79},8592765072627,1,8592765072627,14,null,"8538909999",4.5]
[107105,"DR PMF 12","Spare door for PMF 12","NDC",30.48,0,30.48,8592765071064,1,8592765071064,null,null,"8538909999",1.0900000000000001]
[107106,"DR PMF 24","Spare door for PMF 24","NDC",38.58,0,38.58,8592765071071,1,8592765071071,null,null,"8538909999",1.33]
[107107,"DR PMF 36","Spare door for PMF 36","NDC",46.99,0,46.99,8592765071088,1,8592765071088,null,null,"8538909999",1.76]
[107108,"DR PMF 48","Spare door for PMF 48","NDC",61.86,0,61.86,8592765071095,1,8592765071095,null,null,"8538909999",2.1]
[107263,"DR PMF 60","Spare door for PMF 60","NDC",117.61,{"$f":"NDC","v":0},{"$f":"E5126*(1-F5126)","v":117.61},8592765072634,1,8592765072634,null,null,"8538909999"]
[107120,"SMM PMF","Spare mounting material PMF","NDC",3.15,0,3.15,8592765071217,1,8592765071217,null,null,"8538909999",0.04]
[107121,"SL PMF","Spare lock PMF","NDC",2.13,0,2.13,8592765071224,1,8592765071224,null,null,"8301409000",0.02]
[105494,"LK PM M","Lock with key for PMF, metal","NDC",19.82,0,19.82,8592765054951,1,8592765054951,null,null,"8301409000",0.03]
[107122,"SDDA PMF","Spare door depth adjuster for PMF","NDC",0.74,0,0.74,8592765071231,1,8592765071231,null,null,"8538909999",0.04]
[]
["Multimedia Consumer Units PMF-MM"]
[107264,"PMF-MM 12","Plastic consumer unit with metal door, flush-mounted, multimedia, 12 modules, 1 row","NDC",35.36,{"$f":"NDC","v":0},{"$f":"E5133*(1-F5133)","v":35.36},8592765072641,1,8592765072641,60,null,"8538909999",1.8]
[107265,"PMF-MM 24","Plastic consumer unit with metal door, flush-mounted, multimedia, 24 modules, 2 rows ","NDC",43.96,{"$f":"NDC","v":0},43.96,8592765072658,1,8592765072658,47,null,"8538909999",2.2999999999999998]
[107266,"PMF-MM 36","Plastic consumer unit with metal door, flush-mounted, multimedia, 36 modules, 3 rows ","NDC",56.46,0,56.46,8592765072665,1,8592765072665,33,null,"8538909999",2.8]
[107267,"PMF-MM 48","Plastic consumer unit with metal door, flush-mounted, multimedia, 48 modules, 4 rows","NDC",80.709999999999994,0,80.709999999999994,8592765072672,1,8592765072672,24,null,"8538909999",3.3]
[107268,"PMF-MM 60","Plastic consumer unit with metal door, flush-mounted, multimedia, 60 modules, 5 rows","NDC",117.17,{"$f":"NDC","v":0},117.17,8592765072689,1,8592765072689,14,null,"8538909999",4.3]
[111141,"PMF-MM 12 PT","Flush mounting enclosure for multimedia devices, transparent plastic door - 1 row","NDC",30.06,{"$f":"NDC","v":0},30.06,8592765111418,1,8592765111418,60,null,"8538909999"]
[111142,"PMF-MM 24 PT","Flush mounting enclosure for multimedia devices, transparent plastic door - 2 rows","NDC",37.369999999999997,{"$f":"NDC","v":0},37.369999999999997,8592765111425,1,8592765111425,47,null,"8538909999"]
[110707,"PMF-MM 36 PT","Flush mounting enclosure for multimedia devices, transparent plastic door - 3 rows","NDC",47.99,{"$f":"NDC","v":0},47.99,8592765107077,1,8592765107077,33,null,"8538909999",2.2000000000000002]
[111143,"PMF-MM 12 PW","Flush mounting enclosure for multimedia devices, white plastic door - 1 row","NDC",30.06,0,30.06,8592765111432,1,8592765111432,60,null,"8538909999"]
[111144,"PMF-MM 24 PW","Flush mounting enclosure for multimedia devices, white plastic door - 2 rows","NDC",37.369999999999997,{"$f":"NDC","v":0},37.369999999999997,8592765111449,1,8592765111449,47,null,"8538909999"]
[110708,"PMF-MM 36 PW","Flush mounting enclosure for multimedia devices, white plastic door - 3 rows","NDC",47.99,0,47.99,8592765107084,1,8592765107084,33,null,"8538909999",2.2000000000000002]
[107269,"DR PMF-MM 12","Spare door for PMF-MM 12","NDC",37.1,{"$f":"NDC","v":0},37.1,8592765072696,1,8592765072696,null,null,"8538909999",1.0940000000000001]
[107270,"DR PMF-MM 24","Spare door for PMF-MM 24","NDC",45.75,{"$f":"NDC","v":0},45.75,8592765072702,1,8592765072702,null,null,"8538909999",1.331]
[107271,"DR PMF-MM 36","Spare door for PMF-MM 36","NDC",56.49,{"$f":"NDC","v":0},56.49,8592765072719,1,8592765072719,null,null,"8538909999",1.7589999999999999]
[107272,"DR PMF-MM 48","Spare door for PMF-MM 48","NDC",68.37,{"$f":"NDC","v":0},68.37,8592765072726,1,8592765072726,null,null,"8538909999",2.1]
[107273,"DR PMF-MM 60","Spare door for PMF-MM 60","NDC",117.61,{"$f":"NDC","v":0},117.61,8592765072733,1,8592765072733,null,null,"8538909999",0]
[107280,"VCBP M","Vertical connection bracket PMF","NDC",0.8,0,0.8,8592765072801,1,8592765072801,null,null,"7326909890",0]
[108053,"HCB PM","Horizontal connection bracket PMF","NDC",5.01,0,5.01,8592765080547,1,8592765080547,null,null,"8538909999",0.05]
[107121,"SL PMF","Spare lock PMF","NDC",2.13,0,2.13,8592765071224,1,8592765071224,null,null,"8301409000",0]
[105494,"LK PM M","Lock with key for PMF, metal","NDC",19.82,0,19.82,8592765054951,1,8592765054951,null,null,"8301409000",2.5000000000000001E-2]
[108052,"MP PM","Mounting plate","NDC",6,0,6,8592765080530,1,8592765080530,null,null,"8538909999",0.25]
[109047,"RH PMF-MM","Network devices holder","NDC",5.63,0,5.63,8592765090478,1,8592765090478,null,null,"8538909999",0.1]
[108093,"MF PNF 12","DIN rail (12 MU), PMF","NDC",0.8,0,0.8,8592765080936,1,8592765080936,null,null,"8538909999",0]
[101577,"TH CUB P","Additional insulated terminal 2x15","NDC",4.99,0,4.99,8592765015785,1,8592765015785,null,null,"8536901000",0.03]
[107120,"SMM PMF","Spare mounting material PMF","NDC",3.15,0,3.15,8592765071217,1,8592765071217,null,null,"8538909999",0.04]
[107122,"SDDA PMF","Spare door depth adjuster for PMF","NDC",0.74,0,0.74,8592765071231,1,8592765071231,null,null,"8538909999",0.04]
[]
["Metal flat enclosures EMF"]
[109809,"EMFF2 48W","Metal Flat Flush-mounted enclosure, 2 rows (24MU), 48MU, sheetsteel white door, NPE terminals included","NDD",147.38999999999999,{"$f":"NDD","v":0},{"$f":"E5161*(1-F5161)","v":147.38999999999999},8592765098092,1,8592765098092,null,null,"8538909999",11.5]
[109810,"EMFF3 72W","Metal Flat Flush-mounted enclosure, 3 rows (24MU), 72MU, sheetsteel white door, NPE terminals included","NDD",169.99,{"$f":"NDD","v":0},{"$f":"E5162*(1-F5162)","v":169.99},8592765098108,1,8592765098108,null,null,"8538909999",13.5]
[109811,"EMFF4 96W","Metal Flat Flush-mounted enclosure, 4 rows (24MU), 96MU, sheetsteel white door, NPE terminals included","NDD",184.76,0,184.76,8592765098115,1,8592765098115,null,null,"8538909999",16.5]
[109812,"EMFF5 120W","Metal Flat Flush-mounted enclosure, 5 rows (24MU), 120MU, sheetsteel white door, NPE terminals included","NDD",214.1,0,214.1,8592765098122,1,8592765098122,null,null,"8538909999",18.5]
[109813,"EMFF6 144W","Metal Flat Flush-mounted enclosure, 6 rows (24MU), 144MU, sheetsteel white door, NPE terminals included","NDD",246.85,0,246.85,8592765098139,1,8592765098139,null,null,"8538909999",21.5]
[109814,"EMFS2 48W","Metal Flat Surface-mounted enclosure, 2 rows (24MU), 48MU, sheetsteel white door, NPE terminals included","NDD",172.65,0,172.65,8592765098146,1,8592765098146,null,null,"8538909999",11.5]
[109815,"EMFS3 72W","Metal Flat Surface-mounted enclosure, 3 rows (24MU), 72MU, sheetsteel white door, NPE terminals included","NDD",194.89,0,194.89,8592765098153,1,8592765098153,null,null,"8538909999",14.5]
[109816,"EMFS4 96W","Metal Flat Surface-mounted enclosure, 4 rows (24MU), 96MU, sheetsteel white door, NPE terminals included","NDD",218.3,0,218.3,8592765098160,1,8592765098160,null,null,"8538909999",16.5]
[109817,"EMFS5 120W","Metal Flat Surface-mounted enclosure, 5 rows (24MU), 120MU, sheetsteel white door, NPE terminals included","NDD",240.14,0,240.14,8592765098177,1,8592765098177,null,null,"8538909999",19.5]
[109818,"EMFS6 144W","Metal Flat Surface-mounted enclosure, 6 rows (24MU), 144MU, sheetsteel white door, NPE terminals included","NDD",261.58999999999997,0,261.58999999999997,8592765098184,1,8592765098184,null,null,"8538909999",21.5]
[109819,"EMFF2 66W","Metal Flat Flush-mounted enclosure, 2 rows (33MU), 66MU, sheetsteel white door, NPE terminals included","NDD",181.47,0,181.47,8592765098191,1,8592765098191,null,null,"8538909999",13.5]
[109820,"EMFF3 99W","Metal Flat Flush-mounted enclosure, 3 rows (33MU), 99MU, sheetsteel white door, NPE terminals included","NDD",208.56,0,208.56,8592765098207,1,8592765098207,null,null,"8538909999",16.5]
[109821,"EMFF4 132W","Metal Flat Flush-mounted enclosure, 4 rows (33MU), 132MU, sheetsteel white door, NPE terminals included","NDD",249.92,0,249.92,8592765098214,1,8592765098214,null,null,"8538909999",19.5]
[109822,"EMFF5 165W","Metal Flat Flush-mounted enclosure, 5 rows (33MU), 165MU, sheetsteel white door, NPE terminals included","NDD",283.91000000000003,0,283.91000000000003,8592765098221,1,8592765098221,null,null,"8538909999",22.5]
[109823,"EMFF6 198W","Metal Flat Flush-mounted enclosure, 6 rows (33MU), 198MU, sheetsteel white door, NPE terminals included","NDD",321.02,0,321.02,8592765098238,1,8592765098238,null,null,"8538909999",25.5]
[109824,"EMFS2 66W","Metal Flat Surface-mounted enclosure, 2 rows (33MU), 66MU, sheetsteel white door, NPE terminals included","NDD",188.84,0,188.84,8592765098245,1,8592765098245,null,null,"8538909999",14.5]
[109825,"EMFS3 99W","Metal Flat Surface-mounted enclosure, 3 rows (33MU), 99MU, sheetsteel white door, NPE terminals included","NDD",207.65,0,207.65,8592765098252,1,8592765098252,null,null,"8538909999",17.5]
[109826,"EMFS4 132W","Metal Flat Surface-mounted enclosure, 4 rows (33MU), 132MU, sheetsteel white door, NPE terminals included","NDD",268.76,0,268.76,8592765098269,1,8592765098269,null,null,"8538909999",20.5]
[109827,"EMFS5 165W","Metal Flat Surface-mounted enclosure, 5 rows (33MU), 165MU, sheetsteel white door, NPE terminals included","NDD",303.01,0,303.01,8592765098276,1,8592765098276,null,null,"8538909999",23.5]
[109828,"EMFS6 198W","Metal Flat Surface-mounted enclosure, 6 rows (33MU), 198MU, sheetsteel white door, NPE terminals included","NDD",339.54,0,339.54,8592765098283,1,8592765098283,null,null,"8538909999",26.5]
["Acc."]
[109939,"EMF DR2 48W","Spare door for EMF, white, sheetsteel, 2 rows (24MU), 48MU","NDD",39.35,0,{"$f":"E5182*(1-F5182)","v":39.35},8592765099396,1,8592765099396,null,null,"8538909999",3]
[109940,"EMF DR3 72W","Spare door for EMF, white, sheetsteel, 3 rows (24MU), 72MU","NDD",43.72,0,43.72,8592765099402,1,8592765099402,null,null,"8538909999",3.7]
[109941,"EMF DR4 96W","Spare door for EMF, white, sheetsteel, 4 rows (24MU), 96MU","NDD",48.17,0,48.17,8592765099419,1,8592765099419,null,null,"8538909999",4.5]
[109942,"EMF DR5 120W","Spare door for EMF, white, sheetsteel, 5 rows (24MU), 120MU","NDD",53.49,0,53.49,8592765099426,1,8592765099426,null,null,"8538909999",5.3]
[109943,"EMF DR6 144W","Spare door for EMF, white, sheetsteel, 6 rows (24MU), 144MU","NDD",62.68,0,62.68,8592765099433,1,8592765099433,null,null,"8538909999",6.1]
[109944,"EMF DR2 66W","Spare door for EMF, white, sheetsteel, 2 rows (33MU), 66MU","NDD",37.450000000000003,0,37.450000000000003,8592765099440,1,8592765099440,null,null,"8538909999",3.7]
[109945,"EMF DR3 99W","Spare door for EMF, white, sheetsteel, 3 rows (33MU), 99MU","NDD",46.42,0,46.42,8592765099457,1,8592765099457,null,null,"8538909999",4.7]
[109946,"EMF DR4 132W","Spare door for EMF, white, sheetsteel, 4 rows (33MU), 132MU","NDD",55.36,0,55.36,8592765099464,1,8592765099464,null,null,"8538909999",5.7]
[109947,"EMF DR5 165W","Spare door for EMF, white, sheetsteel, 5 rows (33MU), 165MU","NDD",64.52,0,64.52,8592765099471,1,8592765099471,null,null,"8538909999",6.7]
[109948,"EMF DR6 198W","Spare door for EMF, white, sheetsteel, 6 rows (33MU), 198MU","NDD",73.5,0,73.5,8592765099488,1,8592765099488,null,null,"8538909999",7.7]
[109935,"EMF FP 1 24","Spare metal frontplate with device cutout, white, 1 row, 24MU","NDD",23.05,0,23.05,8592765099358,1,8592765099358,null,null,"8538100000",0.55000000000000004]
[109936,"EMF FP 1 33","Spare metal frontplate with device cutout, white, 1 row, 33MU","NDD",18.57,0,18.57,8592765099365,1,8592765099365,null,null,"8538100000",0.7]
[109937,"EMF FP 1+ 24","Spare metal end frontplate with device cutout, white, 1 row, 24MU","NDD",21.98,0,21.98,8592765099372,1,8592765099372,null,null,"8538100000",0.8]
[109938,"EMF FP 1+ 33","Spare metal end frontplate with device cutout, white, 1 row, 33MU","NDD",21.85,0,21.85,8592765099389,1,8592765099389,null,null,"8538100000",1.04]
[109835,"EMF FPB 0+ 24","Metal end frontplate, blind, white, narrow, 24MU","NDD",16.510000000000002,0,16.510000000000002,8592765098351,1,8592765098351,null,null,"8538100000",0.4]
[109933,"EMF FPB 0+ 33","Metal end frontplate, blind, white, narrow, 33MU","NDD",16.510000000000002,0,16.510000000000002,8592765099334,1,8592765099334,null,null,"8538100000",0.5]
[109836,"EMF UMP 80 24","Universal mounting plate, 80mm, 24MU","NDD",11.55,0,11.55,8592765098368,1,8592765098368,null,null,"8538100000",0.55000000000000004]
[109932,"EMF UEMP 80 33","Universal mounting plate, 80mm, 33MU","NDD",13.77,0,13.77,8592765099327,1,8592765099327,null,null,"8538100000",0.8]
[109838,"EMF UMP 160 24","Universal mounting plate, 160mm, 24MU","NDD",16.440000000000001,0,16.440000000000001,8592765098382,1,8592765098382,null,null,"8538100000",1.1100000000000001]
[109934,"EMF UEMP 160 33","Universal mounting plate, 160mm, 33MU","NDD",16.78,0,16.78,8592765099341,1,8592765099341,null,null,"8538100000",1.6]
[110699,"EMF MP M12 24","Mounting plate for Ex9M1,2, 24MU","NDD",39.21,{"$f":"NDD","v":0},39.21,8592765106995,1,8592765106995,null,null,"8538909999",1.1000000000000001]
[110700,"EMF MP M12 33","Mounting plate for Ex9M1,2, 33MU","NDD",34.99,0,34.99,8592765107008,1,8592765107008,null,null,"8538909999",1.5]
[109837,"EMF HS 24","Horizontal separator, 24MU (vodorovná oddělovací přepážka)","NDD",11.25,0,11.25,8592765098375,1,8592765098375,null,null,"8538100000",0.7]
[109833,"EMFS SMM","Spare mounting material, surface mounted, 1 set","NDD",3.41,0,3.41,8592765098337,1,8592765098337,null,null,"8538909999",0.04]
[109832,"EMFF SMM","Spare mounting material, flush mounted, 1 set","NDD",3.41,0,3.41,8592765098320,1,8592765098320,null,null,"8538909999",0.04]
[109834,"EMF LMS","Set for mounting of Dirak-style lock-key mechanism, white","NDD",7.12,0,7.12,8592765098344,1,8592765098344,null,null,"8538100000",0.03]
[109839,"EMF CFR24","Lišta pro upevnění kabelů, 24MU","NDD",12.44,0,12.44,8592765098399,1,8592765098399,null,null,"8538100000",0.3]
[109831,"EMF SDH","Spare door hinges","NDD",7.65,0,7.65,8592765098313,1,8592765098313,null,null,"8302100090",0.05]
[109931,"EMFF EMH","Set of mounting holders for flush mounting enclosures","NDD",6.68,0,6.68,8592765099310,1,8592765099310,null,null,"8538909999",0.02]
[106831,"MF PDP A4","Plastic documentation pocket, A4, self-adhesive","NDD",10.33,0,10.33,8592765068323,1,8592765068323,null,null,"3926909790",0.2]
[106832,"MF PDP A4S","Plastic documentation pocket, A4, self-adhesive, slim","NDD",7.88,0,7.88,8592765068330,1,8592765068330,null,null,"3926909790",0.1]
[106863,"MF DLK SP6","Lock-key, square pin, 6mm","NDD",14.23,0,14.23,8592765068644,1,8592765068644,null,null,"8301409000",0.03]
[106825,"MF DLK DB3","Lock-key, double pin, 3mm","NDD",12.12,0,12.12,8592765068262,1,8592765068262,null,null,"8301409000",0.03]
[106828,"MF DLK DB5","Lock-key, double pin, 5mm","NDD",12.12,0,12.12,8592765068293,1,8592765068293,null,null,"8301409000",0.03]
[106826,"MF DLK SQ6","Lock-key, square hole, 6mm","NDD",12.79,0,12.79,8592765068279,1,8592765068279,null,null,"8301409000",0.03]
[106830,"MF DLK D","Lock-key, daimler-benz","NDD",14.23,0,14.23,8592765068316,1,8592765068316,null,null,"8301409000",0.03]
[106829,"MF DLK S24","Lock-key, slotted 2x4mm","NDD",14.23,0,14.23,8592765068309,1,8592765068309,null,null,"8301409000",0.03]
[106827,"MF DLK CZ","Lock-key, Czech crescent","NDD",12.12,0,12.12,8592765068286,1,8592765068286,null,null,"8301409000",0.03]
[109048,"MF DLK K","Lock with key","NDD",41.56,0,41.56,8592765090485,1,8592765090485,null,null,"8301409000",0.03]
[109830,"EMF TBH","Horizontal terminal holders","NDD",6.65,0,6.65,8592765098306,1,8592765098306,null,null,"8538100000",0.03]
[109829,"EMF TB45+2","N/PE terminal bar 2x25 + 45x16 mm2","NDD",18.14,0,18.14,8592765098290,1,8592765098290,null,null,"8536901000",0.2]
[106860,"CGQS M16","Cable grommet for EMFS enclosures, 16mm, 1 pc.","NDD",0.76,0,0.76,8592765068613,1,8592765068613,null,null,"4016930090",0.01]
[106208,"CGQS M20","Cable grommet, 20mm, 1 pc.","NDD",0.83,0,0.83,8592765062093,1,8592765062093,null,null,"4016930090",0.01]
[106209,"CGQS M25","Cable grommet, 25mm, 1 pc.","NDD",1.06,0,1.06,8592765062109,1,8592765062109,null,null,"4016930090",0.01]
[106210,"CGQS M32","Cable grommet, 32mm, 1 pc.","NDD",1.43,0,1.43,8592765062116,1,8592765062116,null,null,"4016930090",0.01]
[107841,"MF TL","Empty type label for distribution boards, self-adhesive","NDD",2.99,0,2.99,18592765078428,10,18592765078428,null,null,"8538909999",0.01]
[]
["GRP distribution board, FHS",null,null,null,null,null,null,"","","","","",null,""]
[107192,"FHS-S1 W","GRP distribution board 260x305x160","NDG",139.41999999999999,{"$f":"NDG","v":0},{"$f":"E5230*(1-F5230)","v":139.41999999999999},8592765071927,1,18592765071924,null,28592765071921,"8538909999",2.9710000000000001]
[107193,"FHS-S2 36W","GRP distribution board 340x430x180 36 Modules ","NDG",164.31,{"$f":"NDG","v":0},{"$f":"E5231*(1-F5231)","v":164.31},8592765071934,1,18592765071931,null,28592765071938,"8538909999",4.67]
[107194,"FHS-S3 54W","GRP distribution board 450x505x220 54 Modules ","NDG",220.72,0,220.72,8592765071941,1,18592765071948,null,28592765071945,"8538909999",7.0519999999999996]
[107195,"FHS-S4 72W","GRP distribution board 450x655x220 72 Modules ","NDG",263.52999999999997,0,263.52999999999997,8592765071958,1,18592765071955,null,28592765071952,"8538909999",8.6210000000000004]
[107196,"FHS-S5 96W","GRP distribution board 560x655x260 96 Modules ","NDG",315.3,0,315.3,8592765071965,1,18592765071962,null,28592765071969,"8538909999",10.129]
[107197,"FHS-S6 140W","GRP distribution board 630x810x300 140 Modules ","NDG",423.41,0,423.41,8592765071972,1,18592765071979,null,28592765071976,"8538909999",15.68]
[107198,"FHS-S7 200W","GRP distribution board 850x1060x350 200 Modules ","NDG",666.65,0,666.65,8592765071989,1,18592765071986,null,28592765071983,"8538909999",24.253]
[107206,"MF FHS S2","Frame for board size 2","NDG",68.06,0,68.06,8592765072061,1,18592765072068,null,28592765072065,"7326909890",0.52800000000000002]
[107207,"MF FHS S3","Frame for board size 3","NDG",72.72,0,72.72,8592765072078,1,18592765072075,null,28592765072072,"7326909890",0.64600000000000002]
[107208,"MF FHS S4-5","Frame for board size 4-5","NDG",88.72,0,88.72,8592765072085,1,18592765072082,null,28592765072089,"7326909890",0.86699999999999999]
[107209,"MF FHS S6","Frame for board size 6","NDG",107.64,0,107.64,8592765072092,1,18592765072099,null,28592765072096,"7326909890",1.052]
[107210,"MF FHS S7","Frame for board size 7","NDG",125.59,0,125.59,8592765072108,1,18592765072105,null,28592765072102,"7326909890",1.466]
[107211,"MBP FHS S1","Metal back plate for board size  1","NDG",11.17,0,11.17,8592765072115,1,18592765072112,null,28592765072119,"7326909890",0.51900000000000002]
[107212,"MBP FHS S2","Metal back plate for board size  2","NDG",16.39,0,16.39,8592765072122,1,18592765072129,null,28592765072126,"7326909890",1]
[107213,"MBP FHS S3","Metal back plate for board size  3","NDG",28.17,0,28.17,8592765072139,1,18592765072136,null,28592765072133,"7326909890",2.5950000000000002]
[107214,"MBP FHS S4","Metal back plate for board size  4","NDG",36.81,0,36.81,8592765072146,1,18592765072143,null,28592765072140,"7326909890",3.3849999999999998]
[107215,"MBP FHS S5","Metal back plate for board size  5","NDG",45.65,0,45.65,8592765072153,1,18592765072150,null,28592765072157,"7326909890",4.3810000000000002]
[107216,"MBP FHS S6","Metal back plate for board size  6","NDG",73.34,0,73.34,8592765072160,1,18592765072167,null,28592765072164,"7326909890",6.52]
[107217,"MBP FHS S7","Metal back plate for board size  7","NDG",148.87,0,148.87,8592765072177,1,18592765072174,null,28592765072171,"7326909890",12.52]
[107218,"IBP FHS S1","Back plate GRP for board size  1","NDG",30.17,0,30.17,8592765072184,1,18592765072181,null,28592765072188,"3926909790",0.30299999999999999]
[107219,"IBP FHS S2","Back plate GRP for board size  2","NDG",61.8,0,61.8,8592765072191,1,18592765072198,null,28592765072195,"3926909790",0.60899999999999999]
[107220,"IBP FHS S3","Back plate GRP for board size  3","NDG",88.97,0,88.97,8592765072207,1,18592765072204,null,28592765072201,"3926909790",0.19400000000000001]
[107221,"IBP FHS S4","Back plate GRP for board size  4","NDG",104.69,0,104.69,8592765072214,1,18592765072211,null,28592765072218,"3926909790",1.264]
[107222,"IBP FHS S5","Back plate GRP for board size  5","NDG",120.32,0,120.32,8592765072221,1,18592765072228,null,28592765072225,"3926909790",1.65]
[107223,"IBP FHS S6","Back plate GRP for board size  6","NDG",190.99,0,190.99,8592765072238,1,18592765072235,null,28592765072232,"3926909790",2.4]
[107224,"PW FHS S2","Panel with windows 12 mod size 2","NDG",17.95,0,17.95,8592765072245,1,18592765072242,null,28592765072249,"8538909999",0.48]
[107225,"PW FHS S3-4","Panel with windows 18 mod size 3-4","NDG",29.45,0,29.45,8592765072252,1,18592765072259,null,28592765072256,"8538909999",0.69199999999999995]
[107226,"PW FHS S5","Panel with windows 24 mod size 5","NDG",32.869999999999997,0,32.869999999999997,8592765072269,1,18592765072266,null,28592765072263,"8538909999",0.875]
[107227,"PW FHS S6","Panel with windows 28 mod size 6","NDG",34.72,0,34.72,8592765072276,1,18592765072273,null,28592765072270,"8538909999",0.96099999999999997]
[107228,"PW FHS S7","Panel with windows 40 mod size 7","NDG",45.79,0,45.79,8592765072283,1,18592765072280,null,28592765072287,"8538909999",1.286]
[107229,"BP FHS S2","Blind panel for board size 2","NDG",7.97,0,7.97,8592765072290,1,18592765072297,null,28592765072294,"3926909790",0.308]
[107230,"BP FHS S3-4","Blind panel for board size 3-4","NDG",11.4,0,11.4,8592765072306,1,18592765072303,null,28592765072300,"3926909790",0.32400000000000001]
[107231,"BP FHS S5","Blind panel for board size 5","NDG",19.28,0,19.28,8592765072313,1,18592765072310,null,28592765072317,"3926909790",0.42]
[107232,"BP FHS S6","Blind panel for board size 6","NDG",22.85,0,22.85,8592765072320,1,18592765072327,null,28592765072324,"3926909790",0.501]
[107233,"BP FHS S7","Blind panel for board size 7","NDG",24.79,0,24.79,8592765072337,1,18592765072334,null,28592765072331,"3926909790",0.747]
[107234,"DBP FHS S2","Double blind panel for board size 2","NDG",12.01,0,12.01,8592765072344,1,18592765072341,null,28592765072348,"3926909790",0.39800000000000002]
[107235,"DBP FHS S3-4","Double blind panel for board size 3-4","NDG",16.77,0,16.77,8592765072351,1,18592765072358,null,28592765072355,"3926909790",0.57299999999999995]
[107236,"DBP FHS S5","Double blind panel for board size 5","NDG",23.32,0,23.32,8592765072368,1,18592765072365,null,28592765072362,"3926909790",0.69099999999999995]
[107237,"DBP FHS S6","Double blind panel for board size 6","NDG",25.45,0,25.45,8592765072375,1,18592765072372,null,28592765072379,"3926909790",0.78100000000000003]
[107238,"DBP FHS S7","Double blind panel for board size 7","NDG",39.28,0,39.28,8592765072382,1,18592765072389,null,28592765072386,"3926909790",1.5149999999999999]
[107239,"MSB FHS S2","Mod steel backplate H125 boards size 2","NDG",22.09,0,22.09,8592765072399,1,18592765072396,null,28592765072393,"7326909890",0.53]
[107240,"MSB FHS S3-4","Mod steel backplate H150 boards size 3-4","NDG",27.7,0,27.7,8592765072405,1,18592765072402,null,28592765072409,"7326909890",0.85099999999999998]
[107241,"MSB FHS S5","Mod steel backplate H150 boards size 5","NDG",32.01,0,32.01,8592765072412,1,18592765072419,null,28592765072416,"7326909890",1]
[107242,"MSB FHS S6","Mod steel backplate H150 boards size 6","NDG",34.39,0,34.39,8592765072429,1,18592765072426,null,28592765072423,"7326909890",1.26]
[107243,"MSB FHS SIZE 7","Mod steel backplate H200 boards size 7","NDG",51.4,0,51.4,8592765072436,1,18592765072433,null,28592765072430,"7326909890",2.35]
[107244,"GB FHS","4 Galvanized brackets for wall instal","NDG",5,0,5,8592765072443,1,18592765072440,null,28592765072447,"7326909890",0.255]
[107245,"SB FHS","4 Steel brackets for wall installation","NDG",11.26,0,11.26,8592765072450,1,18592765072457,null,28592765072454,"7326909890",0.26800000000000002]
[107246,"PM FHS S1-2","Acc. pole mounting for board sizes 1-2","NDG",99.94,0,99.94,8592765072467,1,18592765072464,null,28592765072461,"7326909890",1.829]
[107247,"PM FHS S3-4-5","Acc. pole mounting for board sizes 3-4-5","NDG",114.33,0,114.33,8592765072474,1,18592765072471,null,28592765072478,"7326909890",2.714]
[107248,"HSL FHS","Security lock with handle","NDG",10.83,0,10.83,8592765072481,1,18592765072488,null,28592765072485,"8301409000",1]
[107249,"TID FHS S2","GRP inner door 260x370 for board size 2","NDG",68.97,0,68.97,8592765072498,1,18592765072495,null,28592765072492,"8538909999",1.2969999999999999]
[107250,"TID FHS S3","GRP inner door 370X445 for board size 3","NDG",78.62,0,78.62,8592765072504,1,18592765072501,null,28592765072508,"8538909999",1.8779999999999999]
[107251,"TID FHS S4","GRP inner door 370x595 for board size 4","NDG",99.08,0,99.08,8592765072511,1,18592765072518,null,28592765072515,"8538909999",2.415]
[107252,"TID FHS S5","GRP inner door 475x595 for board size 5","NDG",108.58,0,108.58,8592765072528,1,18592765072525,null,28592765072522,"8538909999",3.06]
[107253,"TID FHS S6","GRP inner door 550x745 for board size 6","NDG",143.83000000000001,0,143.83000000000001,8592765072535,1,18592765072532,null,28592765072539,"8538909999",4.2480000000000002]
[107254,"TID FHS S7","GRP inner door 765x995 for board size 7","NDG",211.94,0,211.94,8592765072542,1,18592765072549,null,28592765072546,"8538909999",7.5650000000000004]
[107255,"PDP FHS A5","Plastic holder for documents","NDG",7.36,0,7.36,8592765072559,1,18592765072556,null,28592765072553,"3926909790",0.154]
[107256,"SK FHS S2","Retrofit kit for frame size 2","NDG",58.37,0,58.37,8592765072566,1,18592765072563,null,28592765072560,"7318190090",0.19]
[107257,"SK FHS S3-4","Retrofit kit for frame size 3-4","NDG",61.33,{"$f":"NDG","v":0},{"$f":"E5288*(1-F5288)","v":61.33},8592765072573,1,18592765072570,null,28592765072577,"7318190090",0.28299999999999997]
[107258,"SK FHS S5","Retrofit kit for frame size 5","NDG",70.02,{"$f":"NDG","v":0},{"$f":"E5289*(1-F5289)","v":70.02},8592765072580,1,18592765072587,null,28592765072584,"7318190090",0.38]
[107259,"SK FHS S6","Retrofit kit for frame size 6","NDG",76.33,{"$f":"NDG","v":0},{"$f":"E5290*(1-F5290)","v":76.33},8592765072597,1,18592765072594,null,28592765072591,"7318190090",0.47599999999999998]
[107260,"SK FHS S7","Retrofit kit for frame size 7","NDG",81.37,{"$f":"NDG","v":0},{"$f":"E5291*(1-F5291)","v":81.37},8592765072603,1,18592765072600,null,28592765072607,"7318190090",0.59599999999999997]
[107261,"CTS FHS","Cable trunking support","NDG",57.71,{"$f":"NDG","v":0},{"$f":"E5292*(1-F5292)","v":57.71},8592765072610,1,18592765072617,null,28592765072614,"7326909890",5.8000000000000003E-2]
[]
["Metal enclosure IP66"]
[110562,"MHS 30 20 15","Metal enclosure with mounting plate IP66, 300x200x150","NDH",58.05,{"$f":"NDH","v":0},{"$f":"E5295*(1-F5295)","v":58.05},8592765105622,1,8592765105622,1,null,"8538909999",4.2]
[110563,"MHS 30 30 15","Metal enclosure with mounting plate IP66, 300x300x150","NDH",62.77,{"$f":"NDH","v":0},62.77,8592765105639,1,8592765105639,1,null,"8538909999",5.6]
[110564,"MHS 30 30 20","Metal enclosure with mounting plate IP66, 300x300x200","NDH",71.31,0,71.31,8592765105646,1,8592765105646,1,null,"8538909999",6.3]
[110565,"MHS 40 30 15","Metal enclosure with mounting plate IP66, 400x300x150","NDH",75.06,0,75.06,8592765105653,1,8592765105653,1,null,"8538909999",7]
[110566,"MHS 40 30 20","Metal enclosure with mounting plate IP66, 400x300x200","NDH",79.38,0,79.38,8592765105660,1,8592765105660,1,null,"8538909999",8]
[110567,"MHS 40 40 20","Metal enclosure with mounting plate IP66, 400x400x200","NDH",86.1,0,86.1,8592765105677,1,8592765105677,1,null,"8538909999",9.8000000000000007]
[110568,"MHS 50 40 15","Metal enclosure with mounting plate IP66, 500x400x150","NDH",93.18,0,93.18,8592765105684,1,8592765105684,1,null,"8538909999",10.5]
[110569,"MHS 50 40 20","Metal enclosure with mounting plate IP66, 500x400x200","NDH",97.11,0,97.11,8592765105691,1,8592765105691,1,null,"8538909999",11.6]
[110570,"MHS 60 40 20","Metal enclosure with mounting plate IP66, 600x400x200","NDH",106.92,0,106.92,8592765105707,1,8592765105707,1,null,"8538909999",13.5]
[110571,"MHS 60 40 30","Metal enclosure with mounting plate IP66, 600x400x300","NDH",117.73,0,117.73,8592765105714,1,8592765105714,1,null,"8538909999",15.6]
[110572,"MHS 60 50 20","Metal enclosure with mounting plate IP66, 600x500x200","NDH",125.58,0,125.58,8592765105721,1,8592765105721,1,null,"8538909999",16.2]
[110573,"MHS 60 60 20","Metal enclosure with mounting plate IP66, 600x600x200","NDH",139.58000000000001,0,139.58000000000001,8592765105738,1,8592765105738,1,null,"8538909999",20.6]
[110574,"MHS 60 60 30","Metal enclosure with mounting plate IP66, 600x600x300","NDH",165.56,0,165.56,8592765105745,1,8592765105745,1,null,"8538909999",23.2]
[110575,"MHS 60 80 30","Metal enclosure with mounting plate IP55, 600x800x300 (double door)","NDH",220.75,0,220.75,8592765105752,1,8592765105752,1,null,"8538909999",28.3]
[110576,"MHS 70 50 20","Metal enclosure with mounting plate IP66, 700x500x200","NDH",135.44999999999999,0,135.44999999999999,8592765105769,1,8592765105769,1,null,"8538909999",18.5]
[110577,"MHS 70 50 30","Metal enclosure with mounting plate IP66, 700x500x300","NDH",150.29,0,150.29,8592765105776,1,8592765105776,1,null,"8538909999",21.2]
[110578,"MHS 80 60 20","Metal enclosure with mounting plate IP66, 800x600x200","NDH",172.4,0,172.4,8592765105783,1,8592765105783,1,null,"8538909999",26.2]
[110579,"MHS 80 60 30","Metal enclosure with mounting plate IP66, 800x600x300","NDH",201.88,0,201.88,8592765105790,1,8592765105790,1,null,"8538909999",29]
[110580,"MHS 100 60 30","Metal enclosure with mounting plate IP66, 1000x600x300","NDH",228.02,0,228.02,8592765105806,1,8592765105806,1,null,"8538909999",35.200000000000003]
[110581,"MHS 100 80 30","Metal enclosure with mounting plate IP66, 1000x800x300","NDH",286.01,0,286.01,8592765105813,1,8592765105813,1,null,"8538909999",45.3]
[110582,"MHS 100 100 30","Metal enclosure with mounting plate IP55, 1000x1000x300 (double door)","NDH",351.04,0,351.04,8592765105820,1,8592765105820,1,null,"8538909999",60]
[110583,"MHS 120 60 30","Metal enclosure with mounting plate IP66, 1200x600x300","NDH",266.04000000000002,0,266.04000000000002,8592765105837,1,8592765105837,1,null,"8538909999",39.700000000000003]
[110584,"MHS 120 80 30","Metal enclosure with mounting plate IP66, 1200x800x300","NDH",339.84,0,339.84,8592765105844,1,8592765105844,1,null,"8538909999",59]
[110585,"MHS 120 100 30","Metal enclosure with mounting plate IP55, 1200x1000x300 (double door)","NDH",408.54,0,408.54,8592765105851,1,8592765105851,1,null,"8538909999",70]
["Acc."]
[110586,"MP MHS 30 20","Mounting plate for MHS enclosures 300x200mm","NDH",11.31,0,{"$f":"E5320*(1-F5320)","v":11.31},8592765105868,10,18592765105865,null,null,"8538909999",0.6]
[110587,"MP MHS 30 30","Mounting plate for MHS enclosures 300x300mm","NDH",12.33,0,12.33,8592765105875,10,18592765105872,null,null,"8538909999",1]
[110588,"MP MHS 40 30","Mounting plate for MHS enclosures 400x300mm","NDH",13.84,0,13.84,8592765105882,10,18592765105889,null,null,"8538909999",1.4]
[110589,"MP MHS 40 40","Mounting plate for MHS enclosures 400x400mm","NDH",16.98,0,16.98,8592765105899,10,18592765105896,null,null,"8538909999",1.9]
[110590,"MP MHS 50 40","Mounting plate for MHS enclosures 500x400mm","NDH",18.04,0,18.04,8592765105905,10,18592765105902,null,null,"8538909999",2.5]
[110591,"MP MHS 60 40","Mounting plate for MHS enclosures 600x400mm","NDH",20.079999999999998,0,20.079999999999998,8592765105912,2,18592765105919,null,null,"8538909999",3.1]
[110592,"MP MHS 60 50","Mounting plate for MHS enclosures 600x500mm","NDH",24.65,0,24.65,8592765105929,2,18592765105926,null,null,"8538909999",4]
[110593,"MP MHS 70 50","Mounting plate for MHS enclosures 700x500mm","NDH",28.29,0,28.29,8592765105936,2,18592765105933,null,null,"8538909999",4.8]
[110594,"MP MHS 60 60","Mounting plate for MHS enclosures 600x600mm","NDH",32.409999999999997,0,32.409999999999997,8592765105943,2,18592765105940,null,null,"8538909999",5]
[110595,"MP MHS 80 60","Mounting plate for MHS enclosures 800x600mm","NDH",37.51,0,37.51,8592765105950,2,18592765105957,null,null,"8538909999",6.9]
[110596,"MP MHS 100 60","Mounting plate for MHS enclosures 1000x600mm","NDH",40.729999999999997,0,40.729999999999997,8592765105967,2,18592765105964,null,null,"8538909999",8.6999999999999993]
[110597,"MP MHS 120 60","Mounting plate for MHS enclosures 1200x600mm","NDH",46.9,0,46.9,8592765105974,2,18592765105971,null,null,"8538909999",10.199999999999999]
[110598,"MP MHS 60 80","Mounting plate for MHS enclosures 600x800mm","NDH",35.020000000000003,0,35.020000000000003,8592765105981,2,18592765105988,null,null,"8538909999",6.8]
[110599,"MP MHS 100 80","Mounting plate for MHS enclosures 1000x800mm","NDH",50.41,0,50.41,8592765105998,2,18592765105995,null,null,"8538909999",11.7]
[110600,"MP MHS 120 80","Mounting plate for MHS enclosures 1200x800mm","NDH",54.98,0,54.98,8592765106001,2,18592765106008,null,null,"8538909999",14.2]
[110601,"MP MHS 100 100","Mounting plate for MHS enclosures 1000x1000mm","NDH",58.61,0,58.61,8592765106018,2,18592765106015,null,null,"8538909999",14.8]
[110602,"MP MHS 120 100","Mounting plate for MHS enclosures 1200x1000mm","NDH",76.650000000000006,0,76.650000000000006,8592765106025,2,18592765106022,null,null,"8538909999",17.600000000000001]
[110603,"MF MHS 30","Cover plates mounting frame for MHS enclosures H=300mm, set (content 2 pcs)","NDH",17.670000000000002,0,17.670000000000002,8592765106032,1,8592765106032,null,null,"8538909999",0.7]
[110604,"MF MHS 40","Cover plates mounting frame for MHS enclosures H=400mm, set (content 2 pcs)","NDH",21.43,0,21.43,8592765106049,1,8592765106049,null,null,"8538909999",1]
[110605,"MF MHS 50","Cover plates mounting frame for MHS enclosures H=500mm, set (content 2 pcs)","NDH",24.69,0,24.69,8592765106056,1,8592765106056,null,null,"8538909999",1.3]
[110606,"MF MHS 60","Cover plates mounting frame for MHS enclosures H=600mm, set (content 2 pcs)","NDH",29.02,0,29.02,8592765106063,1,8592765106063,null,null,"8538909999",1.5]
[110607,"MF MHS 70","Cover plates mounting frame for MHS enclosures H=700mm, set (content 2 pcs)","NDH",31.59,0,31.59,8592765106070,1,8592765106070,null,null,"8538909999",1.8]
[110608,"MF MHS 80","Cover plates mounting frame for MHS enclosures H=800mm, set (content 2 pcs)","NDH",34.82,0,34.82,8592765106087,1,8592765106087,null,null,"8538909999",2.1]
[110609,"MF MHS 100","Cover plates mounting frame for MHS enclosures H=1000mm, set (content 2 pcs)","NDH",42.49,0,42.49,8592765106094,1,8592765106094,null,null,"8538909999",2.6]
[110610,"MF MHS 120","Cover plates mounting frame for MHS enclosures H=1200mm, set (content 2 pcs)","NDH",58.12,0,58.12,8592765106100,1,8592765106100,null,null,"8538909999",3]
[110611,"CP MHS 10 30","Screw type cover plates, H=100mm, for MHS enclosures W=300mm","NDH",9.18,0,9.18,8592765106117,1,8592765106117,null,null,"8538909999",0.3]
[110612,"CP MHS 12 30","Screw type cover plates, H=120mm, for MHS enclosures W=300mm","NDH",9.6300000000000008,0,9.6300000000000008,8592765106124,1,8592765106124,null,null,"8538909999",0.3]
[110613,"CP MHS 16 30","Screw type cover plates, H=160mm, for MHS enclosures W=300mm","NDH",10.78,0,10.78,8592765106131,1,8592765106131,null,null,"8538909999",0.4]
[110614,"CP MHS 10 40","Screw type cover plates, H=100mm, for MHS enclosures W=400mm","NDH",9.6300000000000008,0,9.6300000000000008,8592765106148,1,8592765106148,null,null,"8538909999",0.3]
[110615,"CP MHS 12 40","Screw type cover plates, H=120mm, for MHS enclosures W=400mm","NDH",10.78,0,10.78,8592765106155,1,8592765106155,null,null,"8538909999",0.4]
[110616,"CP MHS 16 40","Screw type cover plates, H=160mm, for MHS enclosures W=400mm","NDH",11.8,0,11.8,8592765106162,1,8592765106162,null,null,"8538909999",0.5]
[110617,"CP MHS 10 50","Screw type cover plates, H=100mm, for MHS enclosures W=500mm","NDH",10.78,0,10.78,8592765106179,1,8592765106179,null,null,"8538909999",0.4]
[110618,"CP MHS 12 50","Screw type cover plates, H=120mm, for MHS enclosures W=500mm","NDH",11.8,0,11.8,8592765106186,1,8592765106186,null,null,"8538909999",0.4]
[110619,"CP MHS 16 50","Screw type cover plates, H=160mm, for MHS enclosures W=500mm","NDH",13.43,0,13.43,8592765106193,1,8592765106193,null,null,"8538909999",0.7]
[110620,"CP MHS 10 60","Screw type cover plates, H=100mm, for MHS enclosures W=600mm","NDH",11.8,0,11.8,8592765106209,1,8592765106209,null,null,"8538909999",0.5]
[110621,"CP MHS 12 60","Screw type cover plates, H=120mm, for MHS enclosures W=600mm","NDH",12.94,0,12.94,8592765106216,1,8592765106216,null,null,"8538909999",0.6]
[110622,"CP MHS 16 60","Screw type cover plates, H=160mm, for MHS enclosures W=600mm","NDH",14.41,0,14.41,8592765106223,1,8592765106223,null,null,"8538909999",0.8]
[110623,"CP MHS 12 30 12M","Screw type cover plates, 12 modules, H=120mm, for MHS enclosures W=300mm","NDH",11.31,0,11.31,8592765106230,1,8592765106230,null,null,"8538909999",0.2]
[110624,"CP MHS 16 30 12M","Screw type cover plates, 12 modules, H=160mm, for MHS enclosures W=300mm","NDH",11.8,0,11.8,8592765106247,1,8592765106247,null,null,"8538909999",0.3]
[110625,"CP MHS 12 40 18M","Screw type cover plates, 18 modules, H=120mm, for MHS enclosures W=400mm","NDH",12.94,0,12.94,8592765106254,1,8592765106254,null,null,"8538909999",0.3]
[110626,"CP MHS 16 40 18M","Screw type cover plates, 18 modules, H=160mm, for MHS enclosures W=400mm","NDH",13.92,{"$f":"NDH","v":0},13.92,8592765106261,1,8592765106261,null,null,"8538909999",0.4]
[110627,"CP MHS 12 50 24M","Screw type cover plates, 24 modules, H=120mm, for MHS enclosures W=500mm","NDH",14.41,0,14.41,8592765106278,1,8592765106278,null,null,"8538909999",0.4]
[110628,"CP MHS 16 50 24M","Screw type cover plates, 24 modules, H=160mm, for MHS enclosures W=500mm","NDH",15.59,0,15.59,8592765106285,1,8592765106285,null,null,"8538909999",0.5]
[110629,"CP MHS 12 60 29M","Screw type cover plates, 29 modules, H=120mm, for MHS enclosures W=600mm","NDH",15.06,0,15.06,8592765106292,1,8592765106292,null,null,"8538909999",0.4]
[110630,"CP MHS 16 60 29M","Screw type cover plates, 29 modules, H=160mm, for MHS enclosures W=600mm","NDH",16.079999999999998,0,16.079999999999998,8592765106308,1,8592765106308,null,null,"8538909999",0.6]
[110631,"RC MHS 00 30 15","Rain canopy for MHS enclosures 300x150mm","NDH",29.02,0,29.02,8592765106315,1,8592765106315,null,null,"8538909999",1.1000000000000001]
[110632,"RC MHS 00 30 20","Rain canopy for MHS enclosures 300x200mm","NDH",35.22,0,35.22,8592765106322,1,8592765106322,null,null,"8538909999",1.6]
[110633,"RC MHS 00 40 15","Rain canopy for MHS enclosures 400x150mm","NDH",35.22,0,35.22,8592765106339,1,8592765106339,null,null,"8538909999",1.6]
[110634,"RC MHS 00 40 20","Rain canopy for MHS enclosures 400x200mm","NDH",37.06,0,37.06,8592765106346,1,8592765106346,null,null,"8538909999",2]
[110635,"RC MHS 00 40 30","Rain canopy for MHS enclosures 400x300mm","NDH",45.02,0,45.02,8592765106353,1,8592765106353,null,null,"8538909999",2.6]
[110636,"RC MHS 00 50 20","Rain canopy for MHS enclosures 500x200mm","NDH",48.24,0,48.24,8592765106360,1,8592765106360,null,null,"8538909999",2.4]
[110637,"RC MHS 00 50 30","Rain canopy for MHS enclosures 500x300mm","NDH",53.76,0,53.76,8592765106377,1,8592765106377,null,null,"8538909999",3.1]
[110638,"RC MHS 00 60 20","Rain canopy for MHS enclosures 600x200mm","NDH",48.78,0,48.78,8592765106384,1,8592765106384,null,null,"8538909999",2.7]
[110639,"RC MHS 00 60 30","Rain canopy for MHS enclosures 600x300mm","NDH",63.55,0,63.55,8592765106391,1,8592765106391,null,null,"8538909999",3.5]
[110640,"RC MHS 00 80 20","Rain canopy for MHS enclosures 800x200mm","NDH",65.92,0,65.92,8592765106407,1,8592765106407,null,null,"8538909999",3.6]
[110641,"RC MHS 00 80 30","Rain canopy for MHS enclosures 800x300mm","NDH",93.76,0,93.76,8592765106414,1,8592765106414,null,null,"8538909999",4.7]
[110642,"RC MHS 00 100 30","Rain canopy for MHS enclosures 1000x300mm","NDH",114.41,0,114.41,8592765106421,1,8592765106421,null,null,"8538909999",5.8]
[110643,"SD MHS 30 20","Solid door for MHS enclosures 300x200mm","NDH",25.55,0,25.55,8592765106438,1,8592765106438,null,null,"8538909999",0.7]
[110644,"SD MHS 30 30","Solid door for MHS enclosures 300x300mm","NDH",30.69,0,30.69,8592765106445,1,8592765106445,null,null,"8538909999",1.1000000000000001]
[110645,"SD MHS 40 30","Solid door for MHS enclosures 400x300mm","NDH",34.82,0,34.82,8592765106452,1,8592765106452,null,null,"8538909999",1.5]
[110646,"SD MHS 40 40","Solid door for MHS enclosures 400x400mm","NDH",42.69,0,42.69,8592765106469,1,8592765106469,null,null,"8538909999",1.9]
[110647,"SD MHS 50 40","Solid door for MHS enclosures 500x400mm","NDH",48.94,0,48.94,8592765106476,1,8592765106476,null,null,"8538909999",2.2999999999999998]
[110648,"SD MHS 60 40","Solid door for MHS enclosures 600x400mm","NDH",57.22,0,57.22,8592765106483,1,8592765106483,null,null,"8538909999",2.7]
[110649,"SD MHS 60 50","Solid door for MHS enclosures 600x500mm","NDH",63.02,0,63.02,8592765106490,1,8592765106490,null,null,"8538909999",3.5]
[110650,"SD MHS 70 50","Solid door for MHS enclosures 700x500mm","NDH",77.099999999999994,0,{"$f":"E5384*(1-F5384)","v":77.099999999999994},8592765106506,1,8592765106506,null,null,"8538909999",3.9]
[110651,"SD MHS 60 60","Solid door for MHS enclosures 600x600mm","NDH",79.22,0,79.22,8592765106513,1,8592765106513,null,null,"8538909999",3.8]
[110652,"SD MHS 80 60","Solid door for MHS enclosures 800x600mm","NDH",102.94,0,102.94,8592765106520,1,8592765106520,null,null,"8538909999",5.2]
[110653,"SD MHS 100 60","Solid door for MHS enclosures 1000x600mm","NDH",118.73,0,118.73,8592765106537,1,8592765106537,null,null,"8538909999",6.4]
[110654,"SD MHS 120 60","Solid door for MHS enclosures 1200x600mm","NDH",131.06,0,131.06,8592765106544,1,8592765106544,null,null,"8538909999",7.5]
[110655,"SD MHS 60 80","Solid door for MHS enclosures 600x800mm","NDH",98.94,0,98.94,8592765106551,1,8592765106551,null,null,"8538909999",6.5]
[110656,"SD MHS 60 80 D","Solid double door for MHS enclosures 600x800mm","NDH",118.69,0,118.69,8592765106568,1,8592765106568,null,null,"8538909999",0]
[110657,"SD MHS 100 80","Solid door for MHS enclosures 1000x800mm","NDH",144.37,0,144.37,8592765106575,1,8592765106575,null,null,"8538909999",12.5]
[110658,"SD MHS 120 80","Solid door for MHS enclosures 1200x800mm","NDH",166.86,0,166.86,8592765106582,1,8592765106582,null,null,"8538909999",7.9]
[110659,"SD MHS 100 100 D","Solid double door for MHS enclosures 1000x1000mm","NDH",170.9,0,170.9,8592765106599,1,8592765106599,null,null,"8538909999",16.899999999999999]
[110660,"SD MHS 120 100 D","Solid double door for MHS enclosures 1200x1000mm","NDH",200.49,0,200.49,8592765106605,1,8592765106605,null,null,"8538909999",17]
[110661,"GD MHS 30 30","Glazed door for MHS enclosures 300x300mm","NDH",59.8,0,59.8,8592765106612,1,8592765106612,null,null,"8538909999",1.1000000000000001]
[110662,"GD MHS 40 30","Glazed door for MHS enclosures 400x300mm","NDH",67.8,0,67.8,8592765106629,1,8592765106629,null,null,"8538909999",1.6]
[110663,"GD MHS 40 40","Glazed door for MHS enclosures 400x400mm","NDH",78.41,0,78.41,8592765106636,1,8592765106636,null,null,"8538909999",2.1]
[110664,"GD MHS 50 40","Glazed door for MHS enclosures 500x400mm","NDH",83.22,0,83.22,8592765106643,1,8592765106643,null,null,"8538909999",2.5]
[110665,"GD MHS 60 40","Glazed door for MHS enclosures 600x400mm","NDH",89.59,0,89.59,8592765106650,1,8592765106650,null,null,"8538909999",3]
[110666,"GD MHS 60 50","Glazed door for MHS enclosures 600x500mm","NDH",101.27,0,101.27,8592765106667,1,8592765106667,null,null,"8538909999",3.8]
[110667,"GD MHS 70 50","Glazed door for MHS enclosures 700x500mm","NDH",111.96,0,111.96,8592765106674,1,8592765106674,null,null,"8538909999",4.3]
[110668,"GD MHS 60 60","Glazed door for MHS enclosures 600x600mm","NDH",121.14,0,121.14,8592765106681,1,8592765106681,null,null,"8538909999",4.9000000000000004]
[110669,"GD MHS 80 60","Glazed door for MHS enclosures 800x600mm","NDH",138.08000000000001,0,138.08000000000001,8592765106698,1,8592765106698,null,null,"8538909999",9.5]
[110670,"GD MHS 100 60","Glazed door for MHS enclosures 1000x600mm","NDH",157.80000000000001,0,157.80000000000001,8592765106704,1,8592765106704,null,null,"8538909999",7.8]
[110671,"GD MHS 120 60","Glazed door for MHS enclosures 1200x600mm","NDH",196.29,0,196.29,8592765106711,1,8592765106711,null,null,"8538909999",9.1999999999999993]
[110672,"GD MHS 60 80","Glazed door for MHS enclosures 600x800mm","NDH",160.04,0,160.04,8592765106728,1,8592765106728,null,null,"8538909999",6.3]
[110673,"GD MHS 100 80","Glazed door for MHS enclosures 1000x800mm","NDH",228.86,0,228.86,8592765106735,1,8592765106735,null,null,"8538909999",10]
[110674,"GD MHS 120 80","Glazed door for MHS enclosures 1200x800mm","NDH",260.86,0,260.86,8592765106742,1,8592765106742,null,null,"8538909999",11.9]
[110675,"WB MHS 4","Spare wall brackets, 4 pieces, 1 set","NDH",13.71,0,13.71,8592765106759,1,8592765106759,null,null,"8538909999",0.16]
[110676,"WB MHS 6","Spare wall brackets, 6 pieces, 1 set","NDH",18.29,0,18.29,8592765106766,1,8592765106766,null,null,"8538909999",0.25]
[110677,"PM MHS 00 30","Pole mounting set, W=300mm, 2 pieces, 1 set","NDH",119.06,0,119.06,8592765106773,1,8592765106773,null,null,"8538909999",0.9]
[110678,"PM MHS 00 40","Pole mounting set, W=400mm, 2 pieces, 1 set","NDH",125.35,0,125.35,8592765106780,1,8592765106780,null,null,"8538909999",1.3]
[110679,"PM MHS 00 50","Pole mounting set, W=500mm, 2 pieces, 1 set","NDH",131.63,0,131.63,8592765106797,1,8592765106797,null,null,"8538909999",1.6]
[110680,"PM MHS 00 60","Pole mounting set, W=600mm, 2 pieces, 1 set","NDH",137.88,0,137.88,8592765106803,1,8592765106803,null,null,"8538909999",1.9]
[110681,"PM MHS 00 60-3","Pole mounting set, W=600mm, 3 pieces, 1 set","NDH",206.82,0,206.82,8592765106810,1,8592765106810,null,null,"8538909999",2.4]
[110682,"PM MHS 00 80","Pole mounting set, W=800mm, 3 pieces, 1 set","NDH",229.84,0,229.84,8592765106827,1,8592765106827,null,null,"8538909999",2.6]
[110683,"EC MHS","Earthing cable, 190mm, M8-M8","NDH",2.78,0,2.78,8592765106834,100,18592765106831,null,null,"8538909999"]
[110704,"LK MHS K","Lock with key","NDH",16,0,{"$f":"E5418*(1-F5418)","v":16},8592765107046,1,8592765107046,null,null,"8538100000",0.1]
[110811,"CB MHS 5.5","Cable entry brush, height 55 mm, 25 m roll","NDH",1377.55,0,1377.55,8592765108111,1,8592765108111,null,null,"8538909999",5]
[110812,"CB MHS 3.5","Cable entry brush, height 35 mm, 25 m roll","NDH",826.53,0,826.53,8592765108128,1,8592765108128,null,null,"8538909999",5]
[]
["DC SPDs Ex9UEP, Class II, plug-in module design with optical status indication, suitable for PV applications"]
[108016,"Ex9UEP 20 1P 600","DC SPD Ex9UEP, Class II, In=20kA, 600 V DC, 1MU width","NAO",117.37,{"$f":"NAO","v":0},{"$f":"E5423*(1-F5423)","v":117.37},8592765080172,1,8592765080172,96,28592765080176,"8536309090",0.12]
[108017,"Ex9UEP 20R 1P 600","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 600 V DC, 1MU width","NAO",124.08,{"$f":"NAO","v":0},124.08,8592765080189,1,8592765080189,96,28592765080183,"8536309090",0.12]
[108018,"Ex9UEP 20 2P 600","DC SPD Ex9UEP, Class II, In=20kA, 600 V DC, 2MU width, for ungrounded PV systems","NAO",134.13999999999999,0,134.13999999999999,8592765080196,1,8592765080196,81,28592765080190,"8536309090",0.25]
[108019,"Ex9UEP 20R 2P 600","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 600 V DC, 2MU width, for ungrounded PV systems","NAO",140.83000000000001,0,140.83000000000001,8592765080202,1,8592765080202,81,28592765080206,"8536309090",0.25]
[110171,"Ex9UEP 20 1P 750","DC SPD Ex9UEP, Class II, In=20kA, 750 V DC, 1MU width","NAO",122.09,0,122.09,8592765101716,1,8592765101716,96,28592765101710,"8536309090",0.12]
[110172,"Ex9UEP 20R 1P 750","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 750 V DC, 1MU width","NAO",128.6,0,128.6,8592765101723,1,8592765101723,96,28592765101727,"8536309090",0.12]
[110173,"Ex9UEP 20 2P 750","DC SPD Ex9UEP, Class II, In=20kA, 750 V DC, 2MU width, for ungrounded PV systems","NAO",143.25,0,143.25,8592765101730,1,8592765101730,81,28592765101734,"8536309090",0.25]
[110174,"Ex9UEP 20R 2P 750","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 750 V DC, 2MU width, for ungrounded PV systems","NAO",149.76,0,149.76,8592765101747,1,8592765101747,81,28592765101741,"8536309090",0.25]
[108020,"Ex9UEP 20 2P 1200","DC SPD Ex9UEP, Class II, In=20kA, 1200 V DC, 2MU width, for grounded PV systems","NAO",134.13999999999999,0,134.13999999999999,8592765080219,1,8592765080219,81,28592765080213,"8536309090",0.25]
[108021,"Ex9UEP 20R 2P 1200","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 1200 V DC, 2MU width, for grounded PV systems","NAO",140.83000000000001,0,140.83000000000001,8592765080226,1,8592765080226,81,28592765080220,"8536309090",0.25]
[108022,"Ex9UEP 20 3P 1200","DC SPD Ex9UEP, Class II, In=20kA, 1200 V DC, 3MU width, for ungrounded PV systems","NAO",70.569999999999993,0,70.569999999999993,8592765080233,1,8592765080233,54,28592765080237,"8536309090",0.38]
[108023,"Ex9UEP 20R 3P 1200","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 1200 V DC, 3MU width, for ungrounded PV systems","NAO",167.67,0,167.67,8592765080240,1,8592765080240,54,28592765080244,"8536309090",0.38]
[110179,"Ex9UEP 20 2P 1500","DC SPD Ex9UEP, Class II, In=20kA, 1500 V DC, 2MU width, for grounded PV systems","NAO",141.55000000000001,0,141.55000000000001,8592765101792,1,8592765101792,81,28592765101796,"8536309090",0.25]
[110180,"Ex9UEP 20R 2P 1500","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 1500 V DC, 2MU width, for grounded PV systems","NAO",148.62,0,148.62,8592765101808,1,8592765101808,81,28592765101802,"8536309090",0.25]
[110181,"Ex9UEP 20 3P 1500","DC SPD Ex9UEP, Class II, In=20kA, 1500 V DC, 3MU width, for ungrounded PV systems","NAO",169.86,0,169.86,8592765101815,1,8592765101815,54,28592765101819,"8536309090",0.38]
[110182,"Ex9UEP 20R 3P 1500","DC SPD Ex9UEP with remote contact, Class II, In=20kA, 1500 V DC, 3MU width, for ungrounded PV systems","NAO",176.95,0,176.95,8592765101822,1,8592765101822,54,28592765101826,"8536309090",0.38]
[108024,"Ex9UEP 20 1P 600 M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 1P 600 device, Class II, In=20kA, 600 V DC, 1MU width","NAO",50.32,0,50.32,8592765080257,1,8592765080257,96,28592765080251,"8536309090",0.08]
[108025,"Ex9UEP 20 2P 600 M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 2P 600 device, Class II, In=20kA, 600 V DC, 1MU width","NAO",50.32,0,50.32,8592765080264,1,8592765080264,96,28592765080268,"8536309090",0.08]
[110183,"Ex9UEP 20 1P 750M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 1P 750 device, Class II, In=20kA, 750 V DC, 1MU width","NAO",54.41,0,54.41,8592765101839,1,8592765101839,96,28592765101833,"8536309090",0.08]
[110184,"Ex9UEP 20 2P 750M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 2P 750 device, Class II, In=20kA, 750 V DC, 1MU width","NAO",54.41,0,54.41,8592765101846,1,8592765101846,96,28592765101840,"8536309090",0.08]
[108026,"Ex9UEP 20 2P 1200 M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 2P 1200 device, Class II, In=20kA, 600 V DC, 1MU width","NAO",50.32,0,50.32,8592765080271,1,8592765080271,96,28592765080275,"8536309090",0.08]
[108027,"Ex9UEP 20 3P 1200 M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 3P 1200 device, Class II, In=20kA, 600 V DC, 1MU width","NAO",50.32,0,50.32,8592765080288,1,8592765080288,96,28592765080282,"8536309090",0.08]
[110187,"Ex9UEP 20 2P 1500M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 2P 1500 device, Class II, In=20kA, 750 V DC, 1MU width","NAO",54.41,0,54.41,8592765101877,1,8592765101877,96,28592765101871,"8536309090",0.08]
[110188,"Ex9UEP 20 3P 1500M","DC SPD Ex9UEP plug-in module only for Ex9UEP 20 3P 1200 device, Class II, In=20kA, 750 V DC, 1MU width","NAO",54.41,0,54.41,8592765101884,1,8592765101884,96,28592765101888,"8536309090",0.08]
[]
["DC Fuse disconnectors Ex9FP for PV application"]
[101766,"Ex9FP 1P 30A","Fuse disconnectors, 30 A, 1000 V DC, 1-pole, DC-20B, with signalization","NEA",3.66,{"$f":"NEA","v":0},{"$f":"E5449*(1-F5449)","v":3.66},8592765017673,12,18592765017670,144,28592765017677,"8536201090",7.0000000000000007E-2]
[101767,"Ex9FP 2P 30A","Fuse disconnectors, 30 A, 1000 V DC, 2-pole, DC-20B, with signalization","NEA",11.39,{"$f":"NEA","v":0},{"$f":"E5450*(1-F5450)","v":11.39},8592765017680,6,18592765017687,72,28592765017684,"8536201090",0.14000000000000001]
[]
["Cylindrical Fuse Holder Ex9F",null,null,null,null,null,null,"","","","","",null,""]
[104474,"Ex9F 1P 32A","Fuse holder; for fuse 10x38mm 1P 32A ","NEB",4.24,{"$f":"NEB","v":0},{"$f":"E5453*(1-F5453)","v":4.24},8592765044754,12,18592765044751,144,28592765044758,"8536201090",7.0000000000000007E-2]
[104475,"Ex9F 1PN 32A ","Fuse holder; for fuse 10x38mm 1PN 32A ","NEB",8.99,{"$f":"NEB","v":0},8.99,8592765044761,6,18592765044768,72,28592765044765,"8536201090",0.14000000000000001]
[104476,"Ex9F 2P 32A ","Fuse holder; for fuse 10x38mm 2P 32A ","NEB",7.99,0,7.99,8592765044778,6,18592765044775,72,28592765044772,"8536201090",0.14000000000000001]
[104477,"Ex9F 3P 32A ","Fuse holder; for fuse 10x38mm 3P 32A ","NEB",12.05,0,12.05,8592765044785,4,18592765044782,48,28592765044789,"8536201090",0.21]
[104478,"Ex9F 3PN 32A ","Fuse holder; for fuse 10x38mm 3PN 32A ","NEB",17.09,0,17.09,8592765044792,3,18592765044799,36,28592765044796,"8536201090",0.28000000000000003]
[109054,"Ex9F 1P 32A WI","Fuse holder without indicator; for fuse 10x38mm 1P 32A ","NEB",3.4,{"$f":"NEB","v":0},{"$f":"E5458*(1-F5458)","v":3.4},8592765090546,12,18592765090543,144,28592765090540,"8536201090",7.0000000000000007E-2]
[109055,"Ex9F 1PN 32A WI","Fuse holder without indicator; for fuse 10x38mm 1PN 32A ","NEB",7.19,{"$f":"NEB","v":0},{"$f":"E5459*(1-F5459)","v":7.19},8592765090553,6,18592765090550,72,28592765090557,"8536201090",0.14000000000000001]
[109056,"Ex9F 2P 32A WI","Fuse holder without indicator; for fuse 10x38mm 2P 32A ","NEB",6.4,0,6.4,8592765090560,6,18592765090567,72,28592765090564,"8536201090",0.14000000000000001]
[109057,"Ex9F 3P 32A WI","Fuse holder without indicator; for fuse 10x38mm 3P 32A ","NEB",9.64,0,9.64,8592765090577,4,18592765090574,48,28592765090571,"8536201090",0.21]
[109058,"Ex9F 3PN 32A WI","Fuse holder without indicator; for fuse 10x38mm 3PN 32A ","NEB",13.67,0,13.67,8592765090584,3,18592765090581,36,28592765090588,"8536201090",0.28000000000000003]
[104479,"Ex9F-14 1P 50A ","Fuse holder without indicator; for fuse 14x51mm 1P 50A ","NEB",8.99,0,8.99,8592765044808,12,18592765044805,144,28592765044802,"8536201090",0.11]
[104480,"Ex9F-14 1PN 50A ","Fuse holder without indicator; for fuse 14x51mm 1PN 50A ","NEB",19.489999999999998,0,19.489999999999998,8592765044815,6,18592765044812,72,28592765044819,"8536201090",0.22]
[104481,"Ex9F-14 2P 50A ","Fuse holder without indicator; for fuse 14x51mm 2P 50A ","NEB",17.23,0,17.23,8592765044822,6,18592765044829,72,28592765044826,"8536201090",0.22]
[104482,"Ex9F-14 3P 50A ","Fuse holder without indicator; for fuse 14x51mm 3P 50A ","NEB",25.47,0,25.47,8592765044839,4,18592765044836,48,28592765044833,"8536201090",0.33]
[104483,"Ex9F-14 3PN 50A ","Fuse holder without indicator; for fuse 14x51mm 3PN 50A ","NEB",32.97,0,32.97,8592765044846,3,18592765044843,36,28592765044840,"8536201090",0.44]
[104484,"Ex9F-22 1P 100A ","Fuse holder without indicator; for fuse 22x58mm 1P 100A ","NEB",13.48,0,13.48,8592765044853,9,18592765044850,108,28592765044857,"8536209090",0.17]
[104485,"Ex9F-22 1PN 100A ","Fuse holder without indicator; for fuse 22x58mm 1PN 100A ","NEB",29.96,0,29.96,8592765044860,4,18592765044867,48,28592765044864,"8536209090",0.34]
[104486,"Ex9F-22 2P 100A ","Fuse holder without indicator; for fuse 22x58mm 2P 100A ","NEB",25.47,0,25.47,8592765044877,4,18592765044874,48,28592765044871,"8536209090",0.34]
[104487,"Ex9F-22 3P 100A ","Fuse holder without indicator; for fuse 22x58mm 3P 100A ","NEB",38.21,0,38.21,8592765044884,3,18592765044881,36,28592765044888,"8536209090",0.51]
[104488,"Ex9F-22 3PN 100A ","Fuse holder without indicator; for fuse 22x58mm 3PN 100A ","NEB",56.96,0,56.96,8592765044891,2,18592765044898,24,28592765044895,"8536209090",0.68]
[null,null,null,null,null,null,null,"","","","","",null,""]
["DC Modular Isolators Ex9IP for PV application"]
[101750,"Ex9IP 1P 16A","DC Isolator, width 1 module, 1-pole, 16A","NAN",20.99,{"$f":"NAN","v":0},{"$f":"E5475*(1-F5475)","v":20.99},8592765017512,12,18592765017519,144,28592765017516,"8536508090",0.12]
[101751,"Ex9IP 1P 32A","DC Isolator, width 1 module, 1-pole, 32A","NAN",24.97,0,24.97,8592765017529,12,18592765017526,144,28592765017523,"8536508090",0.12]
[101752,"Ex9IP 1P 50A","DC Isolator, width 1 module, 1-pole, 50A","NAN",27.5,0,27.5,8592765017536,12,18592765017533,144,28592765017530,"8536508090",0.12]
[101753,"Ex9IP 1P 63A","DC Isolator, width 1 module, 1-pole, 63A","NAN",30.41,0,30.41,8592765017543,12,18592765017540,144,28592765017547,"8536508090",0.12]
[101754,"Ex9IP 2P 16A","DC Isolator, width 2 modules, 2-pole, 16A","NAN",38.159999999999997,0,38.159999999999997,8592765017550,6,18592765017557,72,28592765017554,"8536508090",0.24]
[101755,"Ex9IP 2P 32A","DC Isolator, width 2 modules, 2-pole, 32A","NAN",45.4,0,45.4,8592765017567,6,18592765017564,72,28592765017561,"8536508090",0.24]
[101756,"Ex9IP 2P 50A","DC Isolator, width 2 modules, 2-pole, 50A","NAN",50.02,0,50.02,8592765017574,6,18592765017571,72,28592765017578,"8536508090",0.24]
[101757,"Ex9IP 2P 63A","DC Isolator, width 2 modules, 2-pole, 63A","NAN",55.27,0,55.27,8592765017581,6,18592765017588,72,28592765017585,"8536508090",0.24]
[101758,"Ex9IP 3P 16A","DC Isolator, width 3 modules, 3-pole, 16A","NAN",69.400000000000006,0,69.400000000000006,8592765017598,4,18592765017595,48,28592765017592,"8536508090",0.36]
[101759,"Ex9IP 3P 32A","DC Isolator, width 3 modules, 3-pole, 32A","NAN",82.54,0,82.54,8592765017604,4,18592765017601,48,28592765017608,"8536508090",0.36]
[101760,"Ex9IP 3P 50A","DC Isolator, width 3 modules, 3-pole, 50A","NAN",90.93,0,90.93,8592765017611,4,18592765017618,48,28592765017615,"8536508090",0.36]
[101761,"Ex9IP 3P 63A","DC Isolator, width 3 modules, 3-pole, 63A","NAN",100.51,0,100.51,8592765017628,4,18592765017625,48,28592765017622,"8536508090",0.36]
[101762,"Ex9IP 4P 16A","DC Isolator, width 4 modules, 4-pole, 16A","NAN",94.41,0,94.41,8592765017635,3,18592765017632,36,28592765017639,"8536508090",0.48]
[101763,"Ex9IP 4P 32A","DC Isolator, width 4 modules, 4-pole, 32A","NAN",112.32,0,112.32,8592765017642,3,18592765017649,36,28592765017646,"8536508090",0.48]
[101764,"Ex9IP 4P 50A","DC Isolator, width 4 modules, 4-pole, 50A","NAN",123.71,0,123.71,8592765017659,3,18592765017656,36,28592765017653,"8536508090",0.48]
[101765,"Ex9IP 4P 63A","DC Isolator, width 4 modules, 4-pole, 63A","NAN",136.74,0,136.74,8592765017666,3,18592765017663,36,28592765017660,"8536508090",0.48]
[]
["Cable EV chargers Ex9EVC"]
[110688,"Ex9EVC1 T1 16A ","Cable EV chargers, Type 1, 1 phase, 16 A","NGD",742.84,{"$f":"NGD","v":0},{"$f":"E5493*(1-F5493)","v":742.84},8592765106889,1,8592765106889,1,null,"8544429090",2.5]
[110689,"Ex9EVC1 T2 16A ","Cable EV chargers, Type 2, 1 phase, 16 A","NGD",742.84,0,742.84,8592765106896,1,8592765106896,1,null,"8544429090",2.5]
[110690,"Ex9EVC1 T1 32A ","Cable EV chargers, Type 1, 1 phase, 32 A","NGD",757.14,0,757.14,8592765106902,1,8592765106902,1,null,"8544429090",3.1]
[110691,"Ex9EVC1 T2 32A ","Cable EV chargers, Type 2, 1 phase, 32 A","NGD",757.14,0,757.14,8592765106919,1,8592765106919,1,null,"8544429090",3.1]
[110692,"Ex9EVC3 T2 16A ","Cable EV chargers, Type 2, 3 phase, 16 A","NGD",842.9,0,842.9,8592765106926,1,8592765106926,1,null,"8544429090",2.9]
[110693,"Ex9EVC3 T2 32A ","Cable EV chargers, Type 2, 3 phase, 32 A","NGD",871.5,0,871.5,8592765106933,1,8592765106933,1,null,"8544429090",3.9]
[]
["Wall - mounted EV chargers Ex9EV"]
[110256,"Ex9EV1 T1 10A","Wall - mounted EV chargers, Type 1, 1 phase, 10 A","NGD",757.14,{"$f":"NGD","v":0},{"$f":"E5501*(1-F5501)","v":757.14},8592765102560,1,8592765102560,1,null,"8544429090",5.95]
[110494,"Ex9EV1 T1 16A","Wall - mounted EV chargers, Type 1, 1 phase, 16 A","NGD",758.04,{"$f":"NGD","v":0},758.04,8592765104946,1,8592765104946,1,null,"8544429090",5.95]
[110495,"Ex9EV1 T1 20A","Wall - mounted EV chargers, Type 1, 1 phase, 20 A","NGD",758.94,0,758.94,8592765104953,1,8592765104953,1,null,"8544429090",5.95]
[110496,"Ex9EV1 T1 25A","Wall - mounted EV chargers, Type 1, 1 phase, 25 A","NGD",759.84,0,759.84,8592765104960,1,8592765104960,1,null,"8544429090",5.95]
[110497,"Ex9EV1 T1 32A","Wall - mounted EV chargers, Type 1, 1 phase, 32 A","NGD",760.74,0,760.74,8592765104977,1,8592765104977,1,null,"8544429090",5.95]
[110257,"Ex9EV1 T2 10A","Wall - mounted EV chargers, Type 2, 1 phase, 10 A","NGD",872.39,0,872.39,8592765102577,1,8592765102577,1,null,"8544429090",5.95]
[110498,"Ex9EV1 T2 16A","Wall - mounted EV chargers, Type 2, 1 phase, 16 A","NGD",873.29,0,873.29,8592765104984,1,8592765104984,1,null,"8544429090",5.95]
[110499,"Ex9EV1 T2 20A","Wall - mounted EV chargers, Type 2, 1 phase, 20 A","NGD",874.19,0,874.19,8592765104991,1,8592765104991,1,null,"8544429090",5.95]
[110500,"Ex9EV1 T2 25A","Wall - mounted EV chargers, Type 2, 1 phase, 25 A","NGD",875.09,0,875.09,8592765105004,1,8592765105004,1,null,"8544429090",5.95]
[110501,"Ex9EV1 T2 32A","Wall - mounted EV chargers, Type 2, 1 phase, 32 A","NGD",875.99,0,875.99,8592765105011,1,8592765105011,1,null,"8544429090",5.95]
[110258,"Ex9EV3 T2 10A","Wall - mounted EV chargers, Type 2, 3 phase, 10 A","NGD",1008,0,1008,8592765102584,1,8592765102584,1,null,"8544429090",7.2]
[110502,"Ex9EV3 T2 16A","Wall - mounted EV chargers, Type 2, 3 phase, 16 A","NGD",1008,0,1008,8592765105028,1,8592765105028,1,null,"8544429090",7.2]
[110503,"Ex9EV3 T2 20A","Wall - mounted EV chargers, Type 2, 3 phase, 20 A","NGD",1008,0,1008,8592765105035,1,8592765105035,1,null,"8544429090",7.2]
[110504,"Ex9EV3 T2 25A","Wall - mounted EV chargers, Type 2, 3 phase, 25 A","NGD",1008,0,1008,8592765105042,1,8592765105042,1,null,"8544429090",7.2]
[110505,"Ex9EV3 T2 32A","Wall - mounted EV chargers, Type 2, 3 phase, 32 A","NGD",1008,0,1008,8592765105059,1,8592765105059,1,null,"8544429090",7.2]
[]
["Plastic Consumer Units with metal door PMF-C combination of DIN rail and mounting plates"]
[110709,"PMF-C 36-1","Flush mounting enclosure for electrical (modular) & IT equipment - 3 rows","NDC",103.67,{"$f":"NDC","v":0},{"$f":"E5518*(1-F5518)","v":103.67},8592765107091,1,18592765107098,33,null,"8538909999",3]
[110710,"PMF-C 48-1","Flush mounting enclosure for electrical (modular) & IT equipment - 4 rows","NDC",131.22,0,131.22,8592765107107,1,18592765107104,24,null,"8538909999",3.5]
[110711,"PMF-C 48-2","Flush mounting enclosure for electrical (modular) & IT equipment - 4 rows","NDC",131.22,0,131.22,8592765107114,1,18592765107111,24,null,"8538909999",2.5]
[110712,"PMF-C 60-1","Flush mounting enclosure for electrical (modular) & IT equipment - 5 rows","NDC",155.71,0,155.71,8592765107121,1,18592765107128,18,null,"8538909999",4.5]
[110713,"PMF-C 60-2","Flush mounting enclosure for electrical (modular) & IT equipment - 5 rows","NDC",155.71,0,155.71,8592765107138,1,18592765107135,18,null,"8538909999",4.5]
[110714,"PMF-C 60-3","Flush mounting enclosure for electrical (modular) & IT equipment - 5 rows","NDC",155.71,0,155.71,8592765107145,1,18592765107142,18,null,"8538909999",4.5]
[110715,"PWS PMF-C","Partition for integrated socket","NDC",3.06,0,3.06,8592765107152,1,18592765107159,null,null,"8538909999",0.05]
[110716,"GS PMF-C","Modular socket 16A, 250V - Schuko socket","NDC",8.98,0,8.98,8592765107169,1,18592765107166,null,null,"8538909999",0.25]
[110717,"FS PMF-C","Modular socket 16A, 250V - French socket","NDC",9.39,0,9.39,8592765107176,1,18592765107173,null,null,"8538909999",0.25]
[110820,"DTH","HOLDER for double terminal (set, two pieces)","NDC",0.82,0,0.82,8592765108203,1,8592765108203,null,null,"3926909790"]

{"sheet":"Discount groups","index":2,"n_rows":65,"n_cols":3,"rows_kept":65,"cut":false,"hidden":false,"merged":[]}
["Discount group","Description","Sale"]
["NA","Installation Devices",0]
["NAA","Miniature Circuit Breakers 10 kA",{"$f":"NA","v":0}]
["NAB","Miniature Circuit Breakers 6 kA",0]
["NAC","Residual Current Devices 10 kA",0]
["NAD","Residual Current Devices 6 kA",0]
["NAE","Residual Current Breakers with Overload protection 10 kA",0]
["NAF","Residual Current Breakers with Overload protection 6 kA",0]
["NAG","Residual Current Devices Add-on Blocks",0]
["NAH","Isolators",0]
["NAI","Miniature Circuit Breakers Ex9PN-N, 6 kA",0]
["NAK","Miniature Circuit Breakers 4,5 kA",0]
["NAL","DC Miniature Circuit Breakers 10 kA, non-polarized",0]
["NAM","DC Miniature Circuit Breakers 6 kA, non-polarized",0]
["NAN","DC Isolators",0]
["NAO","DC SPDs class II for PV",0]
["NAP","DC Miniature Circuit Breakers 10 kA for PV, non-polarized",0]
["NAQ","DC Miniature Circuit Breakers 6 kA for PV, non-polarized",0]
["NAR","AC SPD class 1+2 and 2",0]
["NAS","Installation relays ans contactors",0]
["NAU","Switches, signal lamps and bells",0]
["NAV","DC Miniature Circuit Breakers 10 kA, polarized",0]
["NAW","Miniature Circuit Breakers up to 125 A",0]
["NAX","Timers, Light intensity switches, Staircase switches",0]
["NAZ","Energy meters",0]
["NAAA","1 module RCBO - electronic type",0]
["NAAB","Slim MCB",0]
[]
["NB","Industrial Devices",0]
["NBA","Contactors, Reversible contactors",{"$f":"NB","v":0}]
["NBB","Overload Thermal Relays",0]
["NBC","Contactors for capacity loads",0]
["NBD","Low-power consumption contactors",0]
["NBF","Panel mounted devices",0]
["NBG","Motor protective circuit breakers",0]
["NBH","Plug-in relays",0]
[]
["NC ","Moulded Case and Air Circuit Breakers",0]
["NCA","Moulded Case Circuit Breakers",{"$f":"NC","v":0}]
["NCB","DC Moulded Case Circuit Breakers",{"$f":"NC","v":0}]
["NCC","Air Circuit Breakers and Air Switch Disconnectors",{"$f":"NC","v":0}]
["NCD","AC Switch disconnectors",{"$f":"NC","v":0}]
["NCE","DC Switch disconnectors",{"$f":"NC","v":0}]
["NCF","Molded Case Circuit Breakers with electronic tripping unit ",{"$f":"NC","v":0}]
[]
["ND","Distribution boards and Connection Systems",0]
["NDA","Plastic Consumer Units",{"$f":"ND","v":0}]
["NDB","Busbars",0]
["NDC","Plastic Consumer Units with metal door",0]
["NDD","Metal flat enclosures",0]
["NDE","Distribution blocks",0]
["NDF","Plastic Consumer Units for hollow-walls mounting",0]
["NDG","GRP distribution board",0]
["NDH","Metal enclosure IP66",{"$f":"ND","v":0}]
[]
["NE","Fuse systems",0]
["NEA","Fuse disconnectors",{"$f":"NE","v":0}]
["NEB","Cylindrical Fuse Holder",{"$f":"NE","v":0}]
[]
["NF","Pre-wired boards",0]
["NFB","DC boards for PV applications",{"$f":"NF","v":0}]
[]
["NG","Photovoltaic devices",0]
["NGC","Smart monitoring devices",{"$f":"NG","v":0}]
["NGD","EV chargers",{"$f":"NG","v":0}]

{"sheet":"Order","index":3,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Order No."]
["Supplier:"]
["NOARK Electric Europe s.r.o.",null,null,"ID: 24123846",null,"VAT number: CZ 24123846"]
["Sezemická 2757/2",null,null,"Account: 51-0016810227/0100",null,"Bank: 0100"]
["193 00 Praha 9",null,null,"\"Contact person\"",null,"Tel.:"]
["Czech Republic",null,null,"E-mail:"]
["Buyer:",null,null,"Customer ID:",null,"Date:"]
["NOARK Electric Europe s.r.o.",null,null,"ID: ",null,"VAT number: "]
["Sezemická 2757/2",null,null,"Account:  ",null,"Bank: "]
["193 00 Prague 9",null,null,"\"Contact person\"",null,"Tel.:"]
["Czech Republic",null,null,"E-mail:"]
[]
["Item No.","Article No.","Type","Description","Discount group","Price with discount (EUR)","pieces","Total price (EUR)"]
[null,null,null,null,null,null,null,0]
[]
[]
[]
[null,null,null,null,"Total order price:",null,null,{"$f":"SUM(H14:H14)","v":0}]
[]
["All prices are given without VAT. All price agreements, scope of delivery as well as way of delivery are defined"]
["In General Business Terms or alternatively by Frame Contract and its appendixes."]

{"sheet":"Offer","index":4,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["Offer Nr."]
["Supplier:"]
["NOARK Electric Europe s.r.o.",null,null,"ID: 24123846",null,"VAT number: CZ 24123846"]
["Sezemická 2757/2",null,null,"Account: 51-0016810227/0100",null,"Bank: 0100"]
["193 00 Prague 9",null,null,"\"Contact person\"",null,"Tel.:"]
["Czech Republic",null,null,"E-mail:"]
["Buyer:",null,null,"Customer ID:",null,"Date:"]
["NOARK Electric Europe s.r.o.",null,null,"ID: ",null,"VAT number: "]
["Sezemická 2757/2",null,null,"Account:  ",null,"Bank: "]
["193 00 Praha 9",null,null,"\"Contact person\"",null,"Tel.:"]
["Czech Republic",null,null,"E-mail:"]
[]
["Item No.","Article No.","Type","Description","Discount group","Price with discount (EUR)","Number of pieces","Total price (EUR)"]
[null,null,null,null,null,null,null,0]
[]
[]
[]
[null,null,null,null,"Total offer price:",null,null,{"$f":"SUM(H14:H14)","v":0}]
[]
["All prices are given without VAT. All price agreements, scope of delivery as well as way of delivery are defined"]
["In General Business Terms or alternatively by Frame Contract and its appendixes."]
["The price is valid when all the goods and quantity demanded at once."]
["If demand changes, price also changes depending on products and quantities."]

{"sheet":"Terms and Conditions","index":5,"n_rows":56,"n_cols":2,"rows_kept":56,"cut":false,"hidden":false,"merged":[]}
[]
[null,"_____________________________________________________________________"]
[null,"GENERAL COMMERCIAL TERMS AND CONDITIONS"]
[null,"_____________________________________________________________________"]
[]
[]
[]
[null,"I.           Introductory Provisions"]
[null,"1.1        These General Commercial Terms and Conditions (“GCTC”) of NOARK Electric Europe s.r.o., having its registered office in Prague 9, Horní Počernice, Sezemická 2757/2, postcode: 193 00, registered in the Commercial Register kept by the Municipal Court in Prague, Section C, file No. 181277 (the “Seller”), define the mutual rights and obligations of the Seller and the person (the “Buyer”), who is interested in purchasing the goods offered by the Seller (the “Goods”) in the current price list of the Goods (the “Price List”). "]
[null,"1.2        Where no general agreement (the “General Agreement”) specifying different arrangements under the particular points has been concluded between the Seller and the Buyer (jointly referred to as the “Parties or each individually as the “Party”), these GCTC and the Purchase Contract (as defined below) shall constitute the entire and final agreement between the Parties on the terms and conditions for the delivery and acceptance of the Goods. Any matters not covered herein shall be governed by the relevant provisions of Act No. 89/2012 Coll., the Civil Code, as amended (the “Civil Code”)."]
[null,"II.         Purchase Order for the Goods"]
[null,"2.1        The Buyer was made acquainted by the Seller with the contents of these GCTC and, on the basis of these GCTC and other information provided by the Seller, the Buyer has expressed, by means of a purchase order (the “Purchase Order”) its wish to purchase the Goods from the Seller for the price as indicated in the Price List or as otherwise agreed (the “Purchase Price”)."]
[null,"2.2        A Purchase Order shall always include: (a) identification data of the person authorized to represent  the Buyer, (b) description (code) of the ordered Goods pursuant to the Price List and their quantity, and (c) method of delivery of the Goods and where applicable, other particulars which the Parties have agreed on. The completed Purchase Order shall be delivered by the Buyer to the Seller in person, sent by postal service to the Seller’s registered office address or to the address indicated in the General Agreement, or shall deliver the Purchase Order to the Seller by e-mail or deliver it to the Seller in another manner agreed by the Parties. The Purchase Order shall be deemed to constitute a proposal to sign an individual purchase contract and, consequently, shall become binding upon its delivery to the Seller. By sending the Purchase Order, the Buyer gives its explicit consent with the purchase contract (and any and all obligations arising therefrom) being governed by the GCTC. The Seller shall be obliged to mark the date of this receipt on the delivered Purchase Order. The purchase contract shall be concluded upon the signing of the delivered Purchase Order by the Seller (the “Purchase Contract”)."]
[null,"III.       Purchase Price, Invoicing, Payment Terms and Conditions "]
[null,"3.1        For the Goods delivered, the Buyer shall be obliged to pay to the Seller the purchase price determined pursuant to the valid Price List or otherwise agreed by the Parties plus VAT. In order to rule out all doubts, it is agreed that purchase prices are stipulated in the Price List exclusive of VAT. "]
[null,"3.2        The Seller shall be entitled to make changes to the Price List at any time and on a unilateral basis; however, any change or modification to the Price List shall not apply to any Goods ordered based on the Purchase Orders that were delivered to the Seller prior to the date of such change or modification. An updated Price List indicating the effective date shall be published on the Seller’s website or sent to the Buyer by means of an e-mail message."]
[null,"3.3        Unless agreed otherwise between the Seller and the Buyer, the Purchase Price shall not include the costs of packaging, transport, handling, installation and commissioning of the Goods, or the packaging disposal and recycling costs (“Other Costs”). The amount of Other Costs shall be indicated in the Price List and added to the Purchase Price."]
[null,"3.4        The Purchase Price shall be due and payable within seven (7) days after the issue date of the respective tax document (pro forma invoice), which must meet the particulars required by Act No. 235/2004 Coll., on Value Added Tax, as amended. The respective amount shall be paid by the Buyer by bank transfer to the Seller’s account as indicated in the relevant invoice or otherwise notified to the Buyer. The Purchase Price shall be deemed to have been paid on the date when the full amount is credited to the respective account of the Seller."]
[null,"3.5        If the Buyer is in delay with the payment of any invoice, the Seller shall be entitled to claim a contractual fine amounting to 0.05% of the amount due for each and every day of delay."]
[null,"IV.        Delivery of the Goods"]
[null,"4.1        The Goods may only be delivered once the Purchase Price has been paid in full. The delivery period shall be thirty (30) days from the payment of the Purchase Price unless the Seller determines otherwise. The Seller shall be entitled to suspend the delivery period for the Goods for the duration of the delay by the Buyer with the payment of any amount due arising from the General Agreement or the Purchase Contract.  The Seller shall assume no responsibility for such delay."]
[null,"4.2        The Seller shall be obliged to deliver the Goods to the Buyer by sending them to the Buyer’s address as indicated in the Purchase Contract or, as the case may be, to another address notified to the Seller in writing (the “Shipment”). The Seller’s obligation shall be deemed to have been duly performed and the Goods to have been delivered to the Buyer upon the moment when the Shipment is handed over for transport to the first carrier. The Shipment shall always be clearly and sufficiently marked as a shipment intended for the Buyer; the delivery of the Goods shall thus be effective upon the handover of the Shipment to the first carrier for transportation. In consistence with the Civil Code, the risk of damage to the Goods shall be transferred to the Buyer upon the handover of the Shipment to the first carrier for transport to the place of delivery."]
[null,"4.3        Unless otherwise set out in these GCTC or otherwise agreed between the Seller and the Buyer, the Goods shall be delivered under the CIP term in accordance with INCOTERMS 2010. The place of shipment and place of destination shall be agreed upon in the particular case between the Seller and the Buyer. "]
[null,"V.          Acquisition of the Title to the Goods"]
[null,"5.1        The Buyer shall acquire the title to the Goods upon their handover to the Buyer, provided that the Purchase Price has been paid in full by the Buyer."]
[null,"VI.        Warranty"]
[null,"6.1        The Seller shall provide a quality warranty for the Goods to the Buyer; the warranty period shall be five (5) years after the date of acceptance of the Goods by the Buyer (the “Warranty Period”). With the quality warranty, the Seller undertakes that the Goods purchased by the Buyer shall be fit for the agreed purpose of use throughout the specified Warranty Period."]
[null,"6.2        The Warranty shall particularly not apply to defects caused by or arising from:"]
[null,"(a)   Improper storage of the Goods prior to their installation and commissioning; "]
[null,"(b)   Inappropriate, incorrectly designed or wrongly performed installation of the Goods, or improper use of the Goods;"]
[null,"(c)   Wear and tear related to the natural life cycle of the Goods and their regular use (e.g. the varistor of surge voltage protectors);"]
[null,"(d)   Excessive use of the Goods, i.e. their use contrary to the recommendations or instructions by the Seller (e.g. by exceeding the number of the declared operating cycles);"]
[null,"(e)   Any change or modification to the Goods that was carried out by the Buyer or any third person, except for persons designated or approved by the Seller;"]
[null,"(f)    External factors outside of the control of the Seller;"]
[null,"(g)   Force majeure, covering particularly flooding, fire, lightning, earthquake, strikes or civil riots. "]
[null,"6.3        Exclusions from the Warranty are specified in detail in the claims handling rules, which are available at the Seller’s website (the “Claims Handling Rules”)."]
[null,"In case of discrepancies between the provisions of the Claim Handling Rule and these GCTC the GCTC shall prevail."]
[]
[null,"6.4         Any returning of the Goods by the Purchaser to the Seller is subject to the Seller’s consent. The Goods may be returned only if the Goods is complete and not damaged including packaging no later than two (2) years from their delivery. The price for which the Seller buys such Goods shall be determined by the Purchaser on the basis of a check performed by the Seller. All costs associated with the back sale (postage, packaging fee etc.) to the Seller shall be borne by the Purchaser. At the Seller’s request the Purchaser shall pay the Seller a service charge in order to cover other additional costs incurred by the Seller in connection with the returning of the."]
[]
[null,"VII.      Claims and European Warranty"]
[null,"7.1        The Buyer shall be entitled to exercise rights arising from defective performance in connection with any defects of the Goods occurring during the Warranty Period (the “Claim”) at any branch office of the Seller indicated in the list, which was submitted to the Buyer upon the purchase of the Goods and which is available at the Seller’s website (the “List”). Under the terms and conditions defined in the Claims Handling Rules, the Buyer shall be entitled to file the Claim also outside of the territory of the country, in which the Goods were purchased."]
[null,"7.2        The Buyer shall exercise the rights arising from defective performance concerning the delivered amount of the Goods no later than fourteen (14) days from the delivery of the Goods."]
[null,"7.3        Upon its acceptance the Buyer shall inspect the Goods to the possible extent and report defects (if any) by means of the transporter’s protocol. The rights arising from defective performance concerning defects the Purchaser could have discovered during the acceptance of the Goods shall cease to exist upon the acceptance of the Goods in which case the Claim will not be accepted. However, the Seller shall be authorised but no obligated to accept the Claim even in such an event."]
[null,"7.4        The Buyer hereby acknowledges that the exclusions from the Warranty, the terms and conditions for filing the Claim, and the circumstances under which a Claim will not be accepted as justified shall be governed by the Claims Handling Rules, the contents of which were made known to the Buyer prior to concluding the Purchase Contract."]
[null,"VIII.    Personal Data Processing"]
[null,"8.1        Any personal data of the Buyer in terms of Section 4 (a) of Act No. 101/2000 Coll., on Personal Data Protection, as amended (the “PDP Act”), which were provided by the Buyer to the Seller in connection with the conclusion and performance of the General Agreement or the Purchase Contract or which were obtained by the Seller in other legitimate ways or, as appropriate, created by the processing of such obtained data (the “Personal Data”), shall be processed by the Seller or by a processer authorized by the Seller for the purposes of using such Personal Data in relation to the Seller’s sphere of business, i.e. for activities directly or indirectly related to the Seller’s commercial activities, including commercial offers and customer care, in automated manner (using computer technology) as well as manually. The Personal Data shall be processed by the Seller throughout the duration of the contractual relationship established by the General Agreement or the Purchase Contract as well as for the period of time required by generally binding legal regulations. The Buyer declares to be aware of the scope, method, purpose and duration of Personal Data processing as defined in the General Agreement, the Purchase Contract and these GCTC and, by signing the General Agreement or the Purchase Contract, the Buyer gives an explicit consent to the Seller with such Personal Data processing. In addition, the Buyer agrees that the Personal Data can be processed and transmitted by the Seller and any other administrator, to be understood as also among them or by third parties (including to a third country), in order to duly perform the General Agreement or the Purchase Contract, improve customer care in relation to the Buyer, perform marketing activities or inform other administrators about the Buyer’s solvency and trustworthiness."]
[null,"IX.        Sending of Commercial Communications"]
[null,"9.1        The Buyer hereby acknowledges that commercial communications in terms of Section 2 (f) of Act No. 480/2004 Coll., on Certain Information Society Services, as amended, can be send by the Seller using electronic means to the addresses provided by the Buyer to the Seller in connection with the General Agreement or the Purchase Contract and, by signing the General Agreement or the Purchase Contract, the Buyer gives an explicit consent to the Seller to do so."]
[null,"X.          Notices"]
[null,"10.1      Unless specified otherwise, any and all notices, messages or other communications between the Parties must be made in writing. The Parties shall be obliged to deliver written documents to each other to the addresses indicated in the General Agreement or the Purchase Contract or otherwise notified by the Parties: (a) by personal delivery with receipt confirmation; (b) by registered letter; (c) by a courier service with receipt confirmation; or (d) by e-mail. Any acts affecting the commencement, modification or termination of the General Agreement or the Purchase Contract must be delivered strictly in writing to the address of the registered office or the address indicated in the General Agreement. Any notice shall be deemed duly delivered to the respective Party upon its reaching the addressee’s disposition sphere. Notices shall be deemed to have been delivered under Section 570 of the Civil Code also if the Party that is the addressee intentionally frustrates their delivery. Notices sent with the use of a postal services provider shall be deemed to have been delivered on the third (or the 15th in case of notices sent abroad) business day following their dispatching."]
[null,"10.2      The Parties undertake to notify each other in writing and without delay on any changes in any data indicated in the General Agreement or the Purchase Contract. In the event that either of the Parties violates this obligation, any correspondence sent to the last known address of such Party shall be deemed to have been delivered although the recipient is no longer staying at that address and, consequently, has not had the opportunity to make itself acquainted with the contents of the shipment."]
[null,"XI.        Final Provisions"]
[null,"11.1      The General Agreement and the Purchase Contract (including the relationships arising therefrom) shall be governed by the laws of the Czech Republic.  "]
[null,"11.2      The Parties undertake to settle any and all mutual disputes related to the General Agreement or the Purchase Contract in an amicable way. In the event that an amicable settlement cannot be reached within thirty (30) days after the date when either of the Parties informed the other Party in writing about the rise of a dispute and requested an amicable settlement thereof, such dispute or controversy shall be finally settled by three (3) arbitrators of the Arbitration Court attached to the Economic Chamber of the Czech Republic and the Agricultural Chamber of the Czech Republic, having its seat in Prague (the “Arbitration Court”), in accordance with the Rules of the Arbitration Court. The place of venue of the arbitration shall be Prague. The arbitration proceedings shall be held in Czech language. Each Party shall appoint one (1) arbitrator. Within thirty (30) days after their appointment, the two (2) arbitrators appointed by the Parties shall appoint a third arbitrator to act as the chairman of the arbitration panel. If either of the Parties fails to appoint an arbitrator within the period of thirty (30) days after the receipt of the request of the other Party to appoint an arbitrator, or if the already appointed arbitrators fail to appoint a third arbitrator within the period of thirty (30) days after the appointment of the second arbitrator, the respective arbitrator(s) shall be appointed by the Chairman of the Arbitration Court. The arbitration award shall be binding for the Parties. The Parties undertake to comply with the obligations arising from the arbitration award. This arbitration clause shall be enforceable separately. In the event that certain disputes are excluded from the jurisdiction of the Arbitration Court pursuant to the applicable legal regulations of the Czech Republic, they shall be settled before the competent court."]
[null,"11.3      These GCTC shall be valid and effective as of 1 January 2015."]

{"sheet":"Claims Handling Rules","index":6,"n_rows":46,"n_cols":2,"rows_kept":46,"cut":false,"hidden":false,"merged":[]}
[null,"______________________________________________________"]
[null,"CLAIMS HANDLING RULES"]
[null,"______________________________________________________"]
[]
[]
[null,"I.           OPENING PROVISIONS"]
[null,"1.1        The present Claims Handling Rules (the “Claims Handling Rules”) of NOARK Electric Europe s.r.o., with its registered ofice at Prague 9, Horní Počernice, Sezemická 2757/2, Postcode: 193 00, registered in the commercial register maintained by the Municipal Court in Prague, Section C, file 181277 (the “Seller”) determine the mutual rights and responsibilities resulting from rights arising from defective performance concerning goods supply to the market by Seller (the “Goods”) and the person who has purchased such Goods for the purpose of its use (the “Buyer”). Unless specified otherwise herein, terms with capitalized first letters shall have the meaning specified in the Seller's General Terms and Conditions (the “GTC”), which are available at the Seller’s website."]
[]
[null,"II.         WARRANTY"]
[null,"2.1        The Seller provides the Buyer with a warranty covering the quality of the Goods, lasting for five (5) years following the day of the Goods receipt by the Buyer (the \"Warranty Period”). With this quality warranty, the Seller undertakes that during the Warranty Period, the Goods purchased by the Buyer shall be fit for use for the agreed purpose. "]
[null,"2.2        The warranty does not apply to defects caused or suffered especially as result of:"]
[null,"(a)   improper storage of the Goods prior to installation and commissioning, i.e. by storing them in an area and under conditions that are in conflict with the relevant product standard and the Declaration of Conformity (unless stipulated otherwise by the Seller in writing), conditions specified in the GTC, User Manual, instructions for use, catalogue or another document issued or indicated by the Seller for these purposes;"]
[null,"(b)   improper, wrongly designed or wrongly conducted the Goods installation, which means especially installation carried out in conflict with the conditions and requirements specified in either of the documents specified under point a) above;"]
[null,"(c)   incorrect use of the Goods, meaning especially using the Goods in conflict with either of the documents specified under point a) above;"]
[null,"(d)   using the Goods for purpose other than defined in either of the documents specified under point a) above;"]
[null,"(e)   wear and tear related to the natural life cycle of the Goods and their regular use (e.g. the varistor of surge voltage protectors);"]
[null,"(f)    excessive use of the Goods i.e. use in conflict with the Seller’s recommendation or instructions (e.g. by exceeding the number of declared operating cycles);"]
[null,"(g)   using the Goods in conflict with any operating or installation condition specified in a product standard or any other document specified under point a) above;"]
[null,"(h)   using the Goods in an environment or area under the influence of external impacts and/or if such environment or area does not correspond to the conditions stipulated or recommended by the Seller;"]
[null,"(i)    incorrect maintenance of the Goods, meaning especially maintenance carried out in conflict with any of the documents specified under point a) above;"]
[null,"(j)    connecting the Goods to any other goods or any other product or equipment in a manner other than recommended or stipulated by the Seller in either of the documents specified under point a) above;"]
[null,"(k)   any changes or modifications of the Goods, carried out by the Buyer or any third person except persons determined or approved by the Seller;"]
[null,"(l)    external impacts beyond the Seller’s control, meaning especially the effect of solar or other radiation, electromagnetic field, penetration of liquids, dust, pollen or any other object, overvoltage in the power system, line voltage fluctuations, overvoltage or short-circuit on inputs or outputs, voltage generated by electrostatic discharge (incl. lightning), incorrect feed or input voltage, unsuited voltage polarity or impact of chemical processes; and"]
[null,"(m) acts of Force Majeure, including but not limited to inundation, flood, fire, lightning, earthquake, strike or civil riots."]
[null,"2.3        If the Goods have no defect but do not fulfil the functions foreseen or expected by the Buyer, or if the Goods cannot fulfil such functions because their installation has been designed or carried out in a way even objectively preventing the Goods from fulfilling these functions, such situation is not deemed a conflict with the Purchase Agreement and no warranty claim shall be accepted. Furthermore, no discrepancy in size, colour or shape of the Goods compared to its representation specified in a catalogue or another document of the Seller shall be considered a defect."]
[]
[null,"III.       CLAIMS AND EUROPEAN WARRANTY"]
[null,"3.1        The Buyer is entitled to raise a claim covered by its rights arising from defective performance concerning the Goods that occurred in the course of the Warranty Period (the “Claim”) at either branch store included in the list provided to the Buyer at the moment of purchase of Goods or available at Seller's website (the “List”)."]
[null,"3.2        Under the terms of these Claim Handling Rules the Buyer is entitled to raise the Claim also outside the territory of the country, where the Goods have been purchased, provided that such other country (business premises) is included in the List."]
[null,"3.3        The following conditions shall be met in order to assert the Claim:"]
[null,"(a)   identification of a person that has purchased the Goods and raises the Claim;"]
[null,"(b)   identification of the Goods which are subject of the Claim (type, code and other identification details of the Goods);"]
[null,"(c)   presenting the original certificate of purchase of the Goods; "]
[null,"(d)   completing a claim protocol in the language of the relevant country, where the Claim is being raised;"]
[null,"(e)   a detailed description of the defect in the Goods and how the defect becomes evident;"]
[null,"(f)    a detailed description of the technique of commissioning and use of Goods;"]
[null,"(g)   preferred method of handling the Claim; and"]
[null,"(h)   raising the Claim exclusively in an authorized service workshop specified in the List."]
[null,"3.4        The Claim shall be handled without undue delay in the following manners:"]
[null,"(a)    if the defect is reparable, the Buyer is entitled to require (i) remedy of defect by the Goods repair, (ii) delivery of the missing Goods; or (iii) an adequate Purchase Price discount; and"]
[null,"(b)   if the defect is irreparable, the Buyer is entitled to require (i) replacement of the Goods; (ii) Purchase Price discount; or the Buyer can withdraw from the Purchase Agreement."]
[null,"3.5       The Buyer acknowledges and agrees that if a Claim is raised (i) in a country other than the country where the Goods have been originally purchased; or at (ii) any  party other than the party from which the Goods have been originally purchased (e.g. if the Buyer has purchased the Goods from a third party and raises a Claim directly towards the Seller), shall be, differently from the Article 3.4 of these Claims Handling Rules, handled exclusively by a repair or replacement of the Goods. For avoidance of any doubt about the meaning of this arrangement, it is expressly stated that in cases according to the first sentence of this Article, the Claim cannot be settled by granting a discount and it is impossible to withdraw from the purchase agreement on the basis of which the Goods were purchased. "]
[null,"3.6     The Buyer is entitled to choose the method of remedying the defect of the Goods. This entitlement is limited in the case of Claims under the Article 3.5 of these Claim Handling Rules."]
[]
[null,"IV.        VALIDITY OF CLAIMS HANDLING RULES"]
[null,"4.1        These Claims Handling Rules enter into force as of 1 January 2015."]

{"sheet":"Manual","index":7,"n_rows":18,"n_cols":2,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
[null,"______________________________________________________"]
[null,"MANUAL"]
[null,"______________________________________________________"]
[]
[]
[null,"1. Select list \"Discount groups\" and define discount conditions. You can set it either for basic groups or for detailed groups."]
[null,"2. Discount conditions must be set before you create an order or offer. Consecutive changes are not included in existing order or offer."]
[null,"3. To add an item into an Order select any cell in a row with appropriate product and click on \"Add to order\" button."]
[null,"4. To add an item into an Offer select any cell in a row with appropriate product and click on \"Add to offer\" button."]
[null,"5. After clicking on a button according to 3. or 4. a window will appear. Write down a number of requested pieces and press Enter."]
[null,"6. You can select more products by using Shift or Alt button. Number of pieces windows will be shown step by step."]
[null,"7. Fill in contact details in a header on \"Order\" or \"Offer\" list"]
[null,"8. In case you want to delete any row in an offer or order, select any cell in given row and press \"Delete row\" button."]
[null,"9. You can delete whole list of products from an offer or order by clicking \"Delete all\" button"]
[null,"10. You can save your order or offer as a standatrd Excel procedure."]
[null,"11. You can export your offer or order to pdf file by clicking \"Save as PDF\" button."]
[null,"12. For printing of an offer or order, please use standard Excel printing tools. "]